14:46:29.547104 BSC_Tests.ttcn:1592 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-io_uring/ttcn3-tcpdump-start.sh BSC_Tests.TC_chan_act_nack'.
14:46:30.558828 BSC_Tests.ttcn:1592 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-io_uring/ttcn3-tcpdump-start.sh BSC_Tests.TC_chan_act_nack' was executed successfully (exit status: 0).
14:46:30.559116 BSC_Tests.ttcn:1592 Test case TC_chan_act_nack started.
14:46:30.559233 BSC_Tests.ttcn:1592 Initializing variables, timers and ports of component type BSC_Tests.test_CT inside testcase TC_chan_act_nack.
14:46:30.559513 BSC_Tests.ttcn:1592 Port IPA_CTRL was started.
14:46:30.559606 BSC_Tests.ttcn:1592 Port RSL_CCHAN[0] was started.
14:46:30.559690 BSC_Tests.ttcn:1592 Port RSL_CCHAN[1] was started.
14:46:30.559769 BSC_Tests.ttcn:1592 Port RSL_CCHAN[2] was started.
14:46:30.559867 BSC_Tests.ttcn:1592 Port IPA_RSL[0][0] was started.
14:46:30.559972 BSC_Tests.ttcn:1592 Port IPA_RSL[0][1] was started.
14:46:30.560051 BSC_Tests.ttcn:1592 Port IPA_RSL[0][2] was started.
14:46:30.560223 BSC_Tests.ttcn:1592 Port IPA_RSL[0][3] was started.
14:46:30.560307 BSC_Tests.ttcn:1592 Port IPA_RSL[1][0] was started.
14:46:30.560387 BSC_Tests.ttcn:1592 Port IPA_RSL[1][1] was started.
14:46:30.560463 BSC_Tests.ttcn:1592 Port IPA_RSL[1][2] was started.
14:46:30.560540 BSC_Tests.ttcn:1592 Port IPA_RSL[1][3] was started.
14:46:30.560619 BSC_Tests.ttcn:1592 Port IPA_RSL[2][0] was started.
14:46:30.560696 BSC_Tests.ttcn:1592 Port IPA_RSL[2][1] was started.
14:46:30.560776 BSC_Tests.ttcn:1592 Port IPA_RSL[2][2] was started.
14:46:30.560854 BSC_Tests.ttcn:1592 Port IPA_RSL[2][3] was started.
14:46:30.560932 BSC_Tests.ttcn:1592 Port IPA was started.
14:46:30.561009 BSC_Tests.ttcn:1592 Port SCCPLITE_IPA_CTRL was started.
14:46:30.561087 BSC_Tests.ttcn:1592 Port IPA_CFG_PORT[0][0] was started.
14:46:30.561165 BSC_Tests.ttcn:1592 Port IPA_CFG_PORT[0][1] was started.
14:46:30.561242 BSC_Tests.ttcn:1592 Port IPA_CFG_PORT[0][2] was started.
14:46:30.561320 BSC_Tests.ttcn:1592 Port IPA_CFG_PORT[0][3] was started.
14:46:30.561398 BSC_Tests.ttcn:1592 Port IPA_CFG_PORT[1][0] was started.
14:46:30.561476 BSC_Tests.ttcn:1592 Port IPA_CFG_PORT[1][1] was started.
14:46:30.561559 BSC_Tests.ttcn:1592 Port IPA_CFG_PORT[1][2] was started.
14:46:30.561636 BSC_Tests.ttcn:1592 Port IPA_CFG_PORT[1][3] was started.
14:46:30.561715 BSC_Tests.ttcn:1592 Port IPA_CFG_PORT[2][0] was started.
14:46:30.561794 BSC_Tests.ttcn:1592 Port IPA_CFG_PORT[2][1] was started.
14:46:30.561872 BSC_Tests.ttcn:1592 Port IPA_CFG_PORT[2][2] was started.
14:46:30.561950 BSC_Tests.ttcn:1592 Port IPA_CFG_PORT[2][3] was started.
14:46:30.562027 BSC_Tests.ttcn:1592 Port BSCVTY was started.
14:46:30.562103 BSC_Tests.ttcn:1592 Port STPVTY was started.
14:46:30.562179 BSC_Tests.ttcn:1592 Port SCCPLITE_IPA_CFG_PORT[0] was started.
14:46:30.562255 BSC_Tests.ttcn:1592 Port SCCPLITE_IPA_CFG_PORT[1] was started.
14:46:30.562333 BSC_Tests.ttcn:1592 Port SCCPLITE_IPA_CFG_PORT[2] was started.
14:46:30.562409 BSC_Tests.ttcn:1592 Port BSSAP was started.
14:46:30.562485 BSC_Tests.ttcn:1592 Port BSSAP_LE was started.
14:46:30.562561 BSC_Tests.ttcn:1592 Component type BSC_Tests.test_CT was initialized.
14:46:30.562656 BSC_Tests.ttcn:1265 Start timer T_guard: 30 s
14:46:30.562753 BSC_Tests.ttcn:1266 Altstep as_Tguard was activated as default, id 1
14:46:30.562848 BSC_Tests.ttcn:1097 Mapping port mtc:BSCVTY to system:BSCVTY.
14:46:30.563507 BSC_Tests.ttcn:1097 Message enqueued on BSCVTY from system integer : 2 id 1
14:46:30.563641 BSC_Tests.ttcn:1097 Port BSCVTY was mapped to system:BSCVTY.
14:46:30.563811 BSC_Tests.ttcn:1097 Map operation of mtc:BSCVTY to system:BSCVTY finished.
14:46:30.563960 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 1, prompt := "OsmoBSC> ", has_wildcards := false } }
14:46:30.564066 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 2, prompt := "OsmoBSC# ", has_wildcards := false } }
14:46:30.564190 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 3, prompt := "OsmoBSC(*)", has_wildcards := true } }
14:46:30.564381 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "enable"
14:46:30.564535 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.564648 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:46:30.564736 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:46:30.564820 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:46:30.564903 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:46:30.564986 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:46:30.565076 Osmocom_VTY_Functions.ttcn:86 Matching on port BSCVTY succeeded: 2 with ? matched
14:46:30.565168 Osmocom_VTY_Functions.ttcn:86 Receive operation on port BSCVTY succeeded, message from system(): integer : 2 id 1
14:46:30.565259 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of BSCVTY.
14:46:30.565496 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 2
14:46:30.565701 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.565869 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:30.565967 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
14:46:30.566057 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of BSCVTY.
14:46:30.566150 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.566258 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:46:30.566398 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.566712 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 3
14:46:30.566891 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.567049 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.567241 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.567344 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 3
14:46:30.567437 Osmocom_VTY_Functions.ttcn:74 Message with id 3 was extracted from the queue of BSCVTY.
14:46:30.567533 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.567633 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "cs7 instance 0"
14:46:30.567766 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.568179 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 4
14:46:30.568433 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.568560 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.568696 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.568765 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 4
14:46:30.568847 Osmocom_VTY_Functions.ttcn:74 Message with id 4 was extracted from the queue of BSCVTY.
14:46:30.568914 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.568993 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer ias 420"
14:46:30.569101 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.569243 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 5
14:46:30.569362 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.569456 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.569571 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.569632 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 5
14:46:30.569692 Osmocom_VTY_Functions.ttcn:74 Message with id 5 was extracted from the queue of BSCVTY.
14:46:30.569754 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.569814 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer iar 900"
14:46:30.569890 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.569994 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 6
14:46:30.570084 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.570171 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.570278 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.570339 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 6
14:46:30.570396 Osmocom_VTY_Functions.ttcn:74 Message with id 6 was extracted from the queue of BSCVTY.
14:46:30.570456 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.570513 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
14:46:30.570584 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.570665 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 7
14:46:30.570754 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.570847 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:30.570907 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 7
14:46:30.570964 Osmocom_VTY_Functions.ttcn:73 Message with id 7 was extracted from the queue of BSCVTY.
14:46:30.571023 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.571086 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:46:30.571156 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.571253 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 8
14:46:30.571344 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.571433 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.571537 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.571606 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 8
14:46:30.571663 Osmocom_VTY_Functions.ttcn:74 Message with id 8 was extracted from the queue of BSCVTY.
14:46:30.571724 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.571785 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
14:46:30.571855 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.571970 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 9
14:46:30.572059 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.572145 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.572246 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.572306 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 9
14:46:30.572363 Osmocom_VTY_Functions.ttcn:74 Message with id 9 was extracted from the queue of BSCVTY.
14:46:30.572422 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.572480 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
14:46:30.572549 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.572645 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 10
14:46:30.572730 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.572813 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.572913 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.572972 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 10
14:46:30.573028 Osmocom_VTY_Functions.ttcn:74 Message with id 10 was extracted from the queue of BSCVTY.
14:46:30.573086 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.573141 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:46:30.573209 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.573301 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 11
14:46:30.573385 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.573469 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.573569 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.573627 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 11
14:46:30.573684 Osmocom_VTY_Functions.ttcn:74 Message with id 11 was extracted from the queue of BSCVTY.
14:46:30.573742 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.573797 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:46:30.573864 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.573942 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 12
14:46:30.574028 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.574124 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:30.574183 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 12
14:46:30.574239 Osmocom_VTY_Functions.ttcn:73 Message with id 12 was extracted from the queue of BSCVTY.
14:46:30.574297 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.574359 StatsD_Checker.ttcnpp:416 Creating new PTC with component type StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
14:46:30.584965 StatsD_Checker.ttcnpp:416 PTC was created. Component reference: 315, alive: no, type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
14:46:30.585025 StatsD_Checker.ttcnpp:417 Starting function main("127.0.0.1", 8125, 5.000000) on component VirtMSC-STATS(315).
14:46:30.585277 StatsD_Checker.ttcnpp:417 Function was started.
14:46:30.585330 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0 bssmap reset"
14:46:30.585409 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.585523 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 13
14:46:30.585626 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.585715 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:30.585765 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 13
14:46:30.585814 Osmocom_VTY_Functions.ttcn:73 Message with id 13 was extracted from the queue of BSCVTY.
14:46:30.585864 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.585916 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1 bssmap reset"
14:46:30.585979 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.586075 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 14
14:46:30.586148 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.586222 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:30.586269 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 14
14:46:30.586310 Osmocom_VTY_Functions.ttcn:73 Message with id 14 was extracted from the queue of BSCVTY.
14:46:30.586353 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.586397 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2 bssmap reset"
14:46:30.586448 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.586989 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 15
14:46:30.587253 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.587363 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:30.587412 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 15
14:46:30.587460 Osmocom_VTY_Functions.ttcn:73 Message with id 15 was extracted from the queue of BSCVTY.
14:46:30.587508 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.587659 SCCP_Adapter.ttcnpp:114 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
14:46:30.596967 SCCP_Adapter.ttcnpp:114 PTC was created. Component reference: 316, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
14:46:30.597058 SCCP_Adapter.ttcnpp:123 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
14:46:30.604396 SCCP_Adapter.ttcnpp:123 PTC was created. Component reference: 317, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
14:46:30.604441 SCCP_Adapter.ttcnpp:124 Mapping port VirtMSC-M3UA(317):SCTP_PORT to system:sctp.
14:46:30.607767 SCCP_Adapter.ttcnpp:124 Map operation of VirtMSC-M3UA(317):SCTP_PORT to system:sctp finished.
14:46:30.607823 SCCP_Adapter.ttcnpp:126 Connecting ports VirtMSC-M3UA(317):MTP3_SP_PORT and VirtMSC-SCCP(316):MTP3_SCCP_PORT.
14:46:30.608990 SCCP_Adapter.ttcnpp:126 Connect operation on VirtMSC-M3UA(317):MTP3_SP_PORT and VirtMSC-SCCP(316):MTP3_SCCP_PORT finished.
14:46:30.609052 SCCP_Adapter.ttcnpp:127 Starting function f_M3UA_Emulation({ local_sctp_port := 23905, local_ip_addr := "127.0.0.1", remote_sctp_port := 2905, remote_ip_addr := "127.0.0.1" }, 1) on component VirtMSC-M3UA(317).
14:46:30.609260 SCCP_Adapter.ttcnpp:127 Function was started.
14:46:30.609321 BSC_Tests.ttcn:1223 Connecting ports mtc:BSSAP and VirtMSC-SCCP(316):SCCP_SP_PORT.
14:46:30.609915 BSC_Tests.ttcn:1223 Port BSSAP is waiting for connection from VirtMSC-SCCP(316):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-177eb81d.
14:46:30.610248 BSC_Tests.ttcn:1223 Port BSSAP has accepted the connection from VirtMSC-SCCP(316):SCCP_SP_PORT.
14:46:30.610362 BSC_Tests.ttcn:1223 Connect operation on mtc:BSSAP and VirtMSC-SCCP(316):SCCP_SP_PORT finished.
14:46:30.610420 SCCP_Adapter.ttcnpp:165 Starting function SCCPStart({ sio := { ni := '00'B, prio := '00'B, si := '0011'B }, opc := 185, dpc := 187, sls := 0, sccp_serviceType := "mtp3_itu", ssn := 254 }) on component VirtMSC-SCCP(316).
14:46:30.610649 SCCP_Adapter.ttcnpp:165 Function was started.
14:46:30.610898 BSC_Tests.ttcn:897 Sent on BSSAP to VirtMSC-SCCP(316) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := omit, returnOption := omit, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { reset := { messageType := '30'O ("0"), cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit }
14:46:30.610970 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { reset := { messageType := '30'O ("0"), cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }
14:46:30.611088 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000430040100'O
14:46:30.611165 BSC_Tests.ttcn:897 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := omit, returnOption := omit, userData := '000430040100'O, importance := omit }
14:46:30.611256 BSC_Tests.ttcn:899 Start timer T: 5 s
14:46:30.827201 BSC_Tests.ttcn:900 Message enqueued on BSSAP from VirtMSC-SCCP(316) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := '000430040120'O, importance := omit } id 1
14:46:30.827470 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000430040120'O
14:46:30.828426 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 4, pdu := { bssmap := { reset := { messageType := '30'O ("0"), cause := { elementIdentifier := '04'O, lengthIndicator := 1, causeValue := '0100000'B, extensionCauseValue := '0'B, spare1 := omit }, a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }
14:46:30.828751 BSC_Tests.ttcn:900 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 4, pdu := { bssmap := { reset := { messageType := '30'O ("0"), cause := { elementIdentifier := '04'O, lengthIndicator := 1, causeValue := '0100000'B, extensionCauseValue := '0'B, spare1 := omit }, a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit } id 1
14:46:30.829022 BSC_Tests.ttcn:901 Matching on port BSSAP .userData.pdu.bssmap{ reset := { messageType := '30'O ("0"), cause := { elementIdentifier := '04'O, lengthIndicator := 1, causeValue := '0100000'B, extensionCauseValue := '0'B, spare1 := omit }, a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } with { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := *, osmuxSupport := omit } } unmatched: First message in the queue does not match the template: 
14:46:30.829229 BSC_Tests.ttcn:905 Matching on port BSSAP succeeded:  matched
14:46:30.829369 BSC_Tests.ttcn:905 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(316): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 4, pdu := { bssmap := { reset := { messageType := '30'O ("0"), cause := { elementIdentifier := '04'O, lengthIndicator := 1, causeValue := '0100000'B, extensionCauseValue := '0'B, spare1 := omit }, a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit } id 1
14:46:30.829483 BSC_Tests.ttcn:905 Message with id 1 was extracted from the queue of BSSAP.
14:46:30.829593 BSC_Tests.ttcn:906 BSSMAP: Respoding to inbound RESET with RESET-ACK
14:46:30.829821 BSC_Tests.ttcn:907 Sent on BSSAP to VirtMSC-SCCP(316) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := omit, returnOption := omit, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit }
14:46:30.829960 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }
14:46:30.830155 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000131'O
14:46:30.830280 BSC_Tests.ttcn:907 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := omit, returnOption := omit, userData := '000131'O, importance := omit }
14:46:30.830585 BSC_Tests.ttcn:900 Message enqueued on BSSAP from VirtMSC-SCCP(316) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := '000131'O, importance := omit } id 2
14:46:30.830713 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000131'O
14:46:30.831137 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }
14:46:30.831373 BSC_Tests.ttcn:900 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit } id 2
14:46:30.831641 BSC_Tests.ttcn:901 Matching on port BSSAP succeeded:  matched
14:46:30.831791 BSC_Tests.ttcn:901 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(316): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit } id 2
14:46:30.831958 BSC_Tests.ttcn:901 Message with id 2 was extracted from the queue of BSSAP.
14:46:30.832088 BSC_Tests.ttcn:903 BSSMAP: Received RESET-ACK in response to RESET, we're ready to go!
14:46:30.832296 BSSAP_LE_Adapter.ttcn:95 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
14:46:30.840967 BSSAP_LE_Adapter.ttcn:95 PTC was created. Component reference: 318, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
14:46:30.841049 BSSAP_LE_Adapter.ttcn:101 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
14:46:30.846094 BSSAP_LE_Adapter.ttcn:101 PTC was created. Component reference: 319, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
14:46:30.846138 BSSAP_LE_Adapter.ttcn:102 Mapping port VirtSMLC-M3UA(319):SCTP_PORT to system:sctp.
14:46:30.847820 BSSAP_LE_Adapter.ttcn:102 Map operation of VirtSMLC-M3UA(319):SCTP_PORT to system:sctp finished.
14:46:30.847880 BSSAP_LE_Adapter.ttcn:104 Connecting ports VirtSMLC-M3UA(319):MTP3_SP_PORT and VirtSMLC-SCCP(318):MTP3_SCCP_PORT.
14:46:30.848363 BSSAP_LE_Adapter.ttcn:104 Connect operation on VirtSMLC-M3UA(319):MTP3_SP_PORT and VirtSMLC-SCCP(318):MTP3_SCCP_PORT finished.
14:46:30.848392 BSSAP_LE_Adapter.ttcn:105 Starting function f_M3UA_Emulation({ local_sctp_port := 23908, local_ip_addr := "127.0.0.1", remote_sctp_port := 2905, remote_ip_addr := "127.0.0.1" }, 6) on component VirtSMLC-M3UA(319).
14:46:30.848461 BSSAP_LE_Adapter.ttcn:105 Function was started.
14:46:30.848525 BSC_Tests.ttcn:1290 Connecting ports mtc:BSSAP_LE and VirtSMLC-SCCP(318):SCCP_SP_PORT.
14:46:30.849070 BSC_Tests.ttcn:1290 Port BSSAP_LE is waiting for connection from VirtSMLC-SCCP(318):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-5032e71d.
14:46:30.849228 BSC_Tests.ttcn:1290 Port BSSAP_LE has accepted the connection from VirtSMLC-SCCP(318):SCCP_SP_PORT.
14:46:30.849263 BSC_Tests.ttcn:1290 Connect operation on mtc:BSSAP_LE and VirtSMLC-SCCP(318):SCCP_SP_PORT finished.
14:46:30.849294 BSSAP_LE_Adapter.ttcn:122 Starting function SCCPStart({ sio := { ni := '00'B, prio := '00'B, si := '0011'B }, opc := 190, dpc := 187, sls := 0, sccp_serviceType := "mtp3_itu", ssn := 252 }) on component VirtSMLC-SCCP(318).
14:46:30.849359 BSSAP_LE_Adapter.ttcn:122 Function was started.
14:46:30.849393 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show running-config"
14:46:30.849446 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.852255 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" id 16
14:46:30.852316 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 17
14:46:30.853978 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.855222 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.856343 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
14:46:30.857480 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
14:46:30.858512 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with ? matched
14:46:30.859520 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" id 16
14:46:30.859544 Osmocom_VTY_Functions.ttcn:85 Message with id 16 was extracted from the queue of BSCVTY.
14:46:30.859567 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.859587 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:30.859600 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 17
14:46:30.859612 Osmocom_VTY_Functions.ttcn:73 Message with id 17 was extracted from the queue of BSCVTY.
14:46:30.859625 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.859643 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:46:30.859663 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.859717 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 18
14:46:30.859737 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.859755 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.859779 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.859792 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 18
14:46:30.859806 Osmocom_VTY_Functions.ttcn:74 Message with id 18 was extracted from the queue of BSCVTY.
14:46:30.859819 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.859832 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
14:46:30.859849 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.859875 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 19
14:46:30.859897 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.859916 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.859939 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.859953 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 19
14:46:30.859966 Osmocom_VTY_Functions.ttcn:74 Message with id 19 was extracted from the queue of BSCVTY.
14:46:30.859979 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.859993 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "allow-attach"
14:46:30.860009 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.860030 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 20
14:46:30.860050 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.860068 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.860090 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.860103 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 20
14:46:30.860116 Osmocom_VTY_Functions.ttcn:74 Message with id 20 was extracted from the queue of BSCVTY.
14:46:30.860129 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.860141 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:46:30.860157 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.860176 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 21
14:46:30.860194 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.860212 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.860233 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.860246 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 21
14:46:30.860259 Osmocom_VTY_Functions.ttcn:74 Message with id 21 was extracted from the queue of BSCVTY.
14:46:30.860272 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.860284 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:46:30.860299 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.860315 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 22
14:46:30.860333 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.860355 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:30.860367 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 22
14:46:30.860380 Osmocom_VTY_Functions.ttcn:73 Message with id 22 was extracted from the queue of BSCVTY.
14:46:30.860393 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.860408 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:46:30.860423 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.860443 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 23
14:46:30.860461 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.860479 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.860501 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.860514 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 23
14:46:30.860527 Osmocom_VTY_Functions.ttcn:74 Message with id 23 was extracted from the queue of BSCVTY.
14:46:30.860540 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.860553 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1"
14:46:30.860568 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.860587 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 24
14:46:30.860605 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.860623 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.860644 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.860657 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 24
14:46:30.860670 Osmocom_VTY_Functions.ttcn:74 Message with id 24 was extracted from the queue of BSCVTY.
14:46:30.860683 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.860696 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
14:46:30.860710 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.860730 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 25
14:46:30.860748 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.860765 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.860786 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.860799 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 25
14:46:30.860811 Osmocom_VTY_Functions.ttcn:74 Message with id 25 was extracted from the queue of BSCVTY.
14:46:30.860824 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.860836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:46:30.860851 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.860870 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 26
14:46:30.860889 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.860907 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.860927 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.860939 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 26
14:46:30.860952 Osmocom_VTY_Functions.ttcn:74 Message with id 26 was extracted from the queue of BSCVTY.
14:46:30.860965 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.860977 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:46:30.860991 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.861008 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 27
14:46:30.861026 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.861044 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:30.861057 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 27
14:46:30.861069 Osmocom_VTY_Functions.ttcn:73 Message with id 27 was extracted from the queue of BSCVTY.
14:46:30.861082 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.861096 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:46:30.861111 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.861130 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 28
14:46:30.861148 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.861165 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.861186 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.861200 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 28
14:46:30.861212 Osmocom_VTY_Functions.ttcn:74 Message with id 28 was extracted from the queue of BSCVTY.
14:46:30.861225 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.861238 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2"
14:46:30.861253 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.861273 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 29
14:46:30.861291 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.861308 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.861328 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.861341 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 29
14:46:30.861354 Osmocom_VTY_Functions.ttcn:74 Message with id 29 was extracted from the queue of BSCVTY.
14:46:30.861366 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.861379 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
14:46:30.861394 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.861414 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 30
14:46:30.861432 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.861450 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.861470 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.861483 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 30
14:46:30.861495 Osmocom_VTY_Functions.ttcn:74 Message with id 30 was extracted from the queue of BSCVTY.
14:46:30.861508 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.861520 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:46:30.861535 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.861554 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 31
14:46:30.861572 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.861589 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:30.861609 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:46:30.861622 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 31
14:46:30.861634 Osmocom_VTY_Functions.ttcn:74 Message with id 31 was extracted from the queue of BSCVTY.
14:46:30.861647 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.861659 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:46:30.861673 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:30.861690 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 32
14:46:30.861707 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:30.861725 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:30.861739 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 32
14:46:30.861751 Osmocom_VTY_Functions.ttcn:73 Message with id 32 was extracted from the queue of BSCVTY.
14:46:30.861764 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:30.861778 Osmocom_CTRL_Adapter.ttcn:69 Creating new PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
14:46:30.864094 Osmocom_CTRL_Adapter.ttcn:69 PTC was created. Component reference: 320, alive: no, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
14:46:30.864110 Osmocom_CTRL_Adapter.ttcn:71 Mapping port IPA-CTRL-CLI-IPA(320):IPA_PORT to system:IPA_CODEC_PT.
14:46:30.865076 Osmocom_CTRL_Adapter.ttcn:71 Map operation of IPA-CTRL-CLI-IPA(320):IPA_PORT to system:IPA_CODEC_PT finished.
14:46:30.865089 Osmocom_CTRL_Adapter.ttcn:72 Connecting ports IPA-CTRL-CLI-IPA(320):IPA_CTRL_PORT and mtc:IPA_CTRL.
14:46:30.865244 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL is waiting for connection from IPA-CTRL-CLI-IPA(320):IPA_CTRL_PORT on UNIX pathname /tmp/ttcn3-portconn-6435f21f.
14:46:30.865324 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL has accepted the connection from IPA-CTRL-CLI-IPA(320):IPA_CTRL_PORT.
14:46:30.865344 Osmocom_CTRL_Adapter.ttcn:72 Connect operation on IPA-CTRL-CLI-IPA(320):IPA_CTRL_PORT and mtc:IPA_CTRL finished.
14:46:30.865361 Osmocom_CTRL_Adapter.ttcn:74 Starting function main_client("127.0.0.1", 4249, "", 0, { ser_nr := "", name := "mahlzeit", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "0/1/2", osmo_rand := "" }, false) on component IPA-CTRL-CLI-IPA(320).
14:46:30.865389 Osmocom_CTRL_Adapter.ttcn:74 Function was started.
14:46:30.865402 Osmocom_CTRL_Adapter.ttcn:37 Start timer T: 10 s
14:46:30.866624 Osmocom_CTRL_Adapter.ttcn:38 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(320) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
14:46:30.866641 Osmocom_CTRL_Adapter.ttcn:39 Matching on port IPA_CTRL succeeded:  matched
14:46:30.866655 Osmocom_CTRL_Adapter.ttcn:39 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(320): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
14:46:30.866669 Osmocom_CTRL_Adapter.ttcn:39 Message with id 1 was extracted from the queue of IPA_CTRL.
14:46:30.866686 BSC_Tests.ttcn:1073 Creating new alive PTC with component type MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
14:46:30.869272 BSC_Tests.ttcn:1073 PTC was created. Component reference: 321, alive: yes, type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
14:46:30.869293 BSC_Tests.ttcn:1074 Starting function main({ create_cb := refers(MGCP_Emulation.ExpectedCreateCallback), unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback) }, { callagent_ip := "127.0.0.1", callagent_udp_port := -1, mgw_ip := "127.0.0.1", mgw_udp_port := 2427, multi_conn_mode := false }, "VirtMGW-MGCP-0") on component VirtMGW-MGCP-0(321).
14:46:30.869352 BSC_Tests.ttcn:1074 Function was started.
14:46:30.869373 BSC_Tests.ttcn:1016 Start timer T: 5 s
14:46:30.869393 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.829626.
14:46:30.869418 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(320) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "829625522", variable := "bts.0.oml-connection-state", val := omit } }
14:46:30.869435 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
14:46:30.871462 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(320) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "829625522", variable := "bts.0.oml-connection-state", val := "degraded" } } id 2
14:46:30.871479 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
14:46:30.871491 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(320): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "829625522", variable := "bts.0.oml-connection-state", val := "degraded" } } id 2
14:46:30.871508 Osmocom_CTRL_Functions.ttcn:41 Message with id 2 was extracted from the queue of IPA_CTRL.
14:46:30.871520 BSC_Tests.ttcn:1019 Stop timer T: 5 s
14:46:30.871530 BSC_Tests.ttcn:1022 Start timer T: 1 s
14:46:31.871639 BSC_Tests.ttcn:1023 Timeout T: 1 s
14:46:31.871949 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
14:46:31.884199 BSC_Tests.ttcn:951 PTC was created. Component reference: 322, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
14:46:31.884422 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: { site_id := 1234, bts_id := 0, trx_id := 0 }
14:46:31.884755 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1234/0/0"
14:46:31.884861 BSC_Tests.ttcn:960 Mapping port IPA-BTS0-TRX0-RSL-IPA(322):IPA_PORT to system:IPA_CODEC_PT.
14:46:31.887707 BSC_Tests.ttcn:960 Map operation of IPA-BTS0-TRX0-RSL-IPA(322):IPA_PORT to system:IPA_CODEC_PT finished.
14:46:31.887852 BSC_Tests.ttcn:961 Connecting ports IPA-BTS0-TRX0-RSL-IPA(322):CFG_PORT and mtc:IPA_CFG_PORT[0][0].
14:46:31.889076 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(322):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-68728b6e.
14:46:31.889668 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(322):CFG_PORT.
14:46:31.889932 BSC_Tests.ttcn:961 Connect operation on IPA-BTS0-TRX0-RSL-IPA(322):CFG_PORT and mtc:IPA_CFG_PORT[0][0] finished.
14:46:31.890127 BSC_Tests.ttcn:965 Connecting ports IPA-BTS0-TRX0-RSL-IPA(322):IPA_RSL_PORT and mtc:IPA_RSL[0][0].
14:46:31.891112 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(322):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-b68ab76.
14:46:31.891762 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(322):IPA_RSL_PORT.
14:46:31.891816 BSC_Tests.ttcn:965 Connect operation on IPA-BTS0-TRX0-RSL-IPA(322):IPA_RSL_PORT and mtc:IPA_RSL[0][0] finished.
14:46:31.891856 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 10000, { ser_nr := "", name := "Osmocom TTCN-3 BTS Simulator", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "1234/0/0", osmo_rand := "" }, true) on component IPA-BTS0-TRX0-RSL-IPA(322).
14:46:31.891986 BSC_Tests.ttcn:969 Function was started.
14:46:31.892057 BSC_Tests.ttcn:976 Start timer T: 10 s
14:46:31.896867 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
14:46:31.896921 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
14:46:31.896951 BSC_Tests.ttcn:981 Matching on port IPA_RSL[0][0] succeeded:  matched
14:46:31.896977 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
14:46:31.897002 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[0][0].
14:46:31.899510 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
14:46:31.899685 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] succeeded:  matched
14:46:31.899758 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
14:46:31.899820 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[0][0].
14:46:31.899900 BSC_Tests.ttcn:979 Stop timer T: 10 s
14:46:31.899988 BSC_Tests.ttcn:1016 Start timer T: 5 s
14:46:31.900059 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.363992.
14:46:31.900188 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(320) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "363991733", variable := "bts.0.oml-connection-state", val := omit } }
14:46:31.900318 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
14:46:31.904860 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_1 (1) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '5506198FB38000000000000000000000000000E504002B'O } } } } } } id 3
14:46:31.905513 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(320) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "363991733", variable := "bts.0.oml-connection-state", val := "connected" } } id 3
14:46:31.905811 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
14:46:31.905900 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(320): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "363991733", variable := "bts.0.oml-connection-state", val := "connected" } } id 3
14:46:31.905950 Osmocom_CTRL_Functions.ttcn:41 Message with id 3 was extracted from the queue of IPA_CTRL.
14:46:31.906030 BSC_Tests.ttcn:1019 Stop timer T: 5 s
14:46:31.906187 BSC_Tests.ttcn:1022 Start timer T: 1 s
14:46:31.908853 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2 (2) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '59061A00000000000000000000000000000000FFE50400'O } } } } } } id 4
14:46:31.909021 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2bis (10) } } } } } id 5
14:46:31.909517 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2ter (11) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '4906038E3200000000000000000000000008002B2B2B2B'O } } } } } } id 6
14:46:31.909870 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2quater (41) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O } } } } } } id 7
14:46:31.910319 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_3 (3) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '49061B000000F1100001C9031E174740E504000C132B2B'O } } } } } } id 8
14:46:31.910609 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_4 (4) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O } } } } } } id 9
14:46:31.910810 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_13 (40) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '0106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O } } } } } } id 10
14:46:31.911398 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } } } id 11
14:46:31.911641 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } } } id 12
14:46:31.911989 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } } } id 13
14:46:31.912293 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000000F110000197FF2B'O } } } } } } id 14
14:46:31.912859 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96), ies := { { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } } } id 15
14:46:32.906910 BSC_Tests.ttcn:1023 Timeout T: 1 s
14:46:32.907379 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:46:32.907824 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:32.908283 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 33
14:46:32.908849 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:32.909046 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:32.909434 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:46:32.909578 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 33
14:46:32.909662 Osmocom_VTY_Functions.ttcn:74 Message with id 33 was extracted from the queue of BSCVTY.
14:46:32.909937 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:32.910292 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
14:46:32.910582 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:32.911054 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 34
14:46:32.911331 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:32.911659 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:32.912003 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
14:46:32.912197 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 34
14:46:32.912350 Osmocom_VTY_Functions.ttcn:74 Message with id 34 was extracted from the queue of BSCVTY.
14:46:32.912477 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:32.912576 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
14:46:32.912684 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:32.913024 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 35
14:46:32.913168 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:32.913276 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:32.913409 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
14:46:32.913557 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 35
14:46:32.913628 Osmocom_VTY_Functions.ttcn:74 Message with id 35 was extracted from the queue of BSCVTY.
14:46:32.913703 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:32.913783 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
14:46:32.913879 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:32.914127 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 36
14:46:32.914267 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:32.914461 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:32.914622 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
14:46:32.914739 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 36
14:46:32.914829 Osmocom_VTY_Functions.ttcn:74 Message with id 36 was extracted from the queue of BSCVTY.
14:46:32.915000 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:32.915107 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
14:46:32.915231 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:32.915407 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 37
14:46:32.915716 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:32.915948 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:32.916073 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 37
14:46:32.916184 Osmocom_VTY_Functions.ttcn:73 Message with id 37 was extracted from the queue of BSCVTY.
14:46:32.916287 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:32.916390 Osmocom_VTY_Functions.ttcn:338 "TC_chan_act_nack() start"
14:46:32.916547 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "logp lglobal notice TTCN3 f_logp(): TC_chan_act_nack() start"
14:46:32.916847 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:32.917137 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 38
14:46:32.917305 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:32.917438 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:32.917512 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 38
14:46:32.917614 Osmocom_VTY_Functions.ttcn:73 Message with id 38 was extracted from the queue of BSCVTY.
14:46:32.917779 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:32.917881 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.640960.
14:46:32.917991 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(320) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "640959562", variable := "rate_ctr.abs.bts.0.chan_act:nack", val := omit } }
14:46:32.918119 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
14:46:32.922814 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(320) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "640959562", variable := "rate_ctr.abs.bts.0.chan_act:nack", val := "0" } } id 4
14:46:32.923246 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
14:46:32.923471 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(320): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "640959562", variable := "rate_ctr.abs.bts.0.chan_act:nack", val := "0" } } id 4
14:46:32.923579 Osmocom_CTRL_Functions.ttcn:41 Message with id 4 was extracted from the queue of IPA_CTRL.
14:46:32.923987 BSC_Tests.ttcn:1394 Sent on IPA_RSL[0][0] to IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := omit, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CHAN_RQD (19), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_RACH (17) }, tn := 0 } } }, { iei := RSL_IE_REQ_REFERENCE (19), body := { req_ref := { ra := '33'O ("3"), frame_nr := { t1_p := 0, t3 := 33, t2 := 7 } } } }, { iei := RSL_IE_ACCESS_DELAY (17), body := { access_delay := 0 } } } } }
14:46:32.924111 BSC_Tests.ttcn:1375 Start timer T: 2 s
14:46:32.924388 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_CCHAN (6) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_BCCH_INFO (17) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.924502 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.924681 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_1 (1) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '5506198FB38000000000000000000000000000E504002B'O } } } } } } id 3
14:46:32.924765 BSC_Tests.ttcn:1380 Message with id 3 was extracted from the queue of IPA_RSL[0][0].
14:46:32.924916 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_CCHAN (6) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_BCCH_INFO (17) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.925091 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.925334 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2 (2) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '59061A00000000000000000000000000000000FFE50400'O } } } } } } id 4
14:46:32.925484 BSC_Tests.ttcn:1380 Message with id 4 was extracted from the queue of IPA_RSL[0][0].
14:46:32.925565 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_CCHAN (6) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_BCCH_INFO (17) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.925769 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.925989 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2bis (10) } } } } } id 5
14:46:32.926111 BSC_Tests.ttcn:1380 Message with id 5 was extracted from the queue of IPA_RSL[0][0].
14:46:32.926273 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_CCHAN (6) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_BCCH_INFO (17) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.926432 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.926702 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2ter (11) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '4906038E3200000000000000000000000008002B2B2B2B'O } } } } } } id 6
14:46:32.926995 BSC_Tests.ttcn:1380 Message with id 6 was extracted from the queue of IPA_RSL[0][0].
14:46:32.927241 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_CCHAN (6) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_BCCH_INFO (17) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.927369 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.927499 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2quater (41) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O } } } } } } id 7
14:46:32.927610 BSC_Tests.ttcn:1380 Message with id 7 was extracted from the queue of IPA_RSL[0][0].
14:46:32.927769 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_CCHAN (6) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_BCCH_INFO (17) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.927854 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.928020 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_3 (3) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '49061B000000F1100001C9031E174740E504000C132B2B'O } } } } } } id 8
14:46:32.928163 BSC_Tests.ttcn:1380 Message with id 8 was extracted from the queue of IPA_RSL[0][0].
14:46:32.928285 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_CCHAN (6) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_BCCH_INFO (17) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.928478 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.928608 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_4 (4) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O } } } } } } id 9
14:46:32.928702 BSC_Tests.ttcn:1380 Message with id 9 was extracted from the queue of IPA_RSL[0][0].
14:46:32.928857 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_CCHAN (6) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_BCCH_INFO (17) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.928929 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.929006 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_13 (40) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '0106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O } } } } } } id 10
14:46:32.929096 BSC_Tests.ttcn:1380 Message with id 10 was extracted from the queue of IPA_RSL[0][0].
14:46:32.929173 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_SACCH_FILL (26) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.929263 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.929341 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } } } id 11
14:46:32.929440 BSC_Tests.ttcn:1380 Message with id 11 was extracted from the queue of IPA_RSL[0][0].
14:46:32.929624 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_SACCH_FILL (26) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.929801 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.929948 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } } } id 12
14:46:32.930125 BSC_Tests.ttcn:1380 Message with id 12 was extracted from the queue of IPA_RSL[0][0].
14:46:32.930477 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_SACCH_FILL (26) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.930684 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.930847 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } } } id 13
14:46:32.930955 BSC_Tests.ttcn:1380 Message with id 13 was extracted from the queue of IPA_RSL[0][0].
14:46:32.931035 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_SACCH_FILL (26) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.931103 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.931202 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000000F110000197FF2B'O } } } } } } id 14
14:46:32.931274 BSC_Tests.ttcn:1380 Message with id 14 was extracted from the queue of IPA_RSL[0][0].
14:46:32.931368 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
14:46:32.931476 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
14:46:32.931553 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96), ies := { { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } } } id 15
14:46:32.931615 BSC_Tests.ttcn:1380 Message with id 15 was extracted from the queue of IPA_RSL[0][0].
14:46:32.933897 BSC_Tests.ttcn:1376 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_DCHAN (4), transparent := false }, msg_type := RSL_MT_CHAN_ACTIV (33), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } }, { iei := RSL_IE_ACT_TYPE (3), body := { act_type := { reactivation := false, reserved := 0, a_bits := ACT_REL_TO_IMM_ASSIGN (0) } } }, { iei := RSL_IE_CHAN_MODE (6), body := { chan_mode := { len := 4, reserved := '000000'B, dtx_d := true, dtx_u := true, spd_ind := RSL_SPDI_SIGN (3), ch_rate_type := RSL_CHRT_SDCCH (1), u := { sign := RSL_CMOD_NO_RESOURCE (0) } } } }, { iei := RSL_IE_CHAN_IDENT (5), body := { chan_ident := { len := 6, ch_desc := { iei := '64'O ("d"), v := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 }, tsc := 2, h := false, arfcn := 871, maio_hsn := omit } }, ma := { iei := '72'O ("r"), v := { len := 0, ma := ''B } } } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 7 } } }, { iei := RSL_IE_TIMING_ADVANCE (24), body := { timing_adv := 0 } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 0, params := ''O } } } } } } id 16
14:46:32.934092 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] succeeded:  matched
14:46:32.934230 BSC_Tests.ttcn:1377 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(322): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_DCHAN (4), transparent := false }, msg_type := RSL_MT_CHAN_ACTIV (33), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } }, { iei := RSL_IE_ACT_TYPE (3), body := { act_type := { reactivation := false, reserved := 0, a_bits := ACT_REL_TO_IMM_ASSIGN (0) } } }, { iei := RSL_IE_CHAN_MODE (6), body := { chan_mode := { len := 4, reserved := '000000'B, dtx_d := true, dtx_u := true, spd_ind := RSL_SPDI_SIGN (3), ch_rate_type := RSL_CHRT_SDCCH (1), u := { sign := RSL_CMOD_NO_RESOURCE (0) } } } }, { iei := RSL_IE_CHAN_IDENT (5), body := { chan_ident := { len := 6, ch_desc := { iei := '64'O ("d"), v := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 }, tsc := 2, h := false, arfcn := 871, maio_hsn := omit } }, ma := { iei := '72'O ("r"), v := { len := 0, ma := ''B } } } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 7 } } }, { iei := RSL_IE_TIMING_ADVANCE (24), body := { timing_adv := 0 } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 0, params := ''O } } } } } } id 16
14:46:32.934333 BSC_Tests.ttcn:1377 Message with id 16 was extracted from the queue of IPA_RSL[0][0].
14:46:32.934523 BSC_Tests.ttcn:1378 Stop timer T: 2 s
14:46:32.934964 BSC_Tests.ttcn:1394 Sent on IPA_RSL[0][0] to IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := omit, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_DCHAN (4), transparent := false }, msg_type := RSL_MT_CHAN_ACTIV_NACK (35), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } }, { iei := RSL_IE_CAUSE (26), body := { cause := { len := 0, e := 0, cause := RSL_ERR_EQUIPMENT_FAIL (32), cause_ext := omit } } } } } }
14:46:32.935180 Osmocom_Types.ttcn:126 Start timer T: 0.5 s
14:46:32.938318 Osmocom_Types.ttcn:127 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(322) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_IMMEDIATE_ASSIGN_CMD (22), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_FULL_IMM_ASS_INFO (43), body := { full_imm_ass_info := { len := 23, payload := '4D063A033304270A3304270A3304270A3304270A0B2B2B'O } } } } } } id 17
14:46:33.435394 Osmocom_Types.ttcn:127 Timeout T: 0.5 s
14:46:33.435623 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.974699.
14:46:33.435743 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(320) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "974699066", variable := "rate_ctr.abs.bts.0.chan_act:nack", val := omit } }
14:46:33.435847 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
14:46:33.440121 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(320) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "974699066", variable := "rate_ctr.abs.bts.0.chan_act:nack", val := "1" } } id 5
14:46:33.440257 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
14:46:33.440333 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(320): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "974699066", variable := "rate_ctr.abs.bts.0.chan_act:nack", val := "1" } } id 5
14:46:33.440401 Osmocom_CTRL_Functions.ttcn:41 Message with id 5 was extracted from the queue of IPA_CTRL.
14:46:33.440526 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show talloc-context application full filter \\<struct.bsc_subscr\\>\\|\\<struct.gsm_subscriber_connection\\>"
14:46:33.440639 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:46:33.441985 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "full talloc report on 'osmo-bsc' (total 1467395 bytes in 1346 blocks)" id 39
14:46:33.442232 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 40
14:46:33.442468 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1467395 bytes in 1346 blocks)" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:33.442656 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1467395 bytes in 1346 blocks)" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:46:33.442836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1467395 bytes in 1346 blocks)" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
14:46:33.443004 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1467395 bytes in 1346 blocks)" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
14:46:33.443128 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "full talloc report on 'osmo-bsc' (total 1467395 bytes in 1346 blocks)" with ? matched
14:46:33.443228 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "full talloc report on 'osmo-bsc' (total 1467395 bytes in 1346 blocks)" id 39
14:46:33.443321 Osmocom_VTY_Functions.ttcn:85 Message with id 39 was extracted from the queue of BSCVTY.
14:46:33.443464 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:46:33.443614 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:46:33.443710 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 40
14:46:33.443796 Osmocom_VTY_Functions.ttcn:73 Message with id 40 was extracted from the queue of BSCVTY.
14:46:33.443981 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:46:33.444142 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct bsc_subscr" x 0, expecting 0
14:46:33.444254 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct gsm_subscriber_connection" x 0, expecting 0
14:46:33.444340 BSC_Tests.ttcn:888 Stopping all components.
14:46:33.448447 BSC_Tests.ttcn:888 Connection of port IPA_CTRL to IPA-CTRL-CLI-IPA(320):IPA_CTRL_PORT was closed unexpectedly by the peer.
14:46:33.448574 BSC_Tests.ttcn:888 Port IPA_CTRL was disconnected from IPA-CTRL-CLI-IPA(320):IPA_CTRL_PORT.
14:46:33.448970 BSC_Tests.ttcn:888 All components were stopped.
14:46:33.449035 BSC_Tests.ttcn:889 setverdict(pass): none -> pass
14:46:33.449103 BSC_Tests.ttcn:890 Stopping test component execution.
14:46:33.449219 BSC_Tests.ttcn:1611 Test case TC_chan_act_nack was stopped.
14:46:33.449274 BSC_Tests.ttcn:1611 Terminating component type BSC_Tests.test_CT.
14:46:33.449504 BSC_Tests.ttcn:1611 Default with id 1 (altstep as_Tguard) was deactivated.
14:46:33.449643 BSC_Tests.ttcn:1611 Stop timer T_guard: 30 s
14:46:33.449748 BSC_Tests.ttcn:1611 Port IPA_CTRL was stopped.
14:46:33.449840 BSC_Tests.ttcn:1611 Port RSL_CCHAN[0] was stopped.
14:46:33.449927 BSC_Tests.ttcn:1611 Port RSL_CCHAN[1] was stopped.
14:46:33.450009 BSC_Tests.ttcn:1611 Port RSL_CCHAN[2] was stopped.
14:46:33.450092 BSC_Tests.ttcn:1611 Removing unterminated connection between port IPA_RSL[0][0] and IPA-BTS0-TRX0-RSL-IPA(322):IPA_RSL_PORT.
14:46:33.450268 BSC_Tests.ttcn:1611 Message with id 17 was extracted from the queue of IPA_RSL[0][0].
14:46:33.450515 BSC_Tests.ttcn:1611 Port IPA_RSL[0][0] was stopped.
14:46:33.450937 BSC_Tests.ttcn:1611 Port IPA_RSL[0][1] was stopped.
14:46:33.451255 BSC_Tests.ttcn:1611 Port IPA_RSL[0][2] was stopped.
14:46:33.451545 BSC_Tests.ttcn:1611 Port IPA_RSL[0][3] was stopped.
14:46:33.451825 BSC_Tests.ttcn:1611 Port IPA_RSL[1][0] was stopped.
14:46:33.452114 BSC_Tests.ttcn:1611 Port IPA_RSL[1][1] was stopped.
14:46:33.452241 BSC_Tests.ttcn:1611 Port IPA_RSL[1][2] was stopped.
14:46:33.452341 BSC_Tests.ttcn:1611 Port IPA_RSL[1][3] was stopped.
14:46:33.452564 BSC_Tests.ttcn:1611 Port IPA_RSL[2][0] was stopped.
14:46:33.452683 BSC_Tests.ttcn:1611 Port IPA_RSL[2][1] was stopped.
14:46:33.452772 BSC_Tests.ttcn:1611 Port IPA_RSL[2][2] was stopped.
14:46:33.452853 BSC_Tests.ttcn:1611 Port IPA_RSL[2][3] was stopped.
14:46:33.452934 BSC_Tests.ttcn:1611 Port IPA was stopped.
14:46:33.453015 BSC_Tests.ttcn:1611 Port SCCPLITE_IPA_CTRL was stopped.
14:46:33.453101 BSC_Tests.ttcn:1611 Removing unterminated connection between port IPA_CFG_PORT[0][0] and IPA-BTS0-TRX0-RSL-IPA(322):CFG_PORT.
14:46:33.453268 BSC_Tests.ttcn:1611 Port IPA_CFG_PORT[0][0] was stopped.
14:46:33.453468 BSC_Tests.ttcn:1611 Port IPA_CFG_PORT[0][1] was stopped.
14:46:33.453557 BSC_Tests.ttcn:1611 Port IPA_CFG_PORT[0][2] was stopped.
14:46:33.453639 BSC_Tests.ttcn:1611 Port IPA_CFG_PORT[0][3] was stopped.
14:46:33.453718 BSC_Tests.ttcn:1611 Port IPA_CFG_PORT[1][0] was stopped.
14:46:33.453794 BSC_Tests.ttcn:1611 Port IPA_CFG_PORT[1][1] was stopped.
14:46:33.453865 BSC_Tests.ttcn:1611 Port IPA_CFG_PORT[1][2] was stopped.
14:46:33.453936 BSC_Tests.ttcn:1611 Port IPA_CFG_PORT[1][3] was stopped.
14:46:33.454006 BSC_Tests.ttcn:1611 Port IPA_CFG_PORT[2][0] was stopped.
14:46:33.454077 BSC_Tests.ttcn:1611 Port IPA_CFG_PORT[2][1] was stopped.
14:46:33.454153 BSC_Tests.ttcn:1611 Port IPA_CFG_PORT[2][2] was stopped.
14:46:33.454225 BSC_Tests.ttcn:1611 Port IPA_CFG_PORT[2][3] was stopped.
14:46:33.454297 BSC_Tests.ttcn:1611 Removing unterminated mapping between port BSCVTY and system:BSCVTY.
14:46:33.454448 BSC_Tests.ttcn:1611 Port BSCVTY was unmapped from system:BSCVTY.
14:46:33.454556 BSC_Tests.ttcn:1611 Port BSCVTY was stopped.
14:46:33.454634 BSC_Tests.ttcn:1611 Port STPVTY was stopped.
14:46:33.454711 BSC_Tests.ttcn:1611 Port SCCPLITE_IPA_CFG_PORT[0] was stopped.
14:46:33.454791 BSC_Tests.ttcn:1611 Port SCCPLITE_IPA_CFG_PORT[1] was stopped.
14:46:33.454867 BSC_Tests.ttcn:1611 Port SCCPLITE_IPA_CFG_PORT[2] was stopped.
14:46:33.454933 BSC_Tests.ttcn:1611 Removing unterminated connection between port BSSAP and VirtMSC-SCCP(316):SCCP_SP_PORT.
14:46:33.455038 BSC_Tests.ttcn:1611 Port BSSAP was stopped.
14:46:33.455154 BSC_Tests.ttcn:1611 Removing unterminated connection between port BSSAP_LE and VirtSMLC-SCCP(318):SCCP_SP_PORT.
14:46:33.455255 BSC_Tests.ttcn:1611 Port BSSAP_LE was stopped.
14:46:33.455370 BSC_Tests.ttcn:1611 Component type BSC_Tests.test_CT was shut down inside testcase TC_chan_act_nack.
14:46:33.455447 BSC_Tests.ttcn:1611 Waiting for PTCs to finish.
14:46:33.461013 BSC_Tests.ttcn:1611 Setting final verdict of the test case.
14:46:33.461203 BSC_Tests.ttcn:1611 Local verdict of MTC: pass
14:46:33.461569 BSC_Tests.ttcn:1611 Local verdict of PTC VirtMSC-STATS(315): none (pass -> pass)
14:46:33.462014 BSC_Tests.ttcn:1611 Local verdict of PTC VirtMSC-SCCP(316): none (pass -> pass)
14:46:33.462213 BSC_Tests.ttcn:1611 Local verdict of PTC VirtMSC-M3UA(317): none (pass -> pass)
14:46:33.462364 BSC_Tests.ttcn:1611 Local verdict of PTC VirtSMLC-SCCP(318): none (pass -> pass)
14:46:33.462526 BSC_Tests.ttcn:1611 Local verdict of PTC VirtSMLC-M3UA(319): none (pass -> pass)
14:46:33.462987 BSC_Tests.ttcn:1611 Local verdict of PTC IPA-CTRL-CLI-IPA(320): none (pass -> pass)
14:46:33.463247 BSC_Tests.ttcn:1611 Local verdict of PTC VirtMGW-MGCP-0(321): none (pass -> pass)
14:46:33.463499 BSC_Tests.ttcn:1611 Local verdict of PTC IPA-BTS0-TRX0-RSL-IPA(322): none (pass -> pass)
14:46:33.463728 BSC_Tests.ttcn:1611 Test case TC_chan_act_nack finished. Verdict: pass
14:46:33.464024 BSC_Tests.ttcn:1611 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-io_uring/ttcn3-tcpdump-stop.sh BSC_Tests.TC_chan_act_nack pass'.
14:46:38.822668 BSC_Tests.ttcn:1611 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-io_uring/ttcn3-tcpdump-stop.sh BSC_Tests.TC_chan_act_nack pass' was executed successfully (exit status: 0).
14:46:38.822828 BSC_Tests.ttcn:1615 Switching to log file `BSC_Tests-TC_chan_exhaustion-4ec725da15b5-mtc-9884.log'
