(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "icE1usb - FPGA and related digital")
    (date "2022-09-05")
    (rev "1.1")
    (comment 1 "CERN-OHL-S")
    (comment 2 "(C) 2020-2022 Sylvain Munaut")
  )
  (lib_symbols
    (symbol "74xx:74HC595" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 13.97 0))
      (property "Value" "74HC595" (id 1) (at -7.62 -16.51 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc595.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "HCMOS SR 3State" (id 4) (at 0 0 0))
      (property "ki_description" "8-bit serial in/out Shift Register 3-State Outputs" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*" (id 6) (at 0 0 0))
      (symbol "74HC595_1_0"
        (pin tri_state line (at 10.16 7.62 180) (length 2.54)
          (name "QB")
          (number "1")
        )
        (pin input line (at -10.16 2.54 0) (length 2.54)
          (name "~{SRCLR}")
          (number "10")
        )
        (pin input line (at -10.16 5.08 0) (length 2.54)
          (name "SRCLK")
          (number "11")
        )
        (pin input line (at -10.16 -2.54 0) (length 2.54)
          (name "RCLK")
          (number "12")
        )
        (pin input line (at -10.16 -5.08 0) (length 2.54)
          (name "~{OE}")
          (number "13")
        )
        (pin input line (at -10.16 10.16 0) (length 2.54)
          (name "SER")
          (number "14")
        )
        (pin tri_state line (at 10.16 10.16 180) (length 2.54)
          (name "QA")
          (number "15")
        )
        (pin power_in line (at 0 15.24 270) (length 2.54)
          (name "VCC")
          (number "16")
        )
        (pin tri_state line (at 10.16 5.08 180) (length 2.54)
          (name "QC")
          (number "2")
        )
        (pin tri_state line (at 10.16 2.54 180) (length 2.54)
          (name "QD")
          (number "3")
        )
        (pin tri_state line (at 10.16 0 180) (length 2.54)
          (name "QE")
          (number "4")
        )
        (pin tri_state line (at 10.16 -2.54 180) (length 2.54)
          (name "QF")
          (number "5")
        )
        (pin tri_state line (at 10.16 -5.08 180) (length 2.54)
          (name "QG")
          (number "6")
        )
        (pin tri_state line (at 10.16 -7.62 180) (length 2.54)
          (name "QH")
          (number "7")
        )
        (pin power_in line (at 0 -17.78 90) (length 2.54)
          (name "GND")
          (number "8")
        )
        (pin output line (at 10.16 -12.7 180) (length 2.54)
          (name "QH'")
          (number "9")
        )
      )
      (symbol "74HC595_1_1"
        (rectangle (start -7.62 12.7) (end 7.62 -15.24)
          (fill (type background))
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x04_Odd_Even" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 1.27 5.08 0))
      (property "Value" "Conn_02x04_Odd_Even" (id 1) (at 1.27 -7.62 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_02x04_Odd_Even_1_1"
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 3.81) (end 3.81 -6.35)
          (fill (type background))
        )
        (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
          (fill (type none))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 7.62 -5.08 180) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
      )
    )
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "C_Small" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "capacitor cap" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at -1.27 3.175 0))
      (property "Value" "LED_Small" (id 1) (at -4.445 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 90))
      (property "ki_keywords" "LED diode light-emitting-diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_Small_0_1"
        (polyline
          (pts
            (xy -0.762 -1.016)
            (xy -0.762 1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 0)
            (xy -0.762 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 -1.016)
            (xy -0.762 0)
            (xy 0.762 1.016)
            (xy 0.762 -1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy -0.508 1.27)
            (xy -0.254 1.27)
            (xy -0.508 1.27)
            (xy -0.508 1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.508 1.27)
            (xy 0 1.778)
            (xy 0.254 1.778)
            (xy 0 1.778)
            (xy 0 1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_Small_1_1"
        (pin passive line (at -2.54 0 0) (length 1.778)
          (name "K")
          (number "1")
        )
        (pin passive line (at 2.54 0 180) (length 1.778)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Pack04" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "RN" (id 0) (at -7.62 0 90))
      (property "Value" "R_Pack04" (id 1) (at 5.08 0 90))
      (property "Footprint" "" (id 2) (at 6.985 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R network parallel topology isolated" (id 4) (at 0 0 0))
      (property "ki_description" "4 resistor network, parallel topology" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIP* SOIC* R*Array*Concave* R*Array*Convex*" (id 6) (at 0 0 0))
      (symbol "R_Pack04_0_1"
        (rectangle (start -6.35 -2.413) (end 3.81 2.413)
          (fill (type background))
        )
        (rectangle (start -5.715 1.905) (end -4.445 -1.905)
          (fill (type none))
        )
        (rectangle (start -3.175 1.905) (end -1.905 -1.905)
          (fill (type none))
        )
        (rectangle (start -0.635 1.905) (end 0.635 -1.905)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 -2.54)
            (xy -5.08 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 1.905)
            (xy -5.08 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.54)
            (xy -2.54 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 1.905)
            (xy -2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 0 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.905)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.905)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (rectangle (start 1.905 1.905) (end 3.175 -1.905)
          (fill (type none))
        )
      )
      (symbol "R_Pack04_1_1"
        (pin passive line (at -5.08 -5.08 90) (length 2.54)
          (name "R1.1")
          (number "1")
        )
        (pin passive line (at -2.54 -5.08 90) (length 2.54)
          (name "R2.1")
          (number "2")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "R3.1")
          (number "3")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "R4.1")
          (number "4")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "R4.2")
          (number "5")
        )
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "R3.2")
          (number "6")
        )
        (pin passive line (at -2.54 5.08 270) (length 2.54)
          (name "R2.2")
          (number "7")
        )
        (pin passive line (at -5.08 5.08 270) (length 2.54)
          (name "R1.2")
          (number "8")
        )
      )
    )
    (symbol "Device:R_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 0.762 0.508 0))
      (property "Value" "R_Small" (id 1) (at 0.762 -1.016 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_Small_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (fill (type none))
        )
      )
      (symbol "R_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Switch:SW_Push" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (id 0) (at 1.27 2.54 0))
      (property "Value" "SW_Push" (id 1) (at 0 -1.524 0))
      (property "Footprint" "" (id 2) (at 0 5.08 0))
      (property "Datasheet" "~" (id 3) (at 0 5.08 0))
      (property "ki_keywords" "switch normally-open pushbutton push-button" (id 4) (at 0 0 0))
      (property "ki_description" "Push button switch, generic, two pins" (id 5) (at 0 0 0))
      (symbol "SW_Push_0_1"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.27)
            (xy -2.54 1.27)
          )
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "power:+1V2" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+1V2" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+1V2\"" (id 5) (at 0 0 0))
      (symbol "+1V2_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+1V2_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+1V2")
          (number "1")
        )
      )
    )
    (symbol "power:+3V3" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3V3" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3V3\"" (id 5) (at 0 0 0))
      (symbol "+3V3_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3V3_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "power:PWR_FLAG" (power) (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "#FLG" (id 0) (at 0 1.905 0))
      (property "Value" "PWR_FLAG" (id 1) (at 0 3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Special symbol for telling ERC where power comes from" (id 5) (at 0 0 0))
      (symbol "PWR_FLAG_0_0"
        (pin power_out line (at 0 0 90) (length 0)
          (name "pwr")
          (number "1")
        )
      )
      (symbol "PWR_FLAG_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 1.27)
            (xy -1.016 1.905)
            (xy 0 2.54)
            (xy 1.016 1.905)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
    )
    (symbol "s47-chips:ICE40UP5K-SG48" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -27.94 71.12 0))
      (property "Value" "s47-chips_ICE40UP5K-SG48" (id 1) (at -27.94 68.58 0))
      (property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm" (id 2) (at 0 -77.47 0))
      (property "Datasheet" "" (id 3) (at 7.62 38.1 0))
      (property "ki_fp_filters" "QFN*48*7x7mm*" (id 4) (at 0 0 0))
      (symbol "ICE40UP5K-SG48_0_0"
        (text "Bank 0" (at 0 -36.83 900))
        (text "Bank 0" (at 0 -36.83 900))
        (text "Bank 1" (at 0 13.97 900))
        (text "Bank 1" (at 0 13.97 900))
        (text "Bank 2" (at 0 49.53 900))
        (text "Bank 2" (at 0 49.53 900))
      )
      (symbol "ICE40UP5K-SG48_0_1"
        (rectangle (start -20.32 66.04) (end 20.32 -66.04)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 19.685 -45.72)
            (xy 19.685 -48.26)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 -45.72)
            (xy 19.685 -48.26)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 -40.64)
            (xy 19.685 -43.18)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 -40.64)
            (xy 19.685 -43.18)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 -33.02)
            (xy 19.685 -35.56)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 -33.02)
            (xy 19.685 -35.56)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 -27.94)
            (xy 19.685 -30.48)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 -27.94)
            (xy 19.685 -30.48)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 -20.32)
            (xy 19.685 -22.86)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 -20.32)
            (xy 19.685 -22.86)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 -15.24)
            (xy 19.685 -17.78)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 -15.24)
            (xy 19.685 -17.78)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 10.16)
            (xy 19.685 7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 10.16)
            (xy 19.685 7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 15.24)
            (xy 19.685 12.7)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 15.24)
            (xy 19.685 12.7)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 43.18)
            (xy 19.685 40.64)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 43.18)
            (xy 19.685 40.64)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 50.8)
            (xy 19.685 48.26)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 50.8)
            (xy 19.685 48.26)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 55.88)
            (xy 19.685 53.34)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 19.685 55.88)
            (xy 19.685 53.34)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -13.97)
            (xy 1.27 -15.24)
            (xy 1.27 -58.42)
            (xy 2.54 -59.69)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -13.97)
            (xy 1.27 -15.24)
            (xy 1.27 -58.42)
            (xy 2.54 -59.69)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 34.29)
            (xy 1.27 33.02)
            (xy 1.27 -7.62)
            (xy 2.54 -8.89)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 34.29)
            (xy 1.27 33.02)
            (xy 1.27 -7.62)
            (xy 2.54 -8.89)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 39.37)
            (xy 1.27 40.64)
            (xy 1.27 58.42)
            (xy 2.54 59.69)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 39.37)
            (xy 1.27 40.64)
            (xy 1.27 58.42)
            (xy 2.54 59.69)
          )
          (fill (type none))
        )
      )
      (symbol "ICE40UP5K-SG48_1_1"
        (pin power_in line (at -22.86 58.42 0) (length 2.54)
          (name "VCC_IO2")
          (number "1")
        )
        (pin bidirectional line (at 22.86 20.32 180) (length 2.54)
          (name "IOB_18A")
          (number "10")
        )
        (pin bidirectional line (at 22.86 17.78 180) (length 2.54)
          (name "IOB_20A")
          (number "11")
        )
        (pin bidirectional line (at 22.86 15.24 180) (length 2.54)
          (name "IOB_22A")
          (number "12")
        )
        (pin bidirectional line (at 22.86 10.16 180) (length 2.54)
          (name "IOB_24A")
          (number "13")
        )
        (pin bidirectional line (at 22.86 0 180) (length 2.54)
          (name "SPI_SDO/IOB_32A")
          (number "14")
        )
        (pin bidirectional line (at 22.86 -5.08 180) (length 2.54)
          (name "SPI_SCK/IOB_34A")
          (number "15")
        )
        (pin bidirectional line (at 22.86 -7.62 180) (length 2.54)
          (name "~{SPI_CSn}/IOB_35B")
          (number "16")
        )
        (pin bidirectional line (at 22.86 -2.54 180) (length 2.54)
          (name "SPI_SDI/IOB_33B")
          (number "17")
        )
        (pin bidirectional line (at 22.86 2.54 180) (length 2.54)
          (name "IOB_31B")
          (number "18")
        )
        (pin bidirectional line (at 22.86 5.08 180) (length 2.54)
          (name "IOB_29B")
          (number "19")
        )
        (pin bidirectional line (at 22.86 45.72 180) (length 2.54)
          (name "IOB_6A")
          (number "2")
        )
        (pin bidirectional line (at 22.86 7.62 180) (length 2.54)
          (name "G3/IOB_25B")
          (number "20")
        )
        (pin bidirectional line (at 22.86 12.7 180) (length 2.54)
          (name "IOB_23B")
          (number "21")
        )
        (pin power_in line (at -22.86 33.02 0) (length 2.54)
          (name "VCC_IO1")
          (number "22")
        )
        (pin bidirectional line (at 22.86 -17.78 180) (length 2.54)
          (name "IOT_37A")
          (number "23")
        )
        (pin power_in line (at -7.62 68.58 270) (length 2.54)
          (name "VPP_2V5")
          (number "24")
        )
        (pin bidirectional line (at 22.86 -15.24 180) (length 2.54)
          (name "IOT_36B")
          (number "25")
        )
        (pin bidirectional line (at 22.86 -22.86 180) (length 2.54)
          (name "IOT_39A")
          (number "26")
        )
        (pin bidirectional line (at 22.86 -20.32 180) (length 2.54)
          (name "IOT_38B")
          (number "27")
        )
        (pin bidirectional line (at 22.86 -25.4 180) (length 2.54)
          (name "IOT_41A")
          (number "28")
        )
        (pin power_in line (at -2.54 68.58 270) (length 2.54)
          (name "VCC_PLL")
          (number "29")
        )
        (pin bidirectional line (at 22.86 40.64 180) (length 2.54)
          (name "IOB_9B")
          (number "3")
        )
        (pin power_in line (at 7.62 68.58 270) (length 2.54)
          (name "VCC")
          (number "30")
        )
        (pin bidirectional line (at 22.86 -27.94 180) (length 2.54)
          (name "IOT_42B")
          (number "31")
        )
        (pin bidirectional line (at 22.86 -30.48 180) (length 2.54)
          (name "IOT_43A")
          (number "32")
        )
        (pin power_in line (at -22.86 -15.24 0) (length 2.54)
          (name "VCC_IO0")
          (number "33")
        )
        (pin bidirectional line (at 22.86 -33.02 180) (length 2.54)
          (name "IOT_44B")
          (number "34")
        )
        (pin bidirectional line (at 22.86 -38.1 180) (length 2.54)
          (name "G0/IOT_46B")
          (number "35")
        )
        (pin bidirectional line (at 22.86 -40.64 180) (length 2.54)
          (name "IOT_48B")
          (number "36")
        )
        (pin bidirectional line (at 22.86 -35.56 180) (length 2.54)
          (name "G1/IOT_45A")
          (number "37")
        )
        (pin bidirectional line (at 22.86 -45.72 180) (length 2.54)
          (name "IOT_50B")
          (number "38")
        )
        (pin open_collector line (at 22.86 -58.42 180) (length 2.54)
          (name "RGB0")
          (number "39")
        )
        (pin bidirectional line (at 22.86 43.18 180) (length 2.54)
          (name "IOB_8A")
          (number "4")
        )
        (pin open_collector line (at 22.86 -55.88 180) (length 2.54)
          (name "RGB1")
          (number "40")
        )
        (pin open_collector line (at 22.86 -53.34 180) (length 2.54)
          (name "RGB2")
          (number "41")
        )
        (pin bidirectional line (at 22.86 -48.26 180) (length 2.54)
          (name "IOT_51A")
          (number "42")
        )
        (pin bidirectional line (at 22.86 -43.18 180) (length 2.54)
          (name "IOT_49A")
          (number "43")
        )
        (pin bidirectional line (at 22.86 53.34 180) (length 2.54)
          (name "G6/IOB_3B")
          (number "44")
        )
        (pin bidirectional line (at 22.86 48.26 180) (length 2.54)
          (name "IOB_5B")
          (number "45")
        )
        (pin bidirectional line (at 22.86 58.42 180) (length 2.54)
          (name "IOB_0A")
          (number "46")
        )
        (pin bidirectional line (at 22.86 55.88 180) (length 2.54)
          (name "IOB_2A")
          (number "47")
        )
        (pin bidirectional line (at 22.86 50.8 180) (length 2.54)
          (name "IOB_4A")
          (number "48")
        )
        (pin power_in line (at 0 -68.58 90) (length 2.54)
          (name "GND")
          (number "49")
        )
        (pin power_in line (at 2.54 68.58 270) (length 2.54)
          (name "VCC")
          (number "5")
        )
        (pin bidirectional line (at 22.86 25.4 180) (length 2.54)
          (name "IOB_13B")
          (number "6")
        )
        (pin open_collector line (at 22.86 33.02 180) (length 2.54)
          (name "CDONE")
          (number "7")
        )
        (pin input line (at 22.86 30.48 180) (length 2.54)
          (name "~{CRESET_B}")
          (number "8")
        )
        (pin bidirectional line (at 22.86 22.86 180) (length 2.54)
          (name "IOB_16A")
          (number "9")
        )
      )
    )
    (symbol "s47-chips:IP4220CZ6" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -6.985 -2.54 0))
      (property "Value" "s47-chips_IP4220CZ6" (id 1) (at 6.35 1.27 90))
      (property "Footprint" "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm" (id 2) (at 1.27 1.905 0))
      (property "Datasheet" "" (id 3) (at 1.27 1.905 0))
      (property "ki_fp_filters" "TSOP?6*" (id 4) (at 0 0 0))
      (symbol "IP4220CZ6_0_1"
        (rectangle (start -5.334 3.048) (end 5.08 -3.048)
          (fill (type background))
        )
        (circle (center -3.81 0) (radius 0.127)
          (fill (type none))
        )
        (circle (center -3.81 0) (radius 0.127)
          (fill (type none))
        )
        (circle (center -1.27 -2.54) (radius 0.127)
          (fill (type none))
        )
        (circle (center -1.27 -2.54) (radius 0.127)
          (fill (type none))
        )
        (circle (center -1.27 0) (radius 0.127)
          (fill (type none))
        )
        (circle (center -1.27 0) (radius 0.127)
          (fill (type none))
        )
        (circle (center -1.27 2.54) (radius 0.127)
          (fill (type none))
        )
        (circle (center -1.27 2.54) (radius 0.127)
          (fill (type none))
        )
        (circle (center 0 -2.54) (radius 0.127)
          (fill (type none))
        )
        (circle (center 0 -2.54) (radius 0.127)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.445 -1.27)
            (xy -3.175 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.445 -1.27)
            (xy -3.175 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.445 1.905)
            (xy -3.175 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 -2.54)
            (xy -3.81 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 -2.54)
            (xy 3.81 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 -0.635)
            (xy -3.81 0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 0.635)
            (xy -3.81 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 2.54)
            (xy 3.81 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 2.54)
            (xy 3.81 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -0.635 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -0.635 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 1.905)
            (xy -0.635 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -2.54)
            (xy -1.27 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -2.54)
            (xy -1.27 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0.635)
            (xy -1.27 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0.635)
            (xy -1.27 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.889)
            (xy 0 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.889)
            (xy 0 1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.889)
            (xy 0 1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.016)
            (xy 0 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -1.27)
            (xy 1.905 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -1.27)
            (xy 1.905 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 1.905 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 1.27 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 1.27 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0.635)
            (xy 1.27 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0.635)
            (xy 1.27 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.175 -1.27)
            (xy 4.445 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.175 -1.27)
            (xy 4.445 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.175 1.905)
            (xy 4.445 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 -2.54)
            (xy 3.81 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 0.635)
            (xy 3.81 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 0.635)
            (xy 3.81 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 0.254)
            (xy -0.762 0.254)
            (xy -0.762 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.445 -1.905)
            (xy -3.175 -1.905)
            (xy -3.81 -1.27)
            (xy -4.445 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.445 1.27)
            (xy -3.175 1.27)
            (xy -3.81 1.905)
            (xy -4.445 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.54)
            (xy -2.54 -0.635)
            (xy -3.048 0)
            (xy -3.937 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.54)
            (xy -2.54 0.762)
            (xy -1.905 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -1.905)
            (xy -0.635 -1.905)
            (xy -1.27 -1.27)
            (xy -1.905 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 1.27)
            (xy -0.635 1.27)
            (xy -1.27 1.905)
            (xy -1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.762 -0.508)
            (xy 0.762 -0.508)
            (xy 0 0.254)
            (xy -0.762 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.762 -0.508)
            (xy 0.762 -0.508)
            (xy 0 0.254)
            (xy -0.762 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -1.905)
            (xy 1.905 -1.905)
            (xy 1.27 -1.27)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.27)
            (xy 1.905 1.27)
            (xy 1.27 1.905)
            (xy 0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 -0.508)
            (xy 2.921 0)
            (xy 3.81 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 2.54 0.762)
            (xy 1.905 0)
            (xy 1.143 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.175 -1.905)
            (xy 4.445 -1.905)
            (xy 3.81 -1.27)
            (xy 3.175 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.175 1.27)
            (xy 4.445 1.27)
            (xy 3.81 1.905)
            (xy 3.175 1.27)
          )
          (fill (type none))
        )
        (circle (center 0 2.54) (radius 0.127)
          (fill (type none))
        )
        (circle (center 0 2.54) (radius 0.127)
          (fill (type none))
        )
        (circle (center 1.27 -2.54) (radius 0.127)
          (fill (type none))
        )
        (circle (center 1.27 -2.54) (radius 0.127)
          (fill (type none))
        )
        (circle (center 1.27 0) (radius 0.127)
          (fill (type none))
        )
        (circle (center 1.27 0) (radius 0.127)
          (fill (type none))
        )
        (circle (center 1.27 2.54) (radius 0.127)
          (fill (type none))
        )
        (circle (center 1.27 2.54) (radius 0.127)
          (fill (type none))
        )
        (circle (center 3.81 0) (radius 0.127)
          (fill (type none))
        )
        (circle (center 3.81 0) (radius 0.127)
          (fill (type none))
        )
      )
      (symbol "IP4220CZ6_1_1"
        (pin passive line (at -2.54 -5.08 90) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "~")
          (number "2")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "~")
          (number "3")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "~")
          (number "4")
        )
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "~")
          (number "5")
        )
        (pin passive line (at -2.54 5.08 270) (length 2.54)
          (name "~")
          (number "6")
        )
      )
    )
    (symbol "s47-chips:SPI_FLASH_8P" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 11.43 0))
      (property "Value" "s47-chips_SPI_FLASH_8P" (id 1) (at -7.62 8.89 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "SPI_FLASH_8P_0_0"
        (rectangle (start -7.62 7.62) (end 7.62 -10.16)
          (fill (type background))
        )
      )
      (symbol "SPI_FLASH_8P_1_1"
        (pin input line (at -10.16 -7.62 0) (length 2.54)
          (name "~{CS}")
          (number "1")
        )
        (pin bidirectional line (at -10.16 2.54 0) (length 2.54)
          (name "SIO1/SO")
          (number "2")
        )
        (pin bidirectional line (at -10.16 0 0) (length 2.54)
          (name "SIO2/~{W}")
          (number "3")
        )
        (pin power_in line (at 10.16 -7.62 180) (length 2.54)
          (name "VSS")
          (number "4")
        )
        (pin bidirectional line (at -10.16 5.08 0) (length 2.54)
          (name "SIO0/SI")
          (number "5")
        )
        (pin input line (at -10.16 -5.08 0) (length 2.54)
          (name "SCK")
          (number "6")
        )
        (pin bidirectional line (at -10.16 -2.54 0) (length 2.54)
          (name "SIO3/~{HOLD}")
          (number "7")
        )
        (pin power_in line (at 10.16 5.08 180) (length 2.54)
          (name "VCC")
          (number "8")
        )
      )
    )
    (symbol "s47-device:LED_RBAG" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 9.398 0))
      (property "Value" "s47-device_LED_RBAG" (id 1) (at 0 -8.89 0))
      (property "Footprint" "" (id 2) (at 0 -1.27 0))
      (property "Datasheet" "" (id 3) (at 0 -1.27 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 4) (at 0 0 0))
      (symbol "LED_RBAG_0_0"
        (text "B" (at -1.905 -6.35 0))
        (text "G" (at -1.905 -1.27 0))
        (text "R" (at -1.905 3.81 0))
      )
      (symbol "LED_RBAG_0_1"
        (polyline
          (pts
            (xy -1.27 -5.08)
            (xy -2.54 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -5.08)
            (xy 1.27 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -3.81)
            (xy -1.27 -6.35)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 5.08)
            (xy -2.54 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 5.08)
            (xy 1.27 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 6.35)
            (xy -1.27 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 6.35)
            (xy -1.27 3.81)
            (xy -1.27 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -5.08)
            (xy 2.032 -5.08)
            (xy 2.032 5.08)
            (xy 1.27 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -3.81)
            (xy 1.27 -6.35)
            (xy -1.27 -5.08)
            (xy 1.27 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 6.35)
            (xy 1.27 3.81)
            (xy -1.27 5.08)
            (xy 1.27 6.35)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 -3.81)
            (xy 0.508 -2.286)
            (xy -0.254 -2.286)
            (xy 0.508 -2.286)
            (xy 0.508 -3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 1.27)
            (xy 0.508 2.794)
            (xy -0.254 2.794)
            (xy 0.508 2.794)
            (xy 0.508 2.032)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 6.35)
            (xy 0.508 7.874)
            (xy -0.254 7.874)
            (xy 0.508 7.874)
            (xy 0.508 7.112)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -3.81)
            (xy 1.524 -2.286)
            (xy 0.762 -2.286)
            (xy 1.524 -2.286)
            (xy 1.524 -3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.27)
            (xy 1.524 2.794)
            (xy 0.762 2.794)
            (xy 1.524 2.794)
            (xy 1.524 2.032)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 6.35)
            (xy 1.524 7.874)
            (xy 0.762 7.874)
            (xy 1.524 7.874)
            (xy 1.524 7.112)
          )
          (fill (type none))
        )
        (rectangle (start 1.27 -1.27) (end 1.27 1.27)
          (fill (type none))
        )
        (rectangle (start 1.27 1.27) (end 1.27 1.27)
          (fill (type none))
        )
        (rectangle (start 1.27 3.81) (end 1.27 6.35)
          (fill (type none))
        )
        (rectangle (start 1.27 6.35) (end 1.27 6.35)
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start 2.794 8.382) (end -2.794 -7.62)
          (fill (type background))
        )
      )
      (symbol "LED_RBAG_1_1"
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "RK")
          (number "1")
        )
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "BK")
          (number "2")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "A")
          (number "3")
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "GK")
          (number "4")
        )
      )
    )
    (symbol "s47-device:VCXO_6_TUNE_OE" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 1.27 11.43 0))
      (property "Value" "s47-device_VCXO_6_TUNE_OE" (id 1) (at 1.27 8.89 0))
      (property "Footprint" "s47-misc:Oscillator_SMD_VCXO-6Pin_7.0x5.0mm_P2.54mm" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "VCXO_6_TUNE_OE_1_1"
        (rectangle (start -7.62 7.62) (end 7.62 -7.62)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -1.27 -0.762)
            (xy -1.016 -0.762)
            (xy -1.016 0.762)
            (xy -0.508 0.762)
            (xy -0.508 -0.762)
            (xy 0 -0.762)
            (xy 0 0.762)
            (xy 0.508 0.762)
            (xy 0.508 -0.762)
            (xy 0.762 -0.762)
          )
          (fill (type none))
        )
        (pin input line (at -10.16 -2.54 0) (length 2.54)
          (name "Vctrl")
          (number "1")
        )
        (pin input line (at -10.16 2.54 0) (length 2.54)
          (name "OE")
          (number "2")
        )
        (pin power_in line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "3")
        )
        (pin output line (at 10.16 0 180) (length 2.54)
          (name "OUT")
          (number "4")
        )
        (pin power_in line (at 0 10.16 270) (length 2.54)
          (name "Vcc")
          (number "6")
        )
      )
    )
    (symbol "s47-misc:LightPipe" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "LP" (id 0) (at 0 5.08 0))
      (property "Value" "s47-misc_LightPipe" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "LightPipe_0_1"
        (rectangle (start -5.08 -3.81) (end 5.08 3.81)
          (fill (type background))
        )
        (arc (start -1.27 1.27) (mid -2.1627 0.8927) (end -2.54 0)
          (fill (type none))
        )
        (arc (start -1.27 2.54) (mid -3.0713 1.8013) (end -3.81 0)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.556 -2.667)
            (xy -3.81 -2.667)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.921 -2.667)
            (xy -2.54 -2.667)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.794 -2.286)
            (xy -2.794 -3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy 2.54 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy -1.27 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 0)
            (xy -3.81 -1.27)
            (xy -2.54 -1.27)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.556 -2.286)
            (xy -3.556 -3.048)
            (xy -2.921 -2.667)
            (xy -3.556 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.556 -2.032)
            (xy -3.302 -1.778)
            (xy -3.429 -1.778)
            (xy -3.302 -1.905)
            (xy -3.302 -1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -2.032)
            (xy -2.794 -1.778)
            (xy -2.921 -1.778)
            (xy -2.794 -1.905)
            (xy -2.794 -1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.302 1.651)
            (xy 3.937 1.651)
            (xy 3.81 1.778)
            (xy 3.81 1.524)
            (xy 3.937 1.651)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.302 2.286)
            (xy 3.937 2.286)
            (xy 3.81 2.413)
            (xy 3.81 2.159)
            (xy 3.937 2.286)
          )
          (fill (type none))
        )
        (arc (start 2.54 1.27) (mid 2.803 1.905) (end 2.54 2.54)
          (fill (type none))
        )
      )
    )
  )
  (junction (at 96.52 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 25.4 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 236.22 40.64) (diameter 0) (color 0 0 0 0))
  (junction (at 33.02 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 231.14 109.22) (diameter 0) (color 0 0 0 0))
  (junction (at 66.04 30.48) (diameter 0) (color 0 0 0 0))
  (junction (at 86.36 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 218.44 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 226.06 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 218.44 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 55.88 25.4) (diameter 0) (color 0 0 0 0))
  (junction (at 256.54 147.32) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 30.48) (diameter 0) (color 0 0 0 0))
  (junction (at 228.6 111.76) (diameter 0) (color 0 0 0 0))
  (junction (at 25.4 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 25.4 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 157.48 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 261.62 121.92) (diameter 0) (color 0 0 0 0))
  (junction (at 55.88 35.56) (diameter 0) (color 0 0 0 0))
  (junction (at 223.52 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 134.62 30.48) (diameter 0) (color 0 0 0 0))
  (junction (at 60.96 33.02) (diameter 0) (color 0 0 0 0))
  (junction (at 147.32 175.26) (diameter 0) (color 0 0 0 0))
  (junction (at 81.28 35.56) (diameter 0) (color 0 0 0 0))
  (junction (at 236.22 114.3) (diameter 0) (color 0 0 0 0))
  (junction (at 33.02 132.08) (diameter 0) (color 0 0 0 0))
  (junction (at 33.02 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 220.98 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 261.62 109.22) (diameter 0) (color 0 0 0 0))
  (junction (at 139.7 33.02) (diameter 0) (color 0 0 0 0))
  (junction (at 218.44 104.14) (diameter 0) (color 0 0 0 0))
  (junction (at 226.06 119.38) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 50.8) (diameter 0) (color 0 0 0 0))
  (junction (at 91.44 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 60.96 25.4) (diameter 0) (color 0 0 0 0))
  (junction (at 139.7 48.26) (diameter 0) (color 0 0 0 0))
  (junction (at 223.52 121.92) (diameter 0) (color 0 0 0 0))
  (junction (at 215.9 132.08) (diameter 0) (color 0 0 0 0))
  (junction (at 215.9 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 248.92 30.48) (diameter 0) (color 0 0 0 0))
  (no_connect (at 167.64 116.84))
  (bus_entry (at 177.8 96.52) (size 2.54 -2.54))
  (bus_entry (at 104.14 106.68) (size 2.54 2.54))
  (bus_entry (at 177.8 93.98) (size 2.54 -2.54))
  (bus_entry (at 177.8 106.68) (size 2.54 -2.54))
  (bus_entry (at 177.8 109.22) (size 2.54 -2.54))
  (bus_entry (at 104.14 109.22) (size 2.54 2.54))
  (bus_entry (at 177.8 104.14) (size 2.54 -2.54))
  (bus_entry (at 177.8 99.06) (size 2.54 -2.54))
  (bus_entry (at 104.14 111.76) (size 2.54 2.54))
  (bus_entry (at 177.8 101.6) (size 2.54 -2.54))
  (bus_entry (at 177.8 111.76) (size 2.54 -2.54))
  (wire (pts (xy 96.52 139.7) (xy 81.28 139.7)))
  (wire (pts (xy 220.98 88.9) (xy 223.52 88.9)))
  (wire (pts (xy 81.28 160.02) (xy 96.52 160.02)))
  (bus (pts (xy 180.34 101.6) (xy 180.34 104.14)))
  (wire (pts (xy 81.28 111.76) (xy 104.14 111.76)))
  (wire (pts (xy 55.88 22.86) (xy 55.88 25.4)))
  (wire (pts (xy 66.04 30.48) (xy 66.04 48.26)))
  (wire (pts (xy 81.28 106.68) (xy 104.14 106.68)))
  (wire (pts (xy 137.16 185.42) (xy 147.32 185.42)))
  (wire (pts (xy 58.42 187.96) (xy 58.42 185.42)))
  (wire (pts (xy 48.26 33.02) (xy 48.26 35.56)))
  (wire (pts (xy 25.4 83.82) (xy 33.02 83.82)))
  (wire (pts (xy 215.9 45.72) (xy 215.9 48.26)))
  (wire (pts (xy 215.9 53.34) (xy 215.9 55.88)))
  (wire (pts (xy 81.28 152.4) (xy 96.52 152.4)))
  (wire (pts (xy 180.34 147.32) (xy 180.34 149.86)))
  (wire (pts (xy 96.52 45.72) (xy 96.52 48.26)))
  (bus (pts (xy 180.34 88.9) (xy 180.34 91.44)))
  (wire (pts (xy 205.74 40.64) (xy 193.04 40.64)))
  (bus (pts (xy 180.34 104.14) (xy 180.34 106.68)))
  (wire (pts (xy 220.98 101.6) (xy 220.98 104.14)))
  (wire (pts (xy 248.92 53.34) (xy 248.92 55.88)))
  (wire (pts (xy 226.06 53.34) (xy 226.06 55.88)))
  (wire (pts (xy 81.28 116.84) (xy 96.52 116.84)))
  (wire (pts (xy 251.46 149.86) (xy 254 149.86)))
  (bus (pts (xy 180.34 96.52) (xy 180.34 99.06)))
  (wire (pts (xy 139.7 35.56) (xy 139.7 33.02)))
  (wire (pts (xy 238.76 121.92) (xy 223.52 121.92)))
  (wire (pts (xy 33.02 91.44) (xy 33.02 93.98)))
  (wire (pts (xy 215.9 154.94) (xy 259.08 154.94)))
  (wire (pts (xy 167.64 99.06) (xy 177.8 99.06)))
  (wire (pts (xy 25.4 58.42) (xy 25.4 83.82)))
  (wire (pts (xy 248.92 30.48) (xy 248.92 33.02)))
  (wire (pts (xy 226.06 147.32) (xy 226.06 119.38)))
  (wire (pts (xy 264.16 154.94) (xy 264.16 157.48)))
  (wire (pts (xy 261.62 109.22) (xy 261.62 114.3)))
  (wire (pts (xy 81.28 149.86) (xy 96.52 149.86)))
  (wire (pts (xy 25.4 83.82) (xy 25.4 132.08)))
  (wire (pts (xy 167.64 106.68) (xy 177.8 106.68)))
  (wire (pts (xy 132.08 25.4) (xy 134.62 25.4)))
  (wire (pts (xy 81.28 134.62) (xy 96.52 134.62)))
  (wire (pts (xy 35.56 58.42) (xy 33.02 58.42)))
  (bus (pts (xy 106.68 116.84) (xy 111.76 116.84)))
  (wire (pts (xy 91.44 38.1) (xy 91.44 33.02)))
  (wire (pts (xy 86.36 43.18) (xy 86.36 45.72)))
  (wire (pts (xy 218.44 129.54) (xy 218.44 152.4)))
  (wire (pts (xy 248.92 27.94) (xy 248.92 30.48)))
  (wire (pts (xy 172.72 45.72) (xy 177.8 45.72)))
  (wire (pts (xy 83.82 175.26) (xy 83.82 180.34)))
  (wire (pts (xy 160.02 30.48) (xy 144.78 30.48)))
  (wire (pts (xy 81.28 114.3) (xy 96.52 114.3)))
  (wire (pts (xy 144.78 109.22) (xy 147.32 109.22)))
  (wire (pts (xy 81.28 76.2) (xy 96.52 76.2)))
  (wire (pts (xy 81.28 119.38) (xy 96.52 119.38)))
  (wire (pts (xy 200.66 129.54) (xy 218.44 129.54)))
  (wire (pts (xy 96.52 144.78) (xy 81.28 144.78)))
  (wire (pts (xy 228.6 144.78) (xy 228.6 111.76)))
  (wire (pts (xy 116.84 30.48) (xy 134.62 30.48)))
  (wire (pts (xy 35.56 83.82) (xy 33.02 83.82)))
  (wire (pts (xy 55.88 25.4) (xy 55.88 27.94)))
  (wire (pts (xy 231.14 142.24) (xy 231.14 109.22)))
  (wire (pts (xy 81.28 58.42) (xy 96.52 58.42)))
  (wire (pts (xy 81.28 91.44) (xy 96.52 91.44)))
  (wire (pts (xy 81.28 121.92) (xy 96.52 121.92)))
  (wire (pts (xy 86.36 175.26) (xy 88.9 175.26)))
  (wire (pts (xy 256.54 147.32) (xy 251.46 147.32)))
  (wire (pts (xy 96.52 63.5) (xy 81.28 63.5)))
  (wire (pts (xy 81.28 45.72) (xy 86.36 45.72)))
  (wire (pts (xy 81.28 86.36) (xy 96.52 86.36)))
  (wire (pts (xy 215.9 91.44) (xy 215.9 88.9)))
  (wire (pts (xy 81.28 66.04) (xy 96.52 66.04)))
  (wire (pts (xy 218.44 45.72) (xy 215.9 45.72)))
  (wire (pts (xy 238.76 40.64) (xy 236.22 40.64)))
  (wire (pts (xy 96.52 38.1) (xy 96.52 30.48)))
  (wire (pts (xy 147.32 172.72) (xy 147.32 175.26)))
  (wire (pts (xy 81.28 73.66) (xy 96.52 73.66)))
  (wire (pts (xy 259.08 154.94) (xy 259.08 144.78)))
  (wire (pts (xy 160.02 50.8) (xy 144.78 50.8)))
  (wire (pts (xy 25.4 45.72) (xy 25.4 58.42)))
  (wire (pts (xy 144.78 124.46) (xy 144.78 109.22)))
  (bus (pts (xy 180.34 99.06) (xy 180.34 101.6)))
  (wire (pts (xy 264.16 149.86) (xy 264.16 147.32)))
  (wire (pts (xy 101.6 172.72) (xy 101.6 175.26)))
  (wire (pts (xy 218.44 104.14) (xy 218.44 129.54)))
  (wire (pts (xy 259.08 109.22) (xy 261.62 109.22)))
  (wire (pts (xy 116.84 50.8) (xy 144.78 50.8)))
  (wire (pts (xy 96.52 137.16) (xy 81.28 137.16)))
  (wire (pts (xy 81.28 157.48) (xy 96.52 157.48)))
  (wire (pts (xy 50.8 48.26) (xy 50.8 45.72)))
  (wire (pts (xy 238.76 119.38) (xy 226.06 119.38)))
  (wire (pts (xy 236.22 30.48) (xy 236.22 40.64)))
  (wire (pts (xy 83.82 180.34) (xy 88.9 180.34)))
  (wire (pts (xy 33.02 139.7) (xy 33.02 142.24)))
  (wire (pts (xy 215.9 45.72) (xy 210.82 45.72)))
  (wire (pts (xy 167.64 109.22) (xy 177.8 109.22)))
  (wire (pts (xy 33.02 58.42) (xy 25.4 58.42)))
  (wire (pts (xy 81.28 83.82) (xy 96.52 83.82)))
  (wire (pts (xy 139.7 33.02) (xy 157.48 33.02)))
  (wire (pts (xy 55.88 25.4) (xy 60.96 25.4)))
  (wire (pts (xy 144.78 45.72) (xy 144.78 50.8)))
  (wire (pts (xy 25.4 22.86) (xy 25.4 45.72)))
  (wire (pts (xy 162.56 45.72) (xy 160.02 45.72)))
  (wire (pts (xy 218.44 101.6) (xy 218.44 104.14)))
  (wire (pts (xy 91.44 43.18) (xy 91.44 45.72)))
  (wire (pts (xy 215.9 132.08) (xy 215.9 154.94)))
  (wire (pts (xy 238.76 111.76) (xy 228.6 111.76)))
  (wire (pts (xy 157.48 76.2) (xy 157.48 88.9)))
  (wire (pts (xy 81.28 175.26) (xy 83.82 175.26)))
  (bus (pts (xy 106.68 111.76) (xy 106.68 114.3)))
  (wire (pts (xy 139.7 45.72) (xy 139.7 48.26)))
  (wire (pts (xy 55.88 33.02) (xy 55.88 35.56)))
  (wire (pts (xy 236.22 116.84) (xy 238.76 116.84)))
  (wire (pts (xy 157.48 48.26) (xy 157.48 43.18)))
  (wire (pts (xy 223.52 121.92) (xy 200.66 121.92)))
  (wire (pts (xy 81.28 35.56) (xy 81.28 38.1)))
  (wire (pts (xy 81.28 68.58) (xy 96.52 68.58)))
  (wire (pts (xy 157.48 33.02) (xy 157.48 40.64)))
  (wire (pts (xy 66.04 25.4) (xy 66.04 30.48)))
  (wire (pts (xy 147.32 147.32) (xy 134.62 147.32)))
  (wire (pts (xy 238.76 147.32) (xy 226.06 147.32)))
  (wire (pts (xy 177.8 43.18) (xy 172.72 43.18)))
  (wire (pts (xy 147.32 93.98) (xy 134.62 93.98)))
  (wire (pts (xy 226.06 45.72) (xy 226.06 48.26)))
  (wire (pts (xy 256.54 152.4) (xy 256.54 147.32)))
  (bus (pts (xy 180.34 88.9) (xy 185.42 88.9)))
  (wire (pts (xy 276.86 43.18) (xy 266.7 43.18)))
  (wire (pts (xy 238.76 45.72) (xy 226.06 45.72)))
  (wire (pts (xy 160.02 45.72) (xy 160.02 50.8)))
  (wire (pts (xy 264.16 147.32) (xy 256.54 147.32)))
  (wire (pts (xy 215.9 88.9) (xy 218.44 88.9)))
  (wire (pts (xy 167.64 93.98) (xy 177.8 93.98)))
  (wire (pts (xy 81.28 93.98) (xy 96.52 93.98)))
  (wire (pts (xy 228.6 111.76) (xy 200.66 111.76)))
  (wire (pts (xy 86.36 172.72) (xy 86.36 175.26)))
  (wire (pts (xy 157.48 40.64) (xy 162.56 40.64)))
  (wire (pts (xy 226.06 45.72) (xy 223.52 45.72)))
  (wire (pts (xy 96.52 162.56) (xy 81.28 162.56)))
  (wire (pts (xy 236.22 114.3) (xy 236.22 116.84)))
  (wire (pts (xy 81.28 170.18) (xy 88.9 170.18)))
  (wire (pts (xy 220.98 104.14) (xy 218.44 104.14)))
  (wire (pts (xy 60.96 25.4) (xy 60.96 33.02)))
  (wire (pts (xy 127 25.4) (xy 116.84 25.4)))
  (wire (pts (xy 236.22 86.36) (xy 236.22 114.3)))
  (wire (pts (xy 147.32 185.42) (xy 147.32 182.88)))
  (bus (pts (xy 106.68 109.22) (xy 106.68 111.76)))
  (wire (pts (xy 248.92 30.48) (xy 236.22 30.48)))
  (wire (pts (xy 215.9 40.64) (xy 215.9 45.72)))
  (wire (pts (xy 142.24 45.72) (xy 142.24 53.34)))
  (wire (pts (xy 259.08 121.92) (xy 261.62 121.92)))
  (wire (pts (xy 149.86 187.96) (xy 149.86 182.88)))
  (wire (pts (xy 147.32 175.26) (xy 149.86 175.26)))
  (bus (pts (xy 180.34 106.68) (xy 180.34 109.22)))
  (bus (pts (xy 180.34 93.98) (xy 180.34 96.52)))
  (wire (pts (xy 81.28 154.94) (xy 96.52 154.94)))
  (wire (pts (xy 81.28 96.52) (xy 96.52 96.52)))
  (wire (pts (xy 33.02 58.42) (xy 33.02 60.96)))
  (wire (pts (xy 137.16 187.96) (xy 149.86 187.96)))
  (wire (pts (xy 86.36 45.72) (xy 91.44 45.72)))
  (wire (pts (xy 116.84 48.26) (xy 139.7 48.26)))
  (wire (pts (xy 215.9 101.6) (xy 215.9 132.08)))
  (wire (pts (xy 147.32 99.06) (xy 134.62 99.06)))
  (wire (pts (xy 147.32 106.68) (xy 134.62 106.68)))
  (wire (pts (xy 238.76 114.3) (xy 236.22 114.3)))
  (wire (pts (xy 259.08 144.78) (xy 251.46 144.78)))
  (wire (pts (xy 35.56 132.08) (xy 33.02 132.08)))
  (bus (pts (xy 180.34 91.44) (xy 180.34 93.98)))
  (wire (pts (xy 193.04 45.72) (xy 205.74 45.72)))
  (wire (pts (xy 81.28 104.14) (xy 96.52 104.14)))
  (wire (pts (xy 261.62 121.92) (xy 261.62 124.46)))
  (wire (pts (xy 81.28 35.56) (xy 55.88 35.56)))
  (wire (pts (xy 116.84 33.02) (xy 139.7 33.02)))
  (wire (pts (xy 167.64 104.14) (xy 177.8 104.14)))
  (wire (pts (xy 167.64 96.52) (xy 177.8 96.52)))
  (wire (pts (xy 223.52 101.6) (xy 223.52 121.92)))
  (wire (pts (xy 81.28 101.6) (xy 96.52 101.6)))
  (wire (pts (xy 254 149.86) (xy 254 157.48)))
  (wire (pts (xy 139.7 48.26) (xy 157.48 48.26)))
  (wire (pts (xy 134.62 25.4) (xy 134.62 30.48)))
  (wire (pts (xy 149.86 175.26) (xy 149.86 177.8)))
  (wire (pts (xy 238.76 149.86) (xy 223.52 149.86)))
  (wire (pts (xy 167.64 101.6) (xy 177.8 101.6)))
  (wire (pts (xy 261.62 43.18) (xy 259.08 43.18)))
  (wire (pts (xy 231.14 109.22) (xy 200.66 109.22)))
  (wire (pts (xy 50.8 45.72) (xy 25.4 45.72)))
  (wire (pts (xy 81.28 60.96) (xy 96.52 60.96)))
  (wire (pts (xy 81.28 71.12) (xy 96.52 71.12)))
  (wire (pts (xy 96.52 132.08) (xy 81.28 132.08)))
  (wire (pts (xy 142.24 25.4) (xy 142.24 35.56)))
  (wire (pts (xy 91.44 45.72) (xy 96.52 45.72)))
  (wire (pts (xy 81.28 124.46) (xy 96.52 124.46)))
  (wire (pts (xy 33.02 132.08) (xy 33.02 134.62)))
  (wire (pts (xy 134.62 30.48) (xy 144.78 30.48)))
  (wire (pts (xy 81.28 142.24) (xy 96.52 142.24)))
  (wire (pts (xy 33.02 66.04) (xy 33.02 68.58)))
  (wire (pts (xy 226.06 119.38) (xy 200.66 119.38)))
  (wire (pts (xy 218.44 152.4) (xy 256.54 152.4)))
  (wire (pts (xy 223.52 86.36) (xy 223.52 88.9)))
  (wire (pts (xy 177.8 147.32) (xy 180.34 147.32)))
  (wire (pts (xy 60.96 25.4) (xy 66.04 25.4)))
  (wire (pts (xy 210.82 40.64) (xy 215.9 40.64)))
  (wire (pts (xy 261.62 121.92) (xy 261.62 119.38)))
  (wire (pts (xy 238.76 142.24) (xy 231.14 142.24)))
  (wire (pts (xy 96.52 30.48) (xy 66.04 30.48)))
  (wire (pts (xy 147.32 175.26) (xy 147.32 177.8)))
  (wire (pts (xy 167.64 111.76) (xy 177.8 111.76)))
  (wire (pts (xy 238.76 109.22) (xy 231.14 109.22)))
  (wire (pts (xy 81.28 109.22) (xy 104.14 109.22)))
  (wire (pts (xy 86.36 35.56) (xy 81.28 35.56)))
  (wire (pts (xy 236.22 40.64) (xy 236.22 48.26)))
  (wire (pts (xy 152.4 83.82) (xy 152.4 86.36)))
  (wire (pts (xy 218.44 88.9) (xy 220.98 88.9)))
  (wire (pts (xy 152.4 78.74) (xy 152.4 76.2)))
  (wire (pts (xy 96.52 43.18) (xy 96.52 45.72)))
  (wire (pts (xy 48.26 35.56) (xy 55.88 35.56)))
  (wire (pts (xy 261.62 86.36) (xy 261.62 109.22)))
  (wire (pts (xy 25.4 132.08) (xy 33.02 132.08)))
  (wire (pts (xy 33.02 83.82) (xy 33.02 86.36)))
  (wire (pts (xy 238.76 144.78) (xy 228.6 144.78)))
  (wire (pts (xy 157.48 121.92) (xy 157.48 124.46)))
  (wire (pts (xy 81.28 172.72) (xy 86.36 172.72)))
  (wire (pts (xy 157.48 73.66) (xy 157.48 76.2)))
  (wire (pts (xy 55.88 35.56) (xy 55.88 48.26)))
  (wire (pts (xy 160.02 38.1) (xy 160.02 30.48)))
  (wire (pts (xy 81.28 43.18) (xy 81.28 45.72)))
  (wire (pts (xy 152.4 147.32) (xy 167.64 147.32)))
  (wire (pts (xy 157.48 43.18) (xy 162.56 43.18)))
  (wire (pts (xy 218.44 88.9) (xy 218.44 91.44)))
  (wire (pts (xy 96.52 147.32) (xy 81.28 147.32)))
  (wire (pts (xy 177.8 38.1) (xy 172.72 38.1)))
  (wire (pts (xy 220.98 88.9) (xy 220.98 91.44)))
  (wire (pts (xy 144.78 35.56) (xy 144.78 30.48)))
  (wire (pts (xy 236.22 53.34) (xy 236.22 55.88)))
  (wire (pts (xy 162.56 38.1) (xy 160.02 38.1)))
  (wire (pts (xy 177.8 40.64) (xy 172.72 40.64)))
  (wire (pts (xy 152.4 76.2) (xy 157.48 76.2)))
  (wire (pts (xy 254 142.24) (xy 251.46 142.24)))
  (wire (pts (xy 254 139.7) (xy 254 142.24)))
  (wire (pts (xy 91.44 33.02) (xy 60.96 33.02)))
  (wire (pts (xy 96.52 165.1) (xy 81.28 165.1)))
  (wire (pts (xy 223.52 88.9) (xy 223.52 91.44)))
  (wire (pts (xy 101.6 175.26) (xy 99.06 175.26)))
  (bus (pts (xy 106.68 114.3) (xy 106.68 116.84)))
  (wire (pts (xy 223.52 149.86) (xy 223.52 121.92)))
  (wire (pts (xy 86.36 38.1) (xy 86.36 35.56)))
  (wire (pts (xy 60.96 33.02) (xy 60.96 48.26)))
  (wire (pts (xy 200.66 132.08) (xy 215.9 132.08)))
  (wire (pts (xy 147.32 101.6) (xy 134.62 101.6)))
  (wire (pts (xy 81.28 99.06) (xy 96.52 99.06)))
  (text "Must be Blue !\nNeed High Vf !" (at 269.24 160.02 0))
  (text "f_c_lo = 13.6 Hz\nf_c_hi = 106 Hz\n\n(Dual pole RC with different first resistor)"
    (at 198.12 25.4 0)
  )
  (label "clk_tune_hi" (at 96.52 66.04 180))
  (label "gpio1" (at 96.52 109.22 180))
  (label "~{creset}" (at 200.66 132.08 0))
  (label "flash_miso" (at 96.52 119.38 180))
  (label "i2c_sda" (at 96.52 76.2 180))
  (label "gpio0" (at 96.52 106.68 180))
  (label "flash_sck" (at 200.66 119.38 0))
  (label "e1_led_rclk" (at 134.62 147.32 0))
  (label "cdone" (at 134.62 101.6 0))
  (label "usb_pu_i" (at 96.52 99.06 180))
  (label "e1_led0" (at 177.8 93.98 180))
  (label "i2c_scl" (at 137.16 187.96 0))
  (label "~{boot_sw}" (at 154.94 147.32 0))
  (label "i2c_scl" (at 96.52 73.66 180))
  (label "dbg_tx_i" (at 96.52 101.6 180))
  (label "clk_30m72" (at 96.52 63.5 180))
  (label "e1_led4" (at 177.8 104.14 180))
  (label "dbg_rx_i" (at 96.52 104.14 180))
  (label "gpio2" (at 96.52 111.76 180))
  (label "flash_mosi" (at 134.62 93.98 0))
  (label "e1_led2" (at 177.8 99.06 180))
  (label "usb_pu_i" (at 116.84 25.4 0))
  (label "~{flash_cs}" (at 96.52 124.46 180))
  (label "dbg_rx_i" (at 116.84 50.8 0))
  (label "cdone" (at 96.52 83.82 180))
  (label "~{flash_cs}" (at 200.66 121.92 0))
  (label "clk_tune_lo" (at 193.04 40.64 0))
  (label "e1_led6" (at 177.8 109.22 180))
  (label "usb_dp_i" (at 116.84 30.48 0))
  (label "cdone" (at 200.66 129.54 0))
  (label "flash_mosi" (at 96.52 116.84 180))
  (label "e1_led7" (at 177.8 111.76 180))
  (label "flash_mosi" (at 200.66 109.22 0))
  (label "e1_led_rclk" (at 96.52 114.3 180))
  (label "~{creset}" (at 96.52 86.36 180))
  (label "usb_dn_i" (at 96.52 93.98 180))
  (label "flash_miso" (at 200.66 111.76 0))
  (label "clk_tune_hi" (at 193.04 45.72 0))
  (label "flash_sck" (at 134.62 99.06 0))
  (label "e1_led5" (at 177.8 106.68 180))
  (label "clk_30m72" (at 276.86 43.18 180))
  (label "clk_tune_lo" (at 96.52 68.58 180))
  (label "i2c_sda" (at 137.16 185.42 0))
  (label "flash_sck" (at 96.52 121.92 180))
  (label "e1_led_rclk" (at 134.62 106.68 0))
  (label "usb_dn_i" (at 116.84 33.02 0))
  (label "dbg_tx_i" (at 116.84 48.26 0))
  (label "e1_led3" (at 177.8 101.6 180))
  (label "usb_dp_i" (at 96.52 96.52 180))
  (label "e1_led1" (at 177.8 96.52 180))
  (hierarchical_label "dbg_rx" (shape input) (at 177.8 45.72 0))
  (hierarchical_label "e1B_rx_hi_p" (shape input) (at 96.52 134.62 0))
  (hierarchical_label "e1A_tx_hi" (shape output) (at 96.52 160.02 0))
  (hierarchical_label "e1A_rx_lo_n" (shape input) (at 96.52 144.78 0))
  (hierarchical_label "e1A_tx_lo" (shape output) (at 96.52 157.48 0))
  (hierarchical_label "usb_dn" (shape bidirectional) (at 177.8 40.64 0))
  (hierarchical_label "dbg_tx" (shape output) (at 177.8 43.18 0))
  (hierarchical_label "e1B_rx_lo_n" (shape input) (at 96.52 137.16 0))
  (hierarchical_label "e1_rx_bias0" (shape output) (at 96.52 142.24 0))
  (hierarchical_label "e1B_tx_hi" (shape output) (at 96.52 149.86 0))
  (hierarchical_label "gpio[0..2]" (shape bidirectional) (at 111.76 116.84 0))
  (hierarchical_label "gps_rx" (shape input) (at 96.52 60.96 0))
  (hierarchical_label "e1A_rx_hi_n" (shape input) (at 96.52 162.56 0))
  (hierarchical_label "i2c_scl" (shape bidirectional) (at 96.52 73.66 0))
  (hierarchical_label "gps_pps" (shape input) (at 96.52 71.12 0))
  (hierarchical_label "e1B_tx_lo" (shape output) (at 96.52 152.4 0))
  (hierarchical_label "e1B_rx_lo_p" (shape input) (at 96.52 139.7 0))
  (hierarchical_label "e1A_rx_hi_p" (shape input) (at 96.52 165.1 0))
  (hierarchical_label "usb_dp" (shape bidirectional) (at 177.8 38.1 0))
  (hierarchical_label "e1A_rx_lo_p" (shape input) (at 96.52 147.32 0))
  (hierarchical_label "e1_led[0..7]" (shape output) (at 185.42 88.9 0))
  (hierarchical_label "gps_tx" (shape output) (at 96.52 58.42 0))
  (hierarchical_label "e1B_rx_hi_n" (shape input) (at 96.52 132.08 0))
  (hierarchical_label "e1_rx_bias1" (shape output) (at 96.52 154.94 0))
  (hierarchical_label "~{gps_reset}" (shape tri_state) (at 96.52 91.44 0))
  (hierarchical_label "i2c_sda" (shape bidirectional) (at 96.52 76.2 0))
  (symbol (lib_id "power:GND") (at 58.42 187.96 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR014" (id 0) (at 58.42 194.31 0))
    (property "Value" "GND" (id 1) (at 58.547 192.3542 0))
    (property "Footprint" "" (id 2) (at 58.42 187.96 0))
    (property "Datasheet" "" (id 3) (at 58.42 187.96 0))
    (pin "1")
  )
  (symbol (lib_id "s47-chips:ICE40UP5K-SG48") (at 58.42 116.84 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U1" (id 0) (at 38.1 187.96 0))
    (property "Value" "ICE40UP5K-SG48" (id 1) (at 38.1 185.42 0))
    (property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm" (id 2) (at 58.42 194.31 0))
    (property "Datasheet" "" (id 3) (at 66.04 78.74 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "s47-chips:SPI_FLASH_8P") (at 248.92 114.3 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U5" (id 0) (at 248.92 102.4382 0))
    (property "Value" "W25Q80" (id 1) (at 248.92 104.7496 0))
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 248.92 114.3 0))
    (property "Datasheet" "" (id 3) (at 248.92 114.3 0))
    (property "MPN" "W25Q80DVSNIG" (id 4) (at 248.92 114.3 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "s47-device:LED_RBAG") (at 93.98 175.26 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D1" (id 0) (at 93.98 185.42 0))
    (property "Value" "STATUS" (id 1) (at 93.98 187.96 0))
    (property "Footprint" "s47-device:LED_RGB_2020" (id 2) (at 93.98 176.53 0))
    (property "Datasheet" "~" (id 3) (at 93.98 176.53 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "s47-misc:LightPipe") (at 111.76 180.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "LP1" (id 0) (at 117.5512 179.1716 0))
    (property "Value" "LightPipe" (id 1) (at 117.5512 181.483 0))
    (property "Footprint" "s47-misc:LUMEX_LPF-C011303S" (id 2) (at 111.76 180.34 0))
    (property "Datasheet" "" (id 3) (at 111.76 180.34 0))
  )
  (symbol (lib_id "Switch:SW_Push") (at 172.72 147.32 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW1" (id 0) (at 172.72 140.081 0))
    (property "Value" "SW_Push" (id 1) (at 172.72 142.3924 0))
    (property "Footprint" "s47-misc:SW_HYP_1TS003B" (id 2) (at 172.72 142.24 0))
    (property "Datasheet" "~" (id 3) (at 172.72 142.24 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "s47-device:VCXO_6_TUNE_OE") (at 248.92 43.18 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U4" (id 0) (at 254 30.48 0))
    (property "Value" "30M72" (id 1) (at 254 33.02 0))
    (property "Footprint" "s47-misc:Oscillator_SMD_VCXO-6Pin_7.0x5.0mm_P2.54mm" (id 2) (at 248.92 43.18 0))
    (property "Datasheet" "" (id 3) (at 248.92 43.18 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "6")
  )
  (symbol (lib_id "power:+3V3") (at 101.6 172.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR016" (id 0) (at 101.6 176.53 0))
    (property "Value" "+3V3" (id 1) (at 101.981 168.3258 0))
    (property "Footprint" "" (id 2) (at 101.6 172.72 0))
    (property "Datasheet" "" (id 3) (at 101.6 172.72 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3V3") (at 25.4 22.86 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR09" (id 0) (at 25.4 26.67 0))
    (property "Value" "+3V3" (id 1) (at 25.781 18.4658 0))
    (property "Footprint" "" (id 2) (at 25.4 22.86 0))
    (property "Datasheet" "" (id 3) (at 25.4 22.86 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 33.02 63.5 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C2" (id 0) (at 30.6832 62.3316 0))
    (property "Value" "100n" (id 1) (at 30.6832 64.643 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 33.02 63.5 0))
    (property "Datasheet" "~" (id 3) (at 33.02 63.5 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 33.02 68.58 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR010" (id 0) (at 33.02 74.93 0))
    (property "Value" "GND" (id 1) (at 33.147 72.9742 0))
    (property "Footprint" "" (id 2) (at 33.02 68.58 0))
    (property "Datasheet" "" (id 3) (at 33.02 68.58 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 33.02 88.9 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C3" (id 0) (at 30.6832 87.7316 0))
    (property "Value" "100n" (id 1) (at 30.6832 90.043 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 33.02 88.9 0))
    (property "Datasheet" "~" (id 3) (at 33.02 88.9 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 33.02 137.16 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C4" (id 0) (at 30.6832 135.9916 0))
    (property "Value" "100n" (id 1) (at 30.6832 138.303 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 33.02 137.16 0))
    (property "Datasheet" "~" (id 3) (at 33.02 137.16 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 33.02 93.98 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR011" (id 0) (at 33.02 100.33 0))
    (property "Value" "GND" (id 1) (at 33.147 98.3742 0))
    (property "Footprint" "" (id 2) (at 33.02 93.98 0))
    (property "Datasheet" "" (id 3) (at 33.02 93.98 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 33.02 142.24 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR012" (id 0) (at 33.02 148.59 0))
    (property "Value" "GND" (id 1) (at 33.147 146.6342 0))
    (property "Footprint" "" (id 2) (at 33.02 142.24 0))
    (property "Datasheet" "" (id 3) (at 33.02 142.24 0))
    (pin "1")
  )
  (symbol (lib_id "power:+1V2") (at 55.88 22.86 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR013" (id 0) (at 55.88 26.67 0))
    (property "Value" "+1V2" (id 1) (at 56.261 18.4658 0))
    (property "Footprint" "" (id 2) (at 55.88 22.86 0))
    (property "Datasheet" "" (id 3) (at 55.88 22.86 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 81.28 40.64 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C5" (id 0) (at 81.28 43.18 0))
    (property "Value" "1u" (id 1) (at 83.82 39.37 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 81.28 40.64 0))
    (property "Datasheet" "~" (id 3) (at 81.28 40.64 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 86.36 40.64 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C6" (id 0) (at 86.36 43.18 0))
    (property "Value" "100n" (id 1) (at 88.9 39.37 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 86.36 40.64 0))
    (property "Datasheet" "~" (id 3) (at 86.36 40.64 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 91.44 40.64 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C7" (id 0) (at 91.44 43.18 0))
    (property "Value" "100n" (id 1) (at 93.98 39.37 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 91.44 40.64 0))
    (property "Datasheet" "~" (id 3) (at 91.44 40.64 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 96.52 40.64 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C8" (id 0) (at 96.52 43.18 0))
    (property "Value" "100n" (id 1) (at 99.06 39.37 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 96.52 40.64 0))
    (property "Datasheet" "~" (id 3) (at 96.52 40.64 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small") (at 55.88 30.48 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R4" (id 0) (at 54.4068 29.3116 0))
    (property "Value" "120R" (id 1) (at 54.4068 31.623 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 55.88 30.48 0))
    (property "Datasheet" "~" (id 3) (at 55.88 30.48 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 96.52 48.26 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR015" (id 0) (at 96.52 54.61 0))
    (property "Value" "GND" (id 1) (at 96.647 52.6542 0))
    (property "Footprint" "" (id 2) (at 96.52 48.26 0))
    (property "Datasheet" "" (id 3) (at 96.52 48.26 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 248.92 55.88 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR031" (id 0) (at 248.92 62.23 0))
    (property "Value" "GND" (id 1) (at 249.047 60.2742 0))
    (property "Footprint" "" (id 2) (at 248.92 55.88 0))
    (property "Datasheet" "" (id 3) (at 248.92 55.88 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3V3") (at 248.92 27.94 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR030" (id 0) (at 248.92 31.75 0))
    (property "Value" "+3V3" (id 1) (at 249.301 23.5458 0))
    (property "Footprint" "" (id 2) (at 248.92 27.94 0))
    (property "Datasheet" "" (id 3) (at 248.92 27.94 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3V3") (at 261.62 86.36 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR034" (id 0) (at 261.62 90.17 0))
    (property "Value" "+3V3" (id 1) (at 262.001 81.9658 0))
    (property "Footprint" "" (id 2) (at 261.62 86.36 0))
    (property "Datasheet" "" (id 3) (at 261.62 86.36 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 261.62 124.46 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR035" (id 0) (at 261.62 130.81 0))
    (property "Value" "GND" (id 1) (at 261.747 128.8542 0))
    (property "Footprint" "" (id 2) (at 261.62 124.46 0))
    (property "Datasheet" "" (id 3) (at 261.62 124.46 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 261.62 116.84 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C13" (id 0) (at 263.9568 115.6716 0))
    (property "Value" "100n" (id 1) (at 263.9568 117.983 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 261.62 116.84 0))
    (property "Datasheet" "~" (id 3) (at 261.62 116.84 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector_Generic:Conn_02x04_Odd_Even") (at 246.38 147.32 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J3" (id 0) (at 245.11 136.525 0))
    (property "Value" "SPI" (id 1) (at 245.11 138.8364 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" (id 2) (at 246.38 147.32 0))
    (property "Datasheet" "~" (id 3) (at 246.38 147.32 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "power:GND") (at 254 157.48 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR033" (id 0) (at 254 163.83 0))
    (property "Value" "GND" (id 1) (at 254.127 161.8742 0))
    (property "Footprint" "" (id 2) (at 254 157.48 0))
    (property "Datasheet" "" (id 3) (at 254 157.48 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3V3") (at 254 139.7 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR032" (id 0) (at 254 143.51 0))
    (property "Value" "+3V3" (id 1) (at 254.381 135.3058 0))
    (property "Footprint" "" (id 2) (at 254 139.7 0))
    (property "Datasheet" "" (id 3) (at 254 139.7 0))
    (pin "1")
  )
  (symbol (lib_id "s47-chips:IP4220CZ6") (at 142.24 40.64 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U2" (id 0) (at 148.082 39.4716 0))
    (property "Value" "IP4220CZ6" (id 1) (at 148.082 41.783 0))
    (property "Footprint" "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm" (id 2) (at 143.51 38.735 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/IP4220CZ6.pdf" (id 3) (at 143.51 38.735 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "power:GND") (at 236.22 55.88 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR028" (id 0) (at 236.22 62.23 0))
    (property "Value" "GND" (id 1) (at 236.347 60.2742 0))
    (property "Footprint" "" (id 2) (at 236.22 55.88 0))
    (property "Datasheet" "" (id 3) (at 236.22 55.88 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 236.22 50.8 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C12" (id 0) (at 233.8832 49.6316 0))
    (property "Value" "100n" (id 1) (at 233.8832 51.943 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 236.22 50.8 0))
    (property "Datasheet" "~" (id 3) (at 236.22 50.8 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 215.9 50.8 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C10" (id 0) (at 213.5632 49.6316 0))
    (property "Value" "1u" (id 1) (at 213.5632 51.943 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 215.9 50.8 0))
    (property "Datasheet" "~" (id 3) (at 215.9 50.8 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 226.06 50.8 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C11" (id 0) (at 223.7486 49.6316 0))
    (property "Value" "1u" (id 1) (at 223.7486 51.943 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 226.06 50.8 0))
    (property "Datasheet" "~" (id 3) (at 226.06 50.8 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small") (at 220.98 45.72 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R11" (id 0) (at 220.98 40.7416 90))
    (property "Value" "1k5" (id 1) (at 220.98 43.053 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 220.98 45.72 0))
    (property "Datasheet" "~" (id 3) (at 220.98 45.72 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small") (at 208.28 40.64 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R9" (id 0) (at 208.28 35.6616 90))
    (property "Value" "91k" (id 1) (at 208.28 37.973 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 208.28 40.64 0))
    (property "Datasheet" "~" (id 3) (at 208.28 40.64 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small") (at 208.28 45.72 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R10" (id 0) (at 205.74 48.26 90))
    (property "Value" "1k5" (id 1) (at 205.74 50.8 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 208.28 45.72 0))
    (property "Datasheet" "~" (id 3) (at 208.28 45.72 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 226.06 55.88 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR027" (id 0) (at 226.06 62.23 0))
    (property "Value" "GND" (id 1) (at 226.187 60.2742 0))
    (property "Footprint" "" (id 2) (at 226.06 55.88 0))
    (property "Datasheet" "" (id 3) (at 226.06 55.88 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 215.9 55.88 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR025" (id 0) (at 215.9 62.23 0))
    (property "Value" "GND" (id 1) (at 216.027 60.2742 0))
    (property "Footprint" "" (id 2) (at 215.9 55.88 0))
    (property "Datasheet" "" (id 3) (at 215.9 55.88 0))
    (pin "1")
  )
  (symbol (lib_id "power:PWR_FLAG") (at 48.26 33.02 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#FLG01" (id 0) (at 48.26 31.115 0))
    (property "Value" "PWR_FLAG" (id 1) (at 48.26 28.6258 0))
    (property "Footprint" "" (id 2) (at 48.26 33.02 0))
    (property "Datasheet" "~" (id 3) (at 48.26 33.02 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small") (at 147.32 180.34 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R6" (id 0) (at 145.8468 179.1716 0))
    (property "Value" "5k1" (id 1) (at 145.8468 181.483 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 147.32 180.34 0))
    (property "Datasheet" "~" (id 3) (at 147.32 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small") (at 149.86 180.34 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R8" (id 0) (at 151.3586 179.1716 0))
    (property "Value" "5k1" (id 1) (at 151.3586 181.483 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 149.86 180.34 0))
    (property "Datasheet" "~" (id 3) (at 149.86 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+3V3") (at 147.32 172.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR020" (id 0) (at 147.32 176.53 0))
    (property "Value" "+3V3" (id 1) (at 147.701 168.3258 0))
    (property "Footprint" "" (id 2) (at 147.32 172.72 0))
    (property "Datasheet" "" (id 3) (at 147.32 172.72 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04") (at 220.98 96.52 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN4" (id 0) (at 225.7552 95.3516 0))
    (property "Value" "10k" (id 1) (at 225.7552 97.663 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x0603" (id 2) (at 227.965 96.52 90))
    (property "Datasheet" "~" (id 3) (at 220.98 96.52 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "Device:R_Small") (at 264.16 43.18 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R12" (id 0) (at 264.16 38.2016 90))
    (property "Value" "27R" (id 1) (at 264.16 40.513 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 264.16 43.18 0))
    (property "Datasheet" "~" (id 3) (at 264.16 43.18 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+3V3") (at 236.22 86.36 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR029" (id 0) (at 236.22 90.17 0))
    (property "Value" "+3V3" (id 1) (at 236.601 81.9658 0))
    (property "Footprint" "" (id 2) (at 236.22 86.36 0))
    (property "Datasheet" "" (id 3) (at 236.22 86.36 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3V3") (at 223.52 86.36 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR026" (id 0) (at 223.52 90.17 0))
    (property "Value" "+3V3" (id 1) (at 223.901 81.9658 0))
    (property "Footprint" "" (id 2) (at 223.52 86.36 0))
    (property "Datasheet" "" (id 3) (at 223.52 86.36 0))
    (pin "1")
  )
  (symbol (lib_id "Device:LED_Small") (at 264.16 152.4 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D2" (id 0) (at 265.8872 151.2316 90))
    (property "Value" "DONE" (id 1) (at 265.8872 153.543 90))
    (property "Footprint" "LED_SMD:LED_0603_1608Metric" (id 2) (at 264.16 152.4 90))
    (property "Datasheet" "~" (id 3) (at 264.16 152.4 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 264.16 157.48 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR036" (id 0) (at 264.16 163.83 0))
    (property "Value" "GND" (id 1) (at 264.287 161.8742 0))
    (property "Footprint" "" (id 2) (at 264.16 157.48 0))
    (property "Datasheet" "" (id 3) (at 264.16 157.48 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 180.34 149.86 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR024" (id 0) (at 180.34 156.21 0))
    (property "Value" "GND" (id 1) (at 180.467 154.2542 0))
    (property "Footprint" "" (id 2) (at 180.34 149.86 0))
    (property "Datasheet" "" (id 3) (at 180.34 149.86 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small") (at 149.86 147.32 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R7" (id 0) (at 149.86 142.3416 90))
    (property "Value" "1k5" (id 1) (at 149.86 144.653 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 149.86 147.32 0))
    (property "Datasheet" "~" (id 3) (at 149.86 147.32 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 142.24 53.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR018" (id 0) (at 142.24 59.69 0))
    (property "Value" "GND" (id 1) (at 142.367 57.7342 0))
    (property "Footprint" "" (id 2) (at 142.24 53.34 0))
    (property "Datasheet" "" (id 3) (at 142.24 53.34 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 142.24 25.4 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR017" (id 0) (at 142.24 29.21 0))
    (property "Value" "+5V" (id 1) (at 142.621 21.0058 0))
    (property "Footprint" "" (id 2) (at 142.24 25.4 0))
    (property "Datasheet" "" (id 3) (at 142.24 25.4 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04") (at 167.64 40.64 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN3" (id 0) (at 167.64 51.2318 90))
    (property "Value" "33R" (id 1) (at 167.64 48.9204 90))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x0603" (id 2) (at 167.64 33.655 90))
    (property "Datasheet" "~" (id 3) (at 167.64 40.64 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "Device:R_Small") (at 129.54 25.4 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R5" (id 0) (at 129.54 20.4216 90))
    (property "Value" "1k5" (id 1) (at 129.54 22.733 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 129.54 25.4 0))
    (property "Datasheet" "~" (id 3) (at 129.54 25.4 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74HC595") (at 157.48 104.14 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U3" (id 0) (at 165.1 86.36 0))
    (property "Value" "74HC595" (id 1) (at 165.1 88.9 0))
    (property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (id 2) (at 157.48 104.14 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc595.pdf" (id 3) (at 157.48 104.14 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "power:GND") (at 157.48 124.46 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR023" (id 0) (at 157.48 130.81 0))
    (property "Value" "GND" (id 1) (at 157.607 128.8542 0))
    (property "Footprint" "" (id 2) (at 157.48 124.46 0))
    (property "Datasheet" "" (id 3) (at 157.48 124.46 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3V3") (at 157.48 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR022" (id 0) (at 157.48 77.47 0))
    (property "Value" "+3V3" (id 1) (at 157.861 69.2658 0))
    (property "Footprint" "" (id 2) (at 157.48 73.66 0))
    (property "Datasheet" "" (id 3) (at 157.48 73.66 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 152.4 81.28 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C9" (id 0) (at 150.0632 80.1116 0))
    (property "Value" "100n" (id 1) (at 150.0632 82.423 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 152.4 81.28 0))
    (property "Datasheet" "~" (id 3) (at 152.4 81.28 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 152.4 86.36 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR021" (id 0) (at 152.4 92.71 0))
    (property "Value" "GND" (id 1) (at 149.86 88.9 0))
    (property "Footprint" "" (id 2) (at 152.4 86.36 0))
    (property "Datasheet" "" (id 3) (at 152.4 86.36 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 144.78 124.46 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR019" (id 0) (at 144.78 130.81 0))
    (property "Value" "GND" (id 1) (at 144.907 128.8542 0))
    (property "Footprint" "" (id 2) (at 144.78 124.46 0))
    (property "Datasheet" "" (id 3) (at 144.78 124.46 0))
    (pin "1")
  )
)
