+ CONFIG=generic
+ SITE_ID=1235
+ TRX_NUM=1
+ BTS_FEATURES=-fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX
+ respawn.sh osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
respawn: 0: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;31mDLINP[0;m[38;5;23m stream_cli.c:444 CLICONN(ts-0-1-oml,){CONNECTING} connect failed (-111)[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x562cc6d35290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44395){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x562cc6d34990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x562cc6d34990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x562cc6d34990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 0: stopped pid 9858 with status 0
respawn: 1: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5604221f1290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39635){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5604221f0990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5604221f0990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5604221f0990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 1: stopped pid 10359 with status 0
respawn: 2: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55a6054b6290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46189){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55a6054b5990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55a6054b5990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55a6054b5990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 2: stopped pid 10446 with status 0
respawn: 3: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56472aed6290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41257){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56472aed5990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56472aed5990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56472aed5990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 3: stopped pid 18313 with status 0
respawn: 4: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55fa655bf290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38341){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55fa655be990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55fa655be990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55fa655be990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 4: stopped pid 18395 with status 0
respawn: 5: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56053e3cb290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40567){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56053e3ca990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56053e3ca990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56053e3ca990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 5: stopped pid 18477 with status 0
respawn: 6: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56241122f290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42975){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56241122e990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56241122e990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56241122e990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 6: stopped pid 18561 with status 0
respawn: 7: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56207b35a290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41373){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56207b359990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56207b359990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56207b359990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 7: stopped pid 18645 with status 0
respawn: 8: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x559c923cc290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35713){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x559c923cb990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x559c923cb990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x559c923cb990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 8: stopped pid 18727 with status 0
respawn: 9: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b180825290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33611){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b180824990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b180824990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b180824990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 9: stopped pid 18811 with status 0
respawn: 10: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x563d4d8f9290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38799){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x563d4d8f8990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x563d4d8f8990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x563d4d8f8990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 10: stopped pid 18895 with status 0
respawn: 11: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x556fd54a4290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41319){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x556fd54a3990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x556fd54a3990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x556fd54a3990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 11: stopped pid 18977 with status 0
respawn: 12: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x560c34f30290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40745){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x560c34f2f990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x560c34f2f990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x560c34f2f990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 12: stopped pid 19062 with status 0
respawn: 13: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x560f0c87e290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36301){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x560f0c87d990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x560f0c87d990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x560f0c87d990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 13: stopped pid 19142 with status 0
respawn: 14: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b96ba39290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46741){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b96ba38990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b96ba38990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b96ba38990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 14: stopped pid 19226 with status 0
respawn: 15: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55eff68b3290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46247){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55eff68b2990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55eff68b2990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55eff68b2990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 15: stopped pid 19299 with status 0
respawn: 16: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55596391c290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38165){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55596391b990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55596391b990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55596391b990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 16: stopped pid 19370 with status 0
respawn: 17: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c4ad969290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46385){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c4ad968990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c4ad968990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c4ad968990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 17: stopped pid 19448 with status 0
respawn: 18: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b840310290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39889){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b84030f990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b84030f990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b84030f990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 18: stopped pid 19534 with status 0
respawn: 19: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d009114290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33737){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d009113990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d009113990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d009113990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 19: stopped pid 19609 with status 0
respawn: 20: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ce684c2290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46129){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ce684c1990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ce684c1990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ce684c1990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 20: stopped pid 19685 with status 0
respawn: 21: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ecfe1d4290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35823){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ecfe1d3990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ecfe1d3990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ecfe1d3990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 21: stopped pid 19762 with status 0
respawn: 22: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55a56adee290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39885){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55a56aded990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55a56aded990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55a56aded990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 22: stopped pid 19844 with status 0
respawn: 23: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e16d6c2290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43741){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e16d6c1990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e16d6c1990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e16d6c1990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 23: stopped pid 19924 with status 0
respawn: 24: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55a060b88290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41163){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55a060b87990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55a060b87990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55a060b87990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 24: stopped pid 20237 with status 0
respawn: 25: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55f540ac0290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36635){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55f540abf990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55f540abf990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55f540abf990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 25: stopped pid 20987 with status 0
respawn: 26: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55742dad5290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38661){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55742dad4990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55742dad4990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55742dad4990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 26: stopped pid 21063 with status 0
respawn: 27: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x557c8ed41290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38231){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x557c8ed40990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x557c8ed40990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x557c8ed40990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 27: stopped pid 21145 with status 0
respawn: 28: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d4a8780290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40811){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d4a877f990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d4a877f990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d4a877f990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 28: stopped pid 21222 with status 0
respawn: 29: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561c53bc1290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38297){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561c53bc0990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561c53bc0990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561c53bc0990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 29: stopped pid 21300 with status 0
respawn: 30: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e4c7b05290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35199){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e4c7b04990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e4c7b04990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e4c7b04990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 30: stopped pid 21377 with status 0
respawn: 31: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5597ee774290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44217){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5597ee773990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5597ee773990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5597ee773990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 31: stopped pid 23262 with status 0
respawn: 32: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x562fc1711290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39435){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x562fc1710990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x562fc1710990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x562fc1710990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 32: stopped pid 23351 with status 0
respawn: 33: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55840dee9290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36173){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55840dee8990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55840dee8990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55840dee8990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 33: stopped pid 23443 with status 0
respawn: 34: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x559d06dd7290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44337){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x559d06dd6990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x559d06dd6990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x559d06dd6990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 34: stopped pid 23538 with status 0
respawn: 35: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c2a9131290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35431){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c2a9130990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c2a9130990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c2a9130990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 35: stopped pid 23627 with status 0
respawn: 36: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x559af48c3290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41667){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x559af48c2990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x559af48c2990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x559af48c2990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 36: stopped pid 23718 with status 0
respawn: 37: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x563ea61d3290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36841){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x563ea61d2990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x563ea61d2990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x563ea61d2990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 37: stopped pid 23810 with status 0
respawn: 38: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e5e525c290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36181){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e5e525b990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e5e525b990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e5e525b990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 38: stopped pid 23890 with status 0
respawn: 39: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55580040f290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35745){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55580040e990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55580040e990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55580040e990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 39: stopped pid 23975 with status 0
respawn: 40: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b73ae64290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41469){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b73ae63990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b73ae63990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b73ae63990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 40: stopped pid 24064 with status 0
respawn: 41: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5642ed2b3290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45479){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5642ed2b2990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5642ed2b2990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5642ed2b2990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 41: stopped pid 25134 with status 0
respawn: 42: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x563ebab86290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42651){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x563ebab85990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x563ebab85990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x563ebab85990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 42: stopped pid 25232 with status 0
respawn: 43: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x558855ad4290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37057){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x558855ad3990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x558855ad3990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x558855ad3990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 43: stopped pid 25326 with status 0
respawn: 44: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x564879d84290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40051){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x564879d83990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x564879d83990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x564879d83990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 44: stopped pid 25422 with status 0
respawn: 45: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56476843d290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35627){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56476843c990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56476843c990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56476843c990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 45: stopped pid 25514 with status 0
respawn: 46: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55eb9f8e2290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41805){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55eb9f8e1990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55eb9f8e1990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55eb9f8e1990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 46: stopped pid 25605 with status 0
respawn: 47: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x562953ce8290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39031){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x562953ce7990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x562953ce7990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x562953ce7990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 47: stopped pid 25706 with status 0
respawn: 48: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c452fef290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39729){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c452fee990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c452fee990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c452fee990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 48: stopped pid 25801 with status 0
respawn: 49: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x563ece440290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40965){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x563ece43f990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x563ece43f990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x563ece43f990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 49: stopped pid 26051 with status 0
respawn: 50: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x555fa3d5d290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43041){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x555fa3d5c990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x555fa3d5c990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x555fa3d5c990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 50: stopped pid 26149 with status 0
respawn: 51: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x564acf447290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46463){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x564acf446990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x564acf446990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x564acf446990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 51: stopped pid 26246 with status 0
respawn: 52: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x564c96640290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41649){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x564c9663f990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x564c9663f990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x564c9663f990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 52: stopped pid 26340 with status 0
respawn: 53: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ac81e50290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33269){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;31mDABIS[0;m abis.c:105 OML link was closed early within 4 seconds. If this situation persists, please check your BTS and BSC configuration files for errors. A common error is a mismatch between unit_id configuration parameters of BTS and BSC.
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ac81e4f990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ac81e4f990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ac81e4f990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 53: stopped pid 27144 with status 0
respawn: 54: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x556ba31a6290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37135){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x556ba31a5990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x556ba31a5990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x556ba31a5990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 54: stopped pid 27163 with status 0
respawn: 55: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x565172ba5290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41513){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x565172ba4990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x565172ba4990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x565172ba4990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 55: stopped pid 27901 with status 0
respawn: 56: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55561bb74290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Unlocked -> Locked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1486 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM state already was Locked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33131){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55561bb73990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55561bb73990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55561bb73990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 56: stopped pid 28554 with status 0
respawn: 57: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561b7b804290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38081){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561b7b803990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561b7b803990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561b7b803990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 57: stopped pid 28980 with status 0
respawn: 58: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ba2aeb5290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43001){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ba2aeb4990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ba2aeb4990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ba2aeb4990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 58: stopped pid 29369 with status 0
respawn: 59: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c86550b290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38885){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c86550a990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c86550a990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c86550a990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 59: stopped pid 29457 with status 0
respawn: 60: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x556e57b00290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45583){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x556e57aff990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x556e57aff990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x556e57aff990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 60: stopped pid 29535 with status 0
respawn: 61: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ad5fd28290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34305){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;31mDABIS[0;m abis.c:105 OML link was closed early within 9 seconds. If this situation persists, please check your BTS and BSC configuration files for errors. A common error is a mismatch between unit_id configuration parameters of BTS and BSC.
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ad5fd27990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ad5fd27990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ad5fd27990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 61: stopped pid 31249 with status 0
respawn: 62: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5641da80c290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46147){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5641da80b990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5641da80b990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5641da80b990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 62: stopped pid 31323 with status 0
respawn: 63: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x558f7b960290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42777){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x558f7b95f990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x558f7b95f990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x558f7b95f990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 63: stopped pid 31401 with status 0
respawn: 64: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x562af873e290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36865){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x562af873d990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x562af873d990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x562af873d990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 64: stopped pid 31480 with status 0
respawn: 65: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55850b96e290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41021){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55850b96d990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55850b96d990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55850b96d990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 65: stopped pid 31560 with status 0
respawn: 66: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561a7a49f290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39961){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561a7a49e990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561a7a49e990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561a7a49e990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 66: stopped pid 31640 with status 0
respawn: 67: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55de0f582290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34853){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55de0f581990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55de0f581990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55de0f581990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 67: stopped pid 31718 with status 0
respawn: 68: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55a0e65bf290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41451){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55a0e65be990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55a0e65be990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55a0e65be990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 68: stopped pid 31807 with status 0
respawn: 69: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5555bc308290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33433){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5555bc307990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5555bc307990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5555bc307990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 69: stopped pid 31888 with status 0
respawn: 70: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561e2ef53290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38121){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561e2ef52990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561e2ef52990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561e2ef52990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 70: stopped pid 31971 with status 0
respawn: 71: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e717fac290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42791){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e717fab990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e717fab990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e717fab990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 71: stopped pid 32052 with status 0
respawn: 72: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55dd8faf8290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45447){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55dd8faf7990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55dd8faf7990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55dd8faf7990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 72: stopped pid 32131 with status 0
respawn: 73: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55fb55dba290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42785){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55fb55db9990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55fb55db9990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55fb55db9990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 73: stopped pid 32212 with status 0
respawn: 74: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b63bc43290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44097){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b63bc42990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b63bc42990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b63bc42990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 74: stopped pid 32289 with status 0
respawn: 75: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d454562290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33381){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d454561990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d454561990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d454561990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 75: stopped pid 32373 with status 0
respawn: 76: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x556f6268f290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37571){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x556f6268e990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x556f6268e990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x556f6268e990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 76: stopped pid 32453 with status 0
respawn: 77: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5607aa06c290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39705){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5607aa06b990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5607aa06b990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5607aa06b990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 77: stopped pid 32546 with status 0
respawn: 78: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x560b11220290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44141){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x560b1121f990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x560b1121f990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x560b1121f990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 78: stopped pid 32620 with status 0
respawn: 79: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c9ae992290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42779){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c9ae991990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c9ae991990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c9ae991990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 79: stopped pid 32697 with status 0
respawn: 80: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e353eb3290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38887){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e353eb2990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e353eb2990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e353eb2990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 80: stopped pid 32773 with status 0
respawn: 81: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5584e8e22290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40069){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5584e8e21990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5584e8e21990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5584e8e21990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 81: stopped pid 32855 with status 0
respawn: 82: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x562616f15290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37449){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x562616f14990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x562616f14990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x562616f14990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 82: stopped pid 32932 with status 0
respawn: 83: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5564262d2290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40393){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5564262d1990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5564262d1990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5564262d1990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 83: stopped pid 33011 with status 0
respawn: 84: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x556a7c114290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44079){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x556a7c113990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x556a7c113990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x556a7c113990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 84: stopped pid 33092 with status 0
respawn: 85: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5594c159c290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46431){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5594c159b990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5594c159b990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5594c159b990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 85: stopped pid 33170 with status 0
respawn: 86: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x555d21933290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36389){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x555d21932990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x555d21932990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x555d21932990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 86: stopped pid 33250 with status 0
respawn: 87: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c470ec4290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36681){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c470ec3990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c470ec3990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c470ec3990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 87: stopped pid 33328 with status 0
respawn: 88: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5583fd576290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35295){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5583fd575990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5583fd575990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5583fd575990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 88: stopped pid 33405 with status 0
respawn: 89: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5623fe42c290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42925){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5623fe42b990]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5623fe42b990]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5623fe42b990]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 89: stopped pid 33480 with status 0
respawn: 90: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1086 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d605ba8290]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
