(kicad_pcb (version 20171130) (host pcbnew 5.1.5)
  (general
    (thickness 1.6)
    (drawings 79)
    (tracks 1784)
    (zones 0)
    (modules 116)
    (nets 156)
  )
  (page A4)
  (title_block
    (title icE1usb)
    (date 2020-08-19)
    (rev 0.1)
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.15)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.15)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.5)
    (via_min_drill 0.25)
    (user_via 0.6 0.3)
    (user_via 1 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.2)
    (pcb_text_size 1 1)
    (mod_edge_width 0.1)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.125)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.075)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x210fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plot/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D1-Pad4)")
  (net 5 "Net-(TR1-Pad15)")
  (net 6 "Net-(TR2-Pad15)")
  (net 7 "Net-(J4-Pad2)")
  (net 8 "Net-(J5-Pad6)")
  (net 9 "Net-(J5-Pad2)")
  (net 10 "Net-(J5-Pad7)")
  (net 11 "Net-(J5-Pad3)")
  (net 12 "Net-(TR1-Pad10)")
  (net 13 "Net-(TR1-Pad7)")
  (net 14 "Net-(TR2-Pad10)")
  (net 15 "Net-(TR2-Pad7)")
  (net 16 "Net-(R3-Pad2)")
  (net 17 "Net-(R2-Pad2)")
  (net 18 /e1A_rj1)
  (net 19 /e1B_rj1)
  (net 20 "Net-(C1-Pad2)")
  (net 21 +3V3)
  (net 22 "Net-(C5-Pad1)")
  (net 23 +1V2)
  (net 24 /gps/RF)
  (net 25 /e1B_rj7)
  (net 26 /e1B_rj6)
  (net 27 /e1B_rj5)
  (net 28 /e1B_rj4)
  (net 29 /e1B_rj8)
  (net 30 /e1B_rj2)
  (net 31 /e1B_rj3)
  (net 32 /e1_led2)
  (net 33 /e1_led0)
  (net 34 /e1_led1)
  (net 35 /e1A_rj8)
  (net 36 /e1A_rj6)
  (net 37 /e1A_rj4)
  (net 38 /e1A_rj2)
  (net 39 /e1A_rj7)
  (net 40 /e1A_rj5)
  (net 41 /e1A_rj3)
  (net 42 +5V)
  (net 43 "Net-(F1-Pad2)")
  (net 44 "Net-(F2-Pad2)")
  (net 45 "Net-(F3-Pad2)")
  (net 46 "Net-(F4-Pad2)")
  (net 47 "Net-(F5-Pad2)")
  (net 48 "Net-(F6-Pad2)")
  (net 49 "Net-(F7-Pad2)")
  (net 50 "Net-(F8-Pad2)")
  (net 51 /fpga/flash_mosi)
  (net 52 /fpga/flash_miso)
  (net 53 /fpga/~creset)
  (net 54 /fpga/cdone)
  (net 55 /fpga/~flash_cs)
  (net 56 /fpga/~boot_sw)
  (net 57 /fpga/flash_sck)
  (net 58 "Net-(U10-Pad4)")
  (net 59 /usb_dn)
  (net 60 /usb_dp)
  (net 61 /dbg_rx)
  (net 62 /dbg_tx)
  (net 63 "Net-(J4-Pad7)")
  (net 64 "Net-(J4-Pad6)")
  (net 65 "Net-(J4-Pad3)")
  (net 66 /fpga/clk_tune_lo)
  (net 67 /fpga/clk_tune_hi)
  (net 68 "Net-(RN1-Pad4)")
  (net 69 "Net-(RN1-Pad2)")
  (net 70 "Net-(RN1-Pad3)")
  (net 71 "Net-(RN1-Pad1)")
  (net 72 /fpga/clk_30m72)
  (net 73 "Net-(C17-Pad1)")
  (net 74 "Net-(C10-Pad1)")
  (net 75 "Net-(J1-Pad8)")
  (net 76 "Net-(J1-Pad7)")
  (net 77 "Net-(J1-Pad6)")
  (net 78 "Net-(J1-Pad5)")
  (net 79 "Net-(J1-Pad4)")
  (net 80 "Net-(J1-Pad3)")
  (net 81 "Net-(J1-Pad2)")
  (net 82 "Net-(J1-Pad1)")
  (net 83 "Net-(RN2-Pad4)")
  (net 84 "Net-(RN2-Pad2)")
  (net 85 "Net-(RN2-Pad3)")
  (net 86 "Net-(RN2-Pad1)")
  (net 87 "Net-(U8-Pad5)")
  (net 88 /fpga/e1A_rx_hi_p)
  (net 89 /fpga/e1A_rx_hi_n)
  (net 90 /fpga/e1A_rx_lo_p)
  (net 91 /fpga/e1A_rx_lo_n)
  (net 92 /fpga/e1B_rx_lo_n)
  (net 93 /fpga/e1B_rx_lo_p)
  (net 94 /fpga/e1B_rx_hi_n)
  (net 95 /fpga/e1B_rx_hi_p)
  (net 96 /e1bias/bias_a_p)
  (net 97 /e1bias/bias_a_n)
  (net 98 /e1bias/bias_b_n)
  (net 99 /fpga/i2c_scl)
  (net 100 /gpio2)
  (net 101 /fpga/i2c_sda)
  (net 102 /gpio1)
  (net 103 /gpio0)
  (net 104 /fpga/e1A_tx_hi)
  (net 105 /fpga/e1A_tx_lo)
  (net 106 /fpga/e1B_tx_hi)
  (net 107 /fpga/e1B_tx_lo)
  (net 108 /fpga/~gps_reset)
  (net 109 /fpga/gps_pps)
  (net 110 /fpga/gps_tx)
  (net 111 /fpga/gps_rx)
  (net 112 /fpga/usb_pu_i)
  (net 113 /fpga/usb_dp_i)
  (net 114 /e1_led3)
  (net 115 /e1_led7)
  (net 116 /e1_led6)
  (net 117 /e1_led4)
  (net 118 /e1_led5)
  (net 119 /fpga/usb_dn_i)
  (net 120 /fpga/dbg_rx_i)
  (net 121 /fpga/dbg_tx_i)
  (net 122 /fpga/e1_led_rclk)
  (net 123 /gps/vbackup)
  (net 124 "Net-(D4-Pad1)")
  (net 125 "Net-(L1-Pad1)")
  (net 126 "Net-(C11-Pad1)")
  (net 127 "Net-(C16-Pad1)")
  (net 128 "Net-(C20-Pad1)")
  (net 129 "Net-(C21-Pad2)")
  (net 130 /e1bias/bias_fixed)
  (net 131 /e1bias/bias_0)
  (net 132 "Net-(C35-Pad1)")
  (net 133 "Net-(C36-Pad1)")
  (net 134 "Net-(C39-Pad1)")
  (net 135 "Net-(R16-Pad1)")
  (net 136 "Net-(R27-Pad1)")
  (net 137 /e1bias/bias1)
  (net 138 /e1bias/bias0)
  (net 139 "Net-(U3-Pad9)")
  (net 140 "Net-(U7-Pad5)")
  (net 141 "Net-(U7-Pad2)")
  (net 142 "Net-(U8-Pad18)")
  (net 143 "Net-(U8-Pad13)")
  (net 144 "Net-(U9-Pad4)")
  (net 145 "Net-(U12-Pad5)")
  (net 146 "Net-(U12-Pad2)")
  (net 147 "Net-(X4-PadB8)")
  (net 148 "Net-(X4-PadA8)")
  (net 149 "Net-(R12-Pad2)")
  (net 150 "Net-(R17-Pad1)")
  (net 151 "Net-(R28-Pad1)")
  (net 152 "Net-(RN6-Pad4)")
  (net 153 "Net-(RN6-Pad2)")
  (net 154 "Net-(RN6-Pad3)")
  (net 155 "Net-(RN6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.15)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V2)
    (add_net +3V3)
    (add_net +5V)
    (add_net /dbg_rx)
    (add_net /dbg_tx)
    (add_net /e1A_rj1)
    (add_net /e1A_rj2)
    (add_net /e1A_rj3)
    (add_net /e1A_rj4)
    (add_net /e1A_rj5)
    (add_net /e1A_rj6)
    (add_net /e1A_rj7)
    (add_net /e1A_rj8)
    (add_net /e1B_rj1)
    (add_net /e1B_rj2)
    (add_net /e1B_rj3)
    (add_net /e1B_rj4)
    (add_net /e1B_rj5)
    (add_net /e1B_rj6)
    (add_net /e1B_rj7)
    (add_net /e1B_rj8)
    (add_net /e1_led0)
    (add_net /e1_led1)
    (add_net /e1_led2)
    (add_net /e1_led3)
    (add_net /e1_led4)
    (add_net /e1_led5)
    (add_net /e1_led6)
    (add_net /e1_led7)
    (add_net /e1bias/bias0)
    (add_net /e1bias/bias1)
    (add_net /e1bias/bias_0)
    (add_net /e1bias/bias_a_n)
    (add_net /e1bias/bias_a_p)
    (add_net /e1bias/bias_b_n)
    (add_net /e1bias/bias_fixed)
    (add_net /fpga/cdone)
    (add_net /fpga/clk_30m72)
    (add_net /fpga/clk_tune_hi)
    (add_net /fpga/clk_tune_lo)
    (add_net /fpga/dbg_rx_i)
    (add_net /fpga/dbg_tx_i)
    (add_net /fpga/e1A_rx_hi_n)
    (add_net /fpga/e1A_rx_hi_p)
    (add_net /fpga/e1A_rx_lo_n)
    (add_net /fpga/e1A_rx_lo_p)
    (add_net /fpga/e1A_tx_hi)
    (add_net /fpga/e1A_tx_lo)
    (add_net /fpga/e1B_rx_hi_n)
    (add_net /fpga/e1B_rx_hi_p)
    (add_net /fpga/e1B_rx_lo_n)
    (add_net /fpga/e1B_rx_lo_p)
    (add_net /fpga/e1B_tx_hi)
    (add_net /fpga/e1B_tx_lo)
    (add_net /fpga/e1_led_rclk)
    (add_net /fpga/flash_miso)
    (add_net /fpga/flash_mosi)
    (add_net /fpga/flash_sck)
    (add_net /fpga/gps_pps)
    (add_net /fpga/gps_rx)
    (add_net /fpga/gps_tx)
    (add_net /fpga/i2c_scl)
    (add_net /fpga/i2c_sda)
    (add_net /fpga/usb_dn_i)
    (add_net /fpga/usb_dp_i)
    (add_net /fpga/usb_pu_i)
    (add_net /fpga/~boot_sw)
    (add_net /fpga/~creset)
    (add_net /fpga/~flash_cs)
    (add_net /fpga/~gps_reset)
    (add_net /gpio0)
    (add_net /gpio1)
    (add_net /gpio2)
    (add_net /gps/RF)
    (add_net /gps/vbackup)
    (add_net /usb_dn)
    (add_net /usb_dp)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C35-Pad1)")
    (add_net "Net-(C36-Pad1)")
    (add_net "Net-(C39-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(F2-Pad2)")
    (add_net "Net-(F3-Pad2)")
    (add_net "Net-(F4-Pad2)")
    (add_net "Net-(F5-Pad2)")
    (add_net "Net-(F6-Pad2)")
    (add_net "Net-(F7-Pad2)")
    (add_net "Net-(F8-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R27-Pad1)")
    (add_net "Net-(R28-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(RN1-Pad1)")
    (add_net "Net-(RN1-Pad2)")
    (add_net "Net-(RN1-Pad3)")
    (add_net "Net-(RN1-Pad4)")
    (add_net "Net-(RN2-Pad1)")
    (add_net "Net-(RN2-Pad2)")
    (add_net "Net-(RN2-Pad3)")
    (add_net "Net-(RN2-Pad4)")
    (add_net "Net-(RN6-Pad1)")
    (add_net "Net-(RN6-Pad2)")
    (add_net "Net-(RN6-Pad3)")
    (add_net "Net-(RN6-Pad4)")
    (add_net "Net-(TR1-Pad10)")
    (add_net "Net-(TR1-Pad15)")
    (add_net "Net-(TR1-Pad7)")
    (add_net "Net-(TR2-Pad10)")
    (add_net "Net-(TR2-Pad15)")
    (add_net "Net-(TR2-Pad7)")
    (add_net "Net-(U10-Pad4)")
    (add_net "Net-(U12-Pad2)")
    (add_net "Net-(U12-Pad5)")
    (add_net "Net-(U3-Pad9)")
    (add_net "Net-(U7-Pad2)")
    (add_net "Net-(U7-Pad5)")
    (add_net "Net-(U8-Pad13)")
    (add_net "Net-(U8-Pad18)")
    (add_net "Net-(U8-Pad5)")
    (add_net "Net-(U9-Pad4)")
    (add_net "Net-(X4-PadA8)")
    (add_net "Net-(X4-PadB8)")
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at -16.5 -9.75 270)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN6 (at 0 -2.8 90) (layer F.SilkS) hide)
    (fp_text value 33R (at -1.25 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 0.9 1.2 270) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 99 /fpga/i2c_scl))
    (pad 6 smd rect (at 0.9 0.4 270) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 101 /fpga/i2c_sda))
    (pad 8 smd rect (at 0.9 -1.2 270) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 110 /fpga/gps_tx))
    (pad 7 smd rect (at 0.9 -0.4 270) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 111 /fpga/gps_rx))
    (pad 4 smd rect (at -0.9 1.2 270) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(RN6-Pad4)"))
    (pad 2 smd rect (at -0.9 -0.4 270) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(RN6-Pad2)"))
    (pad 3 smd rect (at -0.9 0.4 270) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(RN6-Pad3)"))
    (pad 1 smd rect (at -0.9 -1.2 270) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(RN6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26 -7.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 1k5 (at 1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /fpga/~boot_sw))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 122 /fpga/e1_led_rclk))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -17.75 -0.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at -1.25 12.5 270)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN7 (at 0 -2.8 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 1.25 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 0.9 1.2 270) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 137 /e1bias/bias1))
    (pad 6 smd rect (at 0.9 0.4 270) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 138 /e1bias/bias0))
    (pad 8 smd rect (at 0.9 -1.2 270) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 7 smd rect (at 0.9 -0.4 270) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.9 1.2 270) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 98 /e1bias/bias_b_n))
    (pad 2 smd rect (at -0.9 -0.4 270) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 130 /e1bias/bias_fixed))
    (pad 3 smd rect (at -0.9 0.4 270) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 131 /e1bias/bias_0))
    (pad 1 smd rect (at -0.9 -1.2 270) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 130 /e1bias/bias_fixed))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -4.25 9.5 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0R (at -1.25 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (fp_text user DNP (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /e1bias/bias_b_n))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /e1bias/bias_a_n))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -2.75 9.5 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0R (at -1.25 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 /e1bias/bias_0))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /e1bias/bias_a_n))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -1.25 9.5 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0R (at -1.25 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (fp_text user DNP (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 /e1bias/bias_0))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /e1bias/bias_a_p))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 0.25 9.5 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0R (at -1.25 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /e1bias/bias_fixed))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /e1bias/bias_a_p))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -4 12.5 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 1u (at 1.25 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /e1bias/bias_b_n))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -5.5 12.5 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 1u (at 1.25 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 /e1bias/bias_0))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 1.5 12.5 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 1u (at 1.25 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /e1bias/bias_fixed))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module s47-conn:Jack_2.5mm_CUI_SJ-2523-SMT_Horizontal (layer F.Cu) (tedit 5F32BCF4)
    (at -36.75 -10.5 90)
    (descr "2.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cuidevices.com/product/resource/sj-252x-smt.pdf))")
    (tags "2.5mm audio cui horizontal jack stereo")
    (attr smd)
    (fp_text reference X2 (at 0 -8.5 90) (layer F.SilkS) hide)
    (fp_text value Serial (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.75 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 3 90) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -3 90) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad T smd rect (at -3.45 5.4 90) (size 2.5 2.4) (layers F.Cu F.Paste F.Mask)
      (net 61 /dbg_rx))
    (pad S smd rect (at -3.3 -4.3 90) (size 2.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad R smd rect (at 3.3 -1.6 90) (size 2.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 62 /dbg_tx))
    (model ${KIUSR3DMOD}/CUI_DEVICES_SJ-2523-SMT-TR.step
      (offset (xyz 0 6 2.55))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connector_RJ:RJ45_Amphenol_RJHSE538X-02 locked (layer F.Cu) (tedit 5F32B9B7)
    (at 36 -11.435 270)
    (descr "Shielded, 2 LED, 2 Ports, http://www.amphenolinfocom.eu/NavData/Drawings/RJHSE-538X-02-REVC.pdf")
    (tags "RJ45 8p8c dual ethernet cat5")
    (fp_text reference X5 (at 11.43 -9.5 270) (layer F.SilkS) hide)
    (fp_text value E1 (at 11.43 -1.5 270) (layer F.Fab))
    (fp_text user %R (at 11.435 -4 270) (layer F.Fab))
    (pad 19 thru_hole circle (at 21.846 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 25 /e1B_rj7))
    (pad 18 thru_hole circle (at 20.83 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 26 /e1B_rj6))
    (pad 17 thru_hole circle (at 19.814 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 27 /e1B_rj5))
    (pad 16 thru_hole circle (at 18.798 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 28 /e1B_rj4))
    (pad 20 thru_hole circle (at 22.862 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 29 /e1B_rj8))
    (pad 13 thru_hole circle (at 15.75 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 19 /e1B_rj1))
    (pad 14 thru_hole circle (at 16.766 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 30 /e1B_rj2))
    (pad 15 thru_hole circle (at 17.782 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 31 /e1B_rj3))
    (pad 21 thru_hole circle (at 12.45 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 83 "Net-(RN2-Pad4)"))
    (pad 24 thru_hole circle (at 26.17 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 86 "Net-(RN2-Pad1)"))
    (pad 23 thru_hole circle (at 23.88 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 84 "Net-(RN2-Pad2)"))
    (pad 22 thru_hole circle (at 14.74 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 85 "Net-(RN2-Pad3)"))
    (pad 12 thru_hole circle (at 10.42 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 71 "Net-(RN1-Pad1)"))
    (pad 11 thru_hole circle (at 8.13 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 69 "Net-(RN1-Pad2)"))
    (pad 10 thru_hole circle (at -1.01 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 70 "Net-(RN1-Pad3)"))
    (pad 9 thru_hole circle (at -3.3 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 68 "Net-(RN1-Pad4)"))
    (pad SH thru_hole circle (at -4.57 0.89 270) (size 2.3 2.3) (drill 1.57) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at 27.43 0.89 270) (size 2.3 2.3) (drill 1.57) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 25.66 -2.54 270) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.79 -2.54 270) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 7.112 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 35 /e1A_rj8))
    (pad 6 thru_hole circle (at 5.08 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 36 /e1A_rj6))
    (pad 4 thru_hole circle (at 3.048 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 37 /e1A_rj4))
    (pad 2 thru_hole circle (at 1.016 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 38 /e1A_rj2))
    (pad 7 thru_hole circle (at 6.096 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 39 /e1A_rj7))
    (pad 5 thru_hole circle (at 4.064 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 40 /e1A_rj5))
    (pad 3 thru_hole circle (at 2.032 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 41 /e1A_rj3))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 18 /e1A_rj1))
    (model ${KIUSR3DMOD}/M-RJHSE-X08X-02-REVT1.step
      (offset (xyz 27.15 7.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 7.75 21.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 5k1 (at 1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /fpga/i2c_scl))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 7.75 22.75 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 5k1 (at 1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 /fpga/i2c_sda))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -7.5 -17.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 330R (at 1.75 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (fp_text user DNP (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 123 /gps/vbackup))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -28.5 -16.75 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 10R (at 0 0.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (fp_text user DNP (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(L1-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 "Net-(C21-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at -28.5 -19.5 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 47n (at 1.25 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /gps/RF))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(L1-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module s47-misc:J_NC_0603_30 (layer B.Cu) (tedit 5BF2400B)
    (at -16.25 -18.25 270)
    (descr "Jumper Normally Closed SMD 0603, 0.30mm connection, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference JP1 (at 0 1.1 90) (layer B.Fab))
    (fp_text value BatBypass (at 0 -1.2 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.575 0 270) (size 0.95 0.9) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 123 /gps/vbackup))
    (pad 1 smd roundrect (at -0.575 0 270) (size 0.95 0.9) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
  )
  (module Diode_SMD:D_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -10.5 -17.5 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value SDM02U30LP3 (at 0 -0.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (fp_text user DNP (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at -30 -19.5 270)
    (descr "Diode SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D3 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value PESD0402-140 (at -3 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /gps/RF))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -13.5 -17.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at -1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 123 /gps/vbackup))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -13.5 -22)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 1u (at -1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -13.5 -19)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at -1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -13.5 -20.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at -1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -30 -16.75 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (fp_text user DNP (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 "Net-(C21-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Battery:Battery_Panasonic_CR1220-VCN_Vertical_CircularHoles (layer F.Cu) (tedit 5C8577EF)
    (at -6.75 -19.25)
    (descr "Panasonic CR-1220/VCN battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D140.pdf")
    (tags "battery CR-1220 coin cell vertical")
    (fp_text reference BT1 (at 1.625 -4) (layer F.SilkS) hide)
    (fp_text value VL-1220/VCN (at 1.625 -0.25) (layer F.Fab) hide)
    (fp_text user + (at -1.46 -0.5) (layer F.SilkS))
    (fp_text user %R (at 1.625 -1.2 180) (layer F.Fab) hide)
    (fp_text user DNP (at 1.5 -1.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.25 -2.45) (size 1.6 1.6) (drill 1.09) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1.09) (layers *.Cu *.Mask)
      (net 123 /gps/vbackup))
    (model ${KISYS3DMOD}/Battery.3dshapes/Battery_Panasonic_CR1220-VCN_Vertical_CircularHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at 26 -5 180)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0 -2.8) (layer F.SilkS) hide)
    (fp_text value 33R (at -1.25 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 0.9 1.2 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 117 /e1_led4))
    (pad 6 smd rect (at 0.9 0.4 180) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 118 /e1_led5))
    (pad 8 smd rect (at 0.9 -1.2 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 115 /e1_led7))
    (pad 7 smd rect (at 0.9 -0.4 180) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 116 /e1_led6))
    (pad 4 smd rect (at -0.9 1.2 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(RN1-Pad4)"))
    (pad 2 smd rect (at -0.9 -0.4 180) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(RN1-Pad2)"))
    (pad 3 smd rect (at -0.9 0.4 180) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(RN1-Pad3)"))
    (pad 1 smd rect (at -0.9 -1.2 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(RN1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-16_4.4x5mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 23.5 0 180)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 -3.55) (layer F.SilkS) hide)
    (fp_text value 74HC595 (at 0 -1) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 16 smd rect (at 2.95 -2.275 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 15 smd rect (at 2.95 -1.625 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 /e1_led0))
    (pad 14 smd rect (at 2.95 -0.975 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 51 /fpga/flash_mosi))
    (pad 13 smd rect (at 2.95 -0.325 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 2.95 0.325 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 122 /fpga/e1_led_rclk))
    (pad 11 smd rect (at 2.95 0.975 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 57 /fpga/flash_sck))
    (pad 10 smd rect (at 2.95 1.625 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 54 /fpga/cdone))
    (pad 9 smd rect (at 2.95 2.275 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(U3-Pad9)"))
    (pad 8 smd rect (at -2.95 2.275 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -2.95 1.625 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 115 /e1_led7))
    (pad 6 smd rect (at -2.95 0.975 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 116 /e1_led6))
    (pad 5 smd rect (at -2.95 0.325 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 118 /e1_led5))
    (pad 4 smd rect (at -2.95 -0.325 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 117 /e1_led4))
    (pad 3 smd rect (at -2.95 -0.975 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 114 /e1_led3))
    (pad 2 smd rect (at -2.95 -1.625 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 /e1_led2))
    (pad 1 smd rect (at -2.95 -2.275 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 /e1_led1))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 18.75 0 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26 10.75 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 5k1 (at -1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 134 "Net-(C39-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26 7.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 5k1 (at 1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 134 "Net-(C39-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 9 -10.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 5k1 (at -1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 128 "Net-(C20-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 9 -7.75 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 5k1 (at 1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 128 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 26 9.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C39 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 134 "Net-(C39-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 0.5 2.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C34 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /e1bias/bias_b_n))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 0.5 4.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C33 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 -0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /e1bias/bias_a_p))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 9 -9.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 128 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 0.5 -2.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 -0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /e1bias/bias_a_n))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 0.5 -4.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /e1bias/bias_a_p))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at 3.75 3.5)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN8 (at 0 -2.8) (layer F.SilkS) hide)
    (fp_text value 10k (at 1.25 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 95 /fpga/e1B_rx_hi_p))
    (pad 6 smd rect (at 0.9 0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 94 /fpga/e1B_rx_hi_n))
    (pad 8 smd rect (at 0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 92 /fpga/e1B_rx_lo_n))
    (pad 7 smd rect (at 0.9 -0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 93 /fpga/e1B_rx_lo_p))
    (pad 4 smd rect (at -0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 96 /e1bias/bias_a_p))
    (pad 2 smd rect (at -0.9 -0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 96 /e1bias/bias_a_p))
    (pad 3 smd rect (at -0.9 0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 98 /e1bias/bias_b_n))
    (pad 1 smd rect (at -0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 98 /e1bias/bias_b_n))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at 3.75 -3.5)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN5 (at 0 -2.8) (layer F.SilkS) hide)
    (fp_text value 10k (at 1.25 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 91 /fpga/e1A_rx_lo_n))
    (pad 6 smd rect (at 0.9 0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 90 /fpga/e1A_rx_lo_p))
    (pad 8 smd rect (at 0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 88 /fpga/e1A_rx_hi_p))
    (pad 7 smd rect (at 0.9 -0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 89 /fpga/e1A_rx_hi_n))
    (pad 4 smd rect (at -0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 97 /e1bias/bias_a_n))
    (pad 2 smd rect (at -0.9 -0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 97 /e1bias/bias_a_n))
    (pad 3 smd rect (at -0.9 0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 96 /e1bias/bias_a_p))
    (pad 1 smd rect (at -0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 96 /e1bias/bias_a_p))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at 26 5 180)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 0 -2.8) (layer F.SilkS) hide)
    (fp_text value 33R (at -1.25 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 0.9 1.2 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 34 /e1_led1))
    (pad 6 smd rect (at 0.9 0.4 180) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 /e1_led2))
    (pad 8 smd rect (at 0.9 -1.2 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 /e1_led0))
    (pad 7 smd rect (at 0.9 -0.4 180) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 114 /e1_led3))
    (pad 4 smd rect (at -0.9 1.2 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(RN2-Pad4)"))
    (pad 2 smd rect (at -0.9 -0.4 180) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(RN2-Pad2)"))
    (pad 3 smd rect (at -0.9 0.4 180) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(RN2-Pad3)"))
    (pad 1 smd rect (at -0.9 -1.2 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(RN2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at -16 19.25 180)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN4 (at 0 -2.8) (layer F.SilkS) hide)
    (fp_text value 10k (at -1.25 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 0.9 1.2 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 6 smd rect (at 0.9 0.4 180) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 8 smd rect (at 0.9 -1.2 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 7 smd rect (at 0.9 -0.4 180) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 4 smd rect (at -0.9 1.2 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 55 /fpga/~flash_cs))
    (pad 2 smd rect (at -0.9 -0.4 180) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 54 /fpga/cdone))
    (pad 3 smd rect (at -0.9 0.4 180) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 54 /fpga/cdone))
    (pad 1 smd rect (at -0.9 -1.2 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 53 /fpga/~creset))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at -31.75 -1.5)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN3 (at 0 -2.8) (layer F.SilkS) hide)
    (fp_text value 33R (at -1.25 -0.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 113 /fpga/usb_dp_i))
    (pad 6 smd rect (at 0.9 0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 119 /fpga/usb_dn_i))
    (pad 8 smd rect (at 0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 120 /fpga/dbg_rx_i))
    (pad 7 smd rect (at 0.9 -0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 121 /fpga/dbg_tx_i))
    (pad 4 smd rect (at -0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 60 /usb_dp))
    (pad 2 smd rect (at -0.9 -0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 62 /dbg_tx))
    (pad 3 smd rect (at -0.9 0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 59 /usb_dn))
    (pad 1 smd rect (at -0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 61 /dbg_rx))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 7 4.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C36 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at -1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 /fpga/e1B_rx_hi_n))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 "Net-(C36-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 7 2.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C37 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at -1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 /fpga/e1B_rx_lo_p))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 "Net-(C36-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 7 1.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C38 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at -1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 /fpga/e1B_rx_lo_n))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 132 "Net-(C35-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 7 5.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C35 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at -1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 /fpga/e1B_rx_hi_p))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 132 "Net-(C35-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 7 -4.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at -1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 /fpga/e1A_rx_hi_n))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 7 -2.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at -1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 /fpga/e1A_rx_lo_p))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 7 -1.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at -1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 /fpga/e1A_rx_lo_n))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 7 -5.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at -1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 /fpga/e1A_rx_hi_p))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 11.25 2 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 120R (at 0 0.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 132 "Net-(C35-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 "Net-(C36-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 11.25 -5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 120R (at 0 0.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 "Net-(C16-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.25 22.75 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F8 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 300mA (at -2 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(F8-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /e1B_rj5))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.25 21.25 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F7 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 300mA (at -2 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(F7-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /e1B_rj4))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.25 19.75 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F5 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 300mA (at -2 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(F5-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /e1B_rj2))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.25 18.25 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F6 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 300mA (at -2 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(F6-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /e1B_rj1))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.25 -18.25 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F4 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 300mA (at -2 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /e1A_rj5))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(F4-Pad2)"))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.25 -19.75 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F3 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 300mA (at -2 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(F3-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /e1A_rj4))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.25 -21.25 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F1 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 300mA (at -2 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(F1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /e1A_rj2))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.25 -22.75 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F2 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 300mA (at -2 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(F2-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /e1A_rj1))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 10.5 4.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 27R (at -1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 /fpga/e1B_tx_hi))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 136 "Net-(R27-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 10.5 5.75 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 27R (at -1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 /fpga/e1B_tx_lo))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 151 "Net-(R28-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 10.5 -2.75 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 27R (at -1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 /fpga/e1A_tx_hi))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 135 "Net-(R16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 10.5 -1.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 27R (at -1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 /fpga/e1A_tx_lo))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 150 "Net-(R17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -0.25 -11 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 27R (at 0 0.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 149 "Net-(R12-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 /fpga/clk_30m72))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -10.5 -10 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 1k5 (at 1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(C10-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 126 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -10.5 -14.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 1k5 (at 1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /fpga/clk_tune_hi))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -10.5 -13 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 91k (at 1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /fpga/clk_tune_lo))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -29.25 2 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 1k5 (at 0 -0.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 /fpga/usb_pu_i))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 113 /fpga/usb_dp_i))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -4.25 6.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 120R (at 0 0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +1V2))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -31.75 1.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 5k1 (at 1.5 0.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -31.75 -4.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 5k1 (at 1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at -31.75 4.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 91k (at -1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 8 18.81 180)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value EXT_IN (at 0.5 3.81 90) (layer F.Fab))
    (fp_text user %R (at 2 3.81 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 /gpio0))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 /gpio1))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 /fpga/i2c_sda))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 /gpio2))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 /fpga/i2c_scl))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 +5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at -22.48 18.81 180)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value EXT_OUT (at 0.52 3.81 90) (layer F.Fab))
    (fp_text user %R (at 2.02 3.81 270) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -16 22)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value DONE (at 0 0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /fpga/cdone))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -10.5 -8.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 1u (at 1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 126 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -10.5 -11.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 1u (at -1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -19 18.5 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -7.25 -15.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -4.25 0.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 -0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -4.25 1.75)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -4.25 -2.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 -0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -8.5 6.75 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -17.75 -2.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -31.75 2.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.75 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at -22.25 -7.25)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U10 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MIC5504-3.3YM5 (at 1.25 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U10-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 +1V2))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 42 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at -22.25 7.25)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U9 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MIC5504-1.2YM5 (at 1.25 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 +1V2))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(U9-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 42 +5V))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 42 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -19.5 -7.25 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C32 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 -0.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -25 -7.25 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C31 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 -0.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -19.5 7.25 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 -0.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -25 7.25 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 -0.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at -4.25 4.75)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 -0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module s47-conn:SMA_TEConnectivity_619540-1_Horizontal locked (layer F.Cu) (tedit 5F259B65)
    (at -36 -20 90)
    (descr https://www.amphenolrf.com/media/downloads/1769/132203-12.pdf)
    (tags "SMA THT Female Jack Horizontal")
    (fp_text reference X1 (at -5.2 0) (layer F.SilkS) hide)
    (fp_text value GPS (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.25 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 24 /gps/RF))
    (pad 2 thru_hole circle (at 2.54 2.54 180) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIUSR3DMOD}/SMA_TEConnectivity_619540-1.step
      (offset (xyz 0 15.8 6.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Package_SO:TSOP-6_1.65x3.05mm_P0.95mm (layer F.Cu) (tedit 5A02F25C)
    (at 26 20.5 90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (attr smd)
    (fp_text reference U12 (at 0 -2.45 90) (layer F.SilkS) hide)
    (fp_text value IP4220CZ6 (at -1.25 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd rect (at 1.16 -0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(F6-Pad2)"))
    (pad 5 smd rect (at 1.16 0 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(U12-Pad5)"))
    (pad 4 smd rect (at 1.16 0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(F5-Pad2)"))
    (pad 3 smd rect (at -1.16 0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(F8-Pad2)"))
    (pad 2 smd rect (at -1.16 0 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(U12-Pad2)"))
    (pad 1 smd rect (at -1.16 -0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(F7-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSOP-6_1.65x3.05mm_P0.95mm (layer F.Cu) (tedit 5A02F25C)
    (at 14.325 3.5 90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (attr smd)
    (fp_text reference U11 (at 0 -2.45 90) (layer F.SilkS) hide)
    (fp_text value IP4220CZ6 (at 1.25 0.175 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd rect (at 1.16 -0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(C35-Pad1)"))
    (pad 5 smd rect (at 1.16 0 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 4 smd rect (at 1.16 0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(C36-Pad1)"))
    (pad 3 smd rect (at -1.16 0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(R27-Pad1)"))
    (pad 2 smd rect (at -1.16 0 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.16 -0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(R28-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSOP-6_1.65x3.05mm_P0.95mm (layer F.Cu) (tedit 5A02F25C)
    (at 26 -20.5 90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (attr smd)
    (fp_text reference U7 (at 0 -2.45 90) (layer F.SilkS) hide)
    (fp_text value IP4220CZ6 (at 1.25 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd rect (at 1.16 -0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(F2-Pad2)"))
    (pad 5 smd rect (at 1.16 0 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(U7-Pad5)"))
    (pad 4 smd rect (at 1.16 0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(F1-Pad2)"))
    (pad 3 smd rect (at -1.16 0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(F4-Pad2)"))
    (pad 2 smd rect (at -1.16 0 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(U7-Pad2)"))
    (pad 1 smd rect (at -1.16 -0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(F3-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSOP-6_1.65x3.05mm_P0.95mm (layer F.Cu) (tedit 5A02F25C)
    (at 14.325 -3.5 90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (attr smd)
    (fp_text reference U6 (at 0 -2.45 90) (layer F.SilkS) hide)
    (fp_text value IP4220CZ6 (at -1.25 0.175 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd rect (at 1.16 -0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(C16-Pad1)"))
    (pad 5 smd rect (at 1.16 0 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 4 smd rect (at 1.16 0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C17-Pad1)"))
    (pad 3 smd rect (at -1.16 0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at -1.16 0 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.16 -0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(R17-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSOP-6_1.65x3.05mm_P0.95mm (layer F.Cu) (tedit 5A02F25C)
    (at -28.25 -1.5 270)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (attr smd)
    (fp_text reference U2 (at 0 -2.45 90) (layer F.SilkS) hide)
    (fp_text value IP4220CZ6 (at -1.25 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd rect (at 1.16 -0.95 270) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 119 /fpga/usb_dn_i))
    (pad 5 smd rect (at 1.16 0 270) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 42 +5V))
    (pad 4 smd rect (at 1.16 0.95 270) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 113 /fpga/usb_dp_i))
    (pad 3 smd rect (at -1.16 0.95 270) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 120 /fpga/dbg_rx_i))
    (pad 2 smd rect (at -1.16 0 270) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.16 -0.95 270) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask)
      (net 121 /fpga/dbg_tx_i))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 21.31 19.23 270)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J5 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value NT/TE (at 2.02 3.81 180) (layer F.Fab))
    (fp_text user %R (at 0.52 3.81) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(F7-Pad2)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J5-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J5-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(F8-Pad2)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(F6-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J5-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(F5-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 13.69 -19.23 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J4 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value NT/TE (at 0.52 3.81 180) (layer F.Fab))
    (fp_text user %R (at 2.02 3.81) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(F3-Pad2)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(J4-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(J4-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(F4-Pad2)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(F2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(F1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at -12.32 21.35 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J3 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value SPI (at 0.35 3.82 180) (layer F.Fab))
    (fp_text user %R (at 2.1 3.82) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /fpga/flash_mosi))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /fpga/flash_miso))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /fpga/~creset))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /fpga/flash_sck))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /fpga/cdone))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /fpga/~flash_cs))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module s47-misc:ublox_MAX (layer F.Cu) (tedit 5E9E8EA6)
    (at -21.75 -17.25 180)
    (descr "ublox MAX 6/7/8, (https://www.u-blox.com/sites/default/files/MAX-8-M8-FW3_HardwareIntegrationManual_%28UBX-15030059%29.pdf)")
    (tags "GPS ublox MAX 6/7/8")
    (attr smd)
    (fp_text reference U8 (at 0 -6) (layer F.SilkS) hide)
    (fp_text value MAX-M8W (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 18 smd roundrect (at 4.75 -4.4 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 142 "Net-(U8-Pad18)"))
    (pad 17 smd roundrect (at 4.75 -3.3 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 152 "Net-(RN6-Pad4)"))
    (pad 16 smd roundrect (at 4.75 -2.2 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 154 "Net-(RN6-Pad3)"))
    (pad 15 smd roundrect (at 4.75 -1.1 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 "Net-(C21-Pad2)"))
    (pad 14 smd roundrect (at 4.75 0 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(L1-Pad1)"))
    (pad 13 smd roundrect (at 4.75 1.1 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 143 "Net-(U8-Pad13)"))
    (pad 12 smd roundrect (at 4.75 2.2 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at 4.75 3.3 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /gps/RF))
    (pad 10 smd roundrect (at 4.75 4.4 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -4.75 4.4 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 /fpga/~gps_reset))
    (pad 8 smd roundrect (at -4.75 3.3 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 7 smd roundrect (at -4.75 2.2 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 6 smd roundrect (at -4.75 1.1 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 123 /gps/vbackup))
    (pad 5 smd roundrect (at -4.75 0 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(U8-Pad5)"))
    (pad 4 smd roundrect (at -4.75 -1.1 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 /fpga/gps_pps))
    (pad 3 smd roundrect (at -4.75 -2.2 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 155 "Net-(RN6-Pad1)"))
    (pad 2 smd roundrect (at -4.75 -3.3 180) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 153 "Net-(RN6-Pad2)"))
    (pad 1 smd roundrect (at -4.75 -4.4 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIUSR3DMOD}/ublox-MAX-M8.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module s47-misc:Oscillator_SMD_VCXO-6Pin_7.0x5.0mm_P2.54mm (layer F.Cu) (tedit 5F259630)
    (at -5 -11 90)
    (descr "SMD Crystal Oscillator IDT https://www.idt.com/document/dst/xu-family-datasheet#page=17, 7.0x5.0mm")
    (tags "SMD SMT crystal oscillator")
    (attr smd)
    (fp_text reference U4 (at 0 -4.63 90) (layer F.SilkS) hide)
    (fp_text value 30M72 (at -0.75 0) (layer F.Fab))
    (fp_text user %R (at 1 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.1 -2.54) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(C11-Pad1)"))
    (pad 3 smd rect (at -2.1 2.54) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.1 2.54) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(R12-Pad2)"))
    (pad 6 smd rect (at 2.1 -2.54) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 2 smd rect (at -2.1 0) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 5 smd rect (at 2.1 0) (size 1.8 2) (layers F.Cu F.Paste F.Mask))
    (model ${KIUSR3DMOD}/Oscillator_SMD_VCXO-6Pin_7.0x5.0mm_P2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module s47-misc:PULSE_BH locked (layer F.Cu) (tedit 5F1316D6)
    (at 17.5 11.25 270)
    (attr smd)
    (fp_text reference TR2 (at 0 -8 90) (layer F.SilkS) hide)
    (fp_text value PULSE_T1094NL (at 0 -1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 9 smd roundrect (at 4.165 4.445 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(J5-Pad7)"))
    (pad 15 smd roundrect (at 4.165 -3.175 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(TR2-Pad15)"))
    (pad 14 smd roundrect (at 4.165 -1.905 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(J5-Pad6)"))
    (pad 11 smd roundrect (at 4.165 1.905 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(J5-Pad3)"))
    (pad 13 smd roundrect (at 4.165 -0.635 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 4.165 3.175 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(TR2-Pad10)"))
    (pad 12 smd roundrect (at 4.165 0.635 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 16 smd roundrect (at 4.165 -4.445 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(J5-Pad2)"))
    (pad 8 smd roundrect (at -4.165 4.445 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 151 "Net-(R28-Pad1)"))
    (pad 7 smd roundrect (at -4.165 3.175 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(TR2-Pad7)"))
    (pad 6 smd roundrect (at -4.165 1.905 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 136 "Net-(R27-Pad1)"))
    (pad 5 smd roundrect (at -4.165 0.635 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -4.165 -0.635 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -4.165 -1.905 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 "Net-(C36-Pad1)"))
    (pad 2 smd roundrect (at -4.165 -3.175 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 134 "Net-(C39-Pad1)"))
    (pad 1 smd roundrect (at -4.165 -4.445 270) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 132 "Net-(C35-Pad1)"))
    (model ${KIUSR3DMOD}/PULSE_BH1.step
      (offset (xyz 0 0 6.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module s47-misc:PULSE_BH locked (layer F.Cu) (tedit 5F1316D6)
    (at 17.5 -11.25 90)
    (attr smd)
    (fp_text reference TR1 (at 0 -8 90) (layer F.SilkS) hide)
    (fp_text value PULSE_T1094NL (at 0 1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 9 smd roundrect (at 4.165 4.445 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(J4-Pad7)"))
    (pad 15 smd roundrect (at 4.165 -3.175 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(TR1-Pad15)"))
    (pad 14 smd roundrect (at 4.165 -1.905 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(J4-Pad6)"))
    (pad 11 smd roundrect (at 4.165 1.905 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(J4-Pad3)"))
    (pad 13 smd roundrect (at 4.165 -0.635 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 4.165 3.175 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(TR1-Pad10)"))
    (pad 12 smd roundrect (at 4.165 0.635 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 16 smd roundrect (at 4.165 -4.445 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(J4-Pad2)"))
    (pad 8 smd roundrect (at -4.165 4.445 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 150 "Net-(R17-Pad1)"))
    (pad 7 smd roundrect (at -4.165 3.175 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(TR1-Pad7)"))
    (pad 6 smd roundrect (at -4.165 1.905 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 135 "Net-(R16-Pad1)"))
    (pad 5 smd roundrect (at -4.165 0.635 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -4.165 -0.635 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -4.165 -1.905 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(C17-Pad1)"))
    (pad 2 smd roundrect (at -4.165 -3.175 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 128 "Net-(C20-Pad1)"))
    (pad 1 smd roundrect (at -4.165 -4.445 90) (size 1.9 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 "Net-(C16-Pad1)"))
    (model ${KIUSR3DMOD}/PULSE_BH1.step
      (offset (xyz 0 0 6.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module s47-misc:SW_HYP_1TS003B locked (layer F.Cu) (tedit 5F149781)
    (at 40.25 20.5 270)
    (descr "HYP (Hongyuan Precision) 1TS003B switches https://datasheet.lcsc.com/szlcsc/HYP-1TS003B-2600-3500A_C319399.pdf")
    (attr smd)
    (fp_text reference SW1 (at 0 2.75 90) (layer F.SilkS) hide)
    (fp_text value SW_Push (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.7 1.4 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 56 /fpga/~boot_sw))
    (pad 1 smd rect (at -1.7 1.4 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.3 -0.6 270) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask))
    (pad "" np_thru_hole circle (at 0.87 0 270) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad 3 smd rect (at 2.3 -0.6 270) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask))
    (pad "" np_thru_hole circle (at -0.85 0 270) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KIUSR3DMOD}/1TS003B.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module s47-misc:LUMEX_LPF-C011303S (layer F.Cu) (tedit 5F148CB8)
    (at -22.25 0 270)
    (descr https://www.lumex.com/spec/LPF-C011303S.pdf)
    (fp_text reference LP1 (at 0 -4 90) (layer F.SilkS) hide)
    (fp_text value LightPipe (at 3 0) (layer F.Fab))
    (fp_text user %R (at -3 0) (layer F.Fab))
    (pad "" np_thru_hole oval (at 3.575 0 270) (size 2 3) (drill oval 2 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at -3.575 0 270) (size 2 3) (drill oval 2 3) (layers *.Cu *.Mask))
    (model ${KIUSR3DMOD}/Lumex_LPF-C011303S.step
      (offset (xyz 0 -2.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module s47-device:LED_RGB_2020 (layer F.Cu) (tedit 5F149206)
    (at -22.25 0 180)
    (descr "LED Tri SMD 2020, reflow soldering")
    (tags "tri led 2020")
    (attr smd)
    (fp_text reference D1 (at 0 0) (layer F.Fab))
    (fp_text value STATUS (at 1.75 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.95 -0.55 180) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 0.95 -0.55 180) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)"))
    (pad 3 smd roundrect (at 0.95 0.55 180) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 4 smd roundrect (at -0.95 0.55 180) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad4)"))
    (model ${KIUSR3DMOD}/FOSHAN-FM-B2020RGBA-HG.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Connector_RJ:RJ45_Amphenol_RJHSE5380 locked (layer F.Cu) (tedit 5AD365F7)
    (at -36 18.57 90)
    (descr "Shielded, https://www.amphenolcanada.com/ProductSearch/drawings/AC/RJHSE538X.pdf")
    (tags "RJ45 8p8c ethernet cat5")
    (fp_text reference X3 (at 3.56 -9.5 90) (layer F.SilkS) hide)
    (fp_text value GPIO (at 3.57 -1.5 90) (layer F.Fab))
    (fp_text user %R (at 3.57 -4 90) (layer F.Fab))
    (pad SH thru_hole circle (at -4.57 0.89 90) (size 2 2) (drill 1.57) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at 11.69 0.89 90) (size 2 2) (drill 1.57) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 9.91 -2.54 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.79 -2.54 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 7.14 1.78 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 75 "Net-(J1-Pad8)"))
    (pad 6 thru_hole circle (at 5.1 1.78 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 77 "Net-(J1-Pad6)"))
    (pad 4 thru_hole circle (at 3.06 1.78 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 79 "Net-(J1-Pad4)"))
    (pad 2 thru_hole circle (at 1.02 1.78 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 81 "Net-(J1-Pad2)"))
    (pad 7 thru_hole circle (at 6.12 0 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 76 "Net-(J1-Pad7)"))
    (pad 5 thru_hole circle (at 4.08 0 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 78 "Net-(J1-Pad5)"))
    (pad 3 thru_hole circle (at 2.04 0 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 80 "Net-(J1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 82 "Net-(J1-Pad1)"))
    (model ${KIUSR3DMOD}/M-RJHSE-5080-REVT1.step
      (offset (xyz 3.5 1.55 3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module s47-conn:USB_C_Receptacle_HRO_TYPE-C-31-M-12 locked (layer F.Cu) (tedit 5F148CC8)
    (at -39.85 0 270)
    (descr "USB Type-C receptacle for USB 2.0 and PD, http://www.krhro.com/uploads/soft/180320/1-1P320120243.pdf")
    (tags "usb usb-c 2.0 pd")
    (attr smd)
    (fp_text reference X4 (at 0 -5.645 90) (layer F.SilkS) hide)
    (fp_text value USB (at 2.5 0.15 180) (layer F.Fab))
    (fp_text user %R (at -2.5 0 180) (layer F.Fab))
    (pad B1 smd roundrect (at 3.25 -4.045 270) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 1 GND))
    (pad A9 smd roundrect (at 2.45 -4.045 270) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 42 +5V))
    (pad B9 smd roundrect (at -2.45 -4.045 270) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 42 +5V))
    (pad B12 smd roundrect (at -3.25 -4.045 270) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 1 GND))
    (pad A1 smd roundrect (at -3.25 -4.045 270) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 1 GND))
    (pad A4 smd roundrect (at -2.45 -4.045 270) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 42 +5V))
    (pad B4 smd roundrect (at 2.45 -4.045 270) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 42 +5V))
    (pad A12 smd roundrect (at 3.25 -4.045 270) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 1 GND))
    (pad B8 smd roundrect (at -1.75 -4.045 270) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 147 "Net-(X4-PadB8)"))
    (pad A5 smd roundrect (at -1.25 -4.045 270) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(R2-Pad2)"))
    (pad B7 smd roundrect (at -0.75 -4.045 270) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /usb_dn))
    (pad A7 smd roundrect (at 0.25 -4.045 270) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /usb_dn))
    (pad B6 smd roundrect (at 0.75 -4.045 270) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /usb_dp))
    (pad A8 smd roundrect (at 1.25 -4.045 270) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 148 "Net-(X4-PadA8)"))
    (pad B5 smd roundrect (at 1.75 -4.045 270) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R3-Pad2)"))
    (pad A6 smd roundrect (at -0.25 -4.045 270) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /usb_dp))
    (pad S1 thru_hole oval (at 4.32 -3.13 270) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 20 "Net-(C1-Pad2)"))
    (pad S1 thru_hole oval (at -4.32 -3.13 270) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 20 "Net-(C1-Pad2)"))
    (pad "" np_thru_hole circle (at -2.89 -2.6 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad S1 thru_hole oval (at -4.32 1.05 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(C1-Pad2)"))
    (pad "" np_thru_hole circle (at 2.89 -2.6 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad S1 thru_hole oval (at 4.32 1.05 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(C1-Pad2)"))
    (model ${KIUSR3DMOD}/HRO_TYPE-C-31-M-12.step
      (offset (xyz -4.465 -3.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_5.23x5.23mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at -15 14 180)
    (descr "SOIC, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf#page=68), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U5 (at 0 -3.56) (layer F.SilkS) hide)
    (fp_text value SPI_FLASH_8P (at 0 -1) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 3.6 -1.905 180) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 7 smd roundrect (at 3.6 -0.635 180) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 6 smd roundrect (at 3.6 0.635 180) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /fpga/flash_sck))
    (pad 5 smd roundrect (at 3.6 1.905 180) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /fpga/flash_mosi))
    (pad 4 smd roundrect (at -3.6 1.905 180) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -3.6 0.635 180) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at -3.6 -0.635 180) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /fpga/flash_miso))
    (pad 1 smd roundrect (at -3.6 -1.905 180) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /fpga/~flash_cs))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_5.23x5.23mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIJ-8_5.3x5.3mm_P1.27mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm (layer F.Cu) (tedit 5C26A111)
    (at -11 0)
    (descr "QFN, 48 Pin (https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2041_datasheet.pdf#page=62), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U1 (at 0 -4.8) (layer F.SilkS) hide)
    (fp_text value ICE40UP5K-SG48 (at 0 1) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 48 smd roundrect (at -2.75 -3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /fpga/clk_tune_hi))
    (pad 47 smd roundrect (at -2.25 -3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 /fpga/gps_rx))
    (pad 46 smd roundrect (at -1.75 -3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 110 /fpga/gps_tx))
    (pad 45 smd roundrect (at -1.25 -3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /fpga/clk_tune_lo))
    (pad 44 smd roundrect (at -0.75 -3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 /fpga/clk_30m72))
    (pad 43 smd roundrect (at -0.25 -3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 /fpga/e1A_tx_hi))
    (pad 42 smd roundrect (at 0.25 -3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 /fpga/e1A_rx_hi_p))
    (pad 41 smd roundrect (at 0.75 -3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad1)"))
    (pad 40 smd roundrect (at 1.25 -3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad4)"))
    (pad 39 smd roundrect (at 1.75 -3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)"))
    (pad 38 smd roundrect (at 2.25 -3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 /fpga/e1A_rx_hi_n))
    (pad 37 smd roundrect (at 2.75 -3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 /fpga/e1B_tx_lo))
    (pad 36 smd roundrect (at 3.45 -2.75) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 /fpga/e1A_tx_lo))
    (pad 35 smd roundrect (at 3.45 -2.25) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 137 /e1bias/bias1))
    (pad 34 smd roundrect (at 3.45 -1.75) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 /fpga/e1B_tx_hi))
    (pad 33 smd roundrect (at 3.45 -1.25) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 32 smd roundrect (at 3.45 -0.75) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 /fpga/e1A_rx_lo_p))
    (pad 31 smd roundrect (at 3.45 -0.25) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 /fpga/e1A_rx_lo_n))
    (pad 30 smd roundrect (at 3.45 0.25) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +1V2))
    (pad 29 smd roundrect (at 3.45 0.75) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C5-Pad1)"))
    (pad 28 smd roundrect (at 3.45 1.25) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 138 /e1bias/bias0))
    (pad 27 smd roundrect (at 3.45 1.75) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 /fpga/e1B_rx_lo_n))
    (pad 26 smd roundrect (at 3.45 2.25) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 /fpga/e1B_rx_lo_p))
    (pad 25 smd roundrect (at 3.45 2.75) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 /fpga/e1B_rx_hi_n))
    (pad 24 smd roundrect (at 2.75 3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 23 smd roundrect (at 2.25 3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 /fpga/e1B_rx_hi_p))
    (pad 22 smd roundrect (at 1.75 3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 21 smd roundrect (at 1.25 3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 120 /fpga/dbg_rx_i))
    (pad 20 smd roundrect (at 0.75 3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 /gpio1))
    (pad 19 smd roundrect (at 0.25 3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 /gpio2))
    (pad 18 smd roundrect (at -0.25 3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 122 /fpga/e1_led_rclk))
    (pad 17 smd roundrect (at -0.75 3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /fpga/flash_miso))
    (pad 16 smd roundrect (at -1.25 3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /fpga/~flash_cs))
    (pad 15 smd roundrect (at -1.75 3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /fpga/flash_sck))
    (pad 14 smd roundrect (at -2.25 3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /fpga/flash_mosi))
    (pad 13 smd roundrect (at -2.75 3.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 /gpio0))
    (pad 12 smd roundrect (at -3.45 2.75) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 121 /fpga/dbg_tx_i))
    (pad 11 smd roundrect (at -3.45 2.25) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 /fpga/usb_pu_i))
    (pad 10 smd roundrect (at -3.45 1.75) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 113 /fpga/usb_dp_i))
    (pad 9 smd roundrect (at -3.45 1.25) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 /fpga/usb_dn_i))
    (pad 8 smd roundrect (at -3.45 0.75) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /fpga/~creset))
    (pad 7 smd roundrect (at -3.45 0.25) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /fpga/cdone))
    (pad 6 smd roundrect (at -3.45 -0.25) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 /fpga/~gps_reset))
    (pad 5 smd roundrect (at -3.45 -0.75) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +1V2))
    (pad 4 smd roundrect (at -3.45 -1.25) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /fpga/i2c_scl))
    (pad 3 smd roundrect (at -3.45 -1.75) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 /fpga/i2c_sda))
    (pad 2 smd roundrect (at -3.45 -2.25) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 /fpga/gps_pps))
    (pad 1 smd roundrect (at -3.45 -2.75) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad "" smd roundrect (at 1.98 1.98) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at 1.98 0.66) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at 1.98 -0.66) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at 1.98 -1.98) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at 0.66 1.98) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at 0.66 0.66) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at 0.66 -0.66) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at 0.66 -1.98) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at -0.66 1.98) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at -0.66 0.66) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at -0.66 -0.66) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at -0.66 -1.98) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at -1.98 1.98) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at -1.98 0.66) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at -1.98 -0.66) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad "" smd roundrect (at -1.98 -1.98) (size 1.07 1.07) (layers F.Paste) (roundrect_rratio 0.233645))
    (pad 49 smd roundrect (at 0 0) (size 5.3 5.3) (layers F.Cu F.Mask) (roundrect_rratio 0.04717)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "rev 0.1 - 202008\n(c) 2020 - Munaut.S\nCERN-OHL-S" (at 0 -15) (layer F.SilkS))
  (gr_text icE1usb (at 0 -17.5) (layer F.SilkS))
  (gr_arc (start 38 26.5) (end 39 26.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -38 26.5) (end -38 25.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 38 -26.5) (end 38 -25.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -38 -26.5) (end -39 -26.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "GPIO\nExt" (at -47.5 15 90) (layer Eco1.User))
  (gr_text SMA (at -57.5 -20 90) (layer Eco1.User))
  (gr_text Serial (at -47.5 -10.5 90) (layer Eco1.User))
  (gr_text USB (at -47.5 0 90) (layer Eco1.User))
  (gr_line (start 39 -26.5) (end 41 -26.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 41 -25) (end 41 -26.5) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -39 26.5) (end -41 26.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -41 25) (end -41 26.5) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 39 26.5) (end 41 26.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 41 25) (end 41 26.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -39 -26.5) (end -41 -26.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -41 -25) (end -41 -26.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "Back\nPanel" (at 44.5 -25.5) (layer Eco1.User))
  (gr_text "Front\nPanel" (at -44.5 -25.5) (layer Eco1.User))
  (gr_line (start -42.5 25) (end -42.5 -25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 38 25.5) (end -38 25.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 42.5 -25) (end 42.5 25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -38 -25.5) (end 38 -25.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 10 -11.25) (xy 27.5 -11.25) (xy 27.5 -2.5) (xy 28 -2) (xy 28 -1.25)
        (xy 27.5 -0.75) (xy 27.5 11.25) (xy 26.75 11.25) (xy 26.25 11.75) (xy 25.75 11.75)
        (xy 25.25 11.25) (xy 10 11.25) (xy 10 25) (xy -5.375 25) (xy -20.5 25)
        (xy -20.5 10.25) (xy -21.5 9.25) (xy -28 9.25) (xy -33 4.25) (xy -42 4.25)
        (xy -42 -25) (xy 10 -25)
      )
    )
  )
  (zone (net 21) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 10 -11.25) (xy 27.5 -11.25) (xy 27.5 11.25) (xy 10 11.25) (xy 10 25)
        (xy -20.5 25) (xy -20.5 10.25) (xy -21.5 9.25) (xy -28 9.25) (xy -33 4.25)
        (xy -42 4.25) (xy -42 -25) (xy 10 -25)
      )
    )
  )
  (zone (net 20) (net_name "Net-(C1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -35.25 -4.75) (xy -35.25 -4) (xy -35.75 -3.5) (xy -37.75 -3.5) (xy -38 -3.25)
        (xy -38 3.25) (xy -37.75 3.5) (xy -35.75 3.5) (xy -35.25 4) (xy -35.25 4.75)
        (xy -35.75 5.25) (xy -41.5 5.25) (xy -42 4.75) (xy -42 -4.75) (xy -41.5 -5.25)
        (xy -35.75 -5.25)
      )
    )
  )
)
