(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "icE1usb - Power Supply")
    (date "2022-09-05")
    (rev "1.1")
    (comment 1 "CERN-OHL-S")
    (comment 2 "(C) 2020-2022 Sylvain Munaut")
  )
  (lib_symbols
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "C_Small" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "capacitor cap" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Regulator_Linear:MIC5504-1.2YM5" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 8.89 0))
      (property "Value" "MIC5504-1.2YM5" (id 1) (at -7.62 6.35 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (id 2) (at 0 -10.16 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf" (id 3) (at -6.35 6.35 0))
      (property "ki_keywords" "Micrel LDO voltage regulator" (id 4) (at 0 0 0))
      (property "ki_description" "300mA Low-dropout Voltage Regulator, Vout 1.2V, Vin up to 5.5V, SOT-23" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?23?5*" (id 6) (at 0 0 0))
      (symbol "MIC5504-1.2YM5_0_1"
        (rectangle (start -7.62 -5.08) (end 7.62 5.08)
          (fill (type background))
        )
      )
      (symbol "MIC5504-1.2YM5_1_1"
        (pin power_in line (at -10.16 2.54 0) (length 2.54)
          (name "VIN")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin input line (at -10.16 -2.54 0) (length 2.54)
          (name "EN")
          (number "3")
        )
        (pin no_connect line (at 7.62 -2.54 180) (length 2.54) hide
          (name "NC")
          (number "4")
        )
        (pin power_out line (at 10.16 2.54 180) (length 2.54)
          (name "VOUT")
          (number "5")
        )
      )
    )
    (symbol "Regulator_Linear:MIC5504-3.3YM5" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 8.89 0))
      (property "Value" "MIC5504-3.3YM5" (id 1) (at -7.62 6.35 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (id 2) (at 0 -10.16 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf" (id 3) (at -6.35 6.35 0))
      (property "ki_keywords" "Micrel LDO voltage regulator" (id 4) (at 0 0 0))
      (property "ki_description" "300mA Low-dropout Voltage Regulator, Vout 3.3V, Vin up to 5.5V, SOT-23" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?23?5*" (id 6) (at 0 0 0))
      (symbol "MIC5504-3.3YM5_0_1"
        (rectangle (start -7.62 -5.08) (end 7.62 5.08)
          (fill (type background))
        )
      )
      (symbol "MIC5504-3.3YM5_1_1"
        (pin power_in line (at -10.16 2.54 0) (length 2.54)
          (name "VIN")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin input line (at -10.16 -2.54 0) (length 2.54)
          (name "EN")
          (number "3")
        )
        (pin no_connect line (at 7.62 -2.54 180) (length 2.54) hide
          (name "NC")
          (number "4")
        )
        (pin power_out line (at 10.16 2.54 180) (length 2.54)
          (name "VOUT")
          (number "5")
        )
      )
    )
    (symbol "power:+1V2" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+1V2" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+1V2\"" (id 5) (at 0 0 0))
      (symbol "+1V2_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+1V2_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+1V2")
          (number "1")
        )
      )
    )
    (symbol "power:+3V3" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3V3" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3V3\"" (id 5) (at 0 0 0))
      (symbol "+3V3_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3V3_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "power:PWR_FLAG" (power) (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "#FLG" (id 0) (at 0 1.905 0))
      (property "Value" "PWR_FLAG" (id 1) (at 0 3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Special symbol for telling ERC where power comes from" (id 5) (at 0 0 0))
      (symbol "PWR_FLAG_0_0"
        (pin power_out line (at 0 0 90) (length 0)
          (name "pwr")
          (number "1")
        )
      )
      (symbol "PWR_FLAG_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 1.27)
            (xy -1.016 1.905)
            (xy 0 2.54)
            (xy 1.016 1.905)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
    )
  )
  (junction (at 96.52 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 127 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 96.52 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 96.52 91.44) (diameter 0) (color 0 0 0 0))
  (junction (at 182.88 86.36) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 182.88 86.36) (xy 182.88 93.98)))
  (wire (pts (xy 182.88 99.06) (xy 182.88 101.6)))
  (wire (pts (xy 121.92 86.36) (xy 127 86.36)))
  (wire (pts (xy 111.76 96.52) (xy 111.76 101.6)))
  (wire (pts (xy 152.4 81.28) (xy 152.4 86.36)))
  (wire (pts (xy 157.48 86.36) (xy 152.4 86.36)))
  (wire (pts (xy 182.88 81.28) (xy 182.88 86.36)))
  (wire (pts (xy 139.7 91.44) (xy 139.7 86.36)))
  (wire (pts (xy 96.52 83.82) (xy 96.52 81.28)))
  (wire (pts (xy 96.52 91.44) (xy 96.52 86.36)))
  (wire (pts (xy 96.52 99.06) (xy 96.52 101.6)))
  (wire (pts (xy 152.4 99.06) (xy 152.4 101.6)))
  (wire (pts (xy 127 81.28) (xy 127 86.36)))
  (wire (pts (xy 152.4 86.36) (xy 152.4 93.98)))
  (wire (pts (xy 167.64 96.52) (xy 167.64 101.6)))
  (wire (pts (xy 101.6 86.36) (xy 96.52 86.36)))
  (wire (pts (xy 127 86.36) (xy 127 93.98)))
  (wire (pts (xy 91.44 81.28) (xy 91.44 83.82)))
  (wire (pts (xy 91.44 99.06) (xy 91.44 101.6)))
  (wire (pts (xy 177.8 86.36) (xy 182.88 86.36)))
  (wire (pts (xy 96.52 91.44) (xy 96.52 93.98)))
  (wire (pts (xy 157.48 91.44) (xy 139.7 91.44)))
  (wire (pts (xy 139.7 86.36) (xy 127 86.36)))
  (wire (pts (xy 96.52 86.36) (xy 96.52 83.82)))
  (wire (pts (xy 127 99.06) (xy 127 101.6)))
  (wire (pts (xy 91.44 83.82) (xy 96.52 83.82)))
  (wire (pts (xy 101.6 91.44) (xy 96.52 91.44)))
  (symbol (lib_id "Regulator_Linear:MIC5504-1.2YM5") (at 111.76 88.9 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U9" (id 0) (at 111.76 79.5782 0))
    (property "Value" "MIC5504-1.2YM5" (id 1) (at 111.76 81.8896 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (id 2) (at 111.76 99.06 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf" (id 3) (at 105.41 82.55 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Regulator_Linear:MIC5504-3.3YM5") (at 167.64 88.9 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U10" (id 0) (at 167.64 79.5782 0))
    (property "Value" "MIC5504-3.3YM5" (id 1) (at 167.64 81.8896 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (id 2) (at 167.64 99.06 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf" (id 3) (at 161.29 82.55 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 111.76 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR062" (id 0) (at 111.76 107.95 0))
    (property "Value" "GND" (id 1) (at 111.887 105.9942 0))
    (property "Footprint" "" (id 2) (at 111.76 101.6 0))
    (property "Datasheet" "" (id 3) (at 111.76 101.6 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 167.64 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR067" (id 0) (at 167.64 107.95 0))
    (property "Value" "GND" (id 1) (at 167.767 105.9942 0))
    (property "Footprint" "" (id 2) (at 167.64 101.6 0))
    (property "Datasheet" "" (id 3) (at 167.64 101.6 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3V3") (at 182.88 81.28 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR068" (id 0) (at 182.88 85.09 0))
    (property "Value" "+3V3" (id 1) (at 183.261 76.8858 0))
    (property "Footprint" "" (id 2) (at 182.88 81.28 0))
    (property "Datasheet" "" (id 3) (at 182.88 81.28 0))
    (pin "1")
  )
  (symbol (lib_id "power:+1V2") (at 127 81.28 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR063" (id 0) (at 127 85.09 0))
    (property "Value" "+1V2" (id 1) (at 127.381 76.8858 0))
    (property "Footprint" "" (id 2) (at 127 81.28 0))
    (property "Datasheet" "" (id 3) (at 127 81.28 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 96.52 81.28 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR060" (id 0) (at 96.52 85.09 0))
    (property "Value" "+5V" (id 1) (at 96.901 76.8858 0))
    (property "Footprint" "" (id 2) (at 96.52 81.28 0))
    (property "Datasheet" "" (id 3) (at 96.52 81.28 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 96.52 96.52 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C29" (id 0) (at 98.8568 95.3516 0))
    (property "Value" "1u" (id 1) (at 98.8568 97.663 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 96.52 96.52 0))
    (property "Datasheet" "~" (id 3) (at 96.52 96.52 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 127 96.52 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C30" (id 0) (at 129.3368 95.3516 0))
    (property "Value" "1u" (id 1) (at 129.3368 97.663 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 127 96.52 0))
    (property "Datasheet" "~" (id 3) (at 127 96.52 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 152.4 96.52 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C31" (id 0) (at 154.7368 95.3516 0))
    (property "Value" "1u" (id 1) (at 154.7368 97.663 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 152.4 96.52 0))
    (property "Datasheet" "~" (id 3) (at 152.4 96.52 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 182.88 96.52 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C32" (id 0) (at 185.2168 95.3516 0))
    (property "Value" "1u" (id 1) (at 185.2168 97.663 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 182.88 96.52 0))
    (property "Datasheet" "~" (id 3) (at 182.88 96.52 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 96.52 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR061" (id 0) (at 96.52 107.95 0))
    (property "Value" "GND" (id 1) (at 96.647 105.9942 0))
    (property "Footprint" "" (id 2) (at 96.52 101.6 0))
    (property "Datasheet" "" (id 3) (at 96.52 101.6 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 127 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR064" (id 0) (at 127 107.95 0))
    (property "Value" "GND" (id 1) (at 127.127 105.9942 0))
    (property "Footprint" "" (id 2) (at 127 101.6 0))
    (property "Datasheet" "" (id 3) (at 127 101.6 0))
    (pin "1")
  )
  (symbol (lib_id "power:PWR_FLAG") (at 91.44 81.28 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#FLG04" (id 0) (at 91.44 79.375 0))
    (property "Value" "PWR_FLAG" (id 1) (at 91.44 76.8858 0))
    (property "Footprint" "" (id 2) (at 91.44 81.28 0))
    (property "Datasheet" "~" (id 3) (at 91.44 81.28 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 152.4 81.28 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR065" (id 0) (at 152.4 85.09 0))
    (property "Value" "+5V" (id 1) (at 152.781 76.8858 0))
    (property "Footprint" "" (id 2) (at 152.4 81.28 0))
    (property "Datasheet" "" (id 3) (at 152.4 81.28 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 152.4 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR066" (id 0) (at 152.4 107.95 0))
    (property "Value" "GND" (id 1) (at 152.527 105.9942 0))
    (property "Footprint" "" (id 2) (at 152.4 101.6 0))
    (property "Datasheet" "" (id 3) (at 152.4 101.6 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 182.88 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR069" (id 0) (at 182.88 107.95 0))
    (property "Value" "GND" (id 1) (at 183.007 105.9942 0))
    (property "Footprint" "" (id 2) (at 182.88 101.6 0))
    (property "Datasheet" "" (id 3) (at 182.88 101.6 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 91.44 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR059" (id 0) (at 91.44 107.95 0))
    (property "Value" "GND" (id 1) (at 91.567 105.9942 0))
    (property "Footprint" "" (id 2) (at 91.44 101.6 0))
    (property "Datasheet" "" (id 3) (at 91.44 101.6 0))
    (pin "1")
  )
  (symbol (lib_id "power:PWR_FLAG") (at 91.44 99.06 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#FLG05" (id 0) (at 91.44 97.155 0))
    (property "Value" "PWR_FLAG" (id 1) (at 91.44 94.6658 0))
    (property "Footprint" "" (id 2) (at 91.44 99.06 0))
    (property "Datasheet" "~" (id 3) (at 91.44 99.06 0))
    (pin "1")
  )
)
