format_version: '2'
name: sysmoOCTSIM
versions:
  api: '1.0'
  backend: 1.8.580
  commit: f3d8d96e294de8dee688333bbbe8d8458a4f6b4c
  content: unknown
  content_pack_name: unknown
  format: '2'
  frontend: 1.8.580
  packs_version_avr8: 1.0.1463
  packs_version_qtouch: unknown
  packs_version_sam: 1.0.1726
  version_backend: 1.8.580
  version_frontend: ''
board:
  identifier: CustomBoard
  device: SAME54N19A-AF
details: null
application: null
middlewares:
  USB_CHAPTER_9:
    user_label: USB_CHAPTER_9
    configuration: {}
    definition: Atmel:USB:0.0.1::USB_Chapter_9
    functionality: USB_Chapter_9
    api: USB:Protocol:Core
    dependencies: {}
  USB_CLASS_CDC:
    user_label: USB_CLASS_CDC
    configuration: {}
    definition: Atmel:USB:0.0.1::USB_Class_CDC
    functionality: USB_Class_CDC
    api: USB:Protocol:CDC
    dependencies:
      USB Chapter 9: USB_CHAPTER_9
  USB_DEVICE_STACK_CORE_INSTANCE:
    user_label: USB_DEVICE_STACK_CORE_INSTANCE
    configuration:
      usbd_hs_sp: false
    definition: Atmel:USB:0.0.1::USB_Device_Core
    functionality: USB_Device_Core
    api: USB:Device:Core
    dependencies:
      USB Chapter 9: USB_CHAPTER_9
      USB Device instance: USB_DEVICE_INSTANCE
  USB_DEVICE_CDC_ACM:
    user_label: USB_DEVICE_CDC_ACM
    configuration:
      usb_cdcd_acm_bcddevice: 256
      usb_cdcd_acm_bcdusb: USB 2.0 version
      usb_cdcd_acm_bconfigval: 1
      usb_cdcd_acm_bmattri: Bus power supply, not support for remote wakeup
      usb_cdcd_acm_bmaxpksz0: 64 bytes
      usb_cdcd_acm_bmaxpower: 50
      usb_cdcd_acm_bnumconfig: 1
      usb_cdcd_acm_comm_baltset: 0
      usb_cdcd_acm_comm_bifcnum: 0
      usb_cdcd_acm_comm_iifc: 0
      usb_cdcd_acm_comm_int_interval: 10
      usb_cdcd_acm_comm_int_maxpksz: 64 bytes
      usb_cdcd_acm_data_baltset: 0
      usb_cdcd_acm_data_bifcnum: 1
      usb_cdcd_acm_data_buckout_maxpksz: 64 bytes
      usb_cdcd_acm_data_buckout_maxpksz_hs: 512 bytes
      usb_cdcd_acm_data_builin_maxpksz: 64 bytes
      usb_cdcd_acm_data_builin_maxpksz_hs: 512 bytes
      usb_cdcd_acm_data_bulkin_epaddr: EndpointAddress = 0x81
      usb_cdcd_acm_data_bulkout_epaddr: EndpointAddress = 0x01
      usb_cdcd_acm_data_iifc: 0
      usb_cdcd_acm_epaddr: EndpointAddress = 0x82
      usb_cdcd_acm_iconfig_en: false
      usb_cdcd_acm_iconfig_str: ''
      usb_cdcd_acm_idproduct: 24897
      usb_cdcd_acm_idvender: 7504
      usb_cdcd_acm_imanufact_en: true
      usb_cdcd_acm_imanufact_str: sysmocom - s.f.m.c. GmbH
      usb_cdcd_acm_iproduct_en: true
      usb_cdcd_acm_iproduct_str: sysmoOCTSIM
      usb_cdcd_acm_iserialnum_en: false
      usb_cdcd_acm_iserialnum_str: 123456789ABCDEF
      usb_cdcd_acm_langid: '0x0409'
      usb_cdcd_acm_str_en: true
    definition: Atmel:USB:0.0.1::USB_Device_CDC_ACM
    functionality: USB_Device_CDC_ACM
    api: USB:Device:CDC_ACM
    dependencies:
      USB Device Stack Core Instance: USB_DEVICE_STACK_CORE_INSTANCE
      USB Class CDC: USB_CLASS_CDC
  M2M_DMA_0:
    user_label: M2M_DMA_0
    configuration:
      conf_channel: 0
    definition: Atmel:MEMORY_DMA:0.0.1::M2M_DMA
    functionality: M2M_DMA
    api: DMA:M2M:Core
    dependencies:
      DMAC: DMAC
  STDIO_REDIRECT_0:
    user_label: STDIO_REDIRECT_0
    configuration: {}
    definition: Atmel:STDIO_redirect:0.0.1::STDIO_Redirect
    functionality: STDIO_Redirect
    api: STDIO:Redirect:IO
    dependencies:
      Target IO: UART_debug
drivers:
  CMCC:
    user_label: CMCC
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::CMCC::driver_config_definition::CMCC::HAL:HPL:CMCC
    functionality: System
    api: HAL:HPL:CMCC
    configuration:
      cache_size: 4 KB
      cmcc_advanced_configuration: false
      cmcc_clock_gating_disable: false
      cmcc_data_cache_disable: false
      cmcc_enable: false
      cmcc_inst_cache_disable: false
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  DMAC:
    user_label: DMAC
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::DMAC::driver_config_definition::DMAC::HAL:HPL:DMAC
    functionality: System
    api: HAL:HPL:DMAC
    configuration:
      dmac_beatsize_0: 8-bit bus transfer
      dmac_beatsize_1: 8-bit bus transfer
      dmac_beatsize_10: 8-bit bus transfer
      dmac_beatsize_11: 8-bit bus transfer
      dmac_beatsize_12: 8-bit bus transfer
      dmac_beatsize_13: 8-bit bus transfer
      dmac_beatsize_14: 8-bit bus transfer
      dmac_beatsize_15: 8-bit bus transfer
      dmac_beatsize_16: 8-bit bus transfer
      dmac_beatsize_17: 8-bit bus transfer
      dmac_beatsize_18: 8-bit bus transfer
      dmac_beatsize_19: 8-bit bus transfer
      dmac_beatsize_2: 8-bit bus transfer
      dmac_beatsize_20: 8-bit bus transfer
      dmac_beatsize_21: 8-bit bus transfer
      dmac_beatsize_22: 8-bit bus transfer
      dmac_beatsize_23: 8-bit bus transfer
      dmac_beatsize_24: 8-bit bus transfer
      dmac_beatsize_25: 8-bit bus transfer
      dmac_beatsize_26: 8-bit bus transfer
      dmac_beatsize_27: 8-bit bus transfer
      dmac_beatsize_28: 8-bit bus transfer
      dmac_beatsize_29: 8-bit bus transfer
      dmac_beatsize_3: 8-bit bus transfer
      dmac_beatsize_30: 8-bit bus transfer
      dmac_beatsize_31: 8-bit bus transfer
      dmac_beatsize_4: 8-bit bus transfer
      dmac_beatsize_5: 8-bit bus transfer
      dmac_beatsize_6: 8-bit bus transfer
      dmac_beatsize_7: 8-bit bus transfer
      dmac_beatsize_8: 8-bit bus transfer
      dmac_beatsize_9: 8-bit bus transfer
      dmac_blockact_0: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_1: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_10: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_11: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_12: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_13: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_14: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_15: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_16: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_17: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_18: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_19: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_2: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_20: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_21: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_22: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_23: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_24: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_25: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_26: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_27: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_28: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_29: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_3: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_30: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_31: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_4: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_5: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_6: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_7: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_8: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_9: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_channel_0_settings: true
      dmac_channel_10_settings: false
      dmac_channel_11_settings: false
      dmac_channel_12_settings: false
      dmac_channel_13_settings: false
      dmac_channel_14_settings: false
      dmac_channel_15_settings: false
      dmac_channel_16_settings: false
      dmac_channel_17_settings: false
      dmac_channel_18_settings: false
      dmac_channel_19_settings: false
      dmac_channel_1_settings: false
      dmac_channel_20_settings: false
      dmac_channel_21_settings: false
      dmac_channel_22_settings: false
      dmac_channel_23_settings: false
      dmac_channel_24_settings: false
      dmac_channel_25_settings: false
      dmac_channel_26_settings: false
      dmac_channel_27_settings: false
      dmac_channel_28_settings: false
      dmac_channel_29_settings: false
      dmac_channel_2_settings: false
      dmac_channel_30_settings: false
      dmac_channel_31_settings: false
      dmac_channel_3_settings: false
      dmac_channel_4_settings: false
      dmac_channel_5_settings: false
      dmac_channel_6_settings: false
      dmac_channel_7_settings: false
      dmac_channel_8_settings: false
      dmac_channel_9_settings: false
      dmac_dbgrun: false
      dmac_dstinc_0: true
      dmac_dstinc_1: false
      dmac_dstinc_10: false
      dmac_dstinc_11: false
      dmac_dstinc_12: false
      dmac_dstinc_13: false
      dmac_dstinc_14: false
      dmac_dstinc_15: false
      dmac_dstinc_16: false
      dmac_dstinc_17: false
      dmac_dstinc_18: false
      dmac_dstinc_19: false
      dmac_dstinc_2: false
      dmac_dstinc_20: false
      dmac_dstinc_21: false
      dmac_dstinc_22: false
      dmac_dstinc_23: false
      dmac_dstinc_24: false
      dmac_dstinc_25: false
      dmac_dstinc_26: false
      dmac_dstinc_27: false
      dmac_dstinc_28: false
      dmac_dstinc_29: false
      dmac_dstinc_3: false
      dmac_dstinc_30: false
      dmac_dstinc_31: false
      dmac_dstinc_4: false
      dmac_dstinc_5: false
      dmac_dstinc_6: false
      dmac_dstinc_7: false
      dmac_dstinc_8: false
      dmac_dstinc_9: false
      dmac_enable: true
      dmac_evact_0: No action
      dmac_evact_1: No action
      dmac_evact_10: No action
      dmac_evact_11: No action
      dmac_evact_12: No action
      dmac_evact_13: No action
      dmac_evact_14: No action
      dmac_evact_15: No action
      dmac_evact_16: No action
      dmac_evact_17: No action
      dmac_evact_18: No action
      dmac_evact_19: No action
      dmac_evact_2: No action
      dmac_evact_20: No action
      dmac_evact_21: No action
      dmac_evact_22: No action
      dmac_evact_23: No action
      dmac_evact_24: No action
      dmac_evact_25: No action
      dmac_evact_26: No action
      dmac_evact_27: No action
      dmac_evact_28: No action
      dmac_evact_29: No action
      dmac_evact_3: No action
      dmac_evact_30: No action
      dmac_evact_31: No action
      dmac_evact_4: No action
      dmac_evact_5: No action
      dmac_evact_6: No action
      dmac_evact_7: No action
      dmac_evact_8: No action
      dmac_evact_9: No action
      dmac_evie_0: false
      dmac_evie_1: false
      dmac_evie_10: false
      dmac_evie_11: false
      dmac_evie_12: false
      dmac_evie_13: false
      dmac_evie_14: false
      dmac_evie_15: false
      dmac_evie_16: false
      dmac_evie_17: false
      dmac_evie_18: false
      dmac_evie_19: false
      dmac_evie_2: false
      dmac_evie_20: false
      dmac_evie_21: false
      dmac_evie_22: false
      dmac_evie_23: false
      dmac_evie_24: false
      dmac_evie_25: false
      dmac_evie_26: false
      dmac_evie_27: false
      dmac_evie_28: false
      dmac_evie_29: false
      dmac_evie_3: false
      dmac_evie_30: false
      dmac_evie_31: false
      dmac_evie_4: false
      dmac_evie_5: false
      dmac_evie_6: false
      dmac_evie_7: false
      dmac_evie_8: false
      dmac_evie_9: false
      dmac_evoe_0: false
      dmac_evoe_1: false
      dmac_evoe_10: false
      dmac_evoe_11: false
      dmac_evoe_12: false
      dmac_evoe_13: false
      dmac_evoe_14: false
      dmac_evoe_15: false
      dmac_evoe_16: false
      dmac_evoe_17: false
      dmac_evoe_18: false
      dmac_evoe_19: false
      dmac_evoe_2: false
      dmac_evoe_20: false
      dmac_evoe_21: false
      dmac_evoe_22: false
      dmac_evoe_23: false
      dmac_evoe_24: false
      dmac_evoe_25: false
      dmac_evoe_26: false
      dmac_evoe_27: false
      dmac_evoe_28: false
      dmac_evoe_29: false
      dmac_evoe_3: false
      dmac_evoe_30: false
      dmac_evoe_31: false
      dmac_evoe_4: false
      dmac_evoe_5: false
      dmac_evoe_6: false
      dmac_evoe_7: false
      dmac_evoe_8: false
      dmac_evoe_9: false
      dmac_evosel_0: Event generation disabled
      dmac_evosel_1: Event generation disabled
      dmac_evosel_10: Event generation disabled
      dmac_evosel_11: Event generation disabled
      dmac_evosel_12: Event generation disabled
      dmac_evosel_13: Event generation disabled
      dmac_evosel_14: Event generation disabled
      dmac_evosel_15: Event generation disabled
      dmac_evosel_16: Event generation disabled
      dmac_evosel_17: Event generation disabled
      dmac_evosel_18: Event generation disabled
      dmac_evosel_19: Event generation disabled
      dmac_evosel_2: Event generation disabled
      dmac_evosel_20: Event generation disabled
      dmac_evosel_21: Event generation disabled
      dmac_evosel_22: Event generation disabled
      dmac_evosel_23: Event generation disabled
      dmac_evosel_24: Event generation disabled
      dmac_evosel_25: Event generation disabled
      dmac_evosel_26: Event generation disabled
      dmac_evosel_27: Event generation disabled
      dmac_evosel_28: Event generation disabled
      dmac_evosel_29: Event generation disabled
      dmac_evosel_3: Event generation disabled
      dmac_evosel_30: Event generation disabled
      dmac_evosel_31: Event generation disabled
      dmac_evosel_4: Event generation disabled
      dmac_evosel_5: Event generation disabled
      dmac_evosel_6: Event generation disabled
      dmac_evosel_7: Event generation disabled
      dmac_evosel_8: Event generation disabled
      dmac_evosel_9: Event generation disabled
      dmac_lvl_0: Channel priority 0
      dmac_lvl_1: Channel priority 0
      dmac_lvl_10: Channel priority 0
      dmac_lvl_11: Channel priority 0
      dmac_lvl_12: Channel priority 0
      dmac_lvl_13: Channel priority 0
      dmac_lvl_14: Channel priority 0
      dmac_lvl_15: Channel priority 0
      dmac_lvl_16: Channel priority 0
      dmac_lvl_17: Channel priority 0
      dmac_lvl_18: Channel priority 0
      dmac_lvl_19: Channel priority 0
      dmac_lvl_2: Channel priority 0
      dmac_lvl_20: Channel priority 0
      dmac_lvl_21: Channel priority 0
      dmac_lvl_22: Channel priority 0
      dmac_lvl_23: Channel priority 0
      dmac_lvl_24: Channel priority 0
      dmac_lvl_25: Channel priority 0
      dmac_lvl_26: Channel priority 0
      dmac_lvl_27: Channel priority 0
      dmac_lvl_28: Channel priority 0
      dmac_lvl_29: Channel priority 0
      dmac_lvl_3: Channel priority 0
      dmac_lvl_30: Channel priority 0
      dmac_lvl_31: Channel priority 0
      dmac_lvl_4: Channel priority 0
      dmac_lvl_5: Channel priority 0
      dmac_lvl_6: Channel priority 0
      dmac_lvl_7: Channel priority 0
      dmac_lvl_8: Channel priority 0
      dmac_lvl_9: Channel priority 0
      dmac_lvlen0: true
      dmac_lvlen1: true
      dmac_lvlen2: true
      dmac_lvlen3: true
      dmac_lvlpri0: 0
      dmac_lvlpri1: 0
      dmac_lvlpri2: 0
      dmac_lvlpri3: 0
      dmac_rrlvlen0: Static arbitration scheme for channel with priority 0
      dmac_rrlvlen1: Static arbitration scheme for channel with priority 1
      dmac_rrlvlen2: Static arbitration scheme for channel with priority 2
      dmac_rrlvlen3: Static arbitration scheme for channel with priority 3
      dmac_runstdby_0: false
      dmac_runstdby_1: false
      dmac_runstdby_10: false
      dmac_runstdby_11: false
      dmac_runstdby_12: false
      dmac_runstdby_13: false
      dmac_runstdby_14: false
      dmac_runstdby_15: false
      dmac_runstdby_16: false
      dmac_runstdby_17: false
      dmac_runstdby_18: false
      dmac_runstdby_19: false
      dmac_runstdby_2: false
      dmac_runstdby_20: false
      dmac_runstdby_21: false
      dmac_runstdby_22: false
      dmac_runstdby_23: false
      dmac_runstdby_24: false
      dmac_runstdby_25: false
      dmac_runstdby_26: false
      dmac_runstdby_27: false
      dmac_runstdby_28: false
      dmac_runstdby_29: false
      dmac_runstdby_3: false
      dmac_runstdby_30: false
      dmac_runstdby_31: false
      dmac_runstdby_4: false
      dmac_runstdby_5: false
      dmac_runstdby_6: false
      dmac_runstdby_7: false
      dmac_runstdby_8: false
      dmac_runstdby_9: false
      dmac_srcinc_0: true
      dmac_srcinc_1: false
      dmac_srcinc_10: false
      dmac_srcinc_11: false
      dmac_srcinc_12: false
      dmac_srcinc_13: false
      dmac_srcinc_14: false
      dmac_srcinc_15: false
      dmac_srcinc_16: false
      dmac_srcinc_17: false
      dmac_srcinc_18: false
      dmac_srcinc_19: false
      dmac_srcinc_2: false
      dmac_srcinc_20: false
      dmac_srcinc_21: false
      dmac_srcinc_22: false
      dmac_srcinc_23: false
      dmac_srcinc_24: false
      dmac_srcinc_25: false
      dmac_srcinc_26: false
      dmac_srcinc_27: false
      dmac_srcinc_28: false
      dmac_srcinc_29: false
      dmac_srcinc_3: false
      dmac_srcinc_30: false
      dmac_srcinc_31: false
      dmac_srcinc_4: false
      dmac_srcinc_5: false
      dmac_srcinc_6: false
      dmac_srcinc_7: false
      dmac_srcinc_8: false
      dmac_srcinc_9: false
      dmac_stepsel_0: Step size settings apply to the destination address
      dmac_stepsel_1: Step size settings apply to the destination address
      dmac_stepsel_10: Step size settings apply to the destination address
      dmac_stepsel_11: Step size settings apply to the destination address
      dmac_stepsel_12: Step size settings apply to the destination address
      dmac_stepsel_13: Step size settings apply to the destination address
      dmac_stepsel_14: Step size settings apply to the destination address
      dmac_stepsel_15: Step size settings apply to the destination address
      dmac_stepsel_16: Step size settings apply to the destination address
      dmac_stepsel_17: Step size settings apply to the destination address
      dmac_stepsel_18: Step size settings apply to the destination address
      dmac_stepsel_19: Step size settings apply to the destination address
      dmac_stepsel_2: Step size settings apply to the destination address
      dmac_stepsel_20: Step size settings apply to the destination address
      dmac_stepsel_21: Step size settings apply to the destination address
      dmac_stepsel_22: Step size settings apply to the destination address
      dmac_stepsel_23: Step size settings apply to the destination address
      dmac_stepsel_24: Step size settings apply to the destination address
      dmac_stepsel_25: Step size settings apply to the destination address
      dmac_stepsel_26: Step size settings apply to the destination address
      dmac_stepsel_27: Step size settings apply to the destination address
      dmac_stepsel_28: Step size settings apply to the destination address
      dmac_stepsel_29: Step size settings apply to the destination address
      dmac_stepsel_3: Step size settings apply to the destination address
      dmac_stepsel_30: Step size settings apply to the destination address
      dmac_stepsel_31: Step size settings apply to the destination address
      dmac_stepsel_4: Step size settings apply to the destination address
      dmac_stepsel_5: Step size settings apply to the destination address
      dmac_stepsel_6: Step size settings apply to the destination address
      dmac_stepsel_7: Step size settings apply to the destination address
      dmac_stepsel_8: Step size settings apply to the destination address
      dmac_stepsel_9: Step size settings apply to the destination address
      dmac_stepsize_0: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_1: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_10: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_11: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_12: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_13: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_14: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_15: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_16: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_17: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_18: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_19: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_2: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_20: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_21: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_22: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_23: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_24: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_25: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_26: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_27: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_28: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_29: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_3: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_30: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_31: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_4: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_5: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_6: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_7: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_8: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_9: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_trifsrc_0: Only software/event triggers
      dmac_trifsrc_1: Only software/event triggers
      dmac_trifsrc_10: Only software/event triggers
      dmac_trifsrc_11: Only software/event triggers
      dmac_trifsrc_12: Only software/event triggers
      dmac_trifsrc_13: Only software/event triggers
      dmac_trifsrc_14: Only software/event triggers
      dmac_trifsrc_15: Only software/event triggers
      dmac_trifsrc_16: Only software/event triggers
      dmac_trifsrc_17: Only software/event triggers
      dmac_trifsrc_18: Only software/event triggers
      dmac_trifsrc_19: Only software/event triggers
      dmac_trifsrc_2: Only software/event triggers
      dmac_trifsrc_20: Only software/event triggers
      dmac_trifsrc_21: Only software/event triggers
      dmac_trifsrc_22: Only software/event triggers
      dmac_trifsrc_23: Only software/event triggers
      dmac_trifsrc_24: Only software/event triggers
      dmac_trifsrc_25: Only software/event triggers
      dmac_trifsrc_26: Only software/event triggers
      dmac_trifsrc_27: Only software/event triggers
      dmac_trifsrc_28: Only software/event triggers
      dmac_trifsrc_29: Only software/event triggers
      dmac_trifsrc_3: Only software/event triggers
      dmac_trifsrc_30: Only software/event triggers
      dmac_trifsrc_31: Only software/event triggers
      dmac_trifsrc_4: Only software/event triggers
      dmac_trifsrc_5: Only software/event triggers
      dmac_trifsrc_6: Only software/event triggers
      dmac_trifsrc_7: Only software/event triggers
      dmac_trifsrc_8: Only software/event triggers
      dmac_trifsrc_9: Only software/event triggers
      dmac_trigact_0: One trigger required for each block transfer
      dmac_trigact_1: One trigger required for each block transfer
      dmac_trigact_10: One trigger required for each block transfer
      dmac_trigact_11: One trigger required for each block transfer
      dmac_trigact_12: One trigger required for each block transfer
      dmac_trigact_13: One trigger required for each block transfer
      dmac_trigact_14: One trigger required for each block transfer
      dmac_trigact_15: One trigger required for each block transfer
      dmac_trigact_16: One trigger required for each block transfer
      dmac_trigact_17: One trigger required for each block transfer
      dmac_trigact_18: One trigger required for each block transfer
      dmac_trigact_19: One trigger required for each block transfer
      dmac_trigact_2: One trigger required for each block transfer
      dmac_trigact_20: One trigger required for each block transfer
      dmac_trigact_21: One trigger required for each block transfer
      dmac_trigact_22: One trigger required for each block transfer
      dmac_trigact_23: One trigger required for each block transfer
      dmac_trigact_24: One trigger required for each block transfer
      dmac_trigact_25: One trigger required for each block transfer
      dmac_trigact_26: One trigger required for each block transfer
      dmac_trigact_27: One trigger required for each block transfer
      dmac_trigact_28: One trigger required for each block transfer
      dmac_trigact_29: One trigger required for each block transfer
      dmac_trigact_3: One trigger required for each block transfer
      dmac_trigact_30: One trigger required for each block transfer
      dmac_trigact_31: One trigger required for each block transfer
      dmac_trigact_4: One trigger required for each block transfer
      dmac_trigact_5: One trigger required for each block transfer
      dmac_trigact_6: One trigger required for each block transfer
      dmac_trigact_7: One trigger required for each block transfer
      dmac_trigact_8: One trigger required for each block transfer
      dmac_trigact_9: One trigger required for each block transfer
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  GCLK:
    user_label: GCLK
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::GCLK::driver_config_definition::GCLK::HAL:HPL:GCLK
    functionality: System
    api: HAL:HPL:GCLK
    configuration:
      $input: 32768
      $input_id: 32kHz Ultra Low Power Internal Oscillator (OSCULP32K)
      RESERVED_InputFreq: 32768
      RESERVED_InputFreq_id: 32kHz Ultra Low Power Internal Oscillator (OSCULP32K)
      _$freq_output_Generic clock generator 0: 120000000
      _$freq_output_Generic clock generator 1: 48000000
      _$freq_output_Generic clock generator 10: 12000000
      _$freq_output_Generic clock generator 11: 2000000
      _$freq_output_Generic clock generator 2: 12500000
      _$freq_output_Generic clock generator 3: 32768
      _$freq_output_Generic clock generator 4: 50000000
      _$freq_output_Generic clock generator 5: 20000000
      _$freq_output_Generic clock generator 6: 7058823.529411765
      _$freq_output_Generic clock generator 7: 12000000
      _$freq_output_Generic clock generator 8: 12000000
      _$freq_output_Generic clock generator 9: 12000000
      enable_gclk_gen_0: true
      enable_gclk_gen_0__externalclock: 1000000
      enable_gclk_gen_1: true
      enable_gclk_gen_10: false
      enable_gclk_gen_10__externalclock: 1000000
      enable_gclk_gen_11: false
      enable_gclk_gen_11__externalclock: 1000000
      enable_gclk_gen_1__externalclock: 1000000
      enable_gclk_gen_2: true
      enable_gclk_gen_2__externalclock: 1000000
      enable_gclk_gen_3: true
      enable_gclk_gen_3__externalclock: 1000000
      enable_gclk_gen_4: true
      enable_gclk_gen_4__externalclock: 1000000
      enable_gclk_gen_5: true
      enable_gclk_gen_5__externalclock: 1000000
      enable_gclk_gen_6: true
      enable_gclk_gen_6__externalclock: 1000000
      enable_gclk_gen_7: false
      enable_gclk_gen_7__externalclock: 1000000
      enable_gclk_gen_8: false
      enable_gclk_gen_8__externalclock: 1000000
      enable_gclk_gen_9: false
      enable_gclk_gen_9__externalclock: 1000000
      gclk_arch_gen_0_enable: true
      gclk_arch_gen_0_idc: false
      gclk_arch_gen_0_oe: false
      gclk_arch_gen_0_oov: false
      gclk_arch_gen_0_runstdby: false
      gclk_arch_gen_10_enable: false
      gclk_arch_gen_10_idc: false
      gclk_arch_gen_10_oe: false
      gclk_arch_gen_10_oov: false
      gclk_arch_gen_10_runstdby: false
      gclk_arch_gen_11_enable: false
      gclk_arch_gen_11_idc: false
      gclk_arch_gen_11_oe: false
      gclk_arch_gen_11_oov: false
      gclk_arch_gen_11_runstdby: false
      gclk_arch_gen_1_enable: true
      gclk_arch_gen_1_idc: false
      gclk_arch_gen_1_oe: false
      gclk_arch_gen_1_oov: false
      gclk_arch_gen_1_runstdby: false
      gclk_arch_gen_2_enable: true
      gclk_arch_gen_2_idc: false
      gclk_arch_gen_2_oe: false
      gclk_arch_gen_2_oov: false
      gclk_arch_gen_2_runstdby: false
      gclk_arch_gen_3_enable: true
      gclk_arch_gen_3_idc: false
      gclk_arch_gen_3_oe: false
      gclk_arch_gen_3_oov: false
      gclk_arch_gen_3_runstdby: false
      gclk_arch_gen_4_enable: true
      gclk_arch_gen_4_idc: false
      gclk_arch_gen_4_oe: true
      gclk_arch_gen_4_oov: false
      gclk_arch_gen_4_runstdby: false
      gclk_arch_gen_5_enable: true
      gclk_arch_gen_5_idc: false
      gclk_arch_gen_5_oe: true
      gclk_arch_gen_5_oov: false
      gclk_arch_gen_5_runstdby: false
      gclk_arch_gen_6_enable: true
      gclk_arch_gen_6_idc: false
      gclk_arch_gen_6_oe: false
      gclk_arch_gen_6_oov: false
      gclk_arch_gen_6_runstdby: false
      gclk_arch_gen_7_enable: false
      gclk_arch_gen_7_idc: false
      gclk_arch_gen_7_oe: false
      gclk_arch_gen_7_oov: false
      gclk_arch_gen_7_runstdby: false
      gclk_arch_gen_8_enable: false
      gclk_arch_gen_8_idc: false
      gclk_arch_gen_8_oe: false
      gclk_arch_gen_8_oov: false
      gclk_arch_gen_8_runstdby: false
      gclk_arch_gen_9_enable: false
      gclk_arch_gen_9_idc: false
      gclk_arch_gen_9_oe: false
      gclk_arch_gen_9_oov: false
      gclk_arch_gen_9_runstdby: false
      gclk_gen_0_div: 1
      gclk_gen_0_div_sel: false
      gclk_gen_0_oscillator: Digital Phase Locked Loop (DPLL0)
      gclk_gen_10_div: 1
      gclk_gen_10_div_sel: false
      gclk_gen_10_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
      gclk_gen_11_div: 6
      gclk_gen_11_div_sel: false
      gclk_gen_11_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
      gclk_gen_1_div: 1
      gclk_gen_1_div_sel: false
      gclk_gen_1_oscillator: Digital Frequency Locked Loop (DFLL48M)
      gclk_gen_2_div: 200
      gclk_gen_2_div_sel: false
      gclk_gen_2_oscillator: Digital Phase Locked Loop (DPLL1)
      gclk_gen_3_div: 1
      gclk_gen_3_div_sel: false
      gclk_gen_3_oscillator: 32kHz Ultra Low Power Internal Oscillator (OSCULP32K)
      gclk_gen_4_div: 2
      gclk_gen_4_div_sel: false
      gclk_gen_4_oscillator: Digital Phase Locked Loop (DPLL1)
      gclk_gen_5_div: 5
      gclk_gen_5_div_sel: false
      gclk_gen_5_oscillator: Digital Phase Locked Loop (DPLL1)
      gclk_gen_6_div: 17
      gclk_gen_6_div_sel: false
      gclk_gen_6_oscillator: Digital Phase Locked Loop (DPLL0)
      gclk_gen_7_div: 1
      gclk_gen_7_div_sel: false
      gclk_gen_7_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
      gclk_gen_8_div: 1
      gclk_gen_8_div_sel: false
      gclk_gen_8_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
      gclk_gen_9_div: 1
      gclk_gen_9_div_sel: false
      gclk_gen_9_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  MCLK:
    user_label: MCLK
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::MCLK::driver_config_definition::MCLK::HAL:HPL:MCLK
    functionality: System
    api: HAL:HPL:MCLK
    configuration:
      $input: 120000000
      $input_id: Generic clock generator 0
      RESERVED_InputFreq: 120000000
      RESERVED_InputFreq_id: Generic clock generator 0
      _$freq_output_CPU: 120000000
      cpu_clock_source: Generic clock generator 0
      cpu_div: '1'
      enable_cpu_clock: true
      mclk_arch_bupdiv: Divide by 8
      mclk_arch_hsdiv: Divide by 1
      mclk_arch_lpdiv: Divide by 4
      nvm_wait_states: '0'
    optional_signals: []
    variant: null
    clocks:
      domain_group:
        nodes:
        - name: CPU
          input: CPU
          external: false
          external_frequency: 0
        configuration: {}
  OSC32KCTRL:
    user_label: OSC32KCTRL
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::OSC32KCTRL::driver_config_definition::OSC32KCTRL::HAL:HPL:OSC32KCTRL
    functionality: System
    api: HAL:HPL:OSC32KCTRL
    configuration:
      $input: 32768
      $input_id: 32kHz Ultra Low Power Internal Oscillator (OSCULP32K)
      RESERVED_InputFreq: 32768
      RESERVED_InputFreq_id: 32kHz Ultra Low Power Internal Oscillator (OSCULP32K)
      _$freq_output_RTC source: 1024
      enable_osculp32k: true
      enable_rtc_source: false
      enable_xosc32k: false
      osculp32k_calib: 0
      osculp32k_calib_enable: false
      rtc_1khz_selection: true
      rtc_source_oscillator: 32kHz Ultra Low Power Internal Oscillator (OSCULP32K)
      xosc32k_arch_cfden: false
      xosc32k_arch_cfdeo: false
      xosc32k_arch_cgm: Standard mode
      xosc32k_arch_en1k: true
      xosc32k_arch_en32k: true
      xosc32k_arch_enable: false
      xosc32k_arch_ondemand: false
      xosc32k_arch_runstdby: true
      xosc32k_arch_startup: 62592us
      xosc32k_arch_swben: false
      xosc32k_arch_xtalen: true
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  OSCCTRL:
    user_label: OSCCTRL
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::OSCCTRL::driver_config_definition::OSCCTRL::HAL:HPL:OSCCTRL
    functionality: System
    api: HAL:HPL:OSCCTRL
    configuration:
      $input: 32768
      $input_id: Generic clock generator 3
      RESERVED_InputFreq: 32768
      RESERVED_InputFreq_id: Generic clock generator 3
      _$freq_output_Digital Frequency Locked Loop (DFLL48M): 48000000
      _$freq_output_Digital Phase Locked Loop (DPLL0): 120000000
      _$freq_output_Digital Phase Locked Loop (DPLL1): 100000000
      _$freq_output_External Crystal Oscillator 8-48MHz (XOSC0): 12000000
      _$freq_output_External Crystal Oscillator 8-48MHz (XOSC1): 12000000
      dfll_arch_bplckc: true
      dfll_arch_calibration: false
      dfll_arch_ccdis: true
      dfll_arch_coarse: 31
      dfll_arch_cstep: 1
      dfll_arch_enable: true
      dfll_arch_fine: 128
      dfll_arch_fstep: 10
      dfll_arch_llaw: false
      dfll_arch_ondemand: false
      dfll_arch_qldis: false
      dfll_arch_runstdby: false
      dfll_arch_stable: true
      dfll_arch_usbcrm: true
      dfll_arch_waitlock: false
      dfll_mode: Closed Loop Mode
      dfll_mul: 48000
      dfll_ref_clock: Generic clock generator 3
      enable_dfll: true
      enable_fdpll0: true
      enable_fdpll1: true
      enable_xosc0: false
      enable_xosc1: true
      fdpll0_arch_dcoen: false
      fdpll0_arch_enable: true
      fdpll0_arch_filter: 0
      fdpll0_arch_lbypass: false
      fdpll0_arch_ltime: No time-out, automatic lock
      fdpll0_arch_ondemand: false
      fdpll0_arch_refclk: XOSC1 clock reference
      fdpll0_arch_runstdby: false
      fdpll0_arch_wuf: false
      fdpll0_clock_dcofilter: 0
      fdpll0_clock_div: 2
      fdpll0_ldr: 59
      fdpll0_ldrfrac: 0
      fdpll0_ref_clock: External Crystal Oscillator 8-48MHz (XOSC1)
      fdpll1_arch_dcoen: false
      fdpll1_arch_enable: true
      fdpll1_arch_filter: 0
      fdpll1_arch_lbypass: false
      fdpll1_arch_ltime: No time-out, automatic lock
      fdpll1_arch_ondemand: false
      fdpll1_arch_refclk: XOSC1 clock reference
      fdpll1_arch_runstdby: false
      fdpll1_arch_wuf: false
      fdpll1_clock_dcofilter: 0
      fdpll1_clock_div: 2
      fdpll1_ldr: 49
      fdpll1_ldrfrac: 0
      fdpll1_ref_clock: External Crystal Oscillator 8-48MHz (XOSC1)
      xosc0_arch_cfden: false
      xosc0_arch_enable: false
      xosc0_arch_enalc: false
      xosc0_arch_lowbufgain: false
      xosc0_arch_ondemand: false
      xosc0_arch_runstdby: false
      xosc0_arch_startup: 31us
      xosc0_arch_swben: false
      xosc0_arch_xtalen: false
      xosc0_frequency: 12000000
      xosc1_arch_cfden: false
      xosc1_arch_enable: true
      xosc1_arch_enalc: false
      xosc1_arch_lowbufgain: false
      xosc1_arch_ondemand: false
      xosc1_arch_runstdby: false
      xosc1_arch_startup: 31us
      xosc1_arch_swben: false
      xosc1_arch_xtalen: true
      xosc1_frequency: 12000000
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  PORT:
    user_label: PORT
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::PORT::driver_config_definition::PORT::HAL:HPL:PORT
    functionality: System
    api: HAL:HPL:PORT
    configuration:
      enable_port_input_event_0: false
      enable_port_input_event_1: false
      enable_port_input_event_2: false
      enable_port_input_event_3: false
      porta_event_action_0: Output register of pin will be set to level of event
      porta_event_action_1: Output register of pin will be set to level of event
      porta_event_action_2: Output register of pin will be set to level of event
      porta_event_action_3: Output register of pin will be set to level of event
      porta_event_pin_identifier_0: 0
      porta_event_pin_identifier_1: 0
      porta_event_pin_identifier_2: 0
      porta_event_pin_identifier_3: 0
      porta_input_event_enable_0: false
      porta_input_event_enable_1: false
      porta_input_event_enable_2: false
      porta_input_event_enable_3: false
      portb_event_action_0: Output register of pin will be set to level of event
      portb_event_action_1: Output register of pin will be set to level of event
      portb_event_action_2: Output register of pin will be set to level of event
      portb_event_action_3: Output register of pin will be set to level of event
      portb_event_pin_identifier_0: 0
      portb_event_pin_identifier_1: 0
      portb_event_pin_identifier_2: 0
      portb_event_pin_identifier_3: 0
      portb_input_event_enable_0: false
      portb_input_event_enable_1: false
      portb_input_event_enable_2: false
      portb_input_event_enable_3: false
      portc_event_action_0: Output register of pin will be set to level of event
      portc_event_action_1: Output register of pin will be set to level of event
      portc_event_action_2: Output register of pin will be set to level of event
      portc_event_action_3: Output register of pin will be set to level of event
      portc_event_pin_identifier_0: 0
      portc_event_pin_identifier_1: 0
      portc_event_pin_identifier_2: 0
      portc_event_pin_identifier_3: 0
      portc_input_event_enable_0: false
      portc_input_event_enable_1: false
      portc_input_event_enable_2: false
      portc_input_event_enable_3: false
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  RAMECC:
    user_label: RAMECC
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::RAMECC::driver_config_definition::RAMECC::HAL:HPL:RAMECC
    functionality: System
    api: HAL:HPL:RAMECC
    configuration: {}
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  CALENDAR_0:
    user_label: CALENDAR_0
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::RTC::driver_config_definition::Calendar::HAL:Driver:Calendar
    functionality: Calendar
    api: HAL:Driver:Calendar
    configuration:
      rtc_arch_init_reset: true
      rtc_arch_prescaler: Peripheral clock divided by 1024
      rtc_cmpeo0: false
      rtc_cmpeo1: false
      rtc_event_control: false
      rtc_ovfeo: false
      rtc_pereo0: false
      rtc_pereo1: false
      rtc_pereo2: false
      rtc_pereo3: false
      rtc_pereo4: false
      rtc_pereo5: false
      rtc_pereo6: false
      rtc_pereo7: false
      rtc_tamper_active_layer_frequency_prescalar: DIV2 CLK_RTC_OUT is CLK_RTC /2
      rtc_tamper_debounce_frequency_prescalar: DIV2 CLK_RTC_DEB is CLK_RTC /2
      rtc_tamper_input_action_0: OFF(Disabled)
      rtc_tamper_input_action_1: OFF(Disabled)
      rtc_tamper_input_action_2: OFF(Disabled)
      rtc_tamper_input_action_3: OFF(Disabled)
      rtc_tamper_input_action_4: OFF(Disabled)
      rtc_tampereo: false
      rtc_tampevei: false
      tamper_debounce_enable_0: false
      tamper_debounce_enable_1: false
      tamper_debounce_enable_2: false
      tamper_debounce_enable_3: false
      tamper_debounce_enable_4: false
      tamper_input_0_settings: false
      tamper_input_1_settings: false
      tamper_input_2_settings: false
      tamper_input_3_settings: false
      tamper_input_4_settings: false
      tamper_level_0: false
      tamper_level_1: false
      tamper_level_2: false
      tamper_level_3: false
      tamper_level_4: false
    optional_signals: []
    variant: null
    clocks:
      domain_group:
        nodes:
        - name: RTC
          input: RTC source
          external: false
          external_frequency: 0
        configuration:
          rtc_clk_selection: RTC source
  SIM0:
    user_label: SIM0
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::SERCOM0::driver_config_definition::USART.with.ISO7816::HAL:Driver:USART.Async
    functionality: USART
    api: HAL:Driver:USART_Async
    configuration:
      usart_advanced: false
      usart_arch_clock_mode: USART with internal clock
      usart_arch_cloden: false
      usart_arch_dbgstop: Keep running
      usart_arch_dord: LSB is transmitted first
      usart_arch_ibon: false
      usart_arch_runstdby: false
      usart_arch_sfde: false
      usart_baud_rate: 6720
      usart_character_size: 8 bits
      usart_dsnack: The successive receive NACK is disable.
      usart_gtime: 2-bit times
      usart_inack: NACK is transmitted when a parity error is received.
      usart_inverse_enabled: false
      usart_iso7816_type: T=1
      usart_maxiter: 7
      usart_parity: Even parity
      usart_rx_enable: true
      usart_stop_bit: Two stop bits
      usart_tx_enable: true
    optional_signals: []
    variant:
      specification: TXPO=2, RXPO=0
      required_signals:
      - name: SERCOM0/PAD/0
        pad: PA04
        label: RX/TX
    clocks:
      domain_group:
        nodes:
        - name: Core
          input: Generic clock generator 2
          external: false
          external_frequency: 0
        - name: Slow
          input: Generic clock generator 3
          external: false
          external_frequency: 0
        configuration:
          core_gclk_selection: Generic clock generator 2
          slow_gclk_selection: Generic clock generator 3
  SIM1:
    user_label: SIM1
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::SERCOM1::driver_config_definition::USART.with.ISO7816::HAL:Driver:USART.Async
    functionality: USART
    api: HAL:Driver:USART_Async
    configuration:
      usart_advanced: false
      usart_arch_clock_mode: USART with internal clock
      usart_arch_cloden: false
      usart_arch_dbgstop: Keep running
      usart_arch_dord: LSB is transmitted first
      usart_arch_ibon: false
      usart_arch_runstdby: false
      usart_arch_sfde: false
      usart_baud_rate: 6720
      usart_character_size: 8 bits
      usart_dsnack: The successive receive NACK is disable.
      usart_gtime: 2-bit times
      usart_inack: NACK is transmitted when a parity error is received.
      usart_inverse_enabled: false
      usart_iso7816_type: T=1
      usart_maxiter: 7
      usart_parity: Even parity
      usart_rx_enable: true
      usart_stop_bit: Two stop bits
      usart_tx_enable: true
    optional_signals: []
    variant:
      specification: TXPO=2, RXPO=0
      required_signals:
      - name: SERCOM1/PAD/0
        pad: PA16
        label: RX/TX
    clocks:
      domain_group:
        nodes:
        - name: Core
          input: Generic clock generator 2
          external: false
          external_frequency: 0
        - name: Slow
          input: Generic clock generator 3
          external: false
          external_frequency: 0
        configuration:
          core_gclk_selection: Generic clock generator 2
          slow_gclk_selection: Generic clock generator 3
  SIM2:
    user_label: SIM2
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::SERCOM2::driver_config_definition::USART.with.ISO7816::HAL:Driver:USART.Async
    functionality: USART
    api: HAL:Driver:USART_Async
    configuration:
      usart_advanced: false
      usart_arch_clock_mode: USART with internal clock
      usart_arch_cloden: false
      usart_arch_dbgstop: Keep running
      usart_arch_dord: LSB is transmitted first
      usart_arch_ibon: false
      usart_arch_runstdby: false
      usart_arch_sfde: false
      usart_baud_rate: 6720
      usart_character_size: 8 bits
      usart_dsnack: The successive receive NACK is disable.
      usart_gtime: 2-bit times
      usart_inack: NACK is transmitted when a parity error is received.
      usart_inverse_enabled: false
      usart_iso7816_type: T=1
      usart_maxiter: 7
      usart_parity: Even parity
      usart_rx_enable: true
      usart_stop_bit: Two stop bits
      usart_tx_enable: true
    optional_signals: []
    variant:
      specification: TXPO=2, RXPO=0
      required_signals:
      - name: SERCOM2/PAD/0
        pad: PA09
        label: RX/TX
    clocks:
      domain_group:
        nodes:
        - name: Core
          input: Generic clock generator 2
          external: false
          external_frequency: 0
        - name: Slow
          input: Generic clock generator 3
          external: false
          external_frequency: 0
        configuration:
          core_gclk_selection: Generic clock generator 2
          slow_gclk_selection: Generic clock generator 3
  SIM3:
    user_label: SIM3
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::SERCOM3::driver_config_definition::USART.with.ISO7816::HAL:Driver:USART.Async
    functionality: USART
    api: HAL:Driver:USART_Async
    configuration:
      usart_advanced: false
      usart_arch_clock_mode: USART with internal clock
      usart_arch_cloden: false
      usart_arch_dbgstop: Keep running
      usart_arch_dord: LSB is transmitted first
      usart_arch_ibon: false
      usart_arch_runstdby: false
      usart_arch_sfde: false
      usart_baud_rate: 6720
      usart_character_size: 8 bits
      usart_dsnack: The successive receive NACK is disable.
      usart_gtime: 2-bit times
      usart_inack: NACK is transmitted when a parity error is received.
      usart_inverse_enabled: false
      usart_iso7816_type: T=1
      usart_maxiter: 7
      usart_parity: Even parity
      usart_rx_enable: true
      usart_stop_bit: Two stop bits
      usart_tx_enable: true
    optional_signals: []
    variant:
      specification: TXPO=2, RXPO=0
      required_signals:
      - name: SERCOM3/PAD/0
        pad: PB20
        label: RX/TX
    clocks:
      domain_group:
        nodes:
        - name: Core
          input: Generic clock generator 2
          external: false
          external_frequency: 0
        - name: Slow
          input: Generic clock generator 3
          external: false
          external_frequency: 0
        configuration:
          core_gclk_selection: Generic clock generator 2
          slow_gclk_selection: Generic clock generator 3
  SIM4:
    user_label: SIM4
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::SERCOM4::driver_config_definition::USART.with.ISO7816::HAL:Driver:USART.Async
    functionality: USART
    api: HAL:Driver:USART_Async
    configuration:
      usart_advanced: false
      usart_arch_clock_mode: USART with internal clock
      usart_arch_cloden: false
      usart_arch_dbgstop: Keep running
      usart_arch_dord: LSB is transmitted first
      usart_arch_ibon: false
      usart_arch_runstdby: false
      usart_arch_sfde: false
      usart_baud_rate: 6720
      usart_character_size: 8 bits
      usart_dsnack: The successive receive NACK is disable.
      usart_gtime: 2-bit times
      usart_inack: NACK is transmitted when a parity error is received.
      usart_inverse_enabled: false
      usart_iso7816_type: T=1
      usart_maxiter: 7
      usart_parity: Even parity
      usart_rx_enable: true
      usart_stop_bit: Two stop bits
      usart_tx_enable: true
    optional_signals: []
    variant:
      specification: TXPO=2, RXPO=0
      required_signals:
      - name: SERCOM4/PAD/0
        pad: PB08
        label: RX/TX
    clocks:
      domain_group:
        nodes:
        - name: Core
          input: Generic clock generator 2
          external: false
          external_frequency: 0
        - name: Slow
          input: Generic clock generator 3
          external: false
          external_frequency: 0
        configuration:
          core_gclk_selection: Generic clock generator 2
          slow_gclk_selection: Generic clock generator 3
  SIM5:
    user_label: SIM5
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::SERCOM5::driver_config_definition::USART.with.ISO7816::HAL:Driver:USART.Async
    functionality: USART
    api: HAL:Driver:USART_Async
    configuration:
      usart_advanced: false
      usart_arch_clock_mode: USART with internal clock
      usart_arch_cloden: false
      usart_arch_dbgstop: Keep running
      usart_arch_dord: LSB is transmitted first
      usart_arch_ibon: false
      usart_arch_runstdby: false
      usart_arch_sfde: false
      usart_baud_rate: 6720
      usart_character_size: 8 bits
      usart_dsnack: The successive receive NACK is disable.
      usart_gtime: 2-bit times
      usart_inack: NACK is transmitted when a parity error is received.
      usart_inverse_enabled: false
      usart_iso7816_type: T=1
      usart_maxiter: 7
      usart_parity: Even parity
      usart_rx_enable: true
      usart_stop_bit: Two stop bits
      usart_tx_enable: true
    optional_signals: []
    variant:
      specification: TXPO=2, RXPO=0
      required_signals:
      - name: SERCOM5/PAD/0
        pad: PB16
        label: RX/TX
    clocks:
      domain_group:
        nodes:
        - name: Core
          input: Generic clock generator 2
          external: false
          external_frequency: 0
        - name: Slow
          input: Generic clock generator 3
          external: false
          external_frequency: 0
        configuration:
          core_gclk_selection: Generic clock generator 2
          slow_gclk_selection: Generic clock generator 3
  SIM6:
    user_label: SIM6
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::SERCOM6::driver_config_definition::USART.with.ISO7816::HAL:Driver:USART.Async
    functionality: USART
    api: HAL:Driver:USART_Async
    configuration:
      usart_advanced: false
      usart_arch_clock_mode: USART with internal clock
      usart_arch_cloden: false
      usart_arch_dbgstop: Keep running
      usart_arch_dord: LSB is transmitted first
      usart_arch_ibon: false
      usart_arch_runstdby: false
      usart_arch_sfde: false
      usart_baud_rate: 6720
      usart_character_size: 8 bits
      usart_dsnack: The successive receive NACK is disable.
      usart_gtime: 2-bit times
      usart_inack: NACK is transmitted when a parity error is received.
      usart_inverse_enabled: false
      usart_iso7816_type: T=1
      usart_maxiter: 7
      usart_parity: Even parity
      usart_rx_enable: true
      usart_stop_bit: Two stop bits
      usart_tx_enable: true
    optional_signals: []
    variant:
      specification: TXPO=2, RXPO=0
      required_signals:
      - name: SERCOM6/PAD/0
        pad: PC16
        label: RX/TX
    clocks:
      domain_group:
        nodes:
        - name: Core
          input: Generic clock generator 2
          external: false
          external_frequency: 0
        - name: Slow
          input: Generic clock generator 3
          external: false
          external_frequency: 0
        configuration:
          core_gclk_selection: Generic clock generator 2
          slow_gclk_selection: Generic clock generator 3
  UART_debug:
    user_label: UART_debug
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::SERCOM7::driver_config_definition::UART::HAL:Driver:USART.Sync
    functionality: USART
    api: HAL:Driver:USART_Sync
    configuration:
      usart_advanced: false
      usart_arch_clock_mode: USART with internal clock
      usart_arch_cloden: false
      usart_arch_dbgstop: Keep running
      usart_arch_dord: LSB is transmitted first
      usart_arch_enc: No encoding
      usart_arch_fractional: 0
      usart_arch_ibon: false
      usart_arch_lin_slave_enable: Disable
      usart_arch_runstdby: false
      usart_arch_sampa: 7-8-9 (3-4-5 8-bit over-sampling)
      usart_arch_sampr: 16x arithmetic
      usart_arch_sfde: false
      usart_baud_rate: 921600
      usart_character_size: 8 bits
      usart_parity: No parity
      usart_rx_enable: true
      usart_stop_bit: One stop bit
      usart_tx_enable: true
    optional_signals: []
    variant:
      specification: TXPO=0, RXPO=1, CMODE=0
      required_signals:
      - name: SERCOM7/PAD/0
        pad: PB30
        label: TX
      - name: SERCOM7/PAD/1
        pad: PB31
        label: RX
    clocks:
      domain_group:
        nodes:
        - name: Core
          input: Generic clock generator 4
          external: false
          external_frequency: 0
        - name: Slow
          input: Generic clock generator 3
          external: false
          external_frequency: 0
        configuration:
          core_gclk_selection: Generic clock generator 4
          slow_gclk_selection: Generic clock generator 3
  USB_DEVICE_INSTANCE:
    user_label: USB_DEVICE_INSTANCE
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::USB::driver_config_definition::USB.Device::HAL:Driver:USB.Device
    functionality: USB
    api: HAL:Driver:USB_Device
    configuration:
      usb_arch_ep0_cache: Cached by 64 bytes buffer
      usb_arch_ep1_cache: Cached by 64 bytes buffer
      usb_arch_ep2_cache: Cached by 64 bytes buffer
      usb_arch_ep3_cache: Cached by 64 bytes buffer
      usb_arch_ep4_cache: Cached by 64 bytes buffer
      usb_arch_ep5_cache: Cached by 64 bytes buffer
      usb_arch_ep6_cache: Cached by 64 bytes buffer
      usb_arch_ep7_cache: Cached by 64 bytes buffer
      usb_ep1_I_CACHE: No cache
      usb_ep2_I_CACHE: No cache
      usb_ep3_I_CACHE: No cache
      usb_ep4_I_CACHE: No cache
      usb_ep5_I_CACHE: No cache
      usb_ep6_I_CACHE: No cache
      usb_ep7_I_CACHE: No cache
      usbd_arch_max_ep_n: 4 (EP 0x84 or 0x04)
      usbd_arch_speed: Full speed
      usbd_num_ep_sp: 7 (EP0 + 6 endpoints)
    optional_signals: []
    variant:
      specification: default
      required_signals:
      - name: USB/DM
        pad: PA24
        label: Data-
      - name: USB/DP
        pad: PA25
        label: Data+
    clocks:
      domain_group:
        nodes:
        - name: USB
          input: Generic clock generator 1
          external: false
          external_frequency: 0
        configuration:
          usb_gclk_selection: Generic clock generator 1
pads:
  SIM0_INT:
    name: PC00
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PC00
    mode: Digital input
    user_label: SIM0_INT
    configuration: null
  SIM1_INT:
    name: PC01
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PC01
    mode: Digital input
    user_label: SIM1_INT
    configuration: null
  SIM2_INT:
    name: PC02
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PC02
    mode: Digital input
    user_label: SIM2_INT
    configuration: null
  SIM3_INT:
    name: PC03
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PC03
    mode: Digital input
    user_label: SIM3_INT
    configuration: null
  SIM4_INT:
    name: PA02
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA02
    mode: Digital input
    user_label: SIM4_INT
    configuration: null
  SIM5_INT:
    name: PA03
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA03
    mode: Digital input
    user_label: SIM5_INT
    configuration: null
  SIM6_INT:
    name: PB04
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB04
    mode: Digital input
    user_label: SIM6_INT
    configuration: null
  SIM7_INT:
    name: PB05
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB05
    mode: Digital input
    user_label: SIM7_INT
    configuration: null
  SCL3:
    name: PB06
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB06
    mode: Digital output
    user_label: SCL3
    configuration: null
  SDA3:
    name: PB07
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB07
    mode: Digital output
    user_label: SDA3
    configuration: null
  SIM4_IO:
    name: PB08
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB08
    mode: Peripheral IO
    user_label: SIM4_IO
    configuration: null
  SIM0_IO:
    name: PA04
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA04
    mode: Peripheral IO
    user_label: SIM0_IO
    configuration: null
  SIM2_IO:
    name: PA09
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA09
    mode: Peripheral IO
    user_label: SIM2_IO
    configuration: null
  RMII_CLOCK:
    name: PA10
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA10
    mode: Advanced
    user_label: RMII_CLOCK
    configuration:
      pad_direction: Out
      pad_function: M
      pad_initial_level: Low
      pad_pull_config: 'Off'
  SIMCLK_20MHZ:
    name: PA11
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA11
    mode: Advanced
    user_label: SIMCLK_20MHZ
    configuration:
      pad_direction: Out
      pad_function: M
      pad_initial_level: Low
      pad_pull_config: 'Off'
  SCL1:
    name: PB14
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB14
    mode: Digital output
    user_label: SCL1
    configuration: null
  SDA1:
    name: PB15
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB15
    mode: Digital output
    user_label: SDA1
    configuration: null
  SWITCH:
    name: PC14
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PC14
    mode: Digital input
    user_label: SWITCH
    configuration: null
  MUX_STAT:
    name: PC15
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PC15
    mode: Digital input
    user_label: MUX_STAT
    configuration: null
  SIM1_IO:
    name: PA16
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA16
    mode: Peripheral IO
    user_label: SIM1_IO
    configuration: null
  SIM6_IO:
    name: PC16
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PC16
    mode: Peripheral IO
    user_label: SIM6_IO
    configuration: null
  SIM5_IO:
    name: PB16
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB16
    mode: Peripheral IO
    user_label: SIM5_IO
    configuration: null
  SIM3_IO:
    name: PB20
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB20
    mode: Peripheral IO
    user_label: SIM3_IO
    configuration: null
  VB0:
    name: PA20
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA20
    mode: Digital input
    user_label: VB0
    configuration: null
  VB1:
    name: PA21
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA21
    mode: Digital input
    user_label: VB1
    configuration: null
  VB2:
    name: PA22
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA22
    mode: Digital input
    user_label: VB2
    configuration: null
  VB3:
    name: PA23
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA23
    mode: Digital input
    user_label: VB3
    configuration: null
  USBUP_D_N:
    name: PA24
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA24
    mode: Advanced
    user_label: USBUP_D_N
    configuration: null
  USBUP_D_P:
    name: PA25
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PA25
    mode: Advanced
    user_label: USBUP_D_P
    configuration: null
  USER_LED:
    name: PC26
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PC26
    mode: Digital output
    user_label: USER_LED
    configuration: null
  SCL4:
    name: PC27
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PC27
    mode: Digital output
    user_label: SCL4
    configuration: null
  SDA4:
    name: PC28
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PC28
    mode: Digital output
    user_label: SDA4
    configuration: null
  UART_TX:
    name: PB30
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB30
    mode: Peripheral IO
    user_label: UART_TX
    configuration: null
  UART_RX:
    name: PB31
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB31
    mode: Peripheral IO
    user_label: UART_RX
    configuration: null
  SCL2:
    name: PB02
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB02
    mode: Digital output
    user_label: SCL2
    configuration: null
  SDA2:
    name: PB03
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54N19A-AF::pad::PB03
    mode: Digital output
    user_label: SDA2
    configuration: null
toolchain_options: []
static_files: []
