+ CONFIG=generic
+ SITE_ID=1235
+ TRX_NUM=1
+ BTS_FEATURES=-fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX
+ respawn.sh osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
respawn: 0: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;31mDLINP[0;m[38;5;23m stream_cli.c:446 CLICONN(ts-0-1-oml,){CONNECTING} connect failed (-111)[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55eacb2de2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33351){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55eacb2dd9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55eacb2dd9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55eacb2dd9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 0: stopped pid 9858 with status 0
respawn: 1: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d6bde422a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37191){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d6bde419a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d6bde419a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d6bde419a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 1: stopped pid 10400 with status 0
respawn: 2: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561df83972a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38861){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561df83969a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561df83969a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561df83969a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 2: stopped pid 10492 with status 0
respawn: 3: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55fe03ed32a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41467){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55fe03ed29a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55fe03ed29a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55fe03ed29a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 3: stopped pid 19036 with status 0
respawn: 4: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56131698a2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33243){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5613169899a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5613169899a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5613169899a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 4: stopped pid 19128 with status 0
respawn: 5: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56258008b2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40415){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56258008a9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56258008a9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56258008a9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 5: stopped pid 19217 with status 0
respawn: 6: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561bbff4f2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45443){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561bbff4e9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561bbff4e9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561bbff4e9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 6: stopped pid 19301 with status 0
respawn: 7: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5593d4ce02a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39029){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5593d4cdf9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5593d4cdf9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5593d4cdf9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 7: stopped pid 19391 with status 0
respawn: 8: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56551061a2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34257){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5655106199a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5655106199a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5655106199a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 8: stopped pid 19474 with status 0
respawn: 9: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5602e79e62a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37871){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5602e79e59a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5602e79e59a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5602e79e59a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 9: stopped pid 19558 with status 0
respawn: 10: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x560e94eb22a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38619){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x560e94eb19a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x560e94eb19a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x560e94eb19a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 10: stopped pid 19647 with status 0
respawn: 11: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e80f81c2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38093){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e80f81b9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e80f81b9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e80f81b9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 11: stopped pid 19734 with status 0
respawn: 12: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5583c54d32a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46815){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5583c54d29a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5583c54d29a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5583c54d29a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 12: stopped pid 19822 with status 0
respawn: 13: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55684bb2d2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40593){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55684bb2c9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55684bb2c9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55684bb2c9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 13: stopped pid 19910 with status 0
respawn: 14: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x556c6a3782a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45075){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x556c6a3779a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x556c6a3779a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x556c6a3779a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 14: stopped pid 19997 with status 0
respawn: 15: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e5d02d02a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44667){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e5d02cf9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e5d02cf9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e5d02cf9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 15: stopped pid 20084 with status 0
respawn: 16: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x559b4151c2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34537){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x559b4151b9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x559b4151b9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x559b4151b9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 16: stopped pid 20161 with status 0
respawn: 17: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c23c0922a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35199){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c23c0919a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c23c0919a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c23c0919a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 17: stopped pid 20242 with status 0
respawn: 18: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x563fae1bf2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35613){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x563fae1be9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x563fae1be9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x563fae1be9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 18: stopped pid 20334 with status 0
respawn: 19: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x563aa62f92a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38153){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x563aa62f89a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x563aa62f89a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x563aa62f89a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 19: stopped pid 20414 with status 0
respawn: 20: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55afcd8e32a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46583){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55afcd8e29a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55afcd8e29a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55afcd8e29a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 20: stopped pid 20496 with status 0
respawn: 21: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ee564e52a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:32965){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ee564e49a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ee564e49a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ee564e49a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 21: stopped pid 20580 with status 0
respawn: 22: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c4890c52a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46883){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c4890c49a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c4890c49a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c4890c49a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 22: stopped pid 20662 with status 0
respawn: 23: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55637f1042a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46717){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55637f1039a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55637f1039a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55637f1039a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 23: stopped pid 20748 with status 0
respawn: 24: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561f71e4c2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42099){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561f71e4b9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561f71e4b9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561f71e4b9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 24: stopped pid 21089 with status 0
respawn: 25: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55afd041f2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39589){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55afd041e9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55afd041e9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55afd041e9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 25: stopped pid 21908 with status 0
respawn: 26: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e82d42a2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37933){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e82d4299a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e82d4299a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e82d4299a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 26: stopped pid 21988 with status 0
respawn: 27: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5615b4ead2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36227){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5615b4eac9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5615b4eac9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5615b4eac9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 27: stopped pid 22071 with status 0
respawn: 28: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5639a03262a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33601){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5639a03259a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5639a03259a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5639a03259a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 28: stopped pid 22155 with status 0
respawn: 29: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b174c302a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39161){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b174c2f9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b174c2f9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b174c2f9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 29: stopped pid 22238 with status 0
respawn: 30: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b278c3d2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43227){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b278c3c9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b278c3c9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b278c3c9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 30: stopped pid 22321 with status 0
respawn: 31: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55bdb3ece2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44925){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55bdb3ecd9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55bdb3ecd9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55bdb3ecd9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 31: stopped pid 24375 with status 0
respawn: 32: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e2ed2072a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40011){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e2ed2069a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e2ed2069a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e2ed2069a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 32: stopped pid 24476 with status 0
respawn: 33: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x559f3d4db2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43347){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x559f3d4da9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x559f3d4da9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x559f3d4da9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 33: stopped pid 24572 with status 0
respawn: 34: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5640ad34b2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34955){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5640ad34a9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5640ad34a9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5640ad34a9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 34: stopped pid 24677 with status 0
respawn: 35: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55be895d02a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33119){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55be895cf9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55be895cf9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55be895cf9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 35: stopped pid 24768 with status 0
respawn: 36: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55f0034442a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43613){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55f0034439a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55f0034439a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55f0034439a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 36: stopped pid 24868 with status 0
respawn: 37: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c444bbe2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36539){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c444bbd9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c444bbd9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c444bbd9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 37: stopped pid 24961 with status 0
respawn: 38: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b3dc14e2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39187){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b3dc14d9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b3dc14d9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b3dc14d9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 38: stopped pid 25047 with status 0
respawn: 39: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5595ab5eb2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33195){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5595ab5ea9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5595ab5ea9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5595ab5ea9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 39: stopped pid 25140 with status 0
respawn: 40: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e996de42a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45083){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e996de39a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e996de39a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e996de39a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 40: stopped pid 25236 with status 0
respawn: 41: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x564a35b442a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35301){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x564a35b439a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x564a35b439a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x564a35b439a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 41: stopped pid 26374 with status 0
respawn: 42: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x559c1f0a42a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37145){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x559c1f0a39a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x559c1f0a39a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x559c1f0a39a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 42: stopped pid 26478 with status 0
respawn: 43: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x560eb39972a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42333){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x560eb39969a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x560eb39969a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x560eb39969a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 43: stopped pid 26577 with status 0
respawn: 44: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b81520d2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34315){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b81520c9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b81520c9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b81520c9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 44: stopped pid 26677 with status 0
respawn: 45: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5610e64f62a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46053){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5610e64f59a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5610e64f59a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5610e64f59a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 45: stopped pid 26778 with status 0
respawn: 46: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d77aa762a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33245){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d77aa759a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d77aa759a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d77aa759a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 46: stopped pid 26878 with status 0
respawn: 47: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5590f08392a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44781){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5590f08389a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5590f08389a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5590f08389a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 47: stopped pid 26982 with status 0
respawn: 48: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5608001c82a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45389){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5608001c79a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5608001c79a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5608001c79a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 48: stopped pid 27079 with status 0
respawn: 49: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5583e59802a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40937){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5583e597f9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5583e597f9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5583e597f9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 49: stopped pid 27352 with status 0
respawn: 50: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x563e2438c2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39277){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x563e2438b9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x563e2438b9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x563e2438b9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 50: stopped pid 27455 with status 0
respawn: 51: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x556643c882a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46193){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x556643c879a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x556643c879a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x556643c879a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 51: stopped pid 27556 with status 0
respawn: 52: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55faf79692a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40589){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55faf79689a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55faf79689a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55faf79689a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 52: stopped pid 27658 with status 0
respawn: 53: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x563cb59a62a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40417){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;31mDABIS[0;m abis.c:105 OML link was closed early within 4 seconds. If this situation persists, please check your BTS and BSC configuration files for errors. A common error is a mismatch between unit_id configuration parameters of BTS and BSC.
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x563cb59a59a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x563cb59a59a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x563cb59a59a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 53: stopped pid 28529 with status 0
respawn: 54: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5578df0672a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34421){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5578df0669a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5578df0669a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5578df0669a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 54: stopped pid 28552 with status 0
respawn: 55: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5585a011b2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41939){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5585a011a9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5585a011a9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5585a011a9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 55: stopped pid 29355 with status 0
respawn: 56: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55de669542a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Unlocked -> Locked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1486 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM state already was Locked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46575){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55de669539a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55de669539a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55de669539a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 56: stopped pid 30055 with status 0
respawn: 57: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c6a264e2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36105){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c6a264d9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c6a264d9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c6a264d9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 57: stopped pid 30518 with status 0
respawn: 58: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5630205fd2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37527){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5630205fc9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5630205fc9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5630205fc9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 58: stopped pid 30937 with status 0
respawn: 59: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56214ace82a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39073){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56214ace79a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56214ace79a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56214ace79a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 59: stopped pid 31021 with status 0
respawn: 60: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x558de13302a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34039){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x558de132f9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x558de132f9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x558de132f9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 60: stopped pid 31109 with status 0
respawn: 61: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5638e35382a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41745){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;31mDABIS[0;m abis.c:105 OML link was closed early within 10 seconds. If this situation persists, please check your BTS and BSC configuration files for errors. A common error is a mismatch between unit_id configuration parameters of BTS and BSC.
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5638e35379a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5638e35379a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5638e35379a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 61: stopped pid 32961 with status 0
respawn: 62: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5642c3afb2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46435){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5642c3afa9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5642c3afa9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5642c3afa9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 62: stopped pid 33043 with status 0
respawn: 63: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x565225bf32a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44491){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x565225bf29a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x565225bf29a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x565225bf29a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 63: stopped pid 33127 with status 0
respawn: 64: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x564b0a6922a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33477){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x564b0a6919a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x564b0a6919a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x564b0a6919a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 64: stopped pid 33211 with status 0
respawn: 65: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55abfb9582a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45263){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55abfb9579a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55abfb9579a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55abfb9579a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 65: stopped pid 33296 with status 0
respawn: 66: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b273eb22a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40935){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b273eb19a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b273eb19a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b273eb19a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 66: stopped pid 33382 with status 0
respawn: 67: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ab694302a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:32973){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ab6942f9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ab6942f9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ab6942f9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 67: stopped pid 33469 with status 0
respawn: 68: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5602a83852a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38991){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5602a83849a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5602a83849a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5602a83849a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 68: stopped pid 33558 with status 0
respawn: 69: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55a13959d2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43557){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55a13959c9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55a13959c9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55a13959c9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 69: stopped pid 33650 with status 0
respawn: 70: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561fd058f2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41857){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561fd058e9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561fd058e9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561fd058e9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 70: stopped pid 33738 with status 0
respawn: 71: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5641632502a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42051){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56416324f9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56416324f9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56416324f9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 71: stopped pid 33824 with status 0
respawn: 72: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55fd9c6912a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38793){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55fd9c6909a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55fd9c6909a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55fd9c6909a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 72: stopped pid 33910 with status 0
respawn: 73: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x559da2a7b2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33789){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x559da2a7a9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x559da2a7a9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x559da2a7a9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 73: stopped pid 33992 with status 0
respawn: 74: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55fd26e002a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37893){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55fd26dff9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55fd26dff9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55fd26dff9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 74: stopped pid 34083 with status 0
respawn: 75: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d8154e72a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41611){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d8154e69a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d8154e69a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d8154e69a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 75: stopped pid 34164 with status 0
respawn: 76: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x556cb3e622a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45123){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x556cb3e619a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x556cb3e619a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x556cb3e619a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 76: stopped pid 34250 with status 0
respawn: 77: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x557c13c362a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45109){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x557c13c359a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x557c13c359a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x557c13c359a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 77: stopped pid 34349 with status 0
respawn: 78: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55aa096422a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39159){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55aa096419a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55aa096419a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55aa096419a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 78: stopped pid 34434 with status 0
respawn: 79: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x558beda742a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40011){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x558beda739a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x558beda739a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x558beda739a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 79: stopped pid 34517 with status 0
respawn: 80: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e40002a2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33383){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e4000299a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e4000299a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e4000299a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 80: stopped pid 34602 with status 0
respawn: 81: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561f8521f2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43721){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561f8521e9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561f8521e9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561f8521e9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 81: stopped pid 34680 with status 0
respawn: 82: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x564b5849d2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46061){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x564b5849c9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x564b5849c9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x564b5849c9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 82: stopped pid 34765 with status 0
respawn: 83: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5627359b22a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46361){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5627359b19a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5627359b19a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5627359b19a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 83: stopped pid 34847 with status 0
respawn: 84: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ee6223d2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38737){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ee6223c9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ee6223c9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ee6223c9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 84: stopped pid 34931 with status 0
respawn: 85: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5560457cd2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40781){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5560457cc9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5560457cc9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5560457cc9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 85: stopped pid 35019 with status 0
respawn: 86: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d08f10b2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39897){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d08f10a9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d08f10a9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d08f10a9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 86: stopped pid 35102 with status 0
respawn: 87: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5575774f42a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41161){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5575774f39a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5575774f39a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5575774f39a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 87: stopped pid 35188 with status 0
respawn: 88: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b7b29ec2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43153){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b7b29eb9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b7b29eb9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b7b29eb9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 88: stopped pid 35271 with status 0
respawn: 89: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5603c31ff2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:569 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46425){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5603c31fe9a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5603c31fe9a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5603c31fe9a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 89: stopped pid 35362 with status 0
respawn: 90: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55dd01f1f2a0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
