<?xml version="1.0" encoding="UTF-8"?>
<section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>Common Commands</title>
  <para>These commands are available on all VTY nodes. They are listed here only once, to unclutter the VTY reference.</para>
  <section>
    <title>end</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>end</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>end</para>
          <para>End current mode and change to enable mode.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>exit</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>exit</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>exit</para>
          <para>Exit current mode and down to previous mode</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>help</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>help</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>help</para>
          <para>Description of the interactive help system</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>list [with-flags]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>list [with-flags]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>list</para>
          <para>Print command list</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[with-flags]</para>
          <para>Also print the VTY attribute flags</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show running-config</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show running-config</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>running-config</para>
          <para>running configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show vty-attributes</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show vty-attributes</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>vty-attributes</para>
          <para>List of VTY attributes</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show vty-attributes (application|library|global)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show vty-attributes (application|library|global)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>vty-attributes</para>
          <para>List of VTY attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application specific attributes only</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>library</para>
          <para>Library specific attributes only</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global attributes only</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>write</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>write</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>write</para>
          <para>Write running configuration to memory, network, or terminal</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>write file [PATH]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>write file [PATH]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>write</para>
          <para>Write running configuration to memory, network, or terminal</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Write to configuration file</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[PATH]</para>
          <para>Set file path to store the config, or replace if already exists</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>write memory</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>write memory</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>write</para>
          <para>Write running configuration to memory, network, or terminal</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>memory</para>
          <para>Write configuration to the file (same as write file)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>write terminal</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>write terminal</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>write</para>
          <para>Write running configuration to memory, network, or terminal</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Write to terminal</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>view</title>
  <para>The view node is the default node when connecting to the
    VTY interface. This node does not require any additional
    permission and allows to introspect the application.</para>
  <section>
    <title>bssgp bvc nsei &lt;0-65535&gt; bvci &lt;0-65535&gt; reset</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>bssgp bvc nsei &lt;0-65535&gt; bvci &lt;0-65535&gt; reset</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bssgp</para>
          <para>Initiate BVC RESET procedure for a given NSEI and BVCI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bvc</para>
          <para>Filter based on BSSGP Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsei</para>
          <para>NSEI of the BVC to be filtered</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Network Service Entity Identifier (NSEI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bvci</para>
          <para>BVCI of the BVC to be filtered</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>BSSGP Virtual Connection Identifier (BVCI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reset</para>
          <para>Perform reset procedure</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>enable [expert-mode]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>enable [expert-mode]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Turn on privileged mode command</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[expert-mode]</para>
          <para>Enable the expert mode (show hidden commands)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging color (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging color (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>color</para>
          <para>Configure color-printing for log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't use color for printing messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Use color for printing messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging disable</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging disable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>disable</para>
          <para>Disables logging to this vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging enable</title>
    <para>This command is required to make logging commands available
      on the telnet VTY.</para>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging enable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Enables logging to this vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter all (0|1)</title>
    <para>Disable/enable general log output on a given target.
      Typically, 'logging filter all 1' allows to see the usual log output on a
      given target. Setting to '0' can be useful when logging to the telnet VTY
      console: mute all log output to allow typing VTY commands on the telnet
      prompt without interference from log output; 'logging filter all 1' then
      re-enables logging in the same log output configuration as before.

      Some applications provide more specific filters, e.g. to log a given IMSI
      only. To employ such filters, set 'logging filter all 0' to disable
      general logging, and then enable a more specific filter instead.
      </para>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter all (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Do you want to log all messages?</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Only print messages matched by other filters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Bypass filter and print all messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter bvc nsei &lt;0-65535&gt; bvci &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter bvc nsei &lt;0-65535&gt; bvci &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bvc</para>
          <para>Filter based on BSSGP Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsei</para>
          <para>NSEI of the BVC to be filtered</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Network Service Entity Identifier (NSEI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bvci</para>
          <para>BVCI of the BVC to be filtered</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>BSSGP Virtual Connection Identifier (BVCI)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter nse nsei &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter nse nsei &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nse</para>
          <para>Filter based on NS Entity</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsei</para>
          <para>Identify NSE by NSEI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Numeric identifier</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter nsvc nsvci &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter nsvc nsvci &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>Filter based on NS Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvci</para>
          <para>Identify NS-VC by NSVCI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Numeric identifier</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level (mm|pag|meas|ref|gprs|llc|sndcp|slhc|ranap|sua|v42bis|gtp|rim|ra|l...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level (mm|pag|meas|ref|gprs|llc|sndcp|slhc|ranap|sua|v42bis|gtp|rim|ra|lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio|ltcap) (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mm</para>
          <para>Layer3 Mobility Management (MM)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>pag</para>
          <para>Paging Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>meas</para>
          <para>Radio Measurement Processing</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ref</para>
          <para>Reference Counting</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gprs</para>
          <para>GPRS Packet Service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llc</para>
          <para>GPRS Logical Link Control Protocol (LLC)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sndcp</para>
          <para>GPRS Sub-Network Dependent Control Protocol (SNDCP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>slhc</para>
          <para>RFC1144 TCP/IP Header compression (SLHC)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ranap</para>
          <para>RAN Application Part (RANAP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation (SUA)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>v42bis</para>
          <para>V.42bis data compression (SNDCP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>GPRS Tunnelling Protocol (GTP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rim</para>
          <para>RAN Information Management (RIM)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ra</para>
          <para>Routing Area</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lglobal</para>
          <para>Library-internal global log family</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llapd</para>
          <para>LAPD in libosmogsm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>linp</para>
          <para>A-bis Intput Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmux</para>
          <para>A-bis B-Subchannel TRAU Frame Multiplex</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmi</para>
          <para>A-bis Input Driver for Signalling</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmib</para>
          <para>A-bis Input Driver for B-Channels (voice)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsms</para>
          <para>Layer3 Short Message Service (SMS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lctrl</para>
          <para>Control Interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgtp</para>
          <para>GPRS GTP library</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lstats</para>
          <para>Statistics messages and logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgsup</para>
          <para>Generic Subscriber Update Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loap</para>
          <para>Osmocom Authentication Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lss7</para>
          <para>libosmo-sigtran Signalling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsccp</para>
          <para>libosmo-sigtran SCCP Implementation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsua</para>
          <para>libosmo-sigtran SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lm3ua</para>
          <para>libosmo-sigtran MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmgcp</para>
          <para>libosmo-mgcp Media Gateway Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ljibuf</para>
          <para>libosmo-netif Jitter Buffer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lrspro</para>
          <para>Remote SIM protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lns</para>
          <para>GPRS NS layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lbssgp</para>
          <para>GPRS BSSGP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnsdata</para>
          <para>GPRS NS layer data PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnssignal</para>
          <para>GPRS NS layer signal PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>liuup</para>
          <para>Iu UP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lpfcp</para>
          <para>libosmo-pfcp Packet Forwarding Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lcsn1</para>
          <para>libosmo-csn1 Concrete Syntax Notation 1 codec</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lio</para>
          <para>libosmocore IO Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ltcap</para>
          <para>TCAP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level force-all (debug|info|notice|error|fatal)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level force-all (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>force-all</para>
          <para>Globally force all logging categories to a specific level. This is released by the 'no logging level force-all' command. Note: any 'logging level &lt;category&gt; &lt;level&gt;' commands will have no visible effect after this, until the forced level is released.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level set-all (debug|info|notice|error|fatal)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level set-all (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>set-all</para>
          <para>Once-off set all categories to the given log level. There is no single command to take back these changes -- each category is set to the given level, period.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print category (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print category (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>category</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with category/subsystem name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print category-hex (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print category-hex (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>category-hex</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with category/subsystem nr in hex ('&lt;000b&gt;')</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print extended-timestamp (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print extended-timestamp (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>extended-timestamp</para>
          <para>Configure log message timestamping</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current timestamp with YYYYMMDDhhmmssnnn</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print file (0|1|basename) [last]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print file (0|1|basename) [last]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with the source file and line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>basename</para>
          <para>Prefix each log message with the source file's basename (strip leading paths) and line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[last]</para>
          <para>Log source file info at the end of a log line. If omitted, log source file info just before the log text.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print level (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print level (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with the log level name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print thread-id (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print thread-id (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>thread-id</para>
          <para>Configure log message logging Thread ID</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current Thread ID</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging set-log-mask MASK</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging set-log-mask MASK</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>set-log-mask</para>
          <para>Set the logmask of this logging target</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>MASK</para>
          <para>List of logging categories to log, e.g. 'abc:mno:xyz'. Available log categories depend on the specific application, refer to the 'logging level' command. Optionally add individual log levels like 'abc,1:mno,3:xyz,5', where the level numbers are LOGL_DEBUG=1 LOGL_INFO=3 LOGL_NOTICE=5 LOGL_ERROR=7 LOGL_FATAL=8</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging timestamp (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging timestamp (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timestamp</para>
          <para>Configure log message timestamping</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current timestamp</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logp (mm|pag|meas|ref|gprs|llc|sndcp|slhc|ranap|sua|v42bis|gtp|rim|ra|lglobal|ll...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logp (mm|pag|meas|ref|gprs|llc|sndcp|slhc|ranap|sua|v42bis|gtp|rim|ra|lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio|ltcap) (debug|info|notice|error|fatal) .LOGMESSAGE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logp</para>
          <para>Print a message on all log outputs; useful for placing markers in test logs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mm</para>
          <para>Layer3 Mobility Management (MM)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>pag</para>
          <para>Paging Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>meas</para>
          <para>Radio Measurement Processing</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ref</para>
          <para>Reference Counting</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gprs</para>
          <para>GPRS Packet Service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llc</para>
          <para>GPRS Logical Link Control Protocol (LLC)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sndcp</para>
          <para>GPRS Sub-Network Dependent Control Protocol (SNDCP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>slhc</para>
          <para>RFC1144 TCP/IP Header compression (SLHC)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ranap</para>
          <para>RAN Application Part (RANAP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation (SUA)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>v42bis</para>
          <para>V.42bis data compression (SNDCP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>GPRS Tunnelling Protocol (GTP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rim</para>
          <para>RAN Information Management (RIM)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ra</para>
          <para>Routing Area</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lglobal</para>
          <para>Library-internal global log family</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llapd</para>
          <para>LAPD in libosmogsm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>linp</para>
          <para>A-bis Intput Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmux</para>
          <para>A-bis B-Subchannel TRAU Frame Multiplex</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmi</para>
          <para>A-bis Input Driver for Signalling</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmib</para>
          <para>A-bis Input Driver for B-Channels (voice)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsms</para>
          <para>Layer3 Short Message Service (SMS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lctrl</para>
          <para>Control Interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgtp</para>
          <para>GPRS GTP library</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lstats</para>
          <para>Statistics messages and logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgsup</para>
          <para>Generic Subscriber Update Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loap</para>
          <para>Osmocom Authentication Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lss7</para>
          <para>libosmo-sigtran Signalling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsccp</para>
          <para>libosmo-sigtran SCCP Implementation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsua</para>
          <para>libosmo-sigtran SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lm3ua</para>
          <para>libosmo-sigtran MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmgcp</para>
          <para>libosmo-mgcp Media Gateway Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ljibuf</para>
          <para>libosmo-netif Jitter Buffer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lrspro</para>
          <para>Remote SIM protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lns</para>
          <para>GPRS NS layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lbssgp</para>
          <para>GPRS BSSGP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnsdata</para>
          <para>GPRS NS layer data PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnssignal</para>
          <para>GPRS NS layer signal PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>liuup</para>
          <para>Iu UP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lpfcp</para>
          <para>libosmo-pfcp Packet Forwarding Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lcsn1</para>
          <para>libosmo-csn1 Concrete Syntax Notation 1 codec</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lio</para>
          <para>libosmocore IO Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ltcap</para>
          <para>TCAP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>.LOGMESSAGE</para>
          <para>Arbitrary message to log on given category and log level</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no logging level force-all</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no logging level force-all</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>force-all</para>
          <para>Release any globally forced log level set with 'logging level force-all &lt;level&gt;'</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show alarms</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show alarms</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>alarms</para>
          <para>Show current logging configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show asciidoc counters</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show asciidoc counters</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asciidoc</para>
          <para>Asciidoc generation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>counters</para>
          <para>Generate table of all registered counters</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show bssgp</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show bssgp</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bssgp</para>
          <para>Show information about the BSSGP protocol</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show bssgp nsei &lt;0-65535&gt; [stats]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show bssgp nsei &lt;0-65535&gt; [stats]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bssgp</para>
          <para>Show information about the BSSGP protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsei</para>
          <para>Show all BVCs on one NSE</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>The NSEI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[stats]</para>
          <para>Include Statistics</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show bssgp stats</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show bssgp stats</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bssgp</para>
          <para>Show information about the BSSGP protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Include statistics</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cpu-sched threads</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cpu-sched threads</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cpu-sched</para>
          <para>Show Sched section information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>threads</para>
          <para>Show information about running threads)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 (sua|m3ua|ipa) (sctp|tcp) [&lt;0-65534&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 (sua|m3ua|ipa) (sctp|tcp) [&lt;0-65534&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp</para>
          <para>SCTP (Stream Control Transmission Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp</para>
          <para>TCP (Transmission Control Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-65534&gt;]</para>
          <para>Local Port Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 (sua|m3ua|ipa) [&lt;0-65534&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 (sua|m3ua|ipa) [&lt;0-65534&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-65534&gt;]</para>
          <para>Local Port Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 config</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 config</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>config</para>
          <para>Currently running cs7 configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; as (active|all|m3ua|sua)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; as (active|all|m3ua|sua)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Application Server (AS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>active</para>
          <para>Display all active ASs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Display all ASs (default)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>Display all m3ua ASs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>Display all SUA ASs</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; as binding-table name AS_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; as binding-table name AS_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Application Server (AS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>binding-table</para>
          <para>Display binding table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Look up AS with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>AS_NAME</para>
          <para>Name of the Application Server (AS)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; as name AS_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; as name AS_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Application Server (AS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Look up AS with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>AS_NAME</para>
          <para>Name of the Application Server (AS)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp name ASP_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp name ASP_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Lookup ASP with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ASP_NAME</para>
          <para>Name of the Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-assoc-status</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-assoc-status</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-assoc-status</para>
          <para>Application Server Process (ASP) SCTP association status</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-assoc-status name ASP_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-assoc-status name ASP_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-assoc-status</para>
          <para>Application Server Process (ASP) SCTP association information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Lookup ASP with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ASP_NAME</para>
          <para>Name of the Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-remaddr</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-remaddr</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-remaddr</para>
          <para>Application Server Process (ASP) remote addresses information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-remaddr name ASP_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-remaddr name ASP_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-remaddr</para>
          <para>Application Server Process (ASP) remote addresses information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Lookup ASP with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ASP_NAME</para>
          <para>Name of the Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; route [POINT_CODE]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; route [POINT_CODE]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route</para>
          <para>Routing Table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[POINT_CODE]</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; route binding-table [POINT_CODE] [all-matches]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; route binding-table [POINT_CODE] [all-matches]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route</para>
          <para>Routing Table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>binding-table</para>
          <para>Display binding table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[POINT_CODE]</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[all-matches]</para>
          <para>Display all matching Combination Links</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; route-lookup POINT_CODE from POINT_CODE sls &lt;0-15&gt; [lis...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; route-lookup POINT_CODE from POINT_CODE sls &lt;0-15&gt; [list-asps]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route-lookup</para>
          <para>Look up route</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Destination PC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>from</para>
          <para>From</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Origin PC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sls</para>
          <para>SLS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>SLS value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[list-asps]</para>
          <para>List ASPs of the AS if route points to an AS</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp addressbook</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp addressbook</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>addressbook</para>
          <para>List all SCCP addressbook entries</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp connections</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp connections</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>connections</para>
          <para>Show List of active SCCP connections</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp ssn &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp ssn &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ssn</para>
          <para>Find an SCCP User registered for the given SSN</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Subsystem Number (SSN)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp timers</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp timers</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signaling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timers</para>
          <para>Show List of SCCP timers</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp users</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp users</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>users</para>
          <para>Show List of SCCP Users registered</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; users</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; users</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>users</para>
          <para>User Table</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show history</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show history</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>history</para>
          <para>Display the session command history</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show llc</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show llc</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llc</para>
          <para>Display information about the LLC protocol</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show logging vty</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show logging vty</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Show current logging configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>vty</para>
          <para>Show current logging configuration for this vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show mm-context all [pdp]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show mm-context all [pdp]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mm-context</para>
          <para>MM Context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All MM Contexts</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[pdp]</para>
          <para>Include PDP Context Information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show mm-context imsi IMSI [pdp]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show mm-context imsi IMSI [pdp]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mm-context</para>
          <para>MM Context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>imsi</para>
          <para>Identify by IMSI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IMSI</para>
          <para>IMSI of the MM Context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[pdp]</para>
          <para>Include PDP Context Information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show ns (nsei|nsvc) &lt;0-65535&gt; [stats]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show ns (nsei|nsvc) &lt;0-65535&gt; [stats]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ns</para>
          <para>Display information about the NS protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsei</para>
          <para>Select one NSE by its NSE Identifier</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>Select one NSE by its NS-VC Identifier</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>The Identifier of selected type</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[stats]</para>
          <para>Include Statistics</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show ns binds [stats]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show ns binds [stats]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ns</para>
          <para>Display information about the NS protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>binds</para>
          <para>Display information about the NS protocol binds</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[stats]</para>
          <para>Include statistic</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show ns entities [stats]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show ns entities [stats]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ns</para>
          <para>Display information about the NS protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>entities</para>
          <para>Display information about the NS protocol entities (NSEs)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[stats]</para>
          <para>Include statistics</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show ns persistent</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show ns persistent</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ns</para>
          <para>Display information about the NS protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>persistent</para>
          <para>Show only persistent NS</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show online-help</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show online-help</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>online-help</para>
          <para>Online help</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show pdp-context all</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show pdp-context all</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>pdp-context</para>
          <para>Display information on PDP Context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Show everything</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show pid</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show pid</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>pid</para>
          <para>Displays the process ID</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show rate-counters [skip-zero]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show rate-counters [skip-zero]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rate-counters</para>
          <para>Show all rate counters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[skip-zero]</para>
          <para>Skip items with total count zero</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show runtime</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show runtime</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>runtime</para>
          <para>Display runtime information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show sgsn</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show sgsn</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sgsn</para>
          <para>Display information about the SGSN</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show sndcp</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show sndcp</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sndcp</para>
          <para>Display information about the SNDCP protocol</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show stats [skip-zero]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show stats [skip-zero]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Show statistical values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[skip-zero]</para>
          <para>Skip items with total count zero</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show stats level (global|peer|subscriber) [skip-zero]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show stats level (global|peer|subscriber) [skip-zero]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Show statistical values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the maximum group level</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Show global groups only</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>peer</para>
          <para>Show global and network peer related groups</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subscriber</para>
          <para>Show global, peer, and subscriber groups</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[skip-zero]</para>
          <para>Skip items with total count zero</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show subscriber cache</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show subscriber cache</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subscriber</para>
          <para>Show information about subscribers</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cache</para>
          <para>Display contents of subscriber cache</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show talloc-context (application|global|all) (full|brief|DEPTH)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show talloc-context (application|global|all) (full|brief|DEPTH)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>talloc-context</para>
          <para>Show talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application's context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global context (OTC_GLOBAL)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All contexts, if NULL-context tracking is enabled</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>full</para>
          <para>Display a full talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>brief</para>
          <para>Display a brief talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DEPTH</para>
          <para>Specify required maximal depth value</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show talloc-context (application|global|all) (full|brief|DEPTH) filter REGEXP</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show talloc-context (application|global|all) (full|brief|DEPTH) filter REGEXP</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>talloc-context</para>
          <para>Show talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application's context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global context (OTC_GLOBAL)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All contexts, if NULL-context tracking is enabled</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>full</para>
          <para>Display a full talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>brief</para>
          <para>Display a brief talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DEPTH</para>
          <para>Specify required maximal depth value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter chunks using regular expression</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>REGEXP</para>
          <para>Regular expression</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show talloc-context (application|global|all) (full|brief|DEPTH) tree ADDRESS</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show talloc-context (application|global|all) (full|brief|DEPTH) tree ADDRESS</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>talloc-context</para>
          <para>Show talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application's context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global context (OTC_GLOBAL)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All contexts, if NULL-context tracking is enabled</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>full</para>
          <para>Display a full talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>brief</para>
          <para>Display a brief talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DEPTH</para>
          <para>Specify required maximal depth value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tree</para>
          <para>Display only a specific memory chunk</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ADDRESS</para>
          <para>Chunk address (e.g. 0xdeadbeef)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show timer [TNNNN]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show timer [TNNNN]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timer</para>
          <para>Show timers</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[TNNNN]</para>
          <para>T- or X-timer-number -- 3GPP compliant timer number of the format '1234' or 'T1234' or 't1234'; Osmocom-specific timer number of the format: 'X1234' or 'x1234'.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show timer gtp [TNNNN]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show timer gtp [TNNNN]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timer</para>
          <para>Show timers</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>GTP (libgtp) timers</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[TNNNN]</para>
          <para>T- or X-timer-number -- 3GPP compliant timer number of the format '1234' or 'T1234' or 't1234'; Osmocom-specific timer number of the format: 'X1234' or 'x1234'.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show uptime</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show uptime</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>uptime</para>
          <para>Displays how long the program has been running</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show version</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show version</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>version</para>
          <para>Displays program version</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>terminal length &lt;0-512&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>terminal length &lt;0-512&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Set terminal line parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>length</para>
          <para>Set number of lines on a screen</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-512&gt;</para>
          <para>Number of lines on screen (0 for no pausing)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>terminal no length</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>terminal no length</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Set terminal line parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>length</para>
          <para>Set number of lines on a screen</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>who</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>who</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>who</para>
          <para>Display who is on vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>enable</title>
  <para>The enable node is a privileged node, allowing to make changes
    to the configuration and to access further commands like 'configure'.
    All commands seen on the view node are also available here.</para>
  <section>
    <title>bssgp bvc nsei &lt;0-65535&gt; bvci &lt;0-65535&gt; reset</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>bssgp bvc nsei &lt;0-65535&gt; bvci &lt;0-65535&gt; reset</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bssgp</para>
          <para>Initiate BVC RESET procedure for a given NSEI and BVCI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bvc</para>
          <para>Filter based on BSSGP Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsei</para>
          <para>NSEI of the BVC to be filtered</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Network Service Entity Identifier (NSEI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bvci</para>
          <para>BVCI of the BVC to be filtered</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>BSSGP Virtual Connection Identifier (BVCI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reset</para>
          <para>Perform reset procedure</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>configure [terminal]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>configure [terminal]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>configure</para>
          <para>Configuration from vty interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[terminal]</para>
          <para>Configuration terminal</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>copy running-config startup-config</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>copy running-config startup-config</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>copy</para>
          <para>Copy configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>running-config</para>
          <para>Copy running config to... </para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>startup-config</para>
          <para>Copy running config to startup config (same as write file)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>cs7 instance &lt;0-15&gt; asp NAME audit point-code POINT_CODE</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cs7 instance &lt;0-15&gt; asp NAME audit point-code POINT_CODE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>Instance related commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>SS7 Instance Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>ASP related commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>audit</para>
          <para>Audit destination Point Code (xUA DAUD)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Destination Point Code to audit</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Destination Point Code value</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>cs7 instance &lt;0-15&gt; asp NAME disconnect</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cs7 instance &lt;0-15&gt; asp NAME disconnect</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>Instance related commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>SS7 Instance Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>ASP related commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>disconnect</para>
          <para>Disconnect the ASP (client will reconnect)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>disable</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>disable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>disable</para>
          <para>Turn off privileged mode command</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging color (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging color (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>color</para>
          <para>Configure color-printing for log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't use color for printing messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Use color for printing messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging disable</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging disable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>disable</para>
          <para>Disables logging to this vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging enable</title>
    <para>This command is required to make logging commands available
      on the telnet VTY.</para>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging enable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Enables logging to this vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter all (0|1)</title>
    <para>Disable/enable general log output on a given target.
      Typically, 'logging filter all 1' allows to see the usual log output on a
      given target. Setting to '0' can be useful when logging to the telnet VTY
      console: mute all log output to allow typing VTY commands on the telnet
      prompt without interference from log output; 'logging filter all 1' then
      re-enables logging in the same log output configuration as before.

      Some applications provide more specific filters, e.g. to log a given IMSI
      only. To employ such filters, set 'logging filter all 0' to disable
      general logging, and then enable a more specific filter instead.
      </para>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter all (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Do you want to log all messages?</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Only print messages matched by other filters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Bypass filter and print all messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter bvc nsei &lt;0-65535&gt; bvci &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter bvc nsei &lt;0-65535&gt; bvci &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bvc</para>
          <para>Filter based on BSSGP Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsei</para>
          <para>NSEI of the BVC to be filtered</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Network Service Entity Identifier (NSEI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bvci</para>
          <para>BVCI of the BVC to be filtered</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>BSSGP Virtual Connection Identifier (BVCI)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter nse nsei &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter nse nsei &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nse</para>
          <para>Filter based on NS Entity</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsei</para>
          <para>Identify NSE by NSEI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Numeric identifier</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter nsvc nsvci &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter nsvc nsvci &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>Filter based on NS Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvci</para>
          <para>Identify NS-VC by NSVCI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Numeric identifier</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level (mm|pag|meas|ref|gprs|llc|sndcp|slhc|ranap|sua|v42bis|gtp|rim|ra|l...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level (mm|pag|meas|ref|gprs|llc|sndcp|slhc|ranap|sua|v42bis|gtp|rim|ra|lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio|ltcap) (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mm</para>
          <para>Layer3 Mobility Management (MM)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>pag</para>
          <para>Paging Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>meas</para>
          <para>Radio Measurement Processing</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ref</para>
          <para>Reference Counting</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gprs</para>
          <para>GPRS Packet Service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llc</para>
          <para>GPRS Logical Link Control Protocol (LLC)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sndcp</para>
          <para>GPRS Sub-Network Dependent Control Protocol (SNDCP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>slhc</para>
          <para>RFC1144 TCP/IP Header compression (SLHC)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ranap</para>
          <para>RAN Application Part (RANAP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation (SUA)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>v42bis</para>
          <para>V.42bis data compression (SNDCP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>GPRS Tunnelling Protocol (GTP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rim</para>
          <para>RAN Information Management (RIM)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ra</para>
          <para>Routing Area</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lglobal</para>
          <para>Library-internal global log family</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llapd</para>
          <para>LAPD in libosmogsm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>linp</para>
          <para>A-bis Intput Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmux</para>
          <para>A-bis B-Subchannel TRAU Frame Multiplex</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmi</para>
          <para>A-bis Input Driver for Signalling</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmib</para>
          <para>A-bis Input Driver for B-Channels (voice)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsms</para>
          <para>Layer3 Short Message Service (SMS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lctrl</para>
          <para>Control Interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgtp</para>
          <para>GPRS GTP library</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lstats</para>
          <para>Statistics messages and logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgsup</para>
          <para>Generic Subscriber Update Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loap</para>
          <para>Osmocom Authentication Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lss7</para>
          <para>libosmo-sigtran Signalling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsccp</para>
          <para>libosmo-sigtran SCCP Implementation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsua</para>
          <para>libosmo-sigtran SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lm3ua</para>
          <para>libosmo-sigtran MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmgcp</para>
          <para>libosmo-mgcp Media Gateway Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ljibuf</para>
          <para>libosmo-netif Jitter Buffer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lrspro</para>
          <para>Remote SIM protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lns</para>
          <para>GPRS NS layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lbssgp</para>
          <para>GPRS BSSGP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnsdata</para>
          <para>GPRS NS layer data PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnssignal</para>
          <para>GPRS NS layer signal PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>liuup</para>
          <para>Iu UP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lpfcp</para>
          <para>libosmo-pfcp Packet Forwarding Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lcsn1</para>
          <para>libosmo-csn1 Concrete Syntax Notation 1 codec</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lio</para>
          <para>libosmocore IO Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ltcap</para>
          <para>TCAP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level force-all (debug|info|notice|error|fatal)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level force-all (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>force-all</para>
          <para>Globally force all logging categories to a specific level. This is released by the 'no logging level force-all' command. Note: any 'logging level &lt;category&gt; &lt;level&gt;' commands will have no visible effect after this, until the forced level is released.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level set-all (debug|info|notice|error|fatal)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level set-all (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>set-all</para>
          <para>Once-off set all categories to the given log level. There is no single command to take back these changes -- each category is set to the given level, period.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print category (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print category (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>category</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with category/subsystem name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print category-hex (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print category-hex (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>category-hex</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with category/subsystem nr in hex ('&lt;000b&gt;')</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print extended-timestamp (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print extended-timestamp (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>extended-timestamp</para>
          <para>Configure log message timestamping</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current timestamp with YYYYMMDDhhmmssnnn</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print file (0|1|basename) [last]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print file (0|1|basename) [last]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with the source file and line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>basename</para>
          <para>Prefix each log message with the source file's basename (strip leading paths) and line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[last]</para>
          <para>Log source file info at the end of a log line. If omitted, log source file info just before the log text.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print level (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print level (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with the log level name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print thread-id (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print thread-id (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>thread-id</para>
          <para>Configure log message logging Thread ID</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current Thread ID</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging set-log-mask MASK</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging set-log-mask MASK</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>set-log-mask</para>
          <para>Set the logmask of this logging target</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>MASK</para>
          <para>List of logging categories to log, e.g. 'abc:mno:xyz'. Available log categories depend on the specific application, refer to the 'logging level' command. Optionally add individual log levels like 'abc,1:mno,3:xyz,5', where the level numbers are LOGL_DEBUG=1 LOGL_INFO=3 LOGL_NOTICE=5 LOGL_ERROR=7 LOGL_FATAL=8</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging timestamp (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging timestamp (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timestamp</para>
          <para>Configure log message timestamping</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current timestamp</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logp (mm|pag|meas|ref|gprs|llc|sndcp|slhc|ranap|sua|v42bis|gtp|rim|ra|lglobal|ll...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logp (mm|pag|meas|ref|gprs|llc|sndcp|slhc|ranap|sua|v42bis|gtp|rim|ra|lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio|ltcap) (debug|info|notice|error|fatal) .LOGMESSAGE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logp</para>
          <para>Print a message on all log outputs; useful for placing markers in test logs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mm</para>
          <para>Layer3 Mobility Management (MM)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>pag</para>
          <para>Paging Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>meas</para>
          <para>Radio Measurement Processing</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ref</para>
          <para>Reference Counting</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gprs</para>
          <para>GPRS Packet Service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llc</para>
          <para>GPRS Logical Link Control Protocol (LLC)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sndcp</para>
          <para>GPRS Sub-Network Dependent Control Protocol (SNDCP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>slhc</para>
          <para>RFC1144 TCP/IP Header compression (SLHC)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ranap</para>
          <para>RAN Application Part (RANAP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation (SUA)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>v42bis</para>
          <para>V.42bis data compression (SNDCP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>GPRS Tunnelling Protocol (GTP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rim</para>
          <para>RAN Information Management (RIM)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ra</para>
          <para>Routing Area</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lglobal</para>
          <para>Library-internal global log family</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llapd</para>
          <para>LAPD in libosmogsm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>linp</para>
          <para>A-bis Intput Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmux</para>
          <para>A-bis B-Subchannel TRAU Frame Multiplex</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmi</para>
          <para>A-bis Input Driver for Signalling</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmib</para>
          <para>A-bis Input Driver for B-Channels (voice)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsms</para>
          <para>Layer3 Short Message Service (SMS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lctrl</para>
          <para>Control Interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgtp</para>
          <para>GPRS GTP library</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lstats</para>
          <para>Statistics messages and logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgsup</para>
          <para>Generic Subscriber Update Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loap</para>
          <para>Osmocom Authentication Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lss7</para>
          <para>libosmo-sigtran Signalling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsccp</para>
          <para>libosmo-sigtran SCCP Implementation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsua</para>
          <para>libosmo-sigtran SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lm3ua</para>
          <para>libosmo-sigtran MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmgcp</para>
          <para>libosmo-mgcp Media Gateway Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ljibuf</para>
          <para>libosmo-netif Jitter Buffer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lrspro</para>
          <para>Remote SIM protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lns</para>
          <para>GPRS NS layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lbssgp</para>
          <para>GPRS BSSGP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnsdata</para>
          <para>GPRS NS layer data PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnssignal</para>
          <para>GPRS NS layer signal PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>liuup</para>
          <para>Iu UP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lpfcp</para>
          <para>libosmo-pfcp Packet Forwarding Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lcsn1</para>
          <para>libosmo-csn1 Concrete Syntax Notation 1 codec</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lio</para>
          <para>libosmocore IO Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ltcap</para>
          <para>TCAP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>.LOGMESSAGE</para>
          <para>Arbitrary message to log on given category and log level</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no logging level force-all</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no logging level force-all</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>force-all</para>
          <para>Release any globally forced log level set with 'logging level force-all &lt;level&gt;'</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>nse &lt;0-65535&gt; restart-sns</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>nse &lt;0-65535&gt; restart-sns</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nse</para>
          <para>NSE specific commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>NS Entity ID (NSEI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>restart-sns</para>
          <para>Restart SNS procedure</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>nsvc &lt;0-65535&gt; (block|unblock|reset)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>nsvc &lt;0-65535&gt; (block|unblock|reset)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>NS Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>NS Virtual Connection ID (NS-VCI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>block</para>
          <para>Block a NSVC. As cause code O&amp;M intervention will be used.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>unblock</para>
          <para>Unblock a NSVC. As cause code O&amp;M intervention will be used.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reset</para>
          <para>Reset a NSVC. As cause code O&amp;M intervention will be used.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>page imsi IMSI</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>page imsi IMSI</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>page</para>
          <para>Send a PS paging request to subscriber</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>imsi</para>
          <para>Use the IMSI to select the subscriber</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IMSI</para>
          <para>The IMSI</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show alarms</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show alarms</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>alarms</para>
          <para>Show current logging configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show asciidoc counters</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show asciidoc counters</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asciidoc</para>
          <para>Asciidoc generation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>counters</para>
          <para>Generate table of all registered counters</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show bssgp</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show bssgp</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bssgp</para>
          <para>Show information about the BSSGP protocol</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show bssgp nsei &lt;0-65535&gt; [stats]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show bssgp nsei &lt;0-65535&gt; [stats]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bssgp</para>
          <para>Show information about the BSSGP protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsei</para>
          <para>Show all BVCs on one NSE</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>The NSEI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[stats]</para>
          <para>Include Statistics</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show bssgp stats</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show bssgp stats</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bssgp</para>
          <para>Show information about the BSSGP protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Include statistics</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cpu-sched threads</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cpu-sched threads</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cpu-sched</para>
          <para>Show Sched section information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>threads</para>
          <para>Show information about running threads)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 (sua|m3ua|ipa) (sctp|tcp) [&lt;0-65534&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 (sua|m3ua|ipa) (sctp|tcp) [&lt;0-65534&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp</para>
          <para>SCTP (Stream Control Transmission Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp</para>
          <para>TCP (Transmission Control Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-65534&gt;]</para>
          <para>Local Port Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 (sua|m3ua|ipa) [&lt;0-65534&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 (sua|m3ua|ipa) [&lt;0-65534&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-65534&gt;]</para>
          <para>Local Port Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 config</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 config</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>config</para>
          <para>Currently running cs7 configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; as (active|all|m3ua|sua)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; as (active|all|m3ua|sua)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Application Server (AS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>active</para>
          <para>Display all active ASs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Display all ASs (default)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>Display all m3ua ASs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>Display all SUA ASs</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; as binding-table name AS_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; as binding-table name AS_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Application Server (AS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>binding-table</para>
          <para>Display binding table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Look up AS with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>AS_NAME</para>
          <para>Name of the Application Server (AS)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; as name AS_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; as name AS_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Application Server (AS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Look up AS with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>AS_NAME</para>
          <para>Name of the Application Server (AS)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp name ASP_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp name ASP_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Lookup ASP with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ASP_NAME</para>
          <para>Name of the Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-assoc-status</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-assoc-status</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-assoc-status</para>
          <para>Application Server Process (ASP) SCTP association status</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-assoc-status name ASP_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-assoc-status name ASP_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-assoc-status</para>
          <para>Application Server Process (ASP) SCTP association information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Lookup ASP with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ASP_NAME</para>
          <para>Name of the Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-remaddr</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-remaddr</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-remaddr</para>
          <para>Application Server Process (ASP) remote addresses information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; asp-remaddr name ASP_NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; asp-remaddr name ASP_NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-remaddr</para>
          <para>Application Server Process (ASP) remote addresses information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>name</para>
          <para>Lookup ASP with a given name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ASP_NAME</para>
          <para>Name of the Application Server Process (ASP)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; route [POINT_CODE]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; route [POINT_CODE]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route</para>
          <para>Routing Table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[POINT_CODE]</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; route binding-table [POINT_CODE] [all-matches]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; route binding-table [POINT_CODE] [all-matches]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route</para>
          <para>Routing Table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>binding-table</para>
          <para>Display binding table</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[POINT_CODE]</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[all-matches]</para>
          <para>Display all matching Combination Links</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; route-lookup POINT_CODE from POINT_CODE sls &lt;0-15&gt; [lis...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; route-lookup POINT_CODE from POINT_CODE sls &lt;0-15&gt; [list-asps]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>route-lookup</para>
          <para>Look up route</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Destination PC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>from</para>
          <para>From</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Origin PC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sls</para>
          <para>SLS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>SLS value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[list-asps]</para>
          <para>List ASPs of the AS if route points to an AS</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp addressbook</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp addressbook</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>addressbook</para>
          <para>List all SCCP addressbook entries</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp connections</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp connections</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>connections</para>
          <para>Show List of active SCCP connections</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp ssn &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp ssn &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ssn</para>
          <para>Find an SCCP User registered for the given SSN</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Subsystem Number (SSN)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp timers</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp timers</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signaling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timers</para>
          <para>Show List of SCCP timers</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; sccp users</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; sccp users</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>users</para>
          <para>Show List of SCCP Users registered</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show cs7 instance &lt;0-15&gt; users</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show cs7 instance &lt;0-15&gt; users</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>users</para>
          <para>User Table</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show history</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show history</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>history</para>
          <para>Display the session command history</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show llc</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show llc</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llc</para>
          <para>Display information about the LLC protocol</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show logging vty</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show logging vty</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Show current logging configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>vty</para>
          <para>Show current logging configuration for this vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show mm-context all [pdp]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show mm-context all [pdp]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mm-context</para>
          <para>MM Context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All MM Contexts</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[pdp]</para>
          <para>Include PDP Context Information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show mm-context imsi IMSI [pdp]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show mm-context imsi IMSI [pdp]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mm-context</para>
          <para>MM Context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>imsi</para>
          <para>Identify by IMSI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IMSI</para>
          <para>IMSI of the MM Context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[pdp]</para>
          <para>Include PDP Context Information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show ns (nsei|nsvc) &lt;0-65535&gt; [stats]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show ns (nsei|nsvc) &lt;0-65535&gt; [stats]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ns</para>
          <para>Display information about the NS protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsei</para>
          <para>Select one NSE by its NSE Identifier</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>Select one NSE by its NS-VC Identifier</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>The Identifier of selected type</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[stats]</para>
          <para>Include Statistics</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show ns binds [stats]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show ns binds [stats]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ns</para>
          <para>Display information about the NS protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>binds</para>
          <para>Display information about the NS protocol binds</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[stats]</para>
          <para>Include statistic</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show ns entities [stats]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show ns entities [stats]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ns</para>
          <para>Display information about the NS protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>entities</para>
          <para>Display information about the NS protocol entities (NSEs)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[stats]</para>
          <para>Include statistics</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show ns persistent</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show ns persistent</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ns</para>
          <para>Display information about the NS protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>persistent</para>
          <para>Show only persistent NS</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show online-help</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show online-help</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>online-help</para>
          <para>Online help</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show pdp-context all</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show pdp-context all</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>pdp-context</para>
          <para>Display information on PDP Context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Show everything</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show rate-counters [skip-zero]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show rate-counters [skip-zero]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rate-counters</para>
          <para>Show all rate counters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[skip-zero]</para>
          <para>Skip items with total count zero</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show runtime</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show runtime</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>runtime</para>
          <para>Display runtime information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show sgsn</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show sgsn</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sgsn</para>
          <para>Display information about the SGSN</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show sndcp</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show sndcp</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sndcp</para>
          <para>Display information about the SNDCP protocol</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show startup-config</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show startup-config</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>startup-config</para>
          <para>Contentes of startup configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show stats [skip-zero]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show stats [skip-zero]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Show statistical values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[skip-zero]</para>
          <para>Skip items with total count zero</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show stats level (global|peer|subscriber) [skip-zero]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show stats level (global|peer|subscriber) [skip-zero]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Show statistical values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the maximum group level</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Show global groups only</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>peer</para>
          <para>Show global and network peer related groups</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subscriber</para>
          <para>Show global, peer, and subscriber groups</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[skip-zero]</para>
          <para>Skip items with total count zero</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show subscriber cache</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show subscriber cache</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subscriber</para>
          <para>Show information about subscribers</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cache</para>
          <para>Display contents of subscriber cache</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show talloc-context (application|global|all) (full|brief|DEPTH)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show talloc-context (application|global|all) (full|brief|DEPTH)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>talloc-context</para>
          <para>Show talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application's context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global context (OTC_GLOBAL)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All contexts, if NULL-context tracking is enabled</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>full</para>
          <para>Display a full talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>brief</para>
          <para>Display a brief talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DEPTH</para>
          <para>Specify required maximal depth value</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show talloc-context (application|global|all) (full|brief|DEPTH) filter REGEXP</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show talloc-context (application|global|all) (full|brief|DEPTH) filter REGEXP</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>talloc-context</para>
          <para>Show talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application's context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global context (OTC_GLOBAL)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All contexts, if NULL-context tracking is enabled</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>full</para>
          <para>Display a full talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>brief</para>
          <para>Display a brief talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DEPTH</para>
          <para>Specify required maximal depth value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter chunks using regular expression</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>REGEXP</para>
          <para>Regular expression</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show talloc-context (application|global|all) (full|brief|DEPTH) tree ADDRESS</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show talloc-context (application|global|all) (full|brief|DEPTH) tree ADDRESS</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>talloc-context</para>
          <para>Show talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>application</para>
          <para>Application's context</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Global context (OTC_GLOBAL)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>All contexts, if NULL-context tracking is enabled</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>full</para>
          <para>Display a full talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>brief</para>
          <para>Display a brief talloc memory hierarchy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DEPTH</para>
          <para>Specify required maximal depth value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tree</para>
          <para>Display only a specific memory chunk</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ADDRESS</para>
          <para>Chunk address (e.g. 0xdeadbeef)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show timer [TNNNN]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show timer [TNNNN]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timer</para>
          <para>Show timers</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[TNNNN]</para>
          <para>T- or X-timer-number -- 3GPP compliant timer number of the format '1234' or 'T1234' or 't1234'; Osmocom-specific timer number of the format: 'X1234' or 'x1234'.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show timer gtp [TNNNN]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show timer gtp [TNNNN]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timer</para>
          <para>Show timers</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>GTP (libgtp) timers</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[TNNNN]</para>
          <para>T- or X-timer-number -- 3GPP compliant timer number of the format '1234' or 'T1234' or 't1234'; Osmocom-specific timer number of the format: 'X1234' or 'x1234'.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show version</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show version</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>version</para>
          <para>Displays program version</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>shutdown</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>shutdown</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>shutdown</para>
          <para>Request a shutdown of the program</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats report</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats report</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Stats related commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>report</para>
          <para>Manurally trigger reporting of stats</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats reset</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats reset</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Stats related commands</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reset</para>
          <para>Reset all rate counter stats</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>terminal length &lt;0-512&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>terminal length &lt;0-512&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Set terminal line parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>length</para>
          <para>Set number of lines on a screen</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-512&gt;</para>
          <para>Number of lines on screen (0 for no pausing)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>terminal monitor</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>terminal monitor</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Set terminal line parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>monitor</para>
          <para>Copy debug output to the current terminal line</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>terminal no length</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>terminal no length</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Set terminal line parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>length</para>
          <para>Set number of lines on a screen</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>terminal no monitor</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>terminal no monitor</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal</para>
          <para>Set terminal line parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>monitor</para>
          <para>Copy debug output to the current terminal line</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>update-subscriber imsi IMSI cancel (update-procedure|subscription-withdraw)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>update-subscriber imsi IMSI cancel (update-procedure|subscription-withdraw)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>update-subscriber</para>
          <para>Update subscriber list</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>imsi</para>
          <para>Use the IMSI to select the subscriber</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IMSI</para>
          <para>The IMSI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cancel</para>
          <para>Cancel (remove) subscriber record</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>update-procedure</para>
          <para>The MS moved to another SGSN</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subscription-withdraw</para>
          <para>The subscription is no longer valid</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>update-subscriber imsi IMSI create</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>update-subscriber imsi IMSI create</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>update-subscriber</para>
          <para>Update subscriber list</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>imsi</para>
          <para>Use the IMSI to select the subscriber</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IMSI</para>
          <para>The IMSI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>create</para>
          <para>Create a subscriber entry</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>update-subscriber imsi IMSI destroy</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>update-subscriber imsi IMSI destroy</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>update-subscriber</para>
          <para>Update subscriber list</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>imsi</para>
          <para>Use the IMSI to select the subscriber</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IMSI</para>
          <para>The IMSI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>destroy</para>
          <para>Destroy a subscriber entry</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>update-subscriber imsi IMSI insert auth-triplet &lt;1-5&gt; sres SRES rand RAND kc KC</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>update-subscriber imsi IMSI insert auth-triplet &lt;1-5&gt; sres SRES rand RAND kc KC</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>update-subscriber</para>
          <para>Update subscriber list</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>imsi</para>
          <para>Use the IMSI to select the subscriber</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IMSI</para>
          <para>The IMSI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>insert</para>
          <para>Insert data into the subscriber record</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>auth-triplet</para>
          <para>Update authentication triplet</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-5&gt;</para>
          <para>Triplet index</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sres</para>
          <para>Set SRES value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>SRES</para>
          <para>SRES value (4 byte) in hex</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rand</para>
          <para>Set RAND value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>RAND</para>
          <para>RAND value (16 byte) in hex</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>kc</para>
          <para>Set Kc value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>KC</para>
          <para>Kc value (8 byte) in hex</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>update-subscriber imsi IMSI update-auth-info</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>update-subscriber imsi IMSI update-auth-info</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>update-subscriber</para>
          <para>Update subscriber list</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>imsi</para>
          <para>Use the IMSI to select the subscriber</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IMSI</para>
          <para>The IMSI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>update-auth-info</para>
          <para>Complete the send authentication info procedure</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>update-subscriber imsi IMSI update-location-result (ok|system-failure|data-missi...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>update-subscriber imsi IMSI update-location-result (ok|system-failure|data-missing|unexpected-data-value|unknown-subscriber|roaming-not-allowed)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>update-subscriber</para>
          <para>Update subscriber list</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>imsi</para>
          <para>Use the IMSI to select the subscriber</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IMSI</para>
          <para>The IMSI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>update-location-result</para>
          <para>Complete the update location procedure</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ok</para>
          <para>The update location request succeeded</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>system-failure</para>
          <para>Force error code SystemFailure</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>data-missing</para>
          <para>Force error code DataMissing</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>unexpected-data-value</para>
          <para>Force error code UnexpectedDataValue</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>unknown-subscriber</para>
          <para>Force error code UnknownSubscriber</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>roaming-not-allowed</para>
          <para>Force error code RoamingNotAllowed</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>who</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>who</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>who</para>
          <para>Display who is on vty</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config</title>
  <para>The config node is the root for all configuration commands,
    which are identical to the config file format. Changes made on the telnet
    VTY can be made persistent with the 'write file' command.</para>
  <section>
    <title>banner motd default</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>banner motd default</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>banner</para>
          <para>Set banner string</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>motd</para>
          <para>Strings for motd</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>default</para>
          <para>Default string</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>banner motd file [FILE]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>banner motd file [FILE]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>banner</para>
          <para>Set banner</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>motd</para>
          <para>Banner for motd</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Banner from a file</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[FILE]</para>
          <para>Filename</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>bssgp</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>bssgp</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bssgp</para>
          <para>Configure the GPRS BSS Gateway Protocol</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>cpu-sched</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cpu-sched</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cpu-sched</para>
          <para>Configure CPU Scheduler related settings</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>cs7 instance &lt;0-15&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cs7 instance &lt;0-15&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7</para>
          <para>ITU-T Signaling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>instance</para>
          <para>Configure a SS7 Instance</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>An instance of the SS7 stack</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>ctrl</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>ctrl</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ctrl</para>
          <para>Configure the Control Interface</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>enable password (8|) WORD</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>enable password (8|) WORD</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Modify enable password parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>password</para>
          <para>Assign the privileged level password</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>8</para>
          <para>Specifies a HIDDEN password will follow</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para/>
          <para>dummy string </para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>WORD</para>
          <para>The HIDDEN 'enable' password string</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>enable password LINE</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>enable password LINE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Modify enable password parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>password</para>
          <para>Assign the privileged level password</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>LINE</para>
          <para>The UNENCRYPTED (cleartext) 'enable' password</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>hostname WORD</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>hostname WORD</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>hostname</para>
          <para>Set system's network name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>WORD</para>
          <para>This system's network name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>line vty</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>line vty</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>line</para>
          <para>Configure a terminal line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>vty</para>
          <para>Virtual terminal</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log alarms &lt;2-32700&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log alarms &lt;2-32700&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>alarms</para>
          <para>Logging alarms to osmo_strrb</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;2-32700&gt;</para>
          <para>Maximum number of messages to log</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log file FILENAME [(nonblocking-io|blocking-io|wq)]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log file FILENAME [(nonblocking-io|blocking-io|wq)]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Logging to text file</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>FILENAME</para>
          <para>Filename</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[nonblocking-io]</para>
          <para>Use non-blocking, synchronous I/O (may lose msgs if file write buffer becomes full) (default)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[blocking-io]</para>
          <para>Use blocking, synchronous I/O (only for debug purposes or when blocking is acceptable)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[wq]</para>
          <para>Use Tx workqueue, asynchronous I/O (may lose msgs if queue becomes full)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log gsmtap [HOSTNAME] [(nonblocking-io|blocking-io|wq)]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log gsmtap [HOSTNAME] [(nonblocking-io|blocking-io|wq)]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gsmtap</para>
          <para>Logging via GSMTAP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[HOSTNAME]</para>
          <para>Host name to send the GSMTAP logging to (UDP port 4729)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[nonblocking-io]</para>
          <para>Use non-blocking, synchronous I/O (may lose msgs if UDP socket send buffer becomes full) (default)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[blocking-io]</para>
          <para>Use blocking, synchronous I/O (only for debug purposes or when blocking is acceptable)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[wq]</para>
          <para>Use Tx workqueue, asynchronous I/O (may lose msgs if queue becomes full)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log stderr [(nonblocking-io|blocking-io|wq)]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log stderr [(nonblocking-io|blocking-io|wq)]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stderr</para>
          <para>Logging via STDERR of the process</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[nonblocking-io]</para>
          <para>Use non-blocking, synchronous I/O (may lose msgs if file write buffer becomes full) (default)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[blocking-io]</para>
          <para>Use blocking, synchronous I/O (only for debug purposes or when blocking is acceptable)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[wq]</para>
          <para>Use Tx workqueue, asynchronous I/O (may lose msgs if queue becomes full)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log syslog (authpriv|cron|daemon|ftp|lpr|mail|news|user|uucp)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log syslog (authpriv|cron|daemon|ftp|lpr|mail|news|user|uucp)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>syslog</para>
          <para>Logging via syslog</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>authpriv</para>
          <para>Security/authorization messages facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cron</para>
          <para>Clock daemon (cron/at) facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>daemon</para>
          <para>General system daemon facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ftp</para>
          <para>Ftp daemon facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lpr</para>
          <para>Line printer facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mail</para>
          <para>Mail facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>news</para>
          <para>News facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>user</para>
          <para>Generic facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>uucp</para>
          <para>UUCP facility</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log syslog local &lt;0-7&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log syslog local &lt;0-7&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>syslog</para>
          <para>Logging via syslog</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local</para>
          <para>Syslog LOCAL facility</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-7&gt;</para>
          <para>Local facility number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>log systemd-journal [raw]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>log systemd-journal [raw]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>systemd-journal</para>
          <para>Logging to systemd-journal</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[raw]</para>
          <para>Offload rendering of the meta information (location, category) to systemd</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no banner motd</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no banner motd</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>banner</para>
          <para>Set banner string</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>motd</para>
          <para>Strings for motd</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no enable password</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no enable password</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Modify enable password parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>password</para>
          <para>Assign the privileged level password</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no hostname [HOSTNAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no hostname [HOSTNAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>hostname</para>
          <para>Reset system's network name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[HOSTNAME]</para>
          <para>Host name of this router</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no log alarms</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no log alarms</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>alarms</para>
          <para>Logging alarms to osmo_strrb</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no log file FILENAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no log file FILENAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Logging to text file</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>FILENAME</para>
          <para>Filename</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no log gsmtap [HOSTNAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no log gsmtap [HOSTNAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gsmtap</para>
          <para>Logging via GSMTAP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[HOSTNAME]</para>
          <para>Host name to send the GSMTAP logging to (UDP port 4729)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no log stderr</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no log stderr</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stderr</para>
          <para>Logging via STDERR of the process</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no log syslog</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no log syslog</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>syslog</para>
          <para>Logging via syslog</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no log systemd-journal</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no log systemd-journal</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Configure logging sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>systemd-journal</para>
          <para>Logging to systemd-journal</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no service advanced-vty</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no service advanced-vty</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>service</para>
          <para>Set up miscellaneous service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>advanced-vty</para>
          <para>Enable advanced mode vty interface</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no service terminal-length [&lt;0-512&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no service terminal-length [&lt;0-512&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>service</para>
          <para>Set up miscellaneous service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal-length</para>
          <para>System wide terminal length configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-512&gt;]</para>
          <para>Number of lines of VTY (0 means no line control)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no stats reporter log [NAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no stats reporter log [NAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reporter</para>
          <para>Configure a stats reporter</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Report to the logger</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[NAME]</para>
          <para>Name of the reporter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no stats reporter statsd [NAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no stats reporter statsd [NAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reporter</para>
          <para>Configure a stats reporter</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>statsd</para>
          <para>Report to a STATSD server</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[NAME]</para>
          <para>Name of the reporter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>ns</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>ns</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ns</para>
          <para>Configure the GPRS Network Service</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>password (8|) WORD</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>password (8|) WORD</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>password</para>
          <para>Assign the terminal connection password</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>8</para>
          <para>Specifies a HIDDEN password will follow</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para/>
          <para>dummy string </para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>WORD</para>
          <para>The HIDDEN line password string</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>password LINE</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>password LINE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>password</para>
          <para>Assign the terminal connection password</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>LINE</para>
          <para>The UNENCRYPTED (cleartext) line password</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>service advanced-vty</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>service advanced-vty</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>service</para>
          <para>Set up miscellaneous service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>advanced-vty</para>
          <para>Enable advanced mode vty interface</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>service terminal-length &lt;0-512&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>service terminal-length &lt;0-512&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>service</para>
          <para>Set up miscellaneous service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>terminal-length</para>
          <para>System wide terminal length configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-512&gt;</para>
          <para>Number of lines of VTY (0 means no line control)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sgsn</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sgsn</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sgsn</para>
          <para>Configure the SGSN</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>show history</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>show history</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>show</para>
          <para>Show running system information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>history</para>
          <para>Display the session command history</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats interval &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats interval &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>interval</para>
          <para>Set the reporting interval</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Interval in seconds (0 disables the reporting interval)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats reporter log [NAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats reporter log [NAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reporter</para>
          <para>Configure a stats reporter</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>log</para>
          <para>Report to the logger</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[NAME]</para>
          <para>Name of the reporter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats reporter statsd [NAME]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats reporter statsd [NAME]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reporter</para>
          <para>Configure a stats reporter</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>statsd</para>
          <para>Report to a STATSD server</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[NAME]</para>
          <para>Name of the reporter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats-tcp batch-size &lt;1-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats-tcp batch-size &lt;1-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats-tcp</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>batch-size</para>
          <para>Set the number of tcp sockets that are processed per stats polling interval</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-65535&gt;</para>
          <para>Number of sockets per interval</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>stats-tcp interval &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>stats-tcp interval &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>stats-tcp</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>interval</para>
          <para>Set the tcp socket stats polling interval</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Interval in seconds (0 disables the polling interval)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-log</title>
  <para>The log node is commonly available in all Osmocom programs and
    allows configuring logging to stderr and/or log files, including logging
    category and level filtering as well as output formatting options.
    Note that the 'logging enable' command is required to make logging commands
    available on the telnet VTY.</para>
  <section>
    <title>logging color (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging color (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>color</para>
          <para>Configure color-printing for log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't use color for printing messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Use color for printing messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter all (0|1)</title>
    <para>Disable/enable general log output on a given target.
      Typically, 'logging filter all 1' allows to see the usual log output on a
      given target. Setting to '0' can be useful when logging to the telnet VTY
      console: mute all log output to allow typing VTY commands on the telnet
      prompt without interference from log output; 'logging filter all 1' then
      re-enables logging in the same log output configuration as before.

      Some applications provide more specific filters, e.g. to log a given IMSI
      only. To employ such filters, set 'logging filter all 0' to disable
      general logging, and then enable a more specific filter instead.
      </para>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter all (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Do you want to log all messages?</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Only print messages matched by other filters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Bypass filter and print all messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter bvc nsei &lt;0-65535&gt; bvci &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter bvc nsei &lt;0-65535&gt; bvci &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bvc</para>
          <para>Filter based on BSSGP Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsei</para>
          <para>NSEI of the BVC to be filtered</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Network Service Entity Identifier (NSEI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bvci</para>
          <para>BVCI of the BVC to be filtered</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>BSSGP Virtual Connection Identifier (BVCI)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter nse nsei &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter nse nsei &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nse</para>
          <para>Filter based on NS Entity</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsei</para>
          <para>Identify NSE by NSEI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Numeric identifier</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging filter nsvc nsvci &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging filter nsvc nsvci &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filter</para>
          <para>Filter log messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>Filter based on NS Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvci</para>
          <para>Identify NS-VC by NSVCI</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Numeric identifier</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level (mm|pag|meas|ref|gprs|llc|sndcp|slhc|ranap|sua|v42bis|gtp|rim|ra|l...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level (mm|pag|meas|ref|gprs|llc|sndcp|slhc|ranap|sua|v42bis|gtp|rim|ra|lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio|ltcap) (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mm</para>
          <para>Layer3 Mobility Management (MM)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>pag</para>
          <para>Paging Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>meas</para>
          <para>Radio Measurement Processing</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ref</para>
          <para>Reference Counting</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gprs</para>
          <para>GPRS Packet Service</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llc</para>
          <para>GPRS Logical Link Control Protocol (LLC)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sndcp</para>
          <para>GPRS Sub-Network Dependent Control Protocol (SNDCP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>slhc</para>
          <para>RFC1144 TCP/IP Header compression (SLHC)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ranap</para>
          <para>RAN Application Part (RANAP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation (SUA)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>v42bis</para>
          <para>V.42bis data compression (SNDCP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>GPRS Tunnelling Protocol (GTP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rim</para>
          <para>RAN Information Management (RIM)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ra</para>
          <para>Routing Area</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lglobal</para>
          <para>Library-internal global log family</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>llapd</para>
          <para>LAPD in libosmogsm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>linp</para>
          <para>A-bis Intput Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmux</para>
          <para>A-bis B-Subchannel TRAU Frame Multiplex</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmi</para>
          <para>A-bis Input Driver for Signalling</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmib</para>
          <para>A-bis Input Driver for B-Channels (voice)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsms</para>
          <para>Layer3 Short Message Service (SMS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lctrl</para>
          <para>Control Interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgtp</para>
          <para>GPRS GTP library</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lstats</para>
          <para>Statistics messages and logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lgsup</para>
          <para>Generic Subscriber Update Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loap</para>
          <para>Osmocom Authentication Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lss7</para>
          <para>libosmo-sigtran Signalling System 7</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsccp</para>
          <para>libosmo-sigtran SCCP Implementation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lsua</para>
          <para>libosmo-sigtran SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lm3ua</para>
          <para>libosmo-sigtran MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lmgcp</para>
          <para>libosmo-mgcp Media Gateway Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ljibuf</para>
          <para>libosmo-netif Jitter Buffer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lrspro</para>
          <para>Remote SIM protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lns</para>
          <para>GPRS NS layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lbssgp</para>
          <para>GPRS BSSGP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnsdata</para>
          <para>GPRS NS layer data PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lnssignal</para>
          <para>GPRS NS layer signal PDU</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>liuup</para>
          <para>Iu UP layer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lpfcp</para>
          <para>libosmo-pfcp Packet Forwarding Control Protocol</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lcsn1</para>
          <para>libosmo-csn1 Concrete Syntax Notation 1 codec</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lio</para>
          <para>libosmocore IO Subsystem</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ltcap</para>
          <para>TCAP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level force-all (debug|info|notice|error|fatal)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level force-all (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>force-all</para>
          <para>Globally force all logging categories to a specific level. This is released by the 'no logging level force-all' command. Note: any 'logging level &lt;category&gt; &lt;level&gt;' commands will have no visible effect after this, until the forced level is released.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging level set-all (debug|info|notice|error|fatal)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging level set-all (debug|info|notice|error|fatal)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>set-all</para>
          <para>Once-off set all categories to the given log level. There is no single command to take back these changes -- each category is set to the given level, period.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Log debug messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>info</para>
          <para>Log informational messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>notice</para>
          <para>Log noticeable messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>error</para>
          <para>Log error messages and higher levels</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fatal</para>
          <para>Log only fatal messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print category (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print category (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>category</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with category/subsystem name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print category-hex (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print category-hex (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>category-hex</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with category/subsystem nr in hex ('&lt;000b&gt;')</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print extended-timestamp (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print extended-timestamp (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>extended-timestamp</para>
          <para>Configure log message timestamping</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current timestamp with YYYYMMDDhhmmssnnn</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print file (0|1|basename) [last]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print file (0|1|basename) [last]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>file</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with the source file and line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>basename</para>
          <para>Prefix each log message with the source file's basename (strip leading paths) and line</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[last]</para>
          <para>Log source file info at the end of a log line. If omitted, log source file info just before the log text.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print level (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print level (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Configure log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with the log level name</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging print thread-id (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging print thread-id (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>print</para>
          <para>Log output settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>thread-id</para>
          <para>Configure log message logging Thread ID</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current Thread ID</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>logging timestamp (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>logging timestamp (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timestamp</para>
          <para>Configure log message timestamping</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Don't prefix each log message</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Prefix each log message with current timestamp</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no logging level force-all</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no logging level force-all</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>logging</para>
          <para>Configure logging</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the log level for a specified category</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>force-all</para>
          <para>Release any globally forced log level set with 'logging level force-all &lt;level&gt;'</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-stats</title>
  <para/>
  <section>
    <title>disable</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>disable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>disable</para>
          <para>Disable the reporter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>enable</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>enable</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enable</para>
          <para>Enable the reporter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>flush-period &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>flush-period &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>flush-period</para>
          <para>Configure stats sub-system</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Send all stats even if they have not changed (i.e. force the flush)every N-th reporting interval. Set to 0 to disable regular flush (default).</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>level (global|peer|subscriber)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>level (global|peer|subscriber)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>level</para>
          <para>Set the maximum group level</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global</para>
          <para>Report global groups only</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>peer</para>
          <para>Report global and network peer related groups</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subscriber</para>
          <para>Report global, peer, and subscriber groups</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>local-ip ADDR</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>local-ip ADDR</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Set the IP address to which we bind locally</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ADDR</para>
          <para>IP Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>mtu &lt;100-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>mtu &lt;100-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mtu</para>
          <para>Set the maximum packet size</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;100-65535&gt;</para>
          <para>Size in byte</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no local-ip</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no local-ip</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Set the IP address to which we bind locally</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no mtu</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no mtu</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mtu</para>
          <para>Set the maximum packet size</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no prefix</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no prefix</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>prefix</para>
          <para>Set the item name prefix</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>prefix PREFIX</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>prefix PREFIX</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>prefix</para>
          <para>Set the item name prefix</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>PREFIX</para>
          <para>The prefix string</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>remote-ip ADDR</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>remote-ip ADDR</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote-ip</para>
          <para>Set the remote IP address to which we connect</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ADDR</para>
          <para>IP Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>remote-port &lt;1-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>remote-port &lt;1-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote-port</para>
          <para>Set the remote port to which we connect</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-65535&gt;</para>
          <para>Remote port number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-line</title>
  <para/>
  <section>
    <title>bind A.B.C.D [&lt;0-65535&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>bind A.B.C.D [&lt;0-65535&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bind</para>
          <para>Accept VTY telnet connections on local interface</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Local interface IP address (default: 127.0.0.1)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-65535&gt;]</para>
          <para>Local TCP port number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>login</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>login</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>login</para>
          <para>Enable password checking</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no login</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no login</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>login</para>
          <para>Enable password checking</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-ns</title>
  <para/>
  <section>
    <title>bind (fr|udp) ID</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>bind (fr|udp) ID</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bind</para>
          <para>Configure local Bind</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fr</para>
          <para>Frame Relay</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>udp</para>
          <para>UDP/IP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ID</para>
          <para>Unique identifier for this bind (to reference from NS-VCs, NSEs, ...)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>ip-sns-default bind ID</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>ip-sns-default bind ID</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ip-sns-default</para>
          <para>Defaults for dynamically created NSEs created by IP-SNS in SGSN role</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bind</para>
          <para>IP SNS binds</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ID</para>
          <para>Name of NS udp bind whose IP endpoint will be used as IP-SNS local endpoint. Can be given multiple times.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no bind ID</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no bind ID</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bind</para>
          <para>Delete a bind</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ID</para>
          <para>Unique identifier for this bind</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no ip-sns-default bind ID</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no ip-sns-default bind ID</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ip-sns-default</para>
          <para>Defaults for dynamically created NSEs created by IP-SNS in SGSN role</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bind</para>
          <para>IP SNS binds</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ID</para>
          <para>Name of NS udp bind whose IP endpoint will be removed as IP-SNS local endpoint.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no nse &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no nse &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nse</para>
          <para>Delete a Persistent NS Entity</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>NS Entity ID (NSEI)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>nse &lt;0-65535&gt; [ip-sns-role-sgsn]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>nse &lt;0-65535&gt; [ip-sns-role-sgsn]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nse</para>
          <para>Persistent NS Entity</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>NS Entity ID (NSEI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[ip-sns-role-sgsn]</para>
          <para>Create NSE in SGSN role (default: BSS)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>timer (tns-block|tns-block-retries|tns-reset|tns-reset-retries|tns-test|tns-aliv...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>timer (tns-block|tns-block-retries|tns-reset|tns-reset-retries|tns-test|tns-alive|tns-alive-retries|tsns-prov|tsns-size-retries|tsns-config-retries|tsns-procedures-retries) &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timer</para>
          <para>Network Service Timer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tns-block</para>
          <para>(un)blocking Timer (Tns-block) timeout</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tns-block-retries</para>
          <para>(un)blocking Timer (Tns-block) number of retries</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tns-reset</para>
          <para>Reset Timer (Tns-reset) timeout</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tns-reset-retries</para>
          <para>Reset Timer (Tns-reset) number of retries</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tns-test</para>
          <para>Test Timer (Tns-test) timeout</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tns-alive</para>
          <para>Alive Timer (Tns-alive) timeout</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tns-alive-retries</para>
          <para>Alive Timer (Tns-alive) number of retries</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tsns-prov</para>
          <para>SNS Provision Timer (Tsns-prov) timeout</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tsns-size-retries</para>
          <para>SNS Size number of retries</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tsns-config-retries</para>
          <para>SNS Config number of retries</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tsns-procedures-retries</para>
          <para>SNS Procedures number of retries</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Timer Value</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>txqueue-max-length &lt;1-4096&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>txqueue-max-length &lt;1-4096&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>txqueue-max-length</para>
          <para>Set the maximum length of the txqueue (for UDP)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-4096&gt;</para>
          <para>Maximum length of the txqueue</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-bssgp</title>
  <para/>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-ctrl</title>
  <para/>
  <section>
    <title>bind A.B.C.D [&lt;0-65535&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>bind A.B.C.D [&lt;0-65535&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bind</para>
          <para>Set bind address to listen for Control connections</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Local IP address (default 127.0.0.1)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-65535&gt;]</para>
          <para>Local TCP port number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7</title>
  <para/>
  <section>
    <title>as NAME (sua|m3ua|ipa)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>as NAME (sua|m3ua|ipa)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Configure an Application Server</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of the Application Server</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>asp NAME &lt;0-65535&gt; &lt;0-65535&gt; (sua|m3ua|ipa)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>asp NAME &lt;0-65535&gt; &lt;0-65535&gt; (sua|m3ua|ipa)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Configure Application Server Process</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Remote port number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Local port number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>asp NAME &lt;0-65535&gt; &lt;0-65535&gt; (sua|m3ua|ipa) (sctp|tcp)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>asp NAME &lt;0-65535&gt; &lt;0-65535&gt; (sua|m3ua|ipa) (sctp|tcp)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Configure Application Server Process</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Remote port number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Local port number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp</para>
          <para>SCTP (Stream Control Transmission Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp</para>
          <para>TCP (Transmission Control Protocol)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>description .TEXT</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>description .TEXT</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>description</para>
          <para>Save human-readable description of the object</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>.TEXT</para>
          <para>Text until the end of the line</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>listen (sua|m3ua|ipa) &lt;0-65534&gt; [(sctp|tcp)]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>listen (sua|m3ua|ipa) &lt;0-65534&gt; [(sctp|tcp)]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>listen</para>
          <para>Configure/Enable xUA Listener</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65534&gt;</para>
          <para>Port number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[sctp]</para>
          <para>SCTP (Stream Control Transmission Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[tcp]</para>
          <para>TCP (Transmission Control Protocol)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>network-indicator (international | national | reserved | spare)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>network-indicator (international | national | reserved | spare)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>network-indicator</para>
          <para>Configure the Network Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>international</para>
          <para>International Network</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>national</para>
          <para>National Network</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reserved</para>
          <para>Reserved Network</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>spare</para>
          <para>Spare Network</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no as NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no as NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>as</para>
          <para>Disable Application Server</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of AS</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no asp NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no asp NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Disable Application Server Process</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no listen (sua|m3ua|ipa) &lt;0-65534&gt; [(sctp|tcp)]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no listen (sua|m3ua|ipa) &lt;0-65534&gt; [(sctp|tcp)]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>listen</para>
          <para>Disable xUA Listener on given port</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sua</para>
          <para>SCCP User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>m3ua</para>
          <para>MTP3 User Adaptation</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>IPA Multiplex (SCCP Lite)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65534&gt;</para>
          <para>Port number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[sctp]</para>
          <para>SCTP (Stream Control Transmission Protocol)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[tcp]</para>
          <para>TCP (Transmission Control Protocol)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no sccp-address NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no sccp-address NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp-address</para>
          <para>Delete an SCCP addressbook entry</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of the SCCP Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code POINT_CODE</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code POINT_CODE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Configure the local Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Point Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code delimiter (default|dash)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code delimiter (default|dash)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>delimiter</para>
          <para>Configure Point Code Delimiter</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>default</para>
          <para>Use dot as delimiter</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dash</para>
          <para>User dash as delimiter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code format &lt;1-24&gt; [&lt;1-23&gt;] [&lt;1-22&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code format &lt;1-24&gt; [&lt;1-23&gt;] [&lt;1-22&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>format</para>
          <para>Configure Point Code Format</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-24&gt;</para>
          <para>Length of first PC component</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;1-23&gt;]</para>
          <para>Length of second PC component</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;1-22&gt;]</para>
          <para>Length of third PC component</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code format default</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code format default</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>format</para>
          <para>Configure Point Code Format</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>default</para>
          <para>Default Point Code Format (3.8.3)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sccp max-optional-data (&lt;0-999999&gt;|standard)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sccp max-optional-data (&lt;0-999999&gt;|standard)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Configure SCCP behavior</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-optional-data</para>
          <para>Adjust the upper bound for the optional data length (the payload) for CR, CC, CREF and RLSD messages. For any Optional Data part larger than this value in octets, send CR, CC, CREF and RLSD messages without any payload, and send the data payload in a separate Data Form 1 message. ITU-T Q.713 sections 4.2 thru 4.5 define a limit of 128 bytes for the 'Data' parameter. This limit can be adjusted here. May be useful for interop with nonstandard SCCP peers.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-999999&gt;</para>
          <para>Set a non-standard maximum allowed number of bytes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>standard</para>
          <para>Use the ITU-T Q.713 4.2 to 4.5 standard value of 128</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sccp-address NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sccp-address NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp-address</para>
          <para>Create/Modify an SCCP addressbook entry</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of the SCCP Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sccp-timer (conn_est|ias|iar|rel|repeat_rel|int|guard|reset|reassembly) &lt;1-99999...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sccp-timer (conn_est|ias|iar|rel|repeat_rel|int|guard|reset|reassembly) &lt;1-999999&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp-timer</para>
          <para>Configure SCCP timer values, see ITU-T Q.714</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>conn_est</para>
          <para>Waiting for connection confirm message, 1 to 2 minutes (default: 60)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ias</para>
          <para>Send keep-alive: on an idle connection, delay before sending an Idle Timer message, 5 to 10 minutes (default: 420)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>iar</para>
          <para>Receive keep-alive: on an idle connection, delay until considering a connection as stale, 11 to 21 minutes (default: 900)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rel</para>
          <para>Waiting for release complete message, 10 to 20 seconds (default: 10)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>repeat_rel</para>
          <para>Waiting for release complete message; or to repeat sending released message after the initial expiry, 10 to 20 seconds (default: 10)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>int</para>
          <para>Waiting for release complete message; or to release connection resources, freeze the LRN and alert a maintenance function after the initial expiry, extending to 1 minute (default: 60)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>guard</para>
          <para>Waiting to resume normal procedure for temporary connection sections during the restart procedure, 23 to 25 minutes (default: 1380)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reset</para>
          <para>Waiting to release temporary connection section or alert maintenance function after reset request message is sent, 10 to 20 seconds (default: 10)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reassembly</para>
          <para>Waiting to receive all the segments of the remaining segments, single segmented message after receiving the first segment, 10 to 20 seconds (default: 10)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-999999&gt;</para>
          <para>Timer value, in seconds</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>secondary-pc POINT_CODE</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>secondary-pc POINT_CODE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>secondary-pc</para>
          <para>Configure the local Secondary Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>Point Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sls-opc-dpc [opc-shift] [&lt;0-8&gt;] [dpc-shift] [&lt;0-8&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sls-opc-dpc [opc-shift] [&lt;0-8&gt;] [dpc-shift] [&lt;0-8&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sls-opc-dpc</para>
          <para>Shift OPC and DPC bits used during routing decision</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[opc-shift]</para>
          <para>Shift OPC bits used during routing decision</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-8&gt;]</para>
          <para>How many bits from ITU OPC field (starting from least-significant-bit) to skip (default=0). 6 bits are always used</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[dpc-shift]</para>
          <para>Shift DPC bits used during routing decision</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-8&gt;]</para>
          <para>How many bits from ITU DPC field (starting from least-significant-bit) to skip (default=0). 6 bits are always used</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sls-shift &lt;0-6&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sls-shift &lt;0-6&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sls-shift</para>
          <para>Shift SLS bits used during routing decision</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-6&gt;</para>
          <para>How many bits from derivated 7-bit extended-SLS (OPC, DPC, SLS) field (starting from least-significant-bit) to skip</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>timer xua (T8|T10) &lt;1-999999&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>timer xua (T8|T10) &lt;1-999999&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timer</para>
          <para>Configure CS7 Instance default timer values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>xua</para>
          <para>Configure CS7 Instance default xua timer values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>T8</para>
          <para>T8 - Transfer prohibited inhibition timer (transient solution) (ms) (default: 1000)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>T10</para>
          <para>T10 - Waiting to repeat signalling route set test message (s) (default: 45)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-999999&gt;</para>
          <para>Timer value, in seconds</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>xua rkm routing-key-allocation (static-only|dynamic-permitted)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>xua rkm routing-key-allocation (static-only|dynamic-permitted)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>xua</para>
          <para>SIGTRAN xxxUA related</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rkm</para>
          <para>Routing Key Management</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>routing-key-allocation</para>
          <para>Routing Key Management Allocation Policy</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>static-only</para>
          <para>Only static (pre-configured) Routing Keys permitted</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dynamic-permitted</para>
          <para>Dynamically allocate Routing Keys for what ASPs request</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7-as</title>
  <para/>
  <section>
    <title>asp NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>asp NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Specify that a given ASP is part of this AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP to be added to AS</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>binding-table reset</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>binding-table reset</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>binding-table</para>
          <para>AS Loadshare binding table operations</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>reset</para>
          <para>Reset loadshare binding table</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>description .TEXT</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>description .TEXT</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>description</para>
          <para>Save human-readable description of the object</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>.TEXT</para>
          <para>Text until the end of the line</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no asp NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no asp NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>Specify ASP to be removed from this AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name of ASP to be removed</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no point-code override (opc|dpc)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no point-code override (opc|dpc)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Point Code Specific Features</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>override</para>
          <para>Override (force) a point-code of messages received at the AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>opc</para>
          <para>Override Source Point Code of received messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dpc</para>
          <para>Override Destination Point Code of received messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no traffic-mode</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no traffic-mode</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>traffic-mode</para>
          <para>Remove explicit traffic mode of operation of this AS</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code override (opc|dpc) PC</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code override (opc|dpc) PC</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Point Code Specific Features</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>override</para>
          <para>Override (force) a point-code of messages received at the AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>opc</para>
          <para>Override Source Point Code of received messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dpc</para>
          <para>Override Destination Point Code of received messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>PC</para>
          <para>New Point Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code override patch-sccp (disabled|both)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code override patch-sccp (disabled|both)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Point Code Specific Features</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>override</para>
          <para>Override (force) a point-code to hard-coded value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>patch-sccp</para>
          <para>Patch point code values into SCCP called/calling address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>disabled</para>
          <para>Don't patch any point codes into SCCP called/calling address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>both</para>
          <para>Patch both origin and destination point codes into SCCP called/calling address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>qos-class &lt;0-7&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>qos-class &lt;0-7&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>qos-class</para>
          <para>Specity QoS Class of AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-7&gt;</para>
          <para>QoS Class</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>recovery-timeout &lt;1-2000&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>recovery-timeout &lt;1-2000&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>recovery-timeout</para>
          <para>Specifies RFC4666 recovery timer T(r) timeout</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-2000&gt;</para>
          <para>Recovery Timeout in Milliseconds</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>routing-key RCONTEXT DPC</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>routing-key RCONTEXT DPC</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>routing-key</para>
          <para>Define a routing key</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>RCONTEXT</para>
          <para>Routing context number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DPC</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>routing-key RCONTEXT DPC si (aal2|bicc|b-isup|h248|isup|sat-isup|sccp|tup)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>routing-key RCONTEXT DPC si (aal2|bicc|b-isup|h248|isup|sat-isup|sccp|tup)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>routing-key</para>
          <para>Define a routing key</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>RCONTEXT</para>
          <para>Routing context number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DPC</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>si</para>
          <para>Match on Service Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>aal2</para>
          <para>ATM Adaption Layer 2</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bicc</para>
          <para>Bearer Independent Call Control</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>b-isup</para>
          <para>Broadband ISDN User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>h248</para>
          <para>H.248</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>isup</para>
          <para>ISDN User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sat-isup</para>
          <para>Sattelite ISDN User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tup</para>
          <para>Telephony User Part</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>routing-key RCONTEXT DPC si (aal2|bicc|b-isup|h248|isup|sat-isup|sccp|tup) ssn S...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>routing-key RCONTEXT DPC si (aal2|bicc|b-isup|h248|isup|sat-isup|sccp|tup) ssn SSN</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>routing-key</para>
          <para>Define a routing key</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>RCONTEXT</para>
          <para>Routing context number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DPC</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>si</para>
          <para>Match on Service Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>aal2</para>
          <para>ATM Adaption Layer 2</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>bicc</para>
          <para>Bearer Independent Call Control</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>b-isup</para>
          <para>Broadband ISDN User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>h248</para>
          <para>H.248</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>isup</para>
          <para>ISDN User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sat-isup</para>
          <para>Sattelite ISDN User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sccp</para>
          <para>Signalling Connection Control Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tup</para>
          <para>Telephony User Part</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ssn</para>
          <para>Match on Sub-System Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>SSN</para>
          <para>Sub-System Number to match on</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>routing-key RCONTEXT DPC ssn SSN</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>routing-key RCONTEXT DPC ssn SSN</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>routing-key</para>
          <para>Define a routing key</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>RCONTEXT</para>
          <para>Routing context number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DPC</para>
          <para>Destination Point Code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ssn</para>
          <para>Match on Sub-System Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>SSN</para>
          <para>Sub-System Number to match on</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sls-shift &lt;0-3&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sls-shift &lt;0-3&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sls-shift</para>
          <para>Shift SLS bits used during routing decision</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-3&gt;</para>
          <para>How many bits from SLS field (starting from least-significant-bit) to skip</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>traffic-mode (broadcast | roundrobin | override)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>traffic-mode (broadcast | roundrobin | override)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>traffic-mode</para>
          <para>Specifies traffic mode of operation of the ASP within the AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>broadcast</para>
          <para>Broadcast to all ASP within AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>roundrobin</para>
          <para>Round-Robin between all ASP within AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>override</para>
          <para>Override</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>traffic-mode loadshare [bindings] [sls] [opc-sls] [opc-shift] [&lt;0-2&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>traffic-mode loadshare [bindings] [sls] [opc-sls] [opc-shift] [&lt;0-2&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>traffic-mode</para>
          <para>Specifies traffic mode of operation of the ASP within the AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>loadshare</para>
          <para>Share Load among all ASP within AS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[bindings]</para>
          <para>Configure Loadshare parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[sls]</para>
          <para>Configure Loadshare SLS generation parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[opc-sls]</para>
          <para>Generate extended SLS with OPC information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[opc-shift]</para>
          <para>Shift OPC bits used during routing decision</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-2&gt;]</para>
          <para>How many bits from ITU OPC field (starting from least-significant-bit) to skip (default=0). 6 bits are always used</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7-asp</title>
  <para/>
  <section>
    <title>asp-identifier &lt;0-4294967295&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>asp-identifier &lt;0-4294967295&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-identifier</para>
          <para>Specify ASP Identifier for this ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-4294967295&gt;</para>
          <para>ASP Identifier</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>block</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>block</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>block</para>
          <para>Allows a SCTP Association with ASP, but doesn't let it become active</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>description .TEXT</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>description .TEXT</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>description</para>
          <para>Save human-readable description of the object</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>.TEXT</para>
          <para>Text until the end of the line</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>destination-audit asp-active</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>destination-audit asp-active</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>destination-audit</para>
          <para>Configure ASP Auditing (xUA DAUD)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-active</para>
          <para>Transmit DAUD after ASP successful activate (for remote PCs in sccp address-book)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>local-ip (A.B.C.D|X:X::X:X) [primary]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>local-ip (A.B.C.D|X:X::X:X) [primary]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Specify Local IP Address from which to contact ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Local IPv4 Address from which to contact of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Local IPv6 Address from which to contact of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[primary]</para>
          <para>Signal the SCTP peer to use this address as Primary Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no asp-identifier</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no asp-identifier</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-identifier</para>
          <para>Specify ASP Identifier for this ASP</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no block</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no block</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>block</para>
          <para>Allows a SCTP Association with ASP, but doesn't let it become active</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no destination-audit asp-active</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no destination-audit asp-active</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>destination-audit</para>
          <para>Configure ASP Auditing (xUA DAUD)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp-active</para>
          <para>Transmit xUA DAUD after ASP successful activate (for remote PCs in sccp address-book)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no local-ip (A.B.C.D|X:X::X:X)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no local-ip (A.B.C.D|X:X::X:X)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Specify Local IP Address from which to contact ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Local IPv4 Address from which to contact of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Local IPv6 Address from which to contact of ASP</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no quirk (no_notify|daud_in_asp|snm_inactive)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no quirk (no_notify|daud_in_asp|snm_inactive)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>quirk</para>
          <para>Disable quirk to work around interop issues</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no_notify</para>
          <para>Peer SG doesn't send NTFY(AS-INACTIVE) after ASP-UP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>daud_in_asp</para>
          <para>Allow Rx of DAUD in ASP role</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>snm_inactive</para>
          <para>Allow Rx of [S]SNM in AS-INACTIVE state</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no remote-ip (A.B.C.D|X:X::X:X)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no remote-ip (A.B.C.D|X:X::X:X)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote-ip</para>
          <para>Specify Remote IP Address of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Remote IPv4 Address of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Remote IPv6 Address of ASP</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no sctp-param init (num-ostreams|max-instreams|max-attempts|timeout)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no sctp-param init (num-ostreams|max-instreams|max-attempts|timeout)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp-param</para>
          <para>Configure SCTP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>init</para>
          <para>Configure INIT related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>num-ostreams</para>
          <para>Configure INIT Number of Outbound Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-instreams</para>
          <para>Configure INIT Maximum Inboud Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-attempts</para>
          <para>Configure INIT Maximum Attempts</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timeout</para>
          <para>Configure INIT Timeout (milliseconds)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no shutdown</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no shutdown</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>shutdown</para>
          <para>Terminates SCTP association; New associations will be rejected</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no tcp-param keepalive</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no tcp-param keepalive</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp-param</para>
          <para>Configure TCP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>keepalive</para>
          <para>Configure TCP keep-alive related parameters</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no tcp-param keepalive (time|intvl|probes)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no tcp-param keepalive (time|intvl|probes)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp-param</para>
          <para>Configure TCP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>keepalive</para>
          <para>Configure TCP keep-alive related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>time</para>
          <para>Configure number of seconds a connection needs to be idle before beggining to send probes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>intvl</para>
          <para>Configure number of seconds between probes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>probes</para>
          <para>Configure max number of probes to send before giving up if no response is obtained</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no tcp-param user-timeout</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no tcp-param user-timeout</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp-param</para>
          <para>Configure TCP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>user-timeout</para>
          <para>Configure TCP User Timeout socket option (TCP_USER_TIMEOUT)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>qos-class &lt;0-7&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>qos-class &lt;0-7&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>qos-class</para>
          <para>Specify QoS Class of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-7&gt;</para>
          <para>QoS Class</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>quirk (no_notify|daud_in_asp|snm_inactive)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>quirk (no_notify|daud_in_asp|snm_inactive)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>quirk</para>
          <para>Enable quirk to work around interop issues</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no_notify</para>
          <para>Peer SG doesn't send NTFY(AS-INACTIVE) after ASP-UP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>daud_in_asp</para>
          <para>Allow Rx of DAUD in ASP role</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>snm_inactive</para>
          <para>Allow Rx of [S]SNM in AS-INACTIVE state</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>remote-ip (A.B.C.D|X:X::X:X) [primary]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>remote-ip (A.B.C.D|X:X::X:X) [primary]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote-ip</para>
          <para>Specify Remote IP Address of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Remote IPv4 Address of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Remote IPv6 Address of ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[primary]</para>
          <para>Set remote address as SCTP Primary Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>role (sg|asp|ipsp)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>role (sg|asp|ipsp)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>role</para>
          <para>Specify the xUA role for this ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sg</para>
          <para>SG (Signaling Gateway)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asp</para>
          <para>ASP (Application Server Process)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipsp</para>
          <para>IPSP (IP Signalling Point)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sctp-param init (num-ostreams|max-instreams|max-attempts|timeout) &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sctp-param init (num-ostreams|max-instreams|max-attempts|timeout) &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp-param</para>
          <para>Configure SCTP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>init</para>
          <para>Configure INIT related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>num-ostreams</para>
          <para>Configure INIT Number of Outbound Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-instreams</para>
          <para>Configure INIT Maximum Inboud Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-attempts</para>
          <para>Configure INIT Maximum Attempts</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timeout</para>
          <para>Configure INIT Timeout (milliseconds)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Value of the parameter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>shutdown</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>shutdown</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>shutdown</para>
          <para>Terminates SCTP association; New associations will be rejected</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>tcp-param keepalive (time|intvl|probes) &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>tcp-param keepalive (time|intvl|probes) &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp-param</para>
          <para>Configure TCP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>keepalive</para>
          <para>Configure TCP keep-alive related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>time</para>
          <para>Configure number of seconds a connection needs to be idle before beggining to send probes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>intvl</para>
          <para>Configure number of seconds between probes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>probes</para>
          <para>Configure max number of probes to send before giving up if no response is obtained</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Value of the parameter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>tcp-param keepalive enabled</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>tcp-param keepalive enabled</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp-param</para>
          <para>Configure TCP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>keepalive</para>
          <para>Configure TCP keep-alive related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>enabled</para>
          <para>Enable TCP keep-alive</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>tcp-param user-timeout &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>tcp-param user-timeout &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>tcp-param</para>
          <para>Configure TCP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>user-timeout</para>
          <para>Configure TCP User Timeout socket option (TCP_USER_TIMEOUT)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Value of the parameter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>timer lm (wait_asp_up|wait_notify|wait_notify_rkm|wait_rk_reg_resp) &lt;1-999999&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>timer lm (wait_asp_up|wait_notify|wait_notify_rkm|wait_rk_reg_resp) &lt;1-999999&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timer</para>
          <para>Configure ASP default timer values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>lm</para>
          <para>Configure ASP default lm timer values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>wait_asp_up</para>
          <para>Restart ASP after timeout waiting for ASP UP (SG role) / ASP UP ACK (ASP role) (s) (default: 20)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>wait_notify</para>
          <para>Restart ASP after timeout waiting for NOTIFY (s) (default: 2)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>wait_notify_rkm</para>
          <para>Restart ASP after timeout waiting for NOTIFY after RKM registration (s) (default: 20)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>wait_rk_reg_resp</para>
          <para>Restart ASP after timeout waiting for RK_REG_RESP (s) (default: 10)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-999999&gt;</para>
          <para>Timer value, in seconds</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>timer xua (ack|beat) &lt;1-999999&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>timer xua (ack|beat) &lt;1-999999&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timer</para>
          <para>Configure ASP default timer values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>xua</para>
          <para>Configure ASP default xua timer values</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ack</para>
          <para>Resend ASP Up/Down/Active/Inactive after timeout waiting for ASP Up/Down/Active/Inactive ACK (ASP role)(s) (default: 2)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>beat</para>
          <para>Heartbeat Timer (0 = disabled) (s) (default: 30)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-999999&gt;</para>
          <para>Timer value, in seconds</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>transport-role (client|server)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>transport-role (client|server)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>transport-role</para>
          <para>Specify the transport layer role for this ASP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>client</para>
          <para>Operate as a client; connect to a server</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>server</para>
          <para>Operate as a server; wait for client connections</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7-listen</title>
  <para/>
  <section>
    <title>accept-asp-connections (pre-configured|dynamic-permitted)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>accept-asp-connections (pre-configured|dynamic-permitted)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>accept-asp-connections</para>
          <para>Define what kind of ASP connections to accept</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>pre-configured</para>
          <para>Accept only pre-configured ASPs (source IP/port)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dynamic-permitted</para>
          <para>Accept any connection and dynamically create an ASP definition</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>local-ip (A.B.C.D|X:X::X:X)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>local-ip (A.B.C.D|X:X::X:X)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Configure the Local IP Address for xUA</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>IPv4 Address to use for XUA</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>IPv6 Address to use for XUA</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no local-ip (A.B.C.D|X:X::X:X)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no local-ip (A.B.C.D|X:X::X:X)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Configure the Local IP Address for xUA</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>IPv4 Address to use for XUA</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>IPv6 Address to use for XUA</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no sctp-param init (num-ostreams|max-instreams)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no sctp-param init (num-ostreams|max-instreams)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp-param</para>
          <para>Configure SCTP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>init</para>
          <para>Configure INIT related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>num-ostreams</para>
          <para>Configure INIT Number of Outbound Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-instreams</para>
          <para>Configure INIT Maximum Inboud Streams</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>sctp-param init (num-ostreams|max-instreams) &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>sctp-param init (num-ostreams|max-instreams) &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: @</para>
          <para>This command applies on VTY node exit</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sctp-param</para>
          <para>Configure SCTP parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>init</para>
          <para>Configure INIT related parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>num-ostreams</para>
          <para>Configure INIT Number of Outbound Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>max-instreams</para>
          <para>Configure INIT Maximum Inboud Streams</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Value of the parameter</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7-sccpaddr</title>
  <para/>
  <section>
    <title>global-title</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>global-title</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global-title</para>
          <para>Add/Modify Global Title</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no global-title</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no global-title</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global-title</para>
          <para>Remove Global Title</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no point-code</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no point-code</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Remove point-code Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no subsystem-number</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no subsystem-number</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subsystem-number</para>
          <para>Remove Subsystem Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>point-code POINT_CODE</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>point-code POINT_CODE</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>point-code</para>
          <para>Add point-code Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>POINT_CODE</para>
          <para>PC</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>routing-indicator (GT|PC|IP)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>routing-indicator (GT|PC|IP)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>routing-indicator</para>
          <para>Add Routing Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>GT</para>
          <para>by global-title</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>PC</para>
          <para>by point-code</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IP</para>
          <para>by ip-address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>subsystem-number &lt;0-4294967295&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>subsystem-number &lt;0-4294967295&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>subsystem-number</para>
          <para>Add Subsystem Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-4294967295&gt;</para>
          <para>SSN</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cs7-sccpaddr-gt</title>
  <para/>
  <section>
    <title>digits DIGITS</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>digits DIGITS</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>digits</para>
          <para>Set Global Title Digits</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>DIGITS</para>
          <para>Number digits</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>global-title-indicator &lt;0-15&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>global-title-indicator &lt;0-15&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>global-title-indicator</para>
          <para>Set Global Title Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>GTI</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>nature-of-address-indicator &lt;0-127&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>nature-of-address-indicator &lt;0-127&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nature-of-address-indicator</para>
          <para>Set Global Title Nature of Address Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-127&gt;</para>
          <para>NAI</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>numbering-plan-indicator &lt;0-15&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>numbering-plan-indicator &lt;0-15&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>numbering-plan-indicator</para>
          <para>Set Global Title Numbering Plan Indicator</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>NPI</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>translation-type &lt;0-255&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>translation-type &lt;0-255&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>translation-type</para>
          <para>Set Global Title Translation Type</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-255&gt;</para>
          <para>TT</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-cpu-sched</title>
  <para/>
  <section>
    <title>cpu-affinity (self|all|&lt;0-4294967295&gt;|THREADNAME) CPUHEXMASK [delay]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cpu-affinity (self|all|&lt;0-4294967295&gt;|THREADNAME) CPUHEXMASK [delay]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cpu-affinity</para>
          <para>Set CPU affinity mask on a (group of) thread(s)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>self</para>
          <para>Set CPU affinity mask on thread running the VTY</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>all</para>
          <para>Set CPU affinity mask on all process' threads</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-4294967295&gt;</para>
          <para>Set CPU affinity mask on a thread with specified PID</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>THREADNAME</para>
          <para>Set CPU affinity mask on a thread with specified thread name</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>CPUHEXMASK</para>
          <para>CPU affinity mask</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[delay]</para>
          <para>If set, delay applying the affinity mask now and let the app handle it at a later point</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>policy rr &lt;1-32&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>policy rr &lt;1-32&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Global attributes</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>Flag: !</para>
          <para>This command applies immediately</para>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>policy</para>
          <para>Set the scheduling policy to use for the process</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rr</para>
          <para>Use the SCHED_RR real-time scheduling algorithm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-32&gt;</para>
          <para>Set the SCHED_RR real-time priority</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-ns-bind</title>
  <para/>
  <section>
    <title>accept-dynamic-ip-sns</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>accept-dynamic-ip-sns</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>accept-dynamic-ip-sns</para>
          <para>Allow to create dynamic NS Entities by IP-SNS PDUs</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>accept-ipaccess</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>accept-ipaccess</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>accept-ipaccess</para>
          <para>Allow to create dynamic NS Entity by NS Reset PDU on UDP (ip.access style)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>dscp &lt;0-63&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>dscp &lt;0-63&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dscp</para>
          <para>Set DSCP/TOS on the UDP socket</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-63&gt;</para>
          <para>DSCP Value</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>fr NETIF (fr|frnet)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>fr NETIF (fr|frnet)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fr</para>
          <para>frame relay</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NETIF</para>
          <para>Interface name(e.g. ep0)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fr</para>
          <para>fr (user) is used by BSS or SGSN attached to UNI of a FR network</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>frnet</para>
          <para>frnet (network) is used by SGSN if BSS is directly attached</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>ip-sns signalling-weight &lt;0-254&gt; data-weight &lt;0-254&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>ip-sns signalling-weight &lt;0-254&gt; data-weight &lt;0-254&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ip-sns</para>
          <para>IP SNS</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>signalling-weight</para>
          <para>signalling weight used by IP-SNS dynamic configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-254&gt;</para>
          <para>signalling weight used by IP-SNS dynamic configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>data-weight</para>
          <para>data weight used by IP-SNS dynamic configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-254&gt;</para>
          <para>data weight used by IP-SNS dynamic configuration</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>listen (A.B.C.D|X:X::X:X) &lt;1-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>listen (A.B.C.D|X:X::X:X) &lt;1-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>listen</para>
          <para>Configure local IP + Port of this bind</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Local IPv4 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Local IPv6 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-65535&gt;</para>
          <para>Local UDP Port</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no accept-dynamic-ip-sns</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no accept-dynamic-ip-sns</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>accept-dynamic-ip-sns</para>
          <para>Disable dynamic creation of NS Entities by IP-SNS PDUs</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no accept-ipaccess</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no accept-ipaccess</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>accept-ipaccess</para>
          <para>Reject NS Reset PDU on UDP (ip.access style)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no dscp</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no dscp</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Set DSCP/TOS on the UDP socket</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dscp</para>
          <para>DSCP Value</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no fr NETIF</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no fr NETIF</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fr</para>
          <para>Delete a frame relay link</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NETIF</para>
          <para>Delete a frame relay link</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no listen</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no listen</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>listen</para>
          <para>Delete a IP/Port assignment</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>socket-priority &lt;0-255&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>socket-priority &lt;0-255&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>socket-priority</para>
          <para>Set socket priority on the UDP socket</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-255&gt;</para>
          <para>Priority Value (&gt;6 requires CAP_NET_ADMIN)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-ns-nse</title>
  <para/>
  <section>
    <title>ip-sns-bind BINDID</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>ip-sns-bind BINDID</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ip-sns-bind</para>
          <para>IP SNS binds</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>BINDID</para>
          <para>Name of NS udp bind whose IP endpoint will be used as IP-SNS local endpoint. Can be given multiple times.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>ip-sns-remote (A.B.C.D|X:X::X:X) &lt;1-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>ip-sns-remote (A.B.C.D|X:X::X:X) &lt;1-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ip-sns-remote</para>
          <para>SNS Initial Endpoint</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>SGSN IPv4 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>SGSN IPv6 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-65535&gt;</para>
          <para>SGSN UDP Port</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no ip-sns-bind BINDID</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no ip-sns-bind BINDID</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ip-sns-bind</para>
          <para>IP SNS binds</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>BINDID</para>
          <para>Name of NS udp bind whose IP endpoint will not be used as IP-SNS local endpoint</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no ip-sns-remote (A.B.C.D|X:X::X:X) &lt;1-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no ip-sns-remote (A.B.C.D|X:X::X:X) &lt;1-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ip-sns-remote</para>
          <para>Delete a SNS Initial Endpoint</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>SGSN IPv4 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>SGSN IPv6 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-65535&gt;</para>
          <para>SGSN UDP Port</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no nsvc fr NETIF dlci &lt;16-1007&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no nsvc fr NETIF dlci &lt;16-1007&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>Delete frame relay NS-VC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fr</para>
          <para>frame relay</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NETIF</para>
          <para>frame relay interface. Must be registered via fr vty</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dlci</para>
          <para>Data Link connection identifier</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;16-1007&gt;</para>
          <para>Data Link connection identifier</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no nsvc ipa BIND (A.B.C.D|X:X::X:X) &lt;1-65535&gt; nsvci &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no nsvc ipa BIND (A.B.C.D|X:X::X:X) &lt;1-65535&gt; nsvci &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>Delete a NS Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>NS over UDP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>BIND</para>
          <para>A unique bind identifier created by ns bind</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Remote IPv4 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Remote IPv6 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-65535&gt;</para>
          <para>Remote UDP Port</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvci</para>
          <para>NS Virtual Connection ID (NS-VCI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>NS Virtual Connection ID (NS-VCI)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no nsvc nsvci &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no nsvc nsvci &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>Delete NSVC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvci</para>
          <para>NS Virtual Connection ID (NS-VCI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>NS Virtual Connection ID (NS-VCI)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no nsvc udp BIND (A.B.C.D|X:X::X:X) &lt;1-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no nsvc udp BIND (A.B.C.D|X:X::X:X) &lt;1-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>Delete a NS Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>udp</para>
          <para>NS over UDP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>BIND</para>
          <para>A unique bind identifier created by ns bind</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Remote IPv4 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Remote IPv6 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-65535&gt;</para>
          <para>Remote UDP Port</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>nsvc fr NETIF dlci &lt;16-1007&gt; nsvci &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>nsvc fr NETIF dlci &lt;16-1007&gt; nsvci &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>NS Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>fr</para>
          <para>frame relay</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NETIF</para>
          <para>frame relay interface. Must be registered via fr vty</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dlci</para>
          <para>NS Virtual Connection ID (NS-VCI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;16-1007&gt;</para>
          <para>NS Virtual Connection ID (NS-VCI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvci</para>
          <para>Data Link connection identifier</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Data Link connection identifier</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>nsvc ipa BIND (A.B.C.D|X:X::X:X) &lt;1-65535&gt; nsvci &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>nsvc ipa BIND (A.B.C.D|X:X::X:X) &lt;1-65535&gt; nsvci &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>NS Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa</para>
          <para>NS over UDP ip.access style (uses RESET/BLOCK)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>BIND</para>
          <para>A unique bind identifier created by ns bind</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Remote IPv4 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Remote IPv6 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-65535&gt;</para>
          <para>Remote UDP Port</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvci</para>
          <para>NS Virtual Connection ID (NS-VCI)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>NS Virtual Connection ID (NS-VCI)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>nsvc udp BIND (A.B.C.D|X:X::X:X) &lt;1-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>nsvc udp BIND (A.B.C.D|X:X::X:X) &lt;1-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>NS Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>udp</para>
          <para>NS over UDP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>BIND</para>
          <para>A unique bind identifier created by ns bind</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Remote IPv4 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Remote IPv6 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-65535&gt;</para>
          <para>Remote UDP Port</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>nsvc udp BIND (A.B.C.D|X:X::X:X) &lt;1-65535&gt; signalling-weight &lt;0-254&gt; data-weight...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>nsvc udp BIND (A.B.C.D|X:X::X:X) &lt;1-65535&gt; signalling-weight &lt;0-254&gt; data-weight &lt;0-254&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>nsvc</para>
          <para>NS Virtual Connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>udp</para>
          <para>NS over UDP</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>BIND</para>
          <para>A unique bind identifier created by ns bind</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>Remote IPv4 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>X:X::X:X</para>
          <para>Remote IPv6 Address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-65535&gt;</para>
          <para>Remote UDP Port</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>signalling-weight</para>
          <para>Signalling weight of the NSVC (default = 1)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-254&gt;</para>
          <para>Signalling weight of the NSVC (default = 1)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>data-weight</para>
          <para>Data weight of the NSVC (default = 1)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-254&gt;</para>
          <para>Data weight of the NSVC (default = 1)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-sgsn</title>
  <para>Configure the remote GGSN, access-control and other
	    attributes of the SGSN</para>
  <section>
    <title>access-point-name NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>access-point-name NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>access-point-name</para>
          <para>Globally allow the given APN name for all subscribers.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Add this NAME to the list</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>apn APNAME ggsn &lt;0-255&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>apn APNAME ggsn &lt;0-255&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>apn</para>
          <para>Configure the information per APN</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>APNAME</para>
          <para>The APN gateway name optionally prefixed by '*' (wildcard)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ggsn</para>
          <para>Select the GGSN to use for the given APN gateway prefix</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-255&gt;</para>
          <para>The GGSN id</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>apn APNAME imsi-prefix IMSIPRE ggsn &lt;0-255&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>apn APNAME imsi-prefix IMSIPRE ggsn &lt;0-255&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>apn</para>
          <para>Configure the information per APN</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>APNAME</para>
          <para>The APN gateway name optionally prefixed by '*' (wildcard)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>imsi-prefix</para>
          <para>Select the GGSN to use for the given APN gateway prefix if and only if the IMSI matches the given prefix.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IMSIPRE</para>
          <para>An IMSI prefix</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ggsn</para>
          <para>Select the GGSN to use when APN gateway and IMSI prefix match</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-255&gt;</para>
          <para>The GGSN id</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>asn1 debug (1|0)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>asn1 debug (1|0)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asn1</para>
          <para>ASN.1 settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>debug</para>
          <para>Enable ASN.1 debug messages</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Log ASN.1 debug messages to stderr</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Do not log ASN.1 debug messages to stderr</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>asn1 xer-print (1|0)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>asn1 xer-print (1|0)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>asn1</para>
          <para>ASN.1 settings</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>xer-print</para>
          <para>Log human readable representations of all ASN.1 messages to stderr</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Log XML representation of all ASN.1 messages to stderr</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Do not log decoded ASN.1 messages to stderr</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>auth-policy (accept-all|closed|acl-only|remote)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>auth-policy (accept-all|closed|acl-only|remote)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>auth-policy</para>
          <para>Configure the Authorization policy of the SGSN. This setting determines which subscribers are permitted to register to the network.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>accept-all</para>
          <para>Accept all IMSIs (DANGEROUS)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>closed</para>
          <para>Accept only home network subscribers or those in the ACL</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>acl-only</para>
          <para>Accept only subscribers in the ACL</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote</para>
          <para>Use remote subscription data only (HLR)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>authentication (optional|required)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>authentication (optional|required)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>authentication</para>
          <para>Whether to enforce MS authentication in GERAN (only with auth-policy remote)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>optional</para>
          <para>Allow MS to attach via GERAN without authentication (default and only possible value for non-remote auth-policy)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>required</para>
          <para>Always require authentication (only available for auth-policy remote, default with that auth-policy)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>cdr filename NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cdr filename NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cdr</para>
          <para>CDR</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filename</para>
          <para>Set the file name for the call-data-record file, logging the data usage of each subscriber.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>filename</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>cdr interval &lt;1-2147483647&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cdr interval &lt;1-2147483647&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cdr</para>
          <para>CDR</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>interval</para>
          <para>Set the interval for the call-data-record file</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-2147483647&gt;</para>
          <para>interval in seconds</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>cdr trap</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cdr trap</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cdr</para>
          <para>CDR</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>trap</para>
          <para>Enable sending CDR via TRAP CTRL messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>compression rfc1144 active slots &lt;1-256&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>compression rfc1144 active slots &lt;1-256&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>compression</para>
          <para>Configure compression</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rfc1144</para>
          <para>RFC1144 Header compression scheme</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>active</para>
          <para>Compression is actively proposed</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>slots</para>
          <para>Number of compression state slots</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-256&gt;</para>
          <para>Number of compression state slots</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>compression rfc1144 passive</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>compression rfc1144 passive</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>compression</para>
          <para>Configure compression</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rfc1144</para>
          <para>RFC1144 Header compression scheme</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>passive</para>
          <para>Compression is available on request</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>compression v42bis active direction (ms|sgsn|both) codewords &lt;512-65535&gt; strlen ...</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>compression v42bis active direction (ms|sgsn|both) codewords &lt;512-65535&gt; strlen &lt;6-250&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>compression</para>
          <para>Configure compression</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>v42bis</para>
          <para>V.42bis data compression scheme</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>active</para>
          <para>Compression is actively proposed</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>direction</para>
          <para>Direction in which the compression shall be active (p0)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ms</para>
          <para>Compress ms-&gt;sgsn direction only</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>sgsn</para>
          <para>Compress sgsn-&gt;ms direction only</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>both</para>
          <para>Both directions</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>codewords</para>
          <para>Number of codewords (p1)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;512-65535&gt;</para>
          <para>Number of codewords</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>strlen</para>
          <para>Maximum string length (p2)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;6-250&gt;</para>
          <para>Maximum string length</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>compression v42bis passive</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>compression v42bis passive</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>compression</para>
          <para>Configure compression</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>v42bis</para>
          <para>V.42bis data compression scheme</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>passive</para>
          <para>Compression is available on request</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>cs7-instance-iu &lt;0-15&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>cs7-instance-iu &lt;0-15&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cs7-instance-iu</para>
          <para>Set SS7 to be used by the Iu-Interface.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-15&gt;</para>
          <para>SS7 instance reference number (default: 0)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>encryption cipher-plugin-path PATH</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>encryption cipher-plugin-path PATH</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>encryption</para>
          <para>Set encryption algorithms for SGSN</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cipher-plugin-path</para>
          <para>Path to gprs encryption cipher plugin directory</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>PATH</para>
          <para>Plugin path</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>encryption gea &lt;0-4&gt; [&lt;0-4&gt;] [&lt;0-4&gt;] [&lt;0-4&gt;] [&lt;0-4&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>encryption gea &lt;0-4&gt; [&lt;0-4&gt;] [&lt;0-4&gt;] [&lt;0-4&gt;] [&lt;0-4&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>encryption</para>
          <para>Set encryption algorithms for SGSN</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gea</para>
          <para>GPRS Encryption Algorithm</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-4&gt;</para>
          <para>GEAn Algorithm Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-4&gt;]</para>
          <para>GEAn Algorithm Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-4&gt;]</para>
          <para>GEAn Algorithm Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-4&gt;]</para>
          <para>GEAn Algorithm Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-4&gt;]</para>
          <para>GEAn Algorithm Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>encryption uea &lt;0-2&gt; [&lt;0-2&gt;] [&lt;0-2&gt;]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>encryption uea &lt;0-2&gt; [&lt;0-2&gt;] [&lt;0-2&gt;]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>encryption</para>
          <para>Set encryption algorithms for SGSN</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>uea</para>
          <para>UTRAN (3G) encryption algorithms to allow: 0 = UEA0 (no encryption), 1 = UEA1, 2 = UEA2.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-2&gt;</para>
          <para>UEAn Algorithm Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-2&gt;]</para>
          <para>UEAn Algorithm Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-2&gt;]</para>
          <para>UEAn Algorithm Number</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>ggsn &lt;0-255&gt; echo-interval &lt;1-36000&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>ggsn &lt;0-255&gt; echo-interval &lt;1-36000&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ggsn</para>
          <para>Configure the GGSN information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-255&gt;</para>
          <para>GGSN Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>echo-interval</para>
          <para>Send an echo request to this static GGSN every interval.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;1-36000&gt;</para>
          <para>Interval between echo requests in seconds.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>ggsn &lt;0-255&gt; gtp-version (0|1)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>ggsn &lt;0-255&gt; gtp-version (0|1)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ggsn</para>
          <para>Configure the GGSN information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-255&gt;</para>
          <para>GGSN Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp-version</para>
          <para>GTP Version</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>0</para>
          <para>Version 0</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>1</para>
          <para>Version 1</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>ggsn &lt;0-255&gt; no echo-interval</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>ggsn &lt;0-255&gt; no echo-interval</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ggsn</para>
          <para>Configure the GGSN information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-255&gt;</para>
          <para>GGSN Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>echo-interval</para>
          <para>Send an echo request to this static GGSN every interval.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>ggsn &lt;0-255&gt; remote-ip A.B.C.D</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>ggsn &lt;0-255&gt; remote-ip A.B.C.D</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ggsn</para>
          <para>Configure the GGSN information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-255&gt;</para>
          <para>GGSN Number</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote-ip</para>
          <para>Configure this static GGSN to use the specified remote IP address.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>IPv4 Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>ggsn dynamic</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>ggsn dynamic</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ggsn</para>
          <para>Configure the GGSN information</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>dynamic</para>
          <para>Enable dynamic resolving of GGSNs based on DNS resolving the APN name like in a GRX-style setup. Changing this setting requires a restart.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>grx-dns-add A.B.C.D</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>grx-dns-add A.B.C.D</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>grx-dns-add</para>
          <para>Use the specified IP address for DNS-resolving the AP names to GGSN IP addresses</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>IPv4 address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>gsup ipa-name NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>gsup ipa-name NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gsup</para>
          <para>GSUP Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ipa-name</para>
          <para>Set the IPA name of this SGSN</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>A unique name for this SGSN. For example: PLMN + redundancy server number: SGSN-901-70-0. This name is used for GSUP routing and must be set if more than one SGSN is connected to the network. The default is 'SGSN-00-00-00-00-00-00'.</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>gsup oap-id &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>gsup oap-id &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gsup</para>
          <para>GSUP Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>oap-id</para>
          <para>Set the OAP client ID for authentication on the GSUP protocol. This setting only applies if 'auth-policy remote' is used.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>OAP client ID (0 == disabled)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>gsup oap-k K</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>gsup oap-k K</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gsup</para>
          <para>GSUP Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>oap-k</para>
          <para>Set the OAP shared secret key K for authentication on the GSUP protocol. This setting only applies if auth-policy remote is used.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>K</para>
          <para>K value (16 byte) hex</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>gsup oap-opc OPC</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>gsup oap-opc OPC</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gsup</para>
          <para>GSUP Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>oap-opc</para>
          <para>Set the OAP shared secret OPC for authentication on the GSUP protocol. This setting only applies if auth-policy remote is used.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>OPC</para>
          <para>OPC value (16 byte) hex</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>gsup remote-ip A.B.C.D</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>gsup remote-ip A.B.C.D</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gsup</para>
          <para>GSUP Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote-ip</para>
          <para>Set the IP address of the remote GSUP server (e.g. OsmoHLR). This setting only applies if 'auth-policy remote' is used.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>IPv4 Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>gsup remote-port &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>gsup remote-port &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gsup</para>
          <para>GSUP Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote-port</para>
          <para>Set the TCP port of the remote GSUP server, see also 'gsup remote-ip'</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>Remote TCP port</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>gtp local-ip A.B.C.D</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>gtp local-ip A.B.C.D</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>GTP Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>local-ip</para>
          <para>Set the IP address for the local GTP bind for the Gp interface (towards the GGSNs). Note: in case you would like to run the GGSN on the same machine as the SGSN, you can not run both on the same IP address, since both sides are specified to use the same GTP port numbers (2123 and 2152). For example, you could use 127.0.0.1 for the SGSN and 127.0.0.2 for the GGSN in such situations.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>IPv4 Address</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>gtp state-dir PATH</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>gtp state-dir PATH</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>GTP Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>state-dir</para>
          <para>Set the directory for the GTP State file</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>PATH</para>
          <para>Local Directory</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>imsi-acl (add|del) IMSI</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>imsi-acl (add|del) IMSI</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>imsi-acl</para>
          <para>Access Control List of foreign IMSIs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>add</para>
          <para>Add IMSI to ACL</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>del</para>
          <para>Remove IMSI from ACL</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>IMSI</para>
          <para>IMSI of subscriber</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>iu rab-assign-addr-enc (x213|v4raw)</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>iu rab-assign-addr-enc (x213|v4raw)</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>iu</para>
          <para>Iu interface protocol options</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rab-assign-addr-enc</para>
          <para>Choose RAB Assignment's Transport Layer Address encoding</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>x213</para>
          <para>ITU-T X.213 compliant address encoding (default)</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>v4raw</para>
          <para>32bit length raw IPv4 address (for ip.access nano3G)</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>mme NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>mme NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mme</para>
          <para>Configure an MME peer</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name identifying the MME peer</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no access-point-name NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no access-point-name NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>access-point-name</para>
          <para>Configure a global list of allowed APNs</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Remove entry with NAME</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no cdr filename</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no cdr filename</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cdr</para>
          <para>CDR</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>filename</para>
          <para>Disable saving CDR to file</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no cdr trap</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no cdr trap</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cdr</para>
          <para>CDR</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>trap</para>
          <para>Disable sending CDR via TRAP CTRL messages</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no compression rfc1144</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no compression rfc1144</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>compression</para>
          <para>Configure compression</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>rfc1144</para>
          <para>disable rfc1144 TCP/IP header compression</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no compression v42bis</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no compression v42bis</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>compression</para>
          <para>Configure compression</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>v42bis</para>
          <para>disable V.42bis data compression</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no encryption cipher-plugin-path PATH</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no encryption cipher-plugin-path PATH</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>encryption</para>
          <para>Set encryption algorithms for SGSN</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>cipher-plugin-path</para>
          <para>Path to gprs encryption cipher plugin directory</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>PATH</para>
          <para>Plugin path</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no mme NAME</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no mme NAME</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>mme</para>
          <para>Delete an MME peer configuration</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>NAME</para>
          <para>Name identifying the MME peer</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>timer [TNNNN] [(&lt;0-2147483647&gt;|default)]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>timer [TNNNN] [(&lt;0-2147483647&gt;|default)]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timer</para>
          <para>Configure or show timers</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[TNNNN]</para>
          <para>T- or X-timer-number -- 3GPP compliant timer number of the format '1234' or 'T1234' or 't1234'; Osmocom-specific timer number of the format: 'X1234' or 'x1234'.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-2147483647&gt;]</para>
          <para>New timer value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[default]</para>
          <para>Set to default timer value</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>timer gtp [TNNNN] [(&lt;0-2147483647&gt;|default)]</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>timer gtp [TNNNN] [(&lt;0-2147483647&gt;|default)]</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>timer</para>
          <para>Configure or show timers</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>GTP (libgtp) timers</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[TNNNN]</para>
          <para>T- or X-timer-number -- 3GPP compliant timer number of the format '1234' or 'T1234' or 't1234'; Osmocom-specific timer number of the format: 'X1234' or 'x1234'.</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[&lt;0-2147483647&gt;]</para>
          <para>New timer value</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>[default]</para>
          <para>Set to default timer value</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section><section xmlns:vty="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <title>config-sgsn-mme</title>
  <para/>
  <section>
    <title>gtp ran-info-relay &lt;0-999&gt; &lt;0-999&gt; &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>gtp ran-info-relay &lt;0-999&gt; &lt;0-999&gt; &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>Configure GTP connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ran-info-relay</para>
          <para>Configure RAN Information Relay routing</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-999&gt;</para>
          <para>MCC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-999&gt;</para>
          <para>MNC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>TAC</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>gtp ran-info-relay default</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>gtp ran-info-relay default</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>Configure GTP connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ran-info-relay</para>
          <para>Configure RAN Information Relay routing</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>default</para>
          <para>Set as default route</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>gtp remote-ip A.B.C.D</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>gtp remote-ip A.B.C.D</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>Configure GTP connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>remote-ip</para>
          <para>Set Remote GTP IP address</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>A.B.C.D</para>
          <para>IP information</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>gummei &lt;0-999&gt; &lt;0-999&gt; &lt;0-65535&gt; &lt;0-254&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>gummei &lt;0-999&gt; &lt;0-999&gt; &lt;0-65535&gt; &lt;0-254&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gummei</para>
          <para>Configure the mme</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-999&gt;</para>
          <para>MCC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-999&gt;</para>
          <para>MNC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>MME GroupId</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-254&gt;</para>
          <para>MME Code</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no gtp ran-info-relay &lt;0-999&gt; &lt;0-999&gt; &lt;0-65535&gt;</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no gtp ran-info-relay &lt;0-999&gt; &lt;0-999&gt; &lt;0-65535&gt;</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>Configure GTP connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ran-info-relay</para>
          <para>Configure RAN Information Relay routing</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-999&gt;</para>
          <para>MCC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-999&gt;</para>
          <para>MNC</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>&lt;0-65535&gt;</para>
          <para>TAC</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no gtp ran-info-relay default</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no gtp ran-info-relay default</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gtp</para>
          <para>Configure GTP connection</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>ran-info-relay</para>
          <para>Configure RAN Information Relay routing</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>default</para>
          <para>Set as default route</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
  <section>
    <title>no gummei</title>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Command</para>
          <screen>no gummei</screen>
        </listitem>
      </varlistentry>
    </variablelist>
    <variablelist>
      <varlistentry>
        <listitem>
          <para>Parameters</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>no</para>
          <para>Negate a command or set its defaults</para>
        </listitem>
      </varlistentry>
      <varlistentry>
        <listitem>
          <para>gummei</para>
          <para>Remove gummei</para>
        </listitem>
      </varlistentry>
    </variablelist>
  </section>
</section>
