// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (C) 2019 PHYTEC Messtechnik GmbH
 * Author: Stefan Riedmueller <s.riedmueller@phytec.de>
 */

/dts-v1/;
#include "imx6ull.dtsi"
#include "imx6ull-phytec-phycore-som.dtsi"
#include "imx6ull-phytec-segin.dtsi"
#include "imx6ull-phytec-segin-peb-eval-01.dtsi"
#include "imx6ull-phytec-segin-peb-av-02.dtsi"

/ {
	model = "PHYTEC phyBOARD-Segin i.MX6 ULL Full Featured with eMMC";
	compatible = "phytec,imx6ull-pbacd10-emmc", "phytec,imx6ull-pbacd10",
		     "phytec,imx6ull-pcl063","fsl,imx6ull";
};

&adc1 {
	status = "okay";
};

&can1 {
	status = "okay";
};

&tlv320 {
	status = "okay";
};

&ecspi3 {
	status = "okay";
};

&ethphy1 {
	status = "okay";
};

&ethphy2 {
	status = "okay";
};

&fec1 {
	status = "okay";
};

&fec2 {
	status = "okay";
};

&i2c_rtc {
	status = "okay";
};

&reg_can1_en {
	status = "okay";
};

&reg_sound_1v8 {
	status = "okay";
};

&reg_sound_3v3 {
	status = "okay";
};

&sai2 {
	status = "okay";
};

&sound {
	status = "okay";
};

&uart5 {
	status = "okay";
};

&usbotg1 {
	status = "okay";
};

&usbotg2 {
	status = "okay";
};

&usdhc1 {
	status = "okay";
};

&usdhc2 {
	status = "okay";
};
