What:		/sys/bus/platform/drivers/aspeed-vuart/*/lpc_address
Date:		April 2017
Contact:	Jeremy Kerr <jk@ozlabs.org>
Description:	Configures which IO port the host side of the UART
		will appear on the host <-> BMC LPC bus.
Users:		OpenBMC.  Proposed changes should be mailed to
		openbmc@lists.ozlabs.org

What:		/sys/bus/platform/drivers/aspeed-vuart*/sirq
Date:		April 2017
Contact:	Jeremy Kerr <jk@ozlabs.org>
Description:	Configures which interrupt number the host side of
		the UART will appear on the host <-> BMC LPC bus.
Users:		OpenBMC.  Proposed changes should be mailed to
		openbmc@lists.ozlabs.org
