HDMI Connector
==============

Required properties:
- compatible: "hdmi-connector"
- type: the HDMI connector type: "a", "b", "c", "d" or "e"

Optional properties:
- label: a symbolic name for the connector
- hpd-gpios: HPD GPIO number
- ddc-i2c-bus: phandle link to the I2C controller used for DDC EDID probing

Required nodes:
- Video port for HDMI input

Example
-------

hdmi0: connector@1 {
	compatible = "hdmi-connector";
	label = "hdmi";

	type = "a";

	port {
		hdmi_connector_in: endpoint {
			remote-endpoint = <&tpd12s015_out>;
		};
	};
};
