* Hisilicon Hi3519 System Controller Block

This bindings use the following binding:
Documentation/devicetree/bindings/mfd/syscon.txt

Required properties:
- compatible: "hisilicon,hi3519-sysctrl".
- reg: the register region of this block

Examples:
sysctrl: system-controller@12010000 {
	compatible = "hisilicon,hi3519-sysctrl", "syscon";
	reg = <0x12010000 0x1000>;
};
