Renesas SH-Mobile, R-Mobile, and R-Car Platform Device Tree Bindings
--------------------------------------------------------------------

SoCs:

  - Emma Mobile EV2
    compatible = "renesas,emev2"
  - RZ/A1H (R7S72100)
    compatible = "renesas,r7s72100"
  - SH-Mobile AG5 (R8A73A00/SH73A0)
    compatible = "renesas,sh73a0"
  - R-Mobile APE6 (R8A73A40)
    compatible = "renesas,r8a73a4"
  - R-Mobile A1 (R8A77400)
    compatible = "renesas,r8a7740"
  - RZ/G1H (R8A77420)
    compatible = "renesas,r8a7742"
  - RZ/G1M (R8A77430)
    compatible = "renesas,r8a7743"
  - RZ/G1N (R8A77440)
    compatible = "renesas,r8a7744"
  - RZ/G1E (R8A77450)
    compatible = "renesas,r8a7745"
  - RZ/G1C (R8A77470)
    compatible = "renesas,r8a77470"
  - R-Car M1A (R8A77781)
    compatible = "renesas,r8a7778"
  - R-Car H1 (R8A77790)
    compatible = "renesas,r8a7779"
  - R-Car H2 (R8A77900)
    compatible = "renesas,r8a7790"
  - R-Car M2-W (R8A77910)
    compatible = "renesas,r8a7791"
  - R-Car V2H (R8A77920)
    compatible = "renesas,r8a7792"
  - R-Car M2-N (R8A77930)
    compatible = "renesas,r8a7793"
  - R-Car E2 (R8A77940)
    compatible = "renesas,r8a7794"
  - R-Car H3 (R8A77950)
    compatible = "renesas,r8a7795"
  - R-Car M3-W (R8A77960)
    compatible = "renesas,r8a7796"
  - R-Car M3-N (R8A77965)
    compatible = "renesas,r8a77965"
  - R-Car V3M (R8A77970)
    compatible = "renesas,r8a77970"
  - R-Car V3H (R8A77980)
    compatible = "renesas,r8a77980"
  - R-Car E3 (R8A77990)
    compatible = "renesas,r8a77990"
  - R-Car D3 (R8A77995)
    compatible = "renesas,r8a77995"
  - RZ/N1D (R9A06G032)
    compatible = "renesas,r9a06g032"

Boards:

  - Alt (RTP0RC7794SEB00010S)
    compatible = "renesas,alt", "renesas,r8a7794"
  - APE6-EVM
    compatible = "renesas,ape6evm", "renesas,r8a73a4"
  - Atmark Techno Armadillo-800 EVA
    compatible = "renesas,armadillo800eva", "renesas,r8a7740"
  - Blanche (RTP0RC7792SEB00010S)
    compatible = "renesas,blanche", "renesas,r8a7792"
  - BOCK-W
    compatible = "renesas,bockw", "renesas,r8a7778"
  - Condor (RTP0RC77980SEB0010SS/RTP0RC77980SEB0010SA01)
    compatible = "renesas,condor", "renesas,r8a77980"
  - Draak (RTP0RC77995SEB0010S)
    compatible = "renesas,draak", "renesas,r8a77995"
  - Eagle (RTP0RC77970SEB0010S)
    compatible = "renesas,eagle", "renesas,r8a77970"
  - Ebisu (RTP0RC77990SEB0010S)
    compatible = "renesas,ebisu", "renesas,r8a77990"
  - Genmai (RTK772100BC00000BR)
    compatible = "renesas,genmai", "renesas,r7s72100"
  - GR-Peach (X28A-M01-E/F)
    compatible = "renesas,gr-peach", "renesas,r7s72100"
  - Gose (RTP0RC7793SEB00010S)
    compatible = "renesas,gose", "renesas,r8a7793"
  - H3ULCB (R-Car Starter Kit Premier, RTP0RC7795SKBX0010SA00 (H3 ES1.1))
    H3ULCB (R-Car Starter Kit Premier, RTP0RC77951SKBX010SA00 (H3 ES2.0))
    compatible = "renesas,h3ulcb", "renesas,r8a7795"
  - Henninger
    compatible = "renesas,henninger", "renesas,r8a7791"
  - iWave Systems RZ/G1C Single Board Computer (iW-RainboW-G23S)
    compatible = "iwave,g23s", "renesas,r8a77470"
  - iWave Systems RZ/G1E SODIMM SOM Development Platform (iW-RainboW-G22D)
    compatible = "iwave,g22d", "iwave,g22m", "renesas,r8a7745"
  - iWave Systems RZ/G1E SODIMM System On Module (iW-RainboW-G22M-SM)
    compatible = "iwave,g22m", "renesas,r8a7745"
  - iWave Systems RZ/G1M Qseven Development Platform (iW-RainboW-G20D-Qseven)
    compatible = "iwave,g20d", "iwave,g20m", "renesas,r8a7743"
  - iWave Systems RZ/G1M Qseven System On Module (iW-RainboW-G20M-Qseven)
    compatible = "iwave,g20m", "renesas,r8a7743"
  - Kingfisher (SBEV-RCAR-KF-M03)
    compatible = "shimafuji,kingfisher"
  - Koelsch (RTP0RC7791SEB00010S)
    compatible = "renesas,koelsch", "renesas,r8a7791"
  - Kyoto Microcomputer Co. KZM-A9-Dual
    compatible = "renesas,kzm9d", "renesas,emev2"
  - Kyoto Microcomputer Co. KZM-A9-GT
    compatible = "renesas,kzm9g", "renesas,sh73a0"
  - Lager (RTP0RC7790SEB00010S)
    compatible = "renesas,lager", "renesas,r8a7790"
  - M3ULCB (R-Car Starter Kit Pro, RTP0RC7796SKBX0010SA09 (M3 ES1.0))
    compatible = "renesas,m3ulcb", "renesas,r8a7796"
  - Marzen (R0P7779A00010S)
    compatible = "renesas,marzen", "renesas,r8a7779"
  - Porter (M2-LCDP)
    compatible = "renesas,porter", "renesas,r8a7791"
  - RSKRZA1 (YR0K77210C000BE)
    compatible = "renesas,rskrza1", "renesas,r7s72100"
  - RZN1D-DB (RZ/N1D Demo Board for the RZ/N1D 400 pins package)
    compatible = "renesas,rzn1d400-db", "renesas,r9a06g032"
  - Salvator-X (RTP0RC7795SIPB0010S)
    compatible = "renesas,salvator-x", "renesas,r8a7795"
  - Salvator-X (RTP0RC7796SIPB0011S)
    compatible = "renesas,salvator-x", "renesas,r8a7796"
  - Salvator-X (RTP0RC7796SIPB0011S (M3-N))
    compatible = "renesas,salvator-x", "renesas,r8a77965"
  - Salvator-XS (Salvator-X 2nd version, RTP0RC7795SIPB0012S)
    compatible = "renesas,salvator-xs", "renesas,r8a7795"
  - Salvator-XS (Salvator-X 2nd version, RTP0RC7796SIPB0012S)
    compatible = "renesas,salvator-xs", "renesas,r8a7796"
  - Salvator-XS (Salvator-X 2nd version, RTP0RC77965SIPB012S)
    compatible = "renesas,salvator-xs", "renesas,r8a77965"
  - SILK (RTP0RC7794LCB00011S)
    compatible = "renesas,silk", "renesas,r8a7794"
  - SK-RZG1E (YR8A77450S000BE)
    compatible = "renesas,sk-rzg1e", "renesas,r8a7745"
  - SK-RZG1M (YR8A77430S000BE)
    compatible = "renesas,sk-rzg1m", "renesas,r8a7743"
  - Stout (ADAS Starterkit, Y-R-CAR-ADAS-SKH2-BOARD)
    compatible = "renesas,stout", "renesas,r8a7790"
  - V3HSK (Y-ASK-RCAR-V3H-WS10)
    compatible = "renesas,v3hsk", "renesas,r8a77980"
  - V3MSK (Y-ASK-RCAR-V3M-WS10)
    compatible = "renesas,v3msk", "renesas,r8a77970"
  - Wheat (RTP0RC7792ASKB0000JE)
    compatible = "renesas,wheat", "renesas,r8a7792"


Most Renesas ARM SoCs have a Product Register that allows to retrieve SoC
product and revision information.  If present, a device node for this register
should be added.

Required properties:
  - compatible: Must be "renesas,prr".
  - reg: Base address and length of the register block.


Examples
--------

	prr: chipid@ff000044 {
		compatible = "renesas,prr";
		reg = <0 0xff000044 0 4>;
	};
