* Allwinner Codec Analog Controls

Required properties:
- compatible: must be one of the following compatibles:
		- "allwinner,sun8i-a23-codec-analog"
		- "allwinner,sun8i-h3-codec-analog"
		- "allwinner,sun8i-v3s-codec-analog"

Required properties if not a sub-node of the PRCM node:
- reg: must contain the registers location and length

Example:
prcm: prcm@1f01400 {
	codec_analog: codec-analog {
		compatible = "allwinner,sun8i-a23-codec-analog";
	};
};
