What:		/sys/bus/spi/devices/.../spi-nor/jedec_id
Date:		April 2021
KernelVersion:	5.14
Contact:	linux-mtd@lists.infradead.org
Description:	(RO) The JEDEC ID of the SPI NOR flash as reported by the
		flash device.

		The attribute is not present if the flash doesn't support
		the "Read JEDEC ID" command (9Fh). This is the case for
		non-JEDEC compliant flashes.

What:		/sys/bus/spi/devices/.../spi-nor/manufacturer
Date:		April 2021
KernelVersion:	5.14
Contact:	linux-mtd@lists.infradead.org
Description:	(RO) Manufacturer of the SPI NOR flash.


What:		/sys/bus/spi/devices/.../spi-nor/partname
Date:		April 2021
KernelVersion:	5.14
Contact:	linux-mtd@lists.infradead.org
Description:	(RO) Part name of the SPI NOR flash.


What:		/sys/bus/spi/devices/.../spi-nor/sfdp
Date:		April 2021
KernelVersion:	5.14
Contact:	linux-mtd@lists.infradead.org
Description:	(RO) This attribute is only present if the SPI NOR flash
		device supports the "Read SFDP" command (5Ah).

		If present, it contains the complete SFDP (serial flash
		discoverable parameters) binary data of the flash.
