Mediatek bdpsys controller
============================

The Mediatek bdpsys controller provides various clocks to the system.

Required Properties:

- compatible: Should be:
	- "mediatek,mt2701-bdpsys", "syscon"
	- "mediatek,mt2712-bdpsys", "syscon"
	- "mediatek,mt7623-bdpsys", "mediatek,mt2701-bdpsys", "syscon"
- #clock-cells: Must be 1

The bdpsys controller uses the common clk binding from
Documentation/devicetree/bindings/clock/clock-bindings.txt
The available clocks are defined in dt-bindings/clock/mt*-clk.h.

Example:

bdpsys: clock-controller@1c000000 {
	compatible = "mediatek,mt2701-bdpsys", "syscon";
	reg = <0 0x1c000000 0 0x1000>;
	#clock-cells = <1>;
};
