16:57:43.374888 BTS_Tests.ttcn:3545 Starting external command `../ttcn3-tcpdump-start.sh BTS_Tests.TC_rsl_ms_pwr_dyn_up'.
16:57:44.383975 BTS_Tests.ttcn:3545 External command `../ttcn3-tcpdump-start.sh BTS_Tests.TC_rsl_ms_pwr_dyn_up' was executed successfully (exit status: 0).
16:57:44.384167 BTS_Tests.ttcn:3545 Test case TC_rsl_ms_pwr_dyn_up started.
16:57:44.384214 BTS_Tests.ttcn:3545 Initializing variables, timers and ports of component type BTS_Tests.test_CT inside testcase TC_rsl_ms_pwr_dyn_up.
16:57:44.384368 BTS_Tests.ttcn:3545 Port IPA_CTRL was started.
16:57:44.384397 BTS_Tests.ttcn:3545 Port RSL_CCHAN was started.
16:57:44.384419 BTS_Tests.ttcn:3545 Port L1CTL was started.
16:57:44.384440 BTS_Tests.ttcn:3545 Port BTS_TRXC was started.
16:57:44.384460 BTS_Tests.ttcn:3545 Port BTSVTY was started.
16:57:44.384480 BTS_Tests.ttcn:3545 Port BSCVTY was started.
16:57:44.384500 BTS_Tests.ttcn:3545 Port PCU was started.
16:57:44.384521 BTS_Tests.ttcn:3545 Component type BTS_Tests.test_CT was initialized.
16:57:44.384758 BTS_Tests.ttcn:456 Mapping port mtc:BTSVTY to system:BTSVTY.
16:57:44.385748 BTS_Tests.ttcn:456 Message enqueued on BTSVTY from system integer : 2 id 1
16:57:44.385885 BTS_Tests.ttcn:456 Port BTSVTY was mapped to system:BTSVTY.
16:57:44.386236 BTS_Tests.ttcn:456 Map operation of mtc:BTSVTY to system:BTSVTY finished.
16:57:44.386384 Osmocom_VTY_Functions.ttcn:59 Sent on BTSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 1, prompt := "OsmoBTS> ", has_wildcards := false } }
16:57:44.386434 Osmocom_VTY_Functions.ttcn:59 Sent on BTSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 2, prompt := "OsmoBTS# ", has_wildcards := false } }
16:57:44.386463 Osmocom_VTY_Functions.ttcn:59 Sent on BTSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 3, prompt := "OsmoBTS(*)", has_wildcards := true } }
16:57:44.386577 Osmocom_VTY_Functions.ttcn:105 Sent on BTSVTY to system charstring : "enable"
16:57:44.386703 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
16:57:44.386751 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY failed: Type of the first message in the queue is not charstring.
16:57:44.386779 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY failed: Type of the first message in the queue is not charstring.
16:57:44.386802 Osmocom_VTY_Functions.ttcn:74 Matching on port BTSVTY failed: Type of the first message in the queue is not charstring.
16:57:44.386825 Osmocom_VTY_Functions.ttcn:75 Matching on port BTSVTY failed: Type of the first message in the queue is not charstring.
16:57:44.386849 Osmocom_VTY_Functions.ttcn:85 Matching on port BTSVTY failed: Type of the first message in the queue is not charstring.
16:57:44.386878 Osmocom_VTY_Functions.ttcn:86 Matching on port BTSVTY succeeded: 2 with ? matched
16:57:44.386910 Osmocom_VTY_Functions.ttcn:86 Receive operation on port BTSVTY succeeded, message from system(): integer : 2 id 1
16:57:44.386943 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of BTSVTY.
16:57:44.386997 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "OsmoBTS# " id 2
16:57:44.387105 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "OsmoBTS# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:57:44.387186 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY succeeded: "OsmoBTS# " with pattern "[\w-]+\# " matched
16:57:44.387217 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BTSVTY succeeded, message from system(): charstring : "OsmoBTS# " id 2
16:57:44.387248 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of BTSVTY.
16:57:44.387280 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
16:57:44.387312 Osmocom_VTY_Functions.ttcn:338 "TC_rsl_ms_pwr_dyn_up() start"
16:57:44.387372 Osmocom_VTY_Functions.ttcn:105 Sent on BTSVTY to system charstring : "logp lglobal notice TTCN3 f_logp(): TC_rsl_ms_pwr_dyn_up() start"
16:57:44.387423 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
16:57:44.387902 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "OsmoBTS# " id 3
16:57:44.388123 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "OsmoBTS# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:57:44.388221 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY succeeded: "OsmoBTS# " with pattern "[\w-]+\# " matched
16:57:44.388257 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BTSVTY succeeded, message from system(): charstring : "OsmoBTS# " id 3
16:57:44.388292 Osmocom_VTY_Functions.ttcn:73 Message with id 3 was extracted from the queue of BTSVTY.
16:57:44.388327 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
16:57:44.388376 BTS_Tests.ttcn:244 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: TC_rsl_ms_pwr_dyn_up-RSL-IPA.
16:57:44.394831 BTS_Tests.ttcn:244 PTC was created. Component reference: 352, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: TC_rsl_ms_pwr_dyn_up-RSL-IPA.
16:57:44.394979 BTS_Tests.ttcn:245 Creating new alive PTC with component type RSL_Emulation.RSL_Emulation_CT, component name: TC_rsl_ms_pwr_dyn_up-RSL.
16:57:44.403767 BTS_Tests.ttcn:245 PTC was created. Component reference: 353, alive: yes, type: RSL_Emulation.RSL_Emulation_CT, component name: TC_rsl_ms_pwr_dyn_up-RSL.
16:57:44.403891 BTS_Tests.ttcn:247 Mapping port TC_rsl_ms_pwr_dyn_up-RSL-IPA(352):IPA_PORT to system:IPA_CODEC_PT.
16:57:44.404584 BTS_Tests.ttcn:247 Map operation of TC_rsl_ms_pwr_dyn_up-RSL-IPA(352):IPA_PORT to system:IPA_CODEC_PT finished.
16:57:44.404733 BTS_Tests.ttcn:248 Connecting ports TC_rsl_ms_pwr_dyn_up-RSL-IPA(352):IPA_RSL_PORT and TC_rsl_ms_pwr_dyn_up-RSL(353):IPA_PT.
16:57:44.407623 BTS_Tests.ttcn:248 Connect operation on TC_rsl_ms_pwr_dyn_up-RSL-IPA(352):IPA_RSL_PORT and TC_rsl_ms_pwr_dyn_up-RSL(353):IPA_PT finished.
16:57:44.407751 BTS_Tests.ttcn:249 Connecting ports mtc:RSL_CCHAN and TC_rsl_ms_pwr_dyn_up-RSL(353):CCHAN_PT.
16:57:44.408266 BTS_Tests.ttcn:249 Port RSL_CCHAN is waiting for connection from TC_rsl_ms_pwr_dyn_up-RSL(353):CCHAN_PT on UNIX pathname /tmp/ttcn3-portconn-c04ca21e.
16:57:44.408685 BTS_Tests.ttcn:249 Port RSL_CCHAN has accepted the connection from TC_rsl_ms_pwr_dyn_up-RSL(353):CCHAN_PT.
16:57:44.408905 BTS_Tests.ttcn:249 Connect operation on mtc:RSL_CCHAN and TC_rsl_ms_pwr_dyn_up-RSL(353):CCHAN_PT finished.
16:57:44.409031 BTS_Tests.ttcn:251 Starting function main_server("172.18.92.10", 3003, true, IPA_INIT_SEND_IPA_ID_GET (0), true) on component TC_rsl_ms_pwr_dyn_up-RSL-IPA(352).
16:57:44.409380 BTS_Tests.ttcn:251 Function was started.
16:57:44.409500 BTS_Tests.ttcn:252 Starting function main(false) on component TC_rsl_ms_pwr_dyn_up-RSL(353).
16:57:44.409844 BTS_Tests.ttcn:252 Function was started.
16:57:44.409963 BTS_Tests.ttcn:256 Start timer T: 15 s
16:57:44.933150 BTS_Tests.ttcn:257 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @RSL_Emulation.RSLEm_Event : { ev_type := RSLEM_EV_TRX_UP (0), sid := IPAC_PROTO_RSL_TRX0 (0) } id 1
16:57:44.933180 BTS_Tests.ttcn:259 Matching on port RSL_CCHAN succeeded:  matched
16:57:44.933189 BTS_Tests.ttcn:259 Receive operation on port RSL_CCHAN succeeded, message from TC_rsl_ms_pwr_dyn_up-RSL(353): @RSL_Emulation.RSLEm_Event : { ev_type := RSLEM_EV_TRX_UP (0), sid := IPAC_PROTO_RSL_TRX0 (0) } id 1
16:57:44.933196 BTS_Tests.ttcn:259 Message with id 1 was extracted from the queue of RSL_CCHAN.
16:57:44.933205 BTS_Tests.ttcn:269 1/4 transceiver(s) connected
16:57:44.933449 BTS_Tests.ttcn:257 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @RSL_Emulation.RSLEm_Event : { ev_type := RSLEM_EV_TRX_UP (0), sid := IPAC_PROTO_RSL_TRX1 (1) } id 2
16:57:44.933477 BTS_Tests.ttcn:259 Matching on port RSL_CCHAN succeeded:  matched
16:57:44.933496 BTS_Tests.ttcn:259 Receive operation on port RSL_CCHAN succeeded, message from TC_rsl_ms_pwr_dyn_up-RSL(353): @RSL_Emulation.RSLEm_Event : { ev_type := RSLEM_EV_TRX_UP (0), sid := IPAC_PROTO_RSL_TRX1 (1) } id 2
16:57:44.933515 BTS_Tests.ttcn:259 Message with id 2 was extracted from the queue of RSL_CCHAN.
16:57:44.933544 BTS_Tests.ttcn:269 2/4 transceiver(s) connected
16:57:44.934027 BTS_Tests.ttcn:257 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @RSL_Emulation.RSLEm_Event : { ev_type := RSLEM_EV_TRX_UP (0), sid := IPAC_PROTO_RSL_TRX2 (2) } id 3
16:57:44.934182 BTS_Tests.ttcn:259 Matching on port RSL_CCHAN succeeded:  matched
16:57:44.934249 BTS_Tests.ttcn:259 Receive operation on port RSL_CCHAN succeeded, message from TC_rsl_ms_pwr_dyn_up-RSL(353): @RSL_Emulation.RSLEm_Event : { ev_type := RSLEM_EV_TRX_UP (0), sid := IPAC_PROTO_RSL_TRX2 (2) } id 3
16:57:44.934351 BTS_Tests.ttcn:259 Message with id 3 was extracted from the queue of RSL_CCHAN.
16:57:44.934405 BTS_Tests.ttcn:269 3/4 transceiver(s) connected
16:57:44.936469 BTS_Tests.ttcn:257 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 3, streamId := IPAC_PROTO_RSL_TRX1 (1), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 4
16:57:44.936494 BTS_Tests.ttcn:259 Matching on port RSL_CCHAN failed: Type of the first message in the queue is not @RSL_Emulation.RSLEm_Event.
16:57:44.936515 BTS_Tests.ttcn:273 Matching on port RSL_CCHAN succeeded:  matched
16:57:44.936530 BTS_Tests.ttcn:273 Receive operation on port RSL_CCHAN succeeded, message from TC_rsl_ms_pwr_dyn_up-RSL(353): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 3, streamId := IPAC_PROTO_RSL_TRX1 (1), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 4
16:57:44.936539 BTS_Tests.ttcn:273 Message with id 4 was extracted from the queue of RSL_CCHAN.
16:57:44.936548 BTS_Tests.ttcn:285 1/4 RF Resource Indication(s) received
16:57:44.936725 BTS_Tests.ttcn:257 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 4, streamId := IPAC_PROTO_RSL_TRX2 (2), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 5
16:57:44.936737 BTS_Tests.ttcn:259 Matching on port RSL_CCHAN failed: Type of the first message in the queue is not @RSL_Emulation.RSLEm_Event.
16:57:44.936749 BTS_Tests.ttcn:273 Matching on port RSL_CCHAN succeeded:  matched
16:57:44.936759 BTS_Tests.ttcn:273 Receive operation on port RSL_CCHAN succeeded, message from TC_rsl_ms_pwr_dyn_up-RSL(353): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 4, streamId := IPAC_PROTO_RSL_TRX2 (2), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 5
16:57:44.936767 BTS_Tests.ttcn:273 Message with id 5 was extracted from the queue of RSL_CCHAN.
16:57:44.936775 BTS_Tests.ttcn:285 2/4 RF Resource Indication(s) received
16:57:44.936807 BTS_Tests.ttcn:257 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 6
16:57:44.936816 BTS_Tests.ttcn:259 Matching on port RSL_CCHAN failed: Type of the first message in the queue is not @RSL_Emulation.RSLEm_Event.
16:57:44.936827 BTS_Tests.ttcn:273 Matching on port RSL_CCHAN succeeded:  matched
16:57:44.936836 BTS_Tests.ttcn:273 Receive operation on port RSL_CCHAN succeeded, message from TC_rsl_ms_pwr_dyn_up-RSL(353): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 6
16:57:44.936848 BTS_Tests.ttcn:273 Message with id 6 was extracted from the queue of RSL_CCHAN.
16:57:44.936855 BTS_Tests.ttcn:285 3/4 RF Resource Indication(s) received
16:57:44.937056 BTS_Tests.ttcn:257 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @RSL_Emulation.RSLEm_Event : { ev_type := RSLEM_EV_TRX_UP (0), sid := IPAC_PROTO_RSL_TRX3 (3) } id 7
16:57:44.937084 BTS_Tests.ttcn:259 Matching on port RSL_CCHAN succeeded:  matched
16:57:44.937093 BTS_Tests.ttcn:259 Receive operation on port RSL_CCHAN succeeded, message from TC_rsl_ms_pwr_dyn_up-RSL(353): @RSL_Emulation.RSLEm_Event : { ev_type := RSLEM_EV_TRX_UP (0), sid := IPAC_PROTO_RSL_TRX3 (3) } id 7
16:57:44.937100 BTS_Tests.ttcn:259 Message with id 7 was extracted from the queue of RSL_CCHAN.
16:57:44.937107 BTS_Tests.ttcn:269 4/4 transceiver(s) connected
16:57:44.937171 BTS_Tests.ttcn:257 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 5, streamId := IPAC_PROTO_RSL_TRX3 (3), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 8
16:57:44.937184 BTS_Tests.ttcn:259 Matching on port RSL_CCHAN failed: Type of the first message in the queue is not @RSL_Emulation.RSLEm_Event.
16:57:44.937197 BTS_Tests.ttcn:273 Matching on port RSL_CCHAN succeeded:  matched
16:57:44.937205 BTS_Tests.ttcn:273 Receive operation on port RSL_CCHAN succeeded, message from TC_rsl_ms_pwr_dyn_up-RSL(353): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 5, streamId := IPAC_PROTO_RSL_TRX3 (3), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 8
16:57:44.937212 BTS_Tests.ttcn:273 Message with id 8 was extracted from the queue of RSL_CCHAN.
16:57:44.937219 BTS_Tests.ttcn:285 4/4 RF Resource Indication(s) received
16:57:44.937230 Osmocom_Types.ttcn:126 Start timer T: 0.5 s
16:57:45.437750 Osmocom_Types.ttcn:127 Timeout T: 0.5 s
16:57:45.437813 Osmocom_CTRL_Adapter.ttcn:69 Creating new PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
16:57:45.442511 Osmocom_CTRL_Adapter.ttcn:69 PTC was created. Component reference: 354, alive: no, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
16:57:45.442561 Osmocom_CTRL_Adapter.ttcn:71 Mapping port IPA-CTRL-CLI-IPA(354):IPA_PORT to system:IPA_CODEC_PT.
16:57:45.444424 Osmocom_CTRL_Adapter.ttcn:71 Map operation of IPA-CTRL-CLI-IPA(354):IPA_PORT to system:IPA_CODEC_PT finished.
16:57:45.444443 Osmocom_CTRL_Adapter.ttcn:72 Connecting ports IPA-CTRL-CLI-IPA(354):IPA_CTRL_PORT and mtc:IPA_CTRL.
16:57:45.444637 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL is waiting for connection from IPA-CTRL-CLI-IPA(354):IPA_CTRL_PORT on UNIX pathname /tmp/ttcn3-portconn-c213f21f.
16:57:45.444793 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL has accepted the connection from IPA-CTRL-CLI-IPA(354):IPA_CTRL_PORT.
16:57:45.444884 Osmocom_CTRL_Adapter.ttcn:72 Connect operation on IPA-CTRL-CLI-IPA(354):IPA_CTRL_PORT and mtc:IPA_CTRL finished.
16:57:45.444901 Osmocom_CTRL_Adapter.ttcn:74 Starting function main_client("172.18.92.20", 4238, "", 0, { ser_nr := "", name := "mahlzeit", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "0/1/2", osmo_rand := "" }, false) on component IPA-CTRL-CLI-IPA(354).
16:57:45.445020 Osmocom_CTRL_Adapter.ttcn:74 Function was started.
16:57:45.445034 Osmocom_CTRL_Adapter.ttcn:37 Start timer T: 10 s
16:57:45.447204 Osmocom_CTRL_Adapter.ttcn:38 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(354) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
16:57:45.447224 Osmocom_CTRL_Adapter.ttcn:39 Matching on port IPA_CTRL succeeded:  matched
16:57:45.447236 Osmocom_CTRL_Adapter.ttcn:39 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(354): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
16:57:45.447247 Osmocom_CTRL_Adapter.ttcn:39 Message with id 1 was extracted from the queue of IPA_CTRL.
16:57:45.447321 GSM_SystemInformation.ttcn:246 enc_SystemInformationNoPad(): Encoding @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 18, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_3 (27) }, payload := { si3 := { cell_id := 23, lai := { mcc_mnc := '262F42'H, lac := 42 }, ctrl_chan_desc := { msc_r99 := true, att := true, bs_ag_blks_res := 1, ccch_conf := CCHAN_DESC_1CCCH_COMBINED (1), si22ind := false, cbq3 := CBQ3_IU_MODE_NOT_SUPPORTED (0), spare := '00'B, bs_pa_mfrms := 0, t3212 := 1 }, cell_options := { dn_ind := false, pwrc := false, dtx := MS_MAY_USE_UL_DTX (0), radio_link_tout_div4 := 7 }, cell_sel_par := { cell_resel_hyst_2dB := 2, ms_txpwr_max_cch := 7, acs := '0'B, neci := true, rxlev_access_min := 0 }, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B }, rest_octets := { sel_params := { presence := '0'B, params := omit }, pwr_offset := { presence := '0'B, offset := omit }, si_2ter_ind := '0'B, early_cm_ind := '0'B, sched_where := { presence := '0'B, where := omit }, gprs_ind := { presence := '1'B, ind := { ra_colour := 0, si13_pos := '0'B } }, umts_early_cm_ind := '0'B, si2_quater_ind := { presence := '0'B, ind := omit }, iu_mode_ind := omit, si21_ind := { presence := '0'B, pos := omit } } } } }
16:57:45.447399 GSM_SystemInformation.ttcn:246 enc_SystemInformationNoPad(): Stream after encoding: '49061B001762F224002AC90001074740E504002C2B'O
16:57:45.447416 BTS_Tests.ttcn:451 Setting RSL_SYSTEM_INFO_3 (3): { header := { l2_plen := { l2_plen := 18, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_3 (27) }, payload := { si3 := { cell_id := 23, lai := { mcc_mnc := '262F42'H, lac := 42 }, ctrl_chan_desc := { msc_r99 := true, att := true, bs_ag_blks_res := 1, ccch_conf := CCHAN_DESC_1CCCH_COMBINED (1), si22ind := false, cbq3 := CBQ3_IU_MODE_NOT_SUPPORTED (0), spare := '00'B, bs_pa_mfrms := 0, t3212 := 1 }, cell_options := { dn_ind := false, pwrc := false, dtx := MS_MAY_USE_UL_DTX (0), radio_link_tout_div4 := 7 }, cell_sel_par := { cell_resel_hyst_2dB := 2, ms_txpwr_max_cch := 7, acs := '0'B, neci := true, rxlev_access_min := 0 }, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B }, rest_octets := { sel_params := { presence := '0'B, params := omit }, pwr_offset := { presence := '0'B, offset := omit }, si_2ter_ind := '0'B, early_cm_ind := '0'B, sched_where := { presence := '0'B, where := omit }, gprs_ind := { presence := '1'B, ind := { ra_colour := 0, si13_pos := '0'B } }, umts_early_cm_ind := '0'B, si2_quater_ind := { presence := '0'B, ind := omit }, iu_mode_ind := omit, si21_ind := { presence := '0'B, pos := omit } } } } }
16:57:45.447520 BTS_Tests.ttcn:444 Setting RSL_SYSTEM_INFO_3 (3): '49061B001762F224002AC90001074740E504002C2B2B2B'O
16:57:45.447624 BTS_Tests.ttcn:445 Sent on RSL_CCHAN to TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := omit, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_3 (3) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 0, payload := '49061B001762F224002AC90001074740E504002C2B2B2B'O } } } } } }
16:57:45.447666 GSM_SystemInformation.ttcn:246 enc_SystemInformationNoPad(): Encoding @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 22, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_2 (26) }, payload := { si2 := { bcch_freq_list := '00000000000000000000000000000000'O, ncc_permitted := '11111111'B, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B } } } }
16:57:45.447694 GSM_SystemInformation.ttcn:246 enc_SystemInformationNoPad(): Stream after encoding: '59061A00000000000000000000000000000000FFE50400'O
16:57:45.447706 BTS_Tests.ttcn:451 Setting RSL_SYSTEM_INFO_2 (2): { header := { l2_plen := { l2_plen := 22, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_2 (26) }, payload := { si2 := { bcch_freq_list := '00000000000000000000000000000000'O, ncc_permitted := '11111111'B, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B } } } }
16:57:45.447750 BTS_Tests.ttcn:444 Setting RSL_SYSTEM_INFO_2 (2): '59061A00000000000000000000000000000000FFE50400'O
16:57:45.447787 BTS_Tests.ttcn:445 Sent on RSL_CCHAN to TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := omit, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2 (2) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 0, payload := '59061A00000000000000000000000000000000FFE50400'O } } } } } }
16:57:45.447823 GSM_SystemInformation.ttcn:246 enc_SystemInformationNoPad(): Encoding @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 12, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_4 (28) }, payload := { si4 := { lai := { mcc_mnc := '262F42'H, lac := 42 }, cell_sel_par := { cell_resel_hyst_2dB := 2, ms_txpwr_max_cch := 7, acs := '0'B, neci := true, rxlev_access_min := 0 }, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B }, cbch_chan_desc := omit, cbch_mobile_alloc := omit, rest_octets := { sel_params := { presence := '0'B, params := omit }, pwr_offset := { presence := '0'B, offset := omit }, gprs_ind := { presence := '1'B, ind := { ra_colour := 0, si13_pos := '0'B } }, s_presence := '0'B, s := omit } } } }
16:57:45.447857 GSM_SystemInformation.ttcn:246 enc_SystemInformationNoPad(): Stream after encoding: '31061C62F224002A4740E5040001'O
16:57:45.447868 BTS_Tests.ttcn:451 Setting RSL_SYSTEM_INFO_4 (4): { header := { l2_plen := { l2_plen := 12, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_4 (28) }, payload := { si4 := { lai := { mcc_mnc := '262F42'H, lac := 42 }, cell_sel_par := { cell_resel_hyst_2dB := 2, ms_txpwr_max_cch := 7, acs := '0'B, neci := true, rxlev_access_min := 0 }, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B }, cbch_chan_desc := omit, cbch_mobile_alloc := omit, rest_octets := { sel_params := { presence := '0'B, params := omit }, pwr_offset := { presence := '0'B, offset := omit }, gprs_ind := { presence := '1'B, ind := { ra_colour := 0, si13_pos := '0'B } }, s_presence := '0'B, s := omit } } } }
16:57:45.447929 BTS_Tests.ttcn:444 Setting RSL_SYSTEM_INFO_4 (4): '31061C62F224002A4740E50400012B2B2B2B2B2B2B2B2B'O
16:57:45.447964 BTS_Tests.ttcn:445 Sent on RSL_CCHAN to TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := omit, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_4 (4) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 0, payload := '31061C62F224002A4740E50400012B2B2B2B2B2B2B2B2B'O } } } } } }
16:57:45.447985 BTS_Tests.ttcn:612 Mapping port mtc:BTS_TRXC to system:BTS_TRXC.
16:57:45.448024 BTS_Tests.ttcn:612 Port BTS_TRXC was mapped to system:BTS_TRXC.
16:57:45.448049 BTS_Tests.ttcn:612 Map operation of mtc:BTS_TRXC to system:BTS_TRXC finished.
16:57:45.448064 BTS_Tests.ttcn:508 entering f__IPL4__PROVIDER__connect: :-1 -> 172.18.92.21:5701 / UDP
16:57:45.448076 BTS_Tests.ttcn:508 entering f__IPL4__PROVIDER__listen: :-1 / UDP
16:57:45.448137 TRXC_CodecPort.ttcn:77 Sent on BTS_TRXC to system @TRXC_CodecPort.TRXC_Send : { connId := 1, msg := { cmd := { verb := "FAKE_TOA", params := { "512", "0" } } } }
16:57:45.448150 TRXC_CodecPort.ttcn:42 enc_TrxcMessage(): Encoding @TRXC_Types.TrxcMessage: { cmd := { verb := "FAKE_TOA", params := { "512", "0" } } }
16:57:45.448163 TRXC_CodecPort.ttcn:42 enc_TrxcMessage(): Stream after encoding: "CMD FAKE_TOA 512 0"
16:57:45.448177 TRXC_CodecPort.ttcn:77 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : { connId := 1, proto := { udp := { } }, msg := '434D442046414B455F544F41203531322030'O ("CMD FAKE_TOA 512 0") }
16:57:45.448211 TRXC_CodecPort.ttcn:78 Start timer T: 3 s
16:57:45.448339 TRXC_CodecPort.ttcn:79 Message enqueued on BTS_TRXC from system @IPL4asp_Types.ASP_RecvFrom : { connId := 1, remName := "172.18.92.21", remPort := 5701, locName := "0.0.0.0", locPort := 9999, proto := { udp := { } }, userData := 0, msg := '5253502046414B455F544F41203020353132203000'O } id 1
16:57:45.448351 TRXC_CodecPort.ttcn:36 dec_TrxcMessage(): Stream before decoding: "RSP FAKE_TOA 0 512 0" & char(0, 0, 0, 0)
16:57:45.448362 TRXC_CodecPort.ttcn:36 match_begin data: RSP FAKE_TOA 0 512 0
16:57:45.448370 TRXC_CodecPort.ttcn:36 match_begin token: "CMD "
16:57:45.448377 TRXC_CodecPort.ttcn:36 match_begin result: -1
16:57:45.448385 TRXC_CodecPort.ttcn:36 match_begin data: RSP FAKE_TOA 0 512 0
16:57:45.448392 TRXC_CodecPort.ttcn:36 match_begin token: "RSP "
16:57:45.448399 TRXC_CodecPort.ttcn:36 match_begin result: 4
16:57:45.448417 TRXC_CodecPort.ttcn:36 match_begin data: FAKE_TOA 0 512 0
16:57:45.448424 TRXC_CodecPort.ttcn:36 match_begin token: "^(((POWERON)|(POWEROFF)|(CLOCK)|(RXTUNE)|(TXTUNE)|(SETSLOT)|(SETTSC)|(SETBSIC)|(SETPOWER)|(SETMAXDLY)|(SETMAXDLYNB)|(HANDOVER)|(NOHANDOVER)|(MEASURE)|(FAKE_RSSI)|(FAKE_TOA)|(FAKE_CI)|(FAKE_TRXC_DELAY)))"
16:57:45.448449 TRXC_CodecPort.ttcn:36 match_begin regexec result: 0, Success
16:57:45.448456 TRXC_CodecPort.ttcn:36 match_begin result: 8
16:57:45.448463 TRXC_CodecPort.ttcn:36 match_begin data:  0 512 0
16:57:45.448470 TRXC_CodecPort.ttcn:36 match_begin token: " "
16:57:45.448477 TRXC_CodecPort.ttcn:36 match_begin result: 1
16:57:45.448484 TRXC_CodecPort.ttcn:36 match_first data: 0 512 0
16:57:45.448490 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.448497 TRXC_CodecPort.ttcn:36 match_first result: 1
16:57:45.448503 TRXC_CodecPort.ttcn:36 match_list data: 0 512 0
16:57:45.448510 TRXC_CodecPort.ttcn:36 match_list result: 1
16:57:45.448520 TRXC_CodecPort.ttcn:36 match_begin data:  512 0
16:57:45.448526 TRXC_CodecPort.ttcn:36 match_begin token: " "
16:57:45.448533 TRXC_CodecPort.ttcn:36 match_begin result: 1
16:57:45.448540 TRXC_CodecPort.ttcn:36 match_first data: 512 0
16:57:45.448547 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.448558 TRXC_CodecPort.ttcn:36 match_first result: 3
16:57:45.448564 TRXC_CodecPort.ttcn:36 match_first data: 512 0
16:57:45.448570 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.448577 TRXC_CodecPort.ttcn:36 match_first result: 3
16:57:45.448583 TRXC_CodecPort.ttcn:36 match_list data: 512 0
16:57:45.448589 TRXC_CodecPort.ttcn:36 match_list result: 3
16:57:45.448596 TRXC_CodecPort.ttcn:36 match_begin data:  0
16:57:45.448602 TRXC_CodecPort.ttcn:36 match_begin token: " "
16:57:45.448609 TRXC_CodecPort.ttcn:36 match_begin result: 1
16:57:45.448615 TRXC_CodecPort.ttcn:36 match_first data: 0
16:57:45.448622 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.448637 TRXC_CodecPort.ttcn:36 match_first result: -1
16:57:45.448644 TRXC_CodecPort.ttcn:36 match_first data: 0
16:57:45.448650 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.448657 TRXC_CodecPort.ttcn:36 match_first result: -1
16:57:45.448664 TRXC_CodecPort.ttcn:36 match_list data: 0
16:57:45.448670 TRXC_CodecPort.ttcn:36 match_list result: -1
16:57:45.448678 TRXC_CodecPort.ttcn:36 match_begin data: 
16:57:45.448685 TRXC_CodecPort.ttcn:36 match_begin token: " "
16:57:45.448691 TRXC_CodecPort.ttcn:36 match_begin result: -1
16:57:45.448699 TRXC_CodecPort.ttcn:36 dec_TrxcMessage(): Decoded @TRXC_Types.TrxcMessage: { rsp := { verb := "FAKE_TOA", status := 0, params := { "512", "0" } } }
16:57:45.448710 TRXC_CodecPort.ttcn:36 Warning: dec_TrxcMessage(): Data remained at the end of the stream after successful decoding: '00'O
16:57:45.448726 TRXC_CodecPort.ttcn:79 Incoming message was mapped to @TRXC_CodecPort.TRXC_RecvFrom : { connId := 1, remName := "172.18.92.21", remPort := 5701, locName := "0.0.0.0", locPort := 9999, msg := { rsp := { verb := "FAKE_TOA", status := 0, params := { "512", "0" } } } } id 1
16:57:45.448742 TRXC_CodecPort.ttcn:80 Matching on port BTS_TRXC succeeded:  matched
16:57:45.448754 TRXC_CodecPort.ttcn:80 Receive operation on port BTS_TRXC succeeded, message from system(): @TRXC_CodecPort.TRXC_RecvFrom : { connId := 1, remName := "172.18.92.21", remPort := 5701, locName := "0.0.0.0", locPort := 9999, msg := { rsp := { verb := "FAKE_TOA", status := 0, params := { "512", "0" } } } } id 1
16:57:45.448764 TRXC_CodecPort.ttcn:80 Message with id 1 was extracted from the queue of BTS_TRXC.
16:57:45.448780 TRXC_CodecPort.ttcn:77 Sent on BTS_TRXC to system @TRXC_CodecPort.TRXC_Send : { connId := 1, msg := { cmd := { verb := "FAKE_RSSI", params := { "-60", "0" } } } }
16:57:45.448789 TRXC_CodecPort.ttcn:42 enc_TrxcMessage(): Encoding @TRXC_Types.TrxcMessage: { cmd := { verb := "FAKE_RSSI", params := { "-60", "0" } } }
16:57:45.448798 TRXC_CodecPort.ttcn:42 enc_TrxcMessage(): Stream after encoding: "CMD FAKE_RSSI -60 0"
16:57:45.448809 TRXC_CodecPort.ttcn:77 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : { connId := 1, proto := { udp := { } }, msg := '434D442046414B455F52535349202D36302030'O ("CMD FAKE_RSSI -60 0") }
16:57:45.448830 TRXC_CodecPort.ttcn:78 Start timer T: 3 s
16:57:45.448914 TRXC_CodecPort.ttcn:79 Message enqueued on BTS_TRXC from system @IPL4asp_Types.ASP_RecvFrom : { connId := 1, remName := "172.18.92.21", remPort := 5701, locName := "0.0.0.0", locPort := 9999, proto := { udp := { } }, userData := 0, msg := '5253502046414B455F525353492030202D3630203000'O } id 2
16:57:45.448941 TRXC_CodecPort.ttcn:36 dec_TrxcMessage(): Stream before decoding: "RSP FAKE_RSSI 0 -60 0" & char(0, 0, 0, 0)
16:57:45.448955 TRXC_CodecPort.ttcn:36 match_begin data: RSP FAKE_RSSI 0 -60 0
16:57:45.448963 TRXC_CodecPort.ttcn:36 match_begin token: "CMD "
16:57:45.448971 TRXC_CodecPort.ttcn:36 match_begin result: -1
16:57:45.448979 TRXC_CodecPort.ttcn:36 match_begin data: RSP FAKE_RSSI 0 -60 0
16:57:45.448986 TRXC_CodecPort.ttcn:36 match_begin token: "RSP "
16:57:45.448992 TRXC_CodecPort.ttcn:36 match_begin result: 4
16:57:45.449008 TRXC_CodecPort.ttcn:36 match_begin data: FAKE_RSSI 0 -60 0
16:57:45.449014 TRXC_CodecPort.ttcn:36 match_begin token: "^(((POWERON)|(POWEROFF)|(CLOCK)|(RXTUNE)|(TXTUNE)|(SETSLOT)|(SETTSC)|(SETBSIC)|(SETPOWER)|(SETMAXDLY)|(SETMAXDLYNB)|(HANDOVER)|(NOHANDOVER)|(MEASURE)|(FAKE_RSSI)|(FAKE_TOA)|(FAKE_CI)|(FAKE_TRXC_DELAY)))"
16:57:45.449046 TRXC_CodecPort.ttcn:36 match_begin regexec result: 0, Success
16:57:45.449053 TRXC_CodecPort.ttcn:36 match_begin result: 9
16:57:45.449061 TRXC_CodecPort.ttcn:36 match_begin data:  0 -60 0
16:57:45.449068 TRXC_CodecPort.ttcn:36 match_begin token: " "
16:57:45.449075 TRXC_CodecPort.ttcn:36 match_begin result: 1
16:57:45.449082 TRXC_CodecPort.ttcn:36 match_first data: 0 -60 0
16:57:45.449089 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.449095 TRXC_CodecPort.ttcn:36 match_first result: 1
16:57:45.449101 TRXC_CodecPort.ttcn:36 match_list data: 0 -60 0
16:57:45.449107 TRXC_CodecPort.ttcn:36 match_list result: 1
16:57:45.449116 TRXC_CodecPort.ttcn:36 match_begin data:  -60 0
16:57:45.449122 TRXC_CodecPort.ttcn:36 match_begin token: " "
16:57:45.449129 TRXC_CodecPort.ttcn:36 match_begin result: 1
16:57:45.449136 TRXC_CodecPort.ttcn:36 match_first data: -60 0
16:57:45.449143 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.449149 TRXC_CodecPort.ttcn:36 match_first result: 3
16:57:45.449155 TRXC_CodecPort.ttcn:36 match_first data: -60 0
16:57:45.449162 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.449168 TRXC_CodecPort.ttcn:36 match_first result: 3
16:57:45.449174 TRXC_CodecPort.ttcn:36 match_list data: -60 0
16:57:45.449180 TRXC_CodecPort.ttcn:36 match_list result: 3
16:57:45.449187 TRXC_CodecPort.ttcn:36 match_begin data:  0
16:57:45.449193 TRXC_CodecPort.ttcn:36 match_begin token: " "
16:57:45.449199 TRXC_CodecPort.ttcn:36 match_begin result: 1
16:57:45.449206 TRXC_CodecPort.ttcn:36 match_first data: 0
16:57:45.449212 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.449218 TRXC_CodecPort.ttcn:36 match_first result: -1
16:57:45.449225 TRXC_CodecPort.ttcn:36 match_first data: 0
16:57:45.449231 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.449237 TRXC_CodecPort.ttcn:36 match_first result: -1
16:57:45.449243 TRXC_CodecPort.ttcn:36 match_list data: 0
16:57:45.449249 TRXC_CodecPort.ttcn:36 match_list result: -1
16:57:45.449255 TRXC_CodecPort.ttcn:36 match_begin data: 
16:57:45.449261 TRXC_CodecPort.ttcn:36 match_begin token: " "
16:57:45.449268 TRXC_CodecPort.ttcn:36 match_begin result: -1
16:57:45.449275 TRXC_CodecPort.ttcn:36 dec_TrxcMessage(): Decoded @TRXC_Types.TrxcMessage: { rsp := { verb := "FAKE_RSSI", status := 0, params := { "-60", "0" } } }
16:57:45.449286 TRXC_CodecPort.ttcn:36 Warning: dec_TrxcMessage(): Data remained at the end of the stream after successful decoding: '00'O
16:57:45.449303 TRXC_CodecPort.ttcn:79 Incoming message was mapped to @TRXC_CodecPort.TRXC_RecvFrom : { connId := 1, remName := "172.18.92.21", remPort := 5701, locName := "0.0.0.0", locPort := 9999, msg := { rsp := { verb := "FAKE_RSSI", status := 0, params := { "-60", "0" } } } } id 2
16:57:45.449321 TRXC_CodecPort.ttcn:80 Matching on port BTS_TRXC succeeded:  matched
16:57:45.449333 TRXC_CodecPort.ttcn:80 Receive operation on port BTS_TRXC succeeded, message from system(): @TRXC_CodecPort.TRXC_RecvFrom : { connId := 1, remName := "172.18.92.21", remPort := 5701, locName := "0.0.0.0", locPort := 9999, msg := { rsp := { verb := "FAKE_RSSI", status := 0, params := { "-60", "0" } } } } id 2
16:57:45.449343 TRXC_CodecPort.ttcn:80 Message with id 2 was extracted from the queue of BTS_TRXC.
16:57:45.449363 TRXC_CodecPort.ttcn:77 Sent on BTS_TRXC to system @TRXC_CodecPort.TRXC_Send : { connId := 1, msg := { cmd := { verb := "FAKE_CI", params := { "60", "0" } } } }
16:57:45.449372 TRXC_CodecPort.ttcn:42 enc_TrxcMessage(): Encoding @TRXC_Types.TrxcMessage: { cmd := { verb := "FAKE_CI", params := { "60", "0" } } }
16:57:45.449382 TRXC_CodecPort.ttcn:42 enc_TrxcMessage(): Stream after encoding: "CMD FAKE_CI 60 0"
16:57:45.449393 TRXC_CodecPort.ttcn:77 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : { connId := 1, proto := { udp := { } }, msg := '434D442046414B455F43492036302030'O ("CMD FAKE_CI 60 0") }
16:57:45.449668 TRXC_CodecPort.ttcn:78 Start timer T: 3 s
16:57:45.449692 TRXC_CodecPort.ttcn:79 Message enqueued on BTS_TRXC from system @IPL4asp_Types.ASP_RecvFrom : { connId := 1, remName := "172.18.92.21", remPort := 5701, locName := "0.0.0.0", locPort := 9999, proto := { udp := { } }, userData := 0, msg := '5253502046414B455F43492030203630203000'O } id 3
16:57:45.449733 TRXC_CodecPort.ttcn:36 dec_TrxcMessage(): Stream before decoding: "RSP FAKE_CI 0 60 0" & char(0, 0, 0, 0)
16:57:45.449744 TRXC_CodecPort.ttcn:36 match_begin data: RSP FAKE_CI 0 60 0
16:57:45.449751 TRXC_CodecPort.ttcn:36 match_begin token: "CMD "
16:57:45.449758 TRXC_CodecPort.ttcn:36 match_begin result: -1
16:57:45.449765 TRXC_CodecPort.ttcn:36 match_begin data: RSP FAKE_CI 0 60 0
16:57:45.449772 TRXC_CodecPort.ttcn:36 match_begin token: "RSP "
16:57:45.449778 TRXC_CodecPort.ttcn:36 match_begin result: 4
16:57:45.449791 TRXC_CodecPort.ttcn:36 match_begin data: FAKE_CI 0 60 0
16:57:45.449937 TRXC_CodecPort.ttcn:36 match_begin token: "^(((POWERON)|(POWEROFF)|(CLOCK)|(RXTUNE)|(TXTUNE)|(SETSLOT)|(SETTSC)|(SETBSIC)|(SETPOWER)|(SETMAXDLY)|(SETMAXDLYNB)|(HANDOVER)|(NOHANDOVER)|(MEASURE)|(FAKE_RSSI)|(FAKE_TOA)|(FAKE_CI)|(FAKE_TRXC_DELAY)))"
16:57:45.449959 TRXC_CodecPort.ttcn:36 match_begin regexec result: 0, Success
16:57:45.449966 TRXC_CodecPort.ttcn:36 match_begin result: 7
16:57:45.449973 TRXC_CodecPort.ttcn:36 match_begin data:  0 60 0
16:57:45.449980 TRXC_CodecPort.ttcn:36 match_begin token: " "
16:57:45.449987 TRXC_CodecPort.ttcn:36 match_begin result: 1
16:57:45.449993 TRXC_CodecPort.ttcn:36 match_first data: 0 60 0
16:57:45.450000 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.450006 TRXC_CodecPort.ttcn:36 match_first result: 1
16:57:45.450012 TRXC_CodecPort.ttcn:36 match_list data: 0 60 0
16:57:45.450018 TRXC_CodecPort.ttcn:36 match_list result: 1
16:57:45.450026 TRXC_CodecPort.ttcn:36 match_begin data:  60 0
16:57:45.450032 TRXC_CodecPort.ttcn:36 match_begin token: " "
16:57:45.450038 TRXC_CodecPort.ttcn:36 match_begin result: 1
16:57:45.450047 TRXC_CodecPort.ttcn:36 match_first data: 60 0
16:57:45.450052 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.450058 TRXC_CodecPort.ttcn:36 match_first result: 2
16:57:45.450064 TRXC_CodecPort.ttcn:36 match_first data: 60 0
16:57:45.450070 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.450075 TRXC_CodecPort.ttcn:36 match_first result: 2
16:57:45.450081 TRXC_CodecPort.ttcn:36 match_list data: 60 0
16:57:45.450086 TRXC_CodecPort.ttcn:36 match_list result: 2
16:57:45.450092 TRXC_CodecPort.ttcn:36 match_begin data:  0
16:57:45.450098 TRXC_CodecPort.ttcn:36 match_begin token: " "
16:57:45.450104 TRXC_CodecPort.ttcn:36 match_begin result: 1
16:57:45.450109 TRXC_CodecPort.ttcn:36 match_first data: 0
16:57:45.450115 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.450120 TRXC_CodecPort.ttcn:36 match_first result: -1
16:57:45.450126 TRXC_CodecPort.ttcn:36 match_first data: 0
16:57:45.450131 TRXC_CodecPort.ttcn:36 match_first token: " "
16:57:45.450137 TRXC_CodecPort.ttcn:36 match_first result: -1
16:57:45.450143 TRXC_CodecPort.ttcn:36 match_list data: 0
16:57:45.450148 TRXC_CodecPort.ttcn:36 match_list result: -1
16:57:45.450154 TRXC_CodecPort.ttcn:36 match_begin data: 
16:57:45.450159 TRXC_CodecPort.ttcn:36 match_begin token: " "
16:57:45.450165 TRXC_CodecPort.ttcn:36 match_begin result: -1
16:57:45.450171 TRXC_CodecPort.ttcn:36 dec_TrxcMessage(): Decoded @TRXC_Types.TrxcMessage: { rsp := { verb := "FAKE_CI", status := 0, params := { "60", "0" } } }
16:57:45.450180 TRXC_CodecPort.ttcn:36 Warning: dec_TrxcMessage(): Data remained at the end of the stream after successful decoding: '00'O
16:57:45.450193 TRXC_CodecPort.ttcn:79 Incoming message was mapped to @TRXC_CodecPort.TRXC_RecvFrom : { connId := 1, remName := "172.18.92.21", remPort := 5701, locName := "0.0.0.0", locPort := 9999, msg := { rsp := { verb := "FAKE_CI", status := 0, params := { "60", "0" } } } } id 3
16:57:45.450204 TRXC_CodecPort.ttcn:80 Matching on port BTS_TRXC succeeded:  matched
16:57:45.450213 TRXC_CodecPort.ttcn:80 Receive operation on port BTS_TRXC succeeded, message from system(): @TRXC_CodecPort.TRXC_RecvFrom : { connId := 1, remName := "172.18.92.21", remPort := 5701, locName := "0.0.0.0", locPort := 9999, msg := { rsp := { verb := "FAKE_CI", status := 0, params := { "60", "0" } } } } id 3
16:57:45.450223 TRXC_CodecPort.ttcn:80 Message with id 3 was extracted from the queue of BTS_TRXC.
16:57:45.450233 Osmocom_Types.ttcn:126 Start timer T: 0 s
16:57:45.450240 Osmocom_Types.ttcn:127 Timeout T: 0 s
16:57:45.450256 Osmocom_VTY_Functions.ttcn:105 Sent on BTSVTY to system charstring : "configure terminal"
16:57:45.450323 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
16:57:45.450369 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "OsmoBTS(config)# " id 4
16:57:45.450402 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "OsmoBTS(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:57:45.450425 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY "OsmoBTS(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
16:57:45.450451 Osmocom_VTY_Functions.ttcn:74 Matching on port BTSVTY succeeded: "OsmoBTS(config)# " with pattern "[\w-]+\(*\)\# " matched
16:57:45.450460 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BTSVTY succeeded, message from system(): charstring : "OsmoBTS(config)# " id 4
16:57:45.450469 Osmocom_VTY_Functions.ttcn:74 Message with id 4 was extracted from the queue of BTSVTY.
16:57:45.450478 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
16:57:45.450487 Osmocom_VTY_Functions.ttcn:105 Sent on BTSVTY to system charstring : "phy 0"
16:57:45.450529 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
16:57:45.450548 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "OsmoBTS(phy)# " id 5
16:57:45.450567 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "OsmoBTS(phy)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:57:45.450583 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY "OsmoBTS(phy)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
16:57:45.450605 Osmocom_VTY_Functions.ttcn:74 Matching on port BTSVTY succeeded: "OsmoBTS(phy)# " with pattern "[\w-]+\(*\)\# " matched
16:57:45.450614 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BTSVTY succeeded, message from system(): charstring : "OsmoBTS(phy)# " id 5
16:57:45.450622 Osmocom_VTY_Functions.ttcn:74 Message with id 5 was extracted from the queue of BTSVTY.
16:57:45.450630 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
16:57:45.450638 Osmocom_VTY_Functions.ttcn:105 Sent on BTSVTY to system charstring : "osmotrx ms-power-loop -10"
16:57:45.450674 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
16:57:45.450708 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "'osmotrx ms-power-loop <-127-127>' is deprecated, MS Power Control is now managed by BSC" id 6
16:57:45.450716 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "OsmoBTS(phy)# " id 7
16:57:45.450732 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "'osmotrx ms-power-loop <-127-127>' is deprecated, MS Power Control is now managed by BSC" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:57:45.450747 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY "'osmotrx ms-power-loop <-127-127>' is deprecated, MS Power Control is now managed by BSC" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
16:57:45.450762 Osmocom_VTY_Functions.ttcn:74 Matching on port BTSVTY "'osmotrx ms-power-loop <-127-127>' is deprecated, MS Power Control is now managed by BSC" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
16:57:45.450773 Osmocom_VTY_Functions.ttcn:75 Matching on port BTSVTY "'osmotrx ms-power-loop <-127-127>' is deprecated, MS Power Control is now managed by BSC" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
16:57:45.450785 Osmocom_VTY_Functions.ttcn:85 Matching on port BTSVTY succeeded: "'osmotrx ms-power-loop <-127-127>' is deprecated, MS Power Control is now managed by BSC" with ? matched
16:57:45.450794 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BTSVTY succeeded, message from system(): charstring : "'osmotrx ms-power-loop <-127-127>' is deprecated, MS Power Control is now managed by BSC" id 6
16:57:45.450801 Osmocom_VTY_Functions.ttcn:85 Message with id 6 was extracted from the queue of BTSVTY.
16:57:45.450814 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "OsmoBTS(phy)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:57:45.450828 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY "OsmoBTS(phy)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
16:57:45.450846 Osmocom_VTY_Functions.ttcn:74 Matching on port BTSVTY succeeded: "OsmoBTS(phy)# " with pattern "[\w-]+\(*\)\# " matched
16:57:45.450854 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BTSVTY succeeded, message from system(): charstring : "OsmoBTS(phy)# " id 7
16:57:45.450861 Osmocom_VTY_Functions.ttcn:74 Message with id 7 was extracted from the queue of BTSVTY.
16:57:45.450868 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
16:57:45.450875 Osmocom_VTY_Functions.ttcn:105 Sent on BTSVTY to system charstring : "end"
16:57:45.450902 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
16:57:45.450912 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "OsmoBTS# " id 8
16:57:45.450926 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "OsmoBTS# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:57:45.450941 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY succeeded: "OsmoBTS# " with pattern "[\w-]+\# " matched
16:57:45.450949 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BTSVTY succeeded, message from system(): charstring : "OsmoBTS# " id 8
16:57:45.450955 Osmocom_VTY_Functions.ttcn:73 Message with id 8 was extracted from the queue of BTSVTY.
16:57:45.450962 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
16:57:45.451028 Osmocom_VTY_Functions.ttcn:105 Sent on BTSVTY to system charstring : "show bts 0"
16:57:45.451096 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
16:57:45.451228 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "BTS 0 is of type 'osmo-bts-trx', in band DCS1800, has CI 23 LAC 42, BSIC 63 and 4 TRX\n  Description: (null)\n  Unit ID: 1234/0/0, OML Stream ID 0xff\n  NM State: Oper 'Enabled', Admin 'Unlocked', Avail 'OK'\n  Site Mgr NM State: Oper 'Enabled', Admin 'Locked', Avail 'OK'\n  Paging: Queue size 200, occupied 0, lifetime 0s\n  AGCH: Queue limit 12, occupied 0, dropped 0, merged 0, rejected 0, ag-res 13, non-res 7\n  CBCH queue target: 2, hysteresis: 15, maximum: 2\n  CBCH backlog queue length (BASIC): 0\n  CBCH backlog queue length (EXTENDED): 0\n  Paging: queue length 0, buffer space 200\n  OML Link state: connected.\n  PH-RTS.ind FN advance average: 5, min: 5, max: 5\n  Radio Link Timeout (OML): 32 SACCH blocks\n  TRX 0\n    phy 0 \n  TRX 1\n    phy 1 \n  TRX 2\n    phy 2 \n  TRX 3\n    phy 3 \n  Features:\n    001 GPRS                                    \n    002 EGPRS                                   \n    004 Frequency Hopping                       \n    005 Multi-TSC                               \n    006 OML Alerts                              \n    008 CBCH                                    \n    009 Fullrate speech V1                      \n    010 Halfrate speech V1                      \n    011 Fullrate speech EFR                     \n    012 Fullrate speech AMR                     \n    013 Halfrate speech AMR                     \n    014 ETWS Primary Notification via PCH       \n    015 BSS Paging Coordination                 \n    016 NSVC IPv6                               \n    017 FACCH/SACCH Repetition                  \n    018 Cell Change Notification (CCN)          \n    019 VAMOS (Voice services over Adaptive Multi-user channels on One Slot)\n    020 OsmoPCU over OML link IPA multiplex     \n    021 BCCH carrier power reduction mode       \n    022 Dynamic Timeslot configuration as SDCCH8\n    023 FACCH/SACCH Temporary overpower         \n    024 Osmux (Osmocom RTP multiplexing)        \n    025 Voice Broadcast Service                 \n    026 Voice Group Call Service                \n    027 TW-TS-001 RTP format                    \n    028 TW-TS-002 RTP format                    \n  BTS model specific (internal) flags:\n    001 Measurement and Payload data combined   \n    003 Uplink interference measurements        \n  base transceiver station:\n   Received paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Sent paging requests (Um):        0 (0/s 0/m 0/h 0/d)\n   Paging congestion detected (Abis):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Um):     4028 (0/s 0/m 0/h 0/d)\n   Dropped RACH requests (Um):        3 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Handover):       45 (0/s 0/m 0/h 0/d)\n   Received RACH requests (VGCS):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (CS/Abis):     4025 (0/s 0/m 0/h 0/d)\n   Received RACH requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Received AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH DELETE IND (Abis):        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of received RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during preening:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during loopback:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during DL queue overflow:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during V.110 decode:        0 (0/s 0/m 0/h 0/d)\n   Total number of transmitted RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of transmitted RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)" id 9
16:57:45.451246 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "OsmoBTS# " id 10
16:57:45.451366 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "BTS 0 is of type 'osmo-bts-trx', in band DCS1800, has CI 23 LAC 42, BSIC 63 and 4 TRX\n  Description: (null)\n  Unit ID: 1234/0/0, OML Stream ID 0xff\n  NM State: Oper 'Enabled', Admin 'Unlocked', Avail 'OK'\n  Site Mgr NM State: Oper 'Enabled', Admin 'Locked', Avail 'OK'\n  Paging: Queue size 200, occupied 0, lifetime 0s\n  AGCH: Queue limit 12, occupied 0, dropped 0, merged 0, rejected 0, ag-res 13, non-res 7\n  CBCH queue target: 2, hysteresis: 15, maximum: 2\n  CBCH backlog queue length (BASIC): 0\n  CBCH backlog queue length (EXTENDED): 0\n  Paging: queue length 0, buffer space 200\n  OML Link state: connected.\n  PH-RTS.ind FN advance average: 5, min: 5, max: 5\n  Radio Link Timeout (OML): 32 SACCH blocks\n  TRX 0\n    phy 0 \n  TRX 1\n    phy 1 \n  TRX 2\n    phy 2 \n  TRX 3\n    phy 3 \n  Features:\n    001 GPRS                                    \n    002 EGPRS                                   \n    004 Frequency Hopping                       \n    005 Multi-TSC                               \n    006 OML Alerts                              \n    008 CBCH                                    \n    009 Fullrate speech V1                      \n    010 Halfrate speech V1                      \n    011 Fullrate speech EFR                     \n    012 Fullrate speech AMR                     \n    013 Halfrate speech AMR                     \n    014 ETWS Primary Notification via PCH       \n    015 BSS Paging Coordination                 \n    016 NSVC IPv6                               \n    017 FACCH/SACCH Repetition                  \n    018 Cell Change Notification (CCN)          \n    019 VAMOS (Voice services over Adaptive Multi-user channels on One Slot)\n    020 OsmoPCU over OML link IPA multiplex     \n    021 BCCH carrier power reduction mode       \n    022 Dynamic Timeslot configuration as SDCCH8\n    023 FACCH/SACCH Temporary overpower         \n    024 Osmux (Osmocom RTP multiplexing)        \n    025 Voice Broadcast Service                 \n    026 Voice Group Call Service                \n    027 TW-TS-001 RTP format                    \n    028 TW-TS-002 RTP format                    \n  BTS model specific (internal) flags:\n    001 Measurement and Payload data combined   \n    003 Uplink interference measurements        \n  base transceiver station:\n   Received paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Sent paging requests (Um):        0 (0/s 0/m 0/h 0/d)\n   Paging congestion detected (Abis):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Um):     4028 (0/s 0/m 0/h 0/d)\n   Dropped RACH requests (Um):        3 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Handover):       45 (0/s 0/m 0/h 0/d)\n   Received RACH requests (VGCS):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (CS/Abis):     4025 (0/s 0/m 0/h 0/d)\n   Received RACH requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Received AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH DELETE IND (Abis):        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of received RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during preening:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during loopback:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during DL queue overflow:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during V.110 decode:        0 (0/s 0/m 0/h 0/d)\n   Total number of transmitted RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of transmitted RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:57:45.451484 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY "BTS 0 is of type 'osmo-bts-trx', in band DCS1800, has CI 23 LAC 42, BSIC 63 and 4 TRX\n  Description: (null)\n  Unit ID: 1234/0/0, OML Stream ID 0xff\n  NM State: Oper 'Enabled', Admin 'Unlocked', Avail 'OK'\n  Site Mgr NM State: Oper 'Enabled', Admin 'Locked', Avail 'OK'\n  Paging: Queue size 200, occupied 0, lifetime 0s\n  AGCH: Queue limit 12, occupied 0, dropped 0, merged 0, rejected 0, ag-res 13, non-res 7\n  CBCH queue target: 2, hysteresis: 15, maximum: 2\n  CBCH backlog queue length (BASIC): 0\n  CBCH backlog queue length (EXTENDED): 0\n  Paging: queue length 0, buffer space 200\n  OML Link state: connected.\n  PH-RTS.ind FN advance average: 5, min: 5, max: 5\n  Radio Link Timeout (OML): 32 SACCH blocks\n  TRX 0\n    phy 0 \n  TRX 1\n    phy 1 \n  TRX 2\n    phy 2 \n  TRX 3\n    phy 3 \n  Features:\n    001 GPRS                                    \n    002 EGPRS                                   \n    004 Frequency Hopping                       \n    005 Multi-TSC                               \n    006 OML Alerts                              \n    008 CBCH                                    \n    009 Fullrate speech V1                      \n    010 Halfrate speech V1                      \n    011 Fullrate speech EFR                     \n    012 Fullrate speech AMR                     \n    013 Halfrate speech AMR                     \n    014 ETWS Primary Notification via PCH       \n    015 BSS Paging Coordination                 \n    016 NSVC IPv6                               \n    017 FACCH/SACCH Repetition                  \n    018 Cell Change Notification (CCN)          \n    019 VAMOS (Voice services over Adaptive Multi-user channels on One Slot)\n    020 OsmoPCU over OML link IPA multiplex     \n    021 BCCH carrier power reduction mode       \n    022 Dynamic Timeslot configuration as SDCCH8\n    023 FACCH/SACCH Temporary overpower         \n    024 Osmux (Osmocom RTP multiplexing)        \n    025 Voice Broadcast Service                 \n    026 Voice Group Call Service                \n    027 TW-TS-001 RTP format                    \n    028 TW-TS-002 RTP format                    \n  BTS model specific (internal) flags:\n    001 Measurement and Payload data combined   \n    003 Uplink interference measurements        \n  base transceiver station:\n   Received paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Sent paging requests (Um):        0 (0/s 0/m 0/h 0/d)\n   Paging congestion detected (Abis):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Um):     4028 (0/s 0/m 0/h 0/d)\n   Dropped RACH requests (Um):        3 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Handover):       45 (0/s 0/m 0/h 0/d)\n   Received RACH requests (VGCS):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (CS/Abis):     4025 (0/s 0/m 0/h 0/d)\n   Received RACH requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Received AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH DELETE IND (Abis):        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of received RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during preening:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during loopback:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during DL queue overflow:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during V.110 decode:        0 (0/s 0/m 0/h 0/d)\n   Total number of transmitted RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of transmitted RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
16:57:45.451601 Osmocom_VTY_Functions.ttcn:74 Matching on port BTSVTY "BTS 0 is of type 'osmo-bts-trx', in band DCS1800, has CI 23 LAC 42, BSIC 63 and 4 TRX\n  Description: (null)\n  Unit ID: 1234/0/0, OML Stream ID 0xff\n  NM State: Oper 'Enabled', Admin 'Unlocked', Avail 'OK'\n  Site Mgr NM State: Oper 'Enabled', Admin 'Locked', Avail 'OK'\n  Paging: Queue size 200, occupied 0, lifetime 0s\n  AGCH: Queue limit 12, occupied 0, dropped 0, merged 0, rejected 0, ag-res 13, non-res 7\n  CBCH queue target: 2, hysteresis: 15, maximum: 2\n  CBCH backlog queue length (BASIC): 0\n  CBCH backlog queue length (EXTENDED): 0\n  Paging: queue length 0, buffer space 200\n  OML Link state: connected.\n  PH-RTS.ind FN advance average: 5, min: 5, max: 5\n  Radio Link Timeout (OML): 32 SACCH blocks\n  TRX 0\n    phy 0 \n  TRX 1\n    phy 1 \n  TRX 2\n    phy 2 \n  TRX 3\n    phy 3 \n  Features:\n    001 GPRS                                    \n    002 EGPRS                                   \n    004 Frequency Hopping                       \n    005 Multi-TSC                               \n    006 OML Alerts                              \n    008 CBCH                                    \n    009 Fullrate speech V1                      \n    010 Halfrate speech V1                      \n    011 Fullrate speech EFR                     \n    012 Fullrate speech AMR                     \n    013 Halfrate speech AMR                     \n    014 ETWS Primary Notification via PCH       \n    015 BSS Paging Coordination                 \n    016 NSVC IPv6                               \n    017 FACCH/SACCH Repetition                  \n    018 Cell Change Notification (CCN)          \n    019 VAMOS (Voice services over Adaptive Multi-user channels on One Slot)\n    020 OsmoPCU over OML link IPA multiplex     \n    021 BCCH carrier power reduction mode       \n    022 Dynamic Timeslot configuration as SDCCH8\n    023 FACCH/SACCH Temporary overpower         \n    024 Osmux (Osmocom RTP multiplexing)        \n    025 Voice Broadcast Service                 \n    026 Voice Group Call Service                \n    027 TW-TS-001 RTP format                    \n    028 TW-TS-002 RTP format                    \n  BTS model specific (internal) flags:\n    001 Measurement and Payload data combined   \n    003 Uplink interference measurements        \n  base transceiver station:\n   Received paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Sent paging requests (Um):        0 (0/s 0/m 0/h 0/d)\n   Paging congestion detected (Abis):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Um):     4028 (0/s 0/m 0/h 0/d)\n   Dropped RACH requests (Um):        3 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Handover):       45 (0/s 0/m 0/h 0/d)\n   Received RACH requests (VGCS):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (CS/Abis):     4025 (0/s 0/m 0/h 0/d)\n   Received RACH requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Received AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH DELETE IND (Abis):        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of received RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during preening:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during loopback:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during DL queue overflow:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during V.110 decode:        0 (0/s 0/m 0/h 0/d)\n   Total number of transmitted RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of transmitted RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
16:57:45.451737 Osmocom_VTY_Functions.ttcn:75 Matching on port BTSVTY "BTS 0 is of type 'osmo-bts-trx', in band DCS1800, has CI 23 LAC 42, BSIC 63 and 4 TRX\n  Description: (null)\n  Unit ID: 1234/0/0, OML Stream ID 0xff\n  NM State: Oper 'Enabled', Admin 'Unlocked', Avail 'OK'\n  Site Mgr NM State: Oper 'Enabled', Admin 'Locked', Avail 'OK'\n  Paging: Queue size 200, occupied 0, lifetime 0s\n  AGCH: Queue limit 12, occupied 0, dropped 0, merged 0, rejected 0, ag-res 13, non-res 7\n  CBCH queue target: 2, hysteresis: 15, maximum: 2\n  CBCH backlog queue length (BASIC): 0\n  CBCH backlog queue length (EXTENDED): 0\n  Paging: queue length 0, buffer space 200\n  OML Link state: connected.\n  PH-RTS.ind FN advance average: 5, min: 5, max: 5\n  Radio Link Timeout (OML): 32 SACCH blocks\n  TRX 0\n    phy 0 \n  TRX 1\n    phy 1 \n  TRX 2\n    phy 2 \n  TRX 3\n    phy 3 \n  Features:\n    001 GPRS                                    \n    002 EGPRS                                   \n    004 Frequency Hopping                       \n    005 Multi-TSC                               \n    006 OML Alerts                              \n    008 CBCH                                    \n    009 Fullrate speech V1                      \n    010 Halfrate speech V1                      \n    011 Fullrate speech EFR                     \n    012 Fullrate speech AMR                     \n    013 Halfrate speech AMR                     \n    014 ETWS Primary Notification via PCH       \n    015 BSS Paging Coordination                 \n    016 NSVC IPv6                               \n    017 FACCH/SACCH Repetition                  \n    018 Cell Change Notification (CCN)          \n    019 VAMOS (Voice services over Adaptive Multi-user channels on One Slot)\n    020 OsmoPCU over OML link IPA multiplex     \n    021 BCCH carrier power reduction mode       \n    022 Dynamic Timeslot configuration as SDCCH8\n    023 FACCH/SACCH Temporary overpower         \n    024 Osmux (Osmocom RTP multiplexing)        \n    025 Voice Broadcast Service                 \n    026 Voice Group Call Service                \n    027 TW-TS-001 RTP format                    \n    028 TW-TS-002 RTP format                    \n  BTS model specific (internal) flags:\n    001 Measurement and Payload data combined   \n    003 Uplink interference measurements        \n  base transceiver station:\n   Received paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Sent paging requests (Um):        0 (0/s 0/m 0/h 0/d)\n   Paging congestion detected (Abis):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Um):     4028 (0/s 0/m 0/h 0/d)\n   Dropped RACH requests (Um):        3 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Handover):       45 (0/s 0/m 0/h 0/d)\n   Received RACH requests (VGCS):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (CS/Abis):     4025 (0/s 0/m 0/h 0/d)\n   Received RACH requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Received AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH DELETE IND (Abis):        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of received RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during preening:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during loopback:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during DL queue overflow:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during V.110 decode:        0 (0/s 0/m 0/h 0/d)\n   Total number of transmitted RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of transmitted RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
16:57:45.451846 Osmocom_VTY_Functions.ttcn:85 Matching on port BTSVTY succeeded: "BTS 0 is of type 'osmo-bts-trx', in band DCS1800, has CI 23 LAC 42, BSIC 63 and 4 TRX\n  Description: (null)\n  Unit ID: 1234/0/0, OML Stream ID 0xff\n  NM State: Oper 'Enabled', Admin 'Unlocked', Avail 'OK'\n  Site Mgr NM State: Oper 'Enabled', Admin 'Locked', Avail 'OK'\n  Paging: Queue size 200, occupied 0, lifetime 0s\n  AGCH: Queue limit 12, occupied 0, dropped 0, merged 0, rejected 0, ag-res 13, non-res 7\n  CBCH queue target: 2, hysteresis: 15, maximum: 2\n  CBCH backlog queue length (BASIC): 0\n  CBCH backlog queue length (EXTENDED): 0\n  Paging: queue length 0, buffer space 200\n  OML Link state: connected.\n  PH-RTS.ind FN advance average: 5, min: 5, max: 5\n  Radio Link Timeout (OML): 32 SACCH blocks\n  TRX 0\n    phy 0 \n  TRX 1\n    phy 1 \n  TRX 2\n    phy 2 \n  TRX 3\n    phy 3 \n  Features:\n    001 GPRS                                    \n    002 EGPRS                                   \n    004 Frequency Hopping                       \n    005 Multi-TSC                               \n    006 OML Alerts                              \n    008 CBCH                                    \n    009 Fullrate speech V1                      \n    010 Halfrate speech V1                      \n    011 Fullrate speech EFR                     \n    012 Fullrate speech AMR                     \n    013 Halfrate speech AMR                     \n    014 ETWS Primary Notification via PCH       \n    015 BSS Paging Coordination                 \n    016 NSVC IPv6                               \n    017 FACCH/SACCH Repetition                  \n    018 Cell Change Notification (CCN)          \n    019 VAMOS (Voice services over Adaptive Multi-user channels on One Slot)\n    020 OsmoPCU over OML link IPA multiplex     \n    021 BCCH carrier power reduction mode       \n    022 Dynamic Timeslot configuration as SDCCH8\n    023 FACCH/SACCH Temporary overpower         \n    024 Osmux (Osmocom RTP multiplexing)        \n    025 Voice Broadcast Service                 \n    026 Voice Group Call Service                \n    027 TW-TS-001 RTP format                    \n    028 TW-TS-002 RTP format                    \n  BTS model specific (internal) flags:\n    001 Measurement and Payload data combined   \n    003 Uplink interference measurements        \n  base transceiver station:\n   Received paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Sent paging requests (Um):        0 (0/s 0/m 0/h 0/d)\n   Paging congestion detected (Abis):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Um):     4028 (0/s 0/m 0/h 0/d)\n   Dropped RACH requests (Um):        3 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Handover):       45 (0/s 0/m 0/h 0/d)\n   Received RACH requests (VGCS):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (CS/Abis):     4025 (0/s 0/m 0/h 0/d)\n   Received RACH requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Received AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH DELETE IND (Abis):        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of received RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during preening:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during loopback:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during DL queue overflow:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during V.110 decode:        0 (0/s 0/m 0/h 0/d)\n   Total number of transmitted RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of transmitted RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)" with ? matched
16:57:45.451949 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BTSVTY succeeded, message from system(): charstring : "BTS 0 is of type 'osmo-bts-trx', in band DCS1800, has CI 23 LAC 42, BSIC 63 and 4 TRX\n  Description: (null)\n  Unit ID: 1234/0/0, OML Stream ID 0xff\n  NM State: Oper 'Enabled', Admin 'Unlocked', Avail 'OK'\n  Site Mgr NM State: Oper 'Enabled', Admin 'Locked', Avail 'OK'\n  Paging: Queue size 200, occupied 0, lifetime 0s\n  AGCH: Queue limit 12, occupied 0, dropped 0, merged 0, rejected 0, ag-res 13, non-res 7\n  CBCH queue target: 2, hysteresis: 15, maximum: 2\n  CBCH backlog queue length (BASIC): 0\n  CBCH backlog queue length (EXTENDED): 0\n  Paging: queue length 0, buffer space 200\n  OML Link state: connected.\n  PH-RTS.ind FN advance average: 5, min: 5, max: 5\n  Radio Link Timeout (OML): 32 SACCH blocks\n  TRX 0\n    phy 0 \n  TRX 1\n    phy 1 \n  TRX 2\n    phy 2 \n  TRX 3\n    phy 3 \n  Features:\n    001 GPRS                                    \n    002 EGPRS                                   \n    004 Frequency Hopping                       \n    005 Multi-TSC                               \n    006 OML Alerts                              \n    008 CBCH                                    \n    009 Fullrate speech V1                      \n    010 Halfrate speech V1                      \n    011 Fullrate speech EFR                     \n    012 Fullrate speech AMR                     \n    013 Halfrate speech AMR                     \n    014 ETWS Primary Notification via PCH       \n    015 BSS Paging Coordination                 \n    016 NSVC IPv6                               \n    017 FACCH/SACCH Repetition                  \n    018 Cell Change Notification (CCN)          \n    019 VAMOS (Voice services over Adaptive Multi-user channels on One Slot)\n    020 OsmoPCU over OML link IPA multiplex     \n    021 BCCH carrier power reduction mode       \n    022 Dynamic Timeslot configuration as SDCCH8\n    023 FACCH/SACCH Temporary overpower         \n    024 Osmux (Osmocom RTP multiplexing)        \n    025 Voice Broadcast Service                 \n    026 Voice Group Call Service                \n    027 TW-TS-001 RTP format                    \n    028 TW-TS-002 RTP format                    \n  BTS model specific (internal) flags:\n    001 Measurement and Payload data combined   \n    003 Uplink interference measurements        \n  base transceiver station:\n   Received paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (Abis):        0 (0/s 0/m 0/h 0/d)\n   Dropped paging requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Sent paging requests (Um):        0 (0/s 0/m 0/h 0/d)\n   Paging congestion detected (Abis):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Um):     4028 (0/s 0/m 0/h 0/d)\n   Dropped RACH requests (Um):        3 (0/s 0/m 0/h 0/d)\n   Received RACH requests (Handover):       45 (0/s 0/m 0/h 0/d)\n   Received RACH requests (VGCS):        0 (0/s 0/m 0/h 0/d)\n   Received RACH requests (CS/Abis):     4025 (0/s 0/m 0/h 0/d)\n   Received RACH requests (PS/PCU):        0 (0/s 0/m 0/h 0/d)\n   Received AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH requests (Abis):       20 (0/s 0/m 0/h 0/d)\n   Sent AGCH DELETE IND (Abis):        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of received RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during preening:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during loopback:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during DL queue overflow:        0 (0/s 0/m 0/h 0/d)\n   Total number of received RTP packets dropped during V.110 decode:        0 (0/s 0/m 0/h 0/d)\n   Total number of transmitted RTP packets:        0 (0/s 0/m 0/h 0/d)\n   Number of transmitted RTP packets with marker bit set:        0 (0/s 0/m 0/h 0/d)" id 9
16:57:45.451962 Osmocom_VTY_Functions.ttcn:85 Message with id 9 was extracted from the queue of BTSVTY.
16:57:45.451975 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "OsmoBTS# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:57:45.451987 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY succeeded: "OsmoBTS# " with pattern "[\w-]+\# " matched
16:57:45.451993 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BTSVTY succeeded, message from system(): charstring : "OsmoBTS# " id 10
16:57:45.451999 Osmocom_VTY_Functions.ttcn:73 Message with id 10 was extracted from the queue of BTSVTY.
16:57:45.452005 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
16:57:45.452016 Osmocom_VTY_Functions.ttcn:215 regexp(): POSIX ERE equivalent of pattern "BTS 0 is of*type* in band (\w+),*" is: "^BTS 0 is of.*type.* in band ([0-9A-Za-z]+),.*$"
16:57:45.452360 BTS_Tests.ttcn:698 Creating new PTC with component type BTS_Tests.ConnHdlr, component name: TC_rsl_ms_pwr_dyn_up.
16:57:45.454535 BTS_Tests.ttcn:698 PTC was created. Component reference: 355, alive: no, type: BTS_Tests.ConnHdlr, component name: TC_rsl_ms_pwr_dyn_up.
16:57:45.454559 BTS_Tests.ttcn:700 Connecting ports TC_rsl_ms_pwr_dyn_up(355):RSL and TC_rsl_ms_pwr_dyn_up-RSL(353):CLIENT_PT.
16:57:45.456256 BTS_Tests.ttcn:700 Connect operation on TC_rsl_ms_pwr_dyn_up(355):RSL and TC_rsl_ms_pwr_dyn_up-RSL(353):CLIENT_PT finished.
16:57:45.456265 BTS_Tests.ttcn:701 Connecting ports TC_rsl_ms_pwr_dyn_up(355):RSL_PROC and TC_rsl_ms_pwr_dyn_up-RSL(353):RSL_PROC.
16:57:45.456335 BTS_Tests.ttcn:701 Connect operation on TC_rsl_ms_pwr_dyn_up(355):RSL_PROC and TC_rsl_ms_pwr_dyn_up-RSL(353):RSL_PROC finished.
16:57:45.456341 BTS_Tests.ttcn:711 Unmapping port mtc:BTS_TRXC from system:BTS_TRXC.
16:57:45.456363 BTS_Tests.ttcn:711 Port BTS_TRXC was unmapped from system:BTS_TRXC.
16:57:45.456376 BTS_Tests.ttcn:711 Unmap operation of mtc:BTS_TRXC from system:BTS_TRXC finished.
16:57:45.456381 BTS_Tests.ttcn:712 Mapping port TC_rsl_ms_pwr_dyn_up(355):BTS_TRXC to system:BTS_TRXC.
16:57:45.456448 BTS_Tests.ttcn:712 Map operation of TC_rsl_ms_pwr_dyn_up(355):BTS_TRXC to system:BTS_TRXC finished.
16:57:45.456453 BTS_Tests.ttcn:715 Mapping port TC_rsl_ms_pwr_dyn_up(355):L1CTL to system:L1CTL.
16:57:45.456510 BTS_Tests.ttcn:715 Map operation of TC_rsl_ms_pwr_dyn_up(355):L1CTL to system:L1CTL finished.
16:57:45.456515 BTS_Tests.ttcn:723 Starting function f_handler_init(refers(BTS_Tests.f_TC_rsl_ms_pwr_dyn_up), "TC_rsl_ms_pwr_dyn_up", { trx_nr := 0, chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 1 }, chan_mode := { len := 0, reserved := '000000'B, dtx_d := false, dtx_u := false, spd_ind := RSL_SPDI_SIGN (3), ch_rate_type := RSL_CHRT_SDCCH (1), u := { sign := RSL_CMOD_NO_RESOURCE (0) } }, mr_conf := omit, t_guard := 30.000000, l1_pars := { dtx_enabled := false, toa256_enabled := false, meas_valid := true, meas_ul := { full := { rxlev := 10, rxqual := 0 }, sub := { rxlev := 10, rxqual := 0 } }, timing_offset_256syms := 512, bs_power_level := 0, ms_power_level := 7, ms_actual_ta := 0, facch_enabled := false }, spec := omit, encr := omit, bts0_band := "DCS1800", tsc := 7, fhp := { enabled := false, maio_hsn := { maio := 0, hsn := 0 }, ma_map := { len := 0, ma := ''B }, ma := { } }, loc_osmux_cid := 0, rem_osmux_cid := omit }) on component TC_rsl_ms_pwr_dyn_up(355).
16:57:45.456552 BTS_Tests.ttcn:723 Function was started.
16:57:45.935221 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 9
16:57:46.936054 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 10
16:57:47.835242 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 34, info := { { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 1 } }, tn := 0 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 2 } }, tn := 0 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 3 } }, tn := 0 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 2 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 3 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { lm := { tag := '0001'B, sub_chan := 0 } }, tn := 5 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { lm := { tag := '0001'B, sub_chan := 1 } }, tn := 5 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 0 } }, tn := 6 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 1 } }, tn := 6 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 2 } }, tn := 6 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 3 } }, tn := 6 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 4 } }, tn := 6 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 5 } }, tn := 6 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 6 } }, tn := 6 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 7 } }, tn := 6 }, interf_band := 4, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_OSMO_PDCH (24) }, tn := 7 }, interf_band := 4, rfu := '00000'B } } } } } } } } id 11
16:57:47.835961 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 3, streamId := IPAC_PROTO_RSL_TRX1 (1), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 12
16:57:47.836258 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 4, streamId := IPAC_PROTO_RSL_TRX2 (2), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 13
16:57:47.836556 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 5, streamId := IPAC_PROTO_RSL_TRX3 (3), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 14
16:57:47.937182 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 15
16:57:48.936253 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 16
16:57:49.936987 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 17
16:57:50.728070 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 34, info := { { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 1 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 2 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 3 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 2 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 3 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { lm := { tag := '0001'B, sub_chan := 0 } }, tn := 5 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { lm := { tag := '0001'B, sub_chan := 1 } }, tn := 5 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 0 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 1 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 2 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 3 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 4 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 5 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 6 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 7 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_OSMO_PDCH (24) }, tn := 7 }, interf_band := 2, rfu := '00000'B } } } } } } } } id 18
16:57:50.729963 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 3, streamId := IPAC_PROTO_RSL_TRX1 (1), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 19
16:57:50.730302 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 4, streamId := IPAC_PROTO_RSL_TRX2 (2), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 20
16:57:50.730877 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 5, streamId := IPAC_PROTO_RSL_TRX3 (3), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 21
16:57:50.937760 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 22
16:57:51.938841 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 23
16:57:52.939615 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 24
16:57:53.624840 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 34, info := { { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 1 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 2 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 3 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 2 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 3 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { lm := { tag := '0001'B, sub_chan := 0 } }, tn := 5 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { lm := { tag := '0001'B, sub_chan := 1 } }, tn := 5 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 0 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 1 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 2 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 3 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 4 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 5 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 6 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 7 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_OSMO_PDCH (24) }, tn := 7 }, interf_band := 2, rfu := '00000'B } } } } } } } } id 25
16:57:53.625321 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 3, streamId := IPAC_PROTO_RSL_TRX1 (1), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 26
16:57:53.625723 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 4, streamId := IPAC_PROTO_RSL_TRX2 (2), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 27
16:57:53.626402 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 5, streamId := IPAC_PROTO_RSL_TRX3 (3), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 28
16:57:53.940390 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 29
16:57:54.940229 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 30
16:57:55.940680 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 31
16:57:56.536666 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 34, info := { { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 1 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 2 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 3 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 2 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 3 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { lm := { tag := '0001'B, sub_chan := 0 } }, tn := 5 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { lm := { tag := '0001'B, sub_chan := 1 } }, tn := 5 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 0 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 1 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 2 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 3 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 4 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 5 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 6 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 7 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_OSMO_PDCH (24) }, tn := 7 }, interf_band := 2, rfu := '00000'B } } } } } } } } id 32
16:57:56.537631 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 3, streamId := IPAC_PROTO_RSL_TRX1 (1), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 33
16:57:56.538184 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 4, streamId := IPAC_PROTO_RSL_TRX2 (2), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 34
16:57:56.538479 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 5, streamId := IPAC_PROTO_RSL_TRX3 (3), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 35
16:57:56.942283 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 36
16:57:57.940978 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 37
16:57:58.941545 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 38
16:57:59.455831 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 34, info := { { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 1 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 2 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 3 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 2 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 3 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { lm := { tag := '0001'B, sub_chan := 0 } }, tn := 5 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { lm := { tag := '0001'B, sub_chan := 1 } }, tn := 5 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 0 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 1 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 2 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 3 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 4 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 5 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 6 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 7 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_OSMO_PDCH (24) }, tn := 7 }, interf_band := 2, rfu := '00000'B } } } } } } } } id 39
16:57:59.457031 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 3, streamId := IPAC_PROTO_RSL_TRX1 (1), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 40
16:57:59.457282 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 4, streamId := IPAC_PROTO_RSL_TRX2 (2), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 41
16:57:59.457590 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 5, streamId := IPAC_PROTO_RSL_TRX3 (3), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 42
16:57:59.942195 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 43
16:58:00.941926 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 44
16:58:01.942284 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 45
16:58:02.373013 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 34, info := { { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 1 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 2 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 3 } }, tn := 0 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 2 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_Bm_ACCH (1) }, tn := 3 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { lm := { tag := '0001'B, sub_chan := 0 } }, tn := 5 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { lm := { tag := '0001'B, sub_chan := 1 } }, tn := 5 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 0 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 1 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 2 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 3 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 4 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 5 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 6 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { sdcch8 := { tag := '01'B, sub_chan := 7 } }, tn := 6 }, interf_band := 2, rfu := '00000'B }, { chan_nr := { u := { ch0 := RSL_CHAN_NR_OSMO_PDCH (24) }, tn := 7 }, interf_band := 2, rfu := '00000'B } } } } } } } } id 46
16:58:02.373666 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 3, streamId := IPAC_PROTO_RSL_TRX1 (1), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 47
16:58:02.373824 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 4, streamId := IPAC_PROTO_RSL_TRX2 (2), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 48
16:58:02.374113 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 5, streamId := IPAC_PROTO_RSL_TRX3 (3), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_RF_RES_IND (25), ies := { { iei := RSL_IE_RESOURCE_INFO (21), body := { resource_info := { len := 0, info := { } } } } } } } id 49
16:58:02.943111 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 50
16:58:03.943372 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 51
16:58:04.943748 BTS_Tests.ttcn:3554 Message enqueued on RSL_CCHAN from TC_rsl_ms_pwr_dyn_up-RSL(353) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 2, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CCCH_LOAD_IND (18), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_PAGING_LOAD (15), body := { paging_load := 65535 } } } } } id 52
16:58:05.095914 BTS_Tests.ttcn:3554 PTC with component reference 355 is done.
16:58:05.095982 Osmocom_VTY_Functions.ttcn:105 Sent on BTSVTY to system charstring : "configure terminal"
16:58:05.096095 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
16:58:05.096274 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "OsmoBTS(config)# " id 11
16:58:05.096397 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "OsmoBTS(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:58:05.096487 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY "OsmoBTS(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
16:58:05.096591 Osmocom_VTY_Functions.ttcn:74 Matching on port BTSVTY succeeded: "OsmoBTS(config)# " with pattern "[\w-]+\(*\)\# " matched
16:58:05.096648 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BTSVTY succeeded, message from system(): charstring : "OsmoBTS(config)# " id 11
16:58:05.096687 Osmocom_VTY_Functions.ttcn:74 Message with id 11 was extracted from the queue of BTSVTY.
16:58:05.096722 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
16:58:05.096757 Osmocom_VTY_Functions.ttcn:105 Sent on BTSVTY to system charstring : "phy 0"
16:58:05.096821 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
16:58:05.097081 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "OsmoBTS(phy)# " id 12
16:58:05.097270 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "OsmoBTS(phy)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:58:05.097355 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY "OsmoBTS(phy)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
16:58:05.097448 Osmocom_VTY_Functions.ttcn:74 Matching on port BTSVTY succeeded: "OsmoBTS(phy)# " with pattern "[\w-]+\(*\)\# " matched
16:58:05.097482 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BTSVTY succeeded, message from system(): charstring : "OsmoBTS(phy)# " id 12
16:58:05.097515 Osmocom_VTY_Functions.ttcn:74 Message with id 12 was extracted from the queue of BTSVTY.
16:58:05.097548 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
16:58:05.097588 Osmocom_VTY_Functions.ttcn:105 Sent on BTSVTY to system charstring : "no osmotrx ms-power-loop"
16:58:05.097681 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
16:58:05.097803 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "'no osmotrx ms-power-loop' is deprecated, MS Power Control is now managed by BSC" id 13
16:58:05.097836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "OsmoBTS(phy)# " id 14
16:58:05.097895 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "'no osmotrx ms-power-loop' is deprecated, MS Power Control is now managed by BSC" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:58:05.097952 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY "'no osmotrx ms-power-loop' is deprecated, MS Power Control is now managed by BSC" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
16:58:05.098009 Osmocom_VTY_Functions.ttcn:74 Matching on port BTSVTY "'no osmotrx ms-power-loop' is deprecated, MS Power Control is now managed by BSC" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
16:58:05.098049 Osmocom_VTY_Functions.ttcn:75 Matching on port BTSVTY "'no osmotrx ms-power-loop' is deprecated, MS Power Control is now managed by BSC" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
16:58:05.098101 Osmocom_VTY_Functions.ttcn:85 Matching on port BTSVTY succeeded: "'no osmotrx ms-power-loop' is deprecated, MS Power Control is now managed by BSC" with ? matched
16:58:05.098133 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BTSVTY succeeded, message from system(): charstring : "'no osmotrx ms-power-loop' is deprecated, MS Power Control is now managed by BSC" id 13
16:58:05.098162 Osmocom_VTY_Functions.ttcn:85 Message with id 13 was extracted from the queue of BTSVTY.
16:58:05.098212 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "OsmoBTS(phy)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:58:05.098261 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY "OsmoBTS(phy)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
16:58:05.098328 Osmocom_VTY_Functions.ttcn:74 Matching on port BTSVTY succeeded: "OsmoBTS(phy)# " with pattern "[\w-]+\(*\)\# " matched
16:58:05.098355 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BTSVTY succeeded, message from system(): charstring : "OsmoBTS(phy)# " id 14
16:58:05.098380 Osmocom_VTY_Functions.ttcn:74 Message with id 14 was extracted from the queue of BTSVTY.
16:58:05.098406 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
16:58:05.098429 Osmocom_VTY_Functions.ttcn:105 Sent on BTSVTY to system charstring : "end"
16:58:05.098473 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
16:58:05.098531 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BTSVTY from system charstring : "OsmoBTS# " id 15
16:58:05.098587 Osmocom_VTY_Functions.ttcn:72 Matching on port BTSVTY "OsmoBTS# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
16:58:05.098640 Osmocom_VTY_Functions.ttcn:73 Matching on port BTSVTY succeeded: "OsmoBTS# " with pattern "[\w-]+\# " matched
16:58:05.098666 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BTSVTY succeeded, message from system(): charstring : "OsmoBTS# " id 15
16:58:05.098691 Osmocom_VTY_Functions.ttcn:73 Message with id 15 was extracted from the queue of BTSVTY.
16:58:05.098716 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
16:58:05.098741 Misc_Helpers.ttcn:38 Stopping testcase execution from "BTS_Tests.ttcn":3557
16:58:05.098787 Misc_Helpers.ttcn:43 Stopping all components.
16:58:05.101179 Misc_Helpers.ttcn:43 Connection of port IPA_CTRL to IPA-CTRL-CLI-IPA(354):IPA_CTRL_PORT was closed unexpectedly by the peer.
16:58:05.101331 Misc_Helpers.ttcn:43 Port IPA_CTRL was disconnected from IPA-CTRL-CLI-IPA(354):IPA_CTRL_PORT.
16:58:05.101505 Misc_Helpers.ttcn:43 All components were stopped.
16:58:05.101574 Misc_Helpers.ttcn:45 Stopping test component execution.
16:58:05.101688 BTS_Tests.ttcn:3557 Test case TC_rsl_ms_pwr_dyn_up was stopped.
16:58:05.101739 BTS_Tests.ttcn:3557 Terminating component type BTS_Tests.test_CT.
16:58:05.101793 BTS_Tests.ttcn:3557 Port IPA_CTRL was stopped.
16:58:05.101843 BTS_Tests.ttcn:3557 Removing unterminated connection between port RSL_CCHAN and TC_rsl_ms_pwr_dyn_up-RSL(353):CCHAN_PT.
16:58:05.101969 BTS_Tests.ttcn:3557 Message with id 9 was extracted from the queue of RSL_CCHAN.
16:58:05.102034 BTS_Tests.ttcn:3557 Message with id 10 was extracted from the queue of RSL_CCHAN.
16:58:05.102151 BTS_Tests.ttcn:3557 Message with id 11 was extracted from the queue of RSL_CCHAN.
16:58:05.102179 BTS_Tests.ttcn:3557 Message with id 12 was extracted from the queue of RSL_CCHAN.
16:58:05.102197 BTS_Tests.ttcn:3557 Message with id 13 was extracted from the queue of RSL_CCHAN.
16:58:05.102215 BTS_Tests.ttcn:3557 Message with id 14 was extracted from the queue of RSL_CCHAN.
16:58:05.102234 BTS_Tests.ttcn:3557 Message with id 15 was extracted from the queue of RSL_CCHAN.
16:58:05.102252 BTS_Tests.ttcn:3557 Message with id 16 was extracted from the queue of RSL_CCHAN.
16:58:05.102270 BTS_Tests.ttcn:3557 Message with id 17 was extracted from the queue of RSL_CCHAN.
16:58:05.102307 BTS_Tests.ttcn:3557 Message with id 18 was extracted from the queue of RSL_CCHAN.
16:58:05.102325 BTS_Tests.ttcn:3557 Message with id 19 was extracted from the queue of RSL_CCHAN.
16:58:05.102343 BTS_Tests.ttcn:3557 Message with id 20 was extracted from the queue of RSL_CCHAN.
16:58:05.102361 BTS_Tests.ttcn:3557 Message with id 21 was extracted from the queue of RSL_CCHAN.
16:58:05.102378 BTS_Tests.ttcn:3557 Message with id 22 was extracted from the queue of RSL_CCHAN.
16:58:05.102396 BTS_Tests.ttcn:3557 Message with id 23 was extracted from the queue of RSL_CCHAN.
16:58:05.102414 BTS_Tests.ttcn:3557 Message with id 24 was extracted from the queue of RSL_CCHAN.
16:58:05.102436 BTS_Tests.ttcn:3557 Message with id 25 was extracted from the queue of RSL_CCHAN.
16:58:05.102454 BTS_Tests.ttcn:3557 Message with id 26 was extracted from the queue of RSL_CCHAN.
16:58:05.102472 BTS_Tests.ttcn:3557 Message with id 27 was extracted from the queue of RSL_CCHAN.
16:58:05.102489 BTS_Tests.ttcn:3557 Message with id 28 was extracted from the queue of RSL_CCHAN.
16:58:05.102507 BTS_Tests.ttcn:3557 Message with id 29 was extracted from the queue of RSL_CCHAN.
16:58:05.102524 BTS_Tests.ttcn:3557 Message with id 30 was extracted from the queue of RSL_CCHAN.
16:58:05.102542 BTS_Tests.ttcn:3557 Message with id 31 was extracted from the queue of RSL_CCHAN.
16:58:05.102564 BTS_Tests.ttcn:3557 Message with id 32 was extracted from the queue of RSL_CCHAN.
16:58:05.102581 BTS_Tests.ttcn:3557 Message with id 33 was extracted from the queue of RSL_CCHAN.
16:58:05.102600 BTS_Tests.ttcn:3557 Message with id 34 was extracted from the queue of RSL_CCHAN.
16:58:05.102617 BTS_Tests.ttcn:3557 Message with id 35 was extracted from the queue of RSL_CCHAN.
16:58:05.102635 BTS_Tests.ttcn:3557 Message with id 36 was extracted from the queue of RSL_CCHAN.
16:58:05.102653 BTS_Tests.ttcn:3557 Message with id 37 was extracted from the queue of RSL_CCHAN.
16:58:05.102670 BTS_Tests.ttcn:3557 Message with id 38 was extracted from the queue of RSL_CCHAN.
16:58:05.102692 BTS_Tests.ttcn:3557 Message with id 39 was extracted from the queue of RSL_CCHAN.
16:58:05.102709 BTS_Tests.ttcn:3557 Message with id 40 was extracted from the queue of RSL_CCHAN.
16:58:05.102727 BTS_Tests.ttcn:3557 Message with id 41 was extracted from the queue of RSL_CCHAN.
16:58:05.102744 BTS_Tests.ttcn:3557 Message with id 42 was extracted from the queue of RSL_CCHAN.
16:58:05.102762 BTS_Tests.ttcn:3557 Message with id 43 was extracted from the queue of RSL_CCHAN.
16:58:05.102780 BTS_Tests.ttcn:3557 Message with id 44 was extracted from the queue of RSL_CCHAN.
16:58:05.102797 BTS_Tests.ttcn:3557 Message with id 45 was extracted from the queue of RSL_CCHAN.
16:58:05.102820 BTS_Tests.ttcn:3557 Message with id 46 was extracted from the queue of RSL_CCHAN.
16:58:05.102837 BTS_Tests.ttcn:3557 Message with id 47 was extracted from the queue of RSL_CCHAN.
16:58:05.102855 BTS_Tests.ttcn:3557 Message with id 48 was extracted from the queue of RSL_CCHAN.
16:58:05.102873 BTS_Tests.ttcn:3557 Message with id 49 was extracted from the queue of RSL_CCHAN.
16:58:05.102890 BTS_Tests.ttcn:3557 Message with id 50 was extracted from the queue of RSL_CCHAN.
16:58:05.102908 BTS_Tests.ttcn:3557 Message with id 51 was extracted from the queue of RSL_CCHAN.
16:58:05.102926 BTS_Tests.ttcn:3557 Message with id 52 was extracted from the queue of RSL_CCHAN.
16:58:05.102944 BTS_Tests.ttcn:3557 Port RSL_CCHAN was stopped.
16:58:05.102966 BTS_Tests.ttcn:3557 Port L1CTL was stopped.
16:58:05.102983 BTS_Tests.ttcn:3557 Port BTS_TRXC was stopped.
16:58:05.103000 BTS_Tests.ttcn:3557 Removing unterminated mapping between port BTSVTY and system:BTSVTY.
16:58:05.103083 BTS_Tests.ttcn:3557 Port BTSVTY was unmapped from system:BTSVTY.
16:58:05.103112 BTS_Tests.ttcn:3557 Port BTSVTY was stopped.
16:58:05.103129 BTS_Tests.ttcn:3557 Port BSCVTY was stopped.
16:58:05.103145 BTS_Tests.ttcn:3557 Port PCU was stopped.
16:58:05.103162 BTS_Tests.ttcn:3557 Component type BTS_Tests.test_CT was shut down inside testcase TC_rsl_ms_pwr_dyn_up.
16:58:05.103196 BTS_Tests.ttcn:3557 Waiting for PTCs to finish.
16:58:05.104524 BTS_Tests.ttcn:3557 Setting final verdict of the test case.
16:58:05.104704 BTS_Tests.ttcn:3557 Local verdict of MTC: none
16:58:05.104791 BTS_Tests.ttcn:3557 Local verdict of PTC TC_rsl_ms_pwr_dyn_up-RSL-IPA(352): none (none -> none)
16:58:05.104873 BTS_Tests.ttcn:3557 Local verdict of PTC TC_rsl_ms_pwr_dyn_up-RSL(353): none (none -> none)
16:58:05.104947 BTS_Tests.ttcn:3557 Local verdict of PTC IPA-CTRL-CLI-IPA(354): none (none -> none)
16:58:05.105062 BTS_Tests.ttcn:3557 Local verdict of PTC TC_rsl_ms_pwr_dyn_up(355): pass (none -> pass)
16:58:05.105141 BTS_Tests.ttcn:3557 Test case TC_rsl_ms_pwr_dyn_up finished. Verdict: pass
16:58:05.105222 BTS_Tests.ttcn:3557 Starting external command `../ttcn3-tcpdump-stop.sh BTS_Tests.TC_rsl_ms_pwr_dyn_up pass'.
16:58:08.694063 BTS_Tests.ttcn:3557 External command `../ttcn3-tcpdump-stop.sh BTS_Tests.TC_rsl_ms_pwr_dyn_up pass' was executed successfully (exit status: 0).
16:58:08.694142 BTS_Tests.ttcn:3575 Switching to log file `BTS_Tests-TC_rsl_ms_pwr_dyn_down-958f0a91c7aa-mtc-24.log'
