= IPL4asp Test Port for TTCN-3 Toolset with TITAN, Change log
:author: Gábor Szalai
:toc:

= Changes

== R30E

Message dissector function update:

If the callback function detects that the it will be impossible to determine the length of the message, even receiving more octests, should return `_"-2"_`. In this case the connection will be closed and the length calculation error will be reported.

If the callback function returns `_"0"_` run time error will be raised to avoid deadlock.

== R30F

The name of the test port parameters: TLSv1.1, TLSv1.2, DTLSv1.2 changed to TLSv1_1, TLSv1_2, DTLSv1_2

