--  Reference:          3GPP TS 29.002 10.6.0

MAP-TS-Code {
   itu-t identified-organization (4) etsi (0) mobileDomain (0)
   gsm-Network (1) modules (3) map-TS-Code (19) version13 (13)}

DEFINITIONS

::=

BEGIN

TeleserviceCode ::= OCTET STRING (SIZE (1))
	-- This type is used to represent the code identifying a single
	-- teleservice, a group of teleservices, or all teleservices. The
	-- services are defined in TS GSM 22.003 [4].
	-- The internal structure is defined as follows:

	-- bits 87654321: group (bits 8765) and specific service
	-- (bits 4321)

Ext-TeleserviceCode ::= OCTET STRING (SIZE (1..5))
	-- This type is used to represent the code identifying a single
	-- teleservice, a group of teleservices, or all teleservices. The
	-- services are defined in TS GSM 22.003 [4].
	-- The internal structure is defined as follows:

	-- OCTET 1:
	-- bits 87654321: group (bits 8765) and specific service
	-- (bits 4321)

	-- OCTETS 2-5: reserved for future use. If received the
    -- Ext-TeleserviceCode shall be
 	-- treated according to the exception handling defined for the
	-- operation that uses this type.

	-- Ext-TeleserviceCode includes all values defined for TeleserviceCode.

allTeleservices	TeleserviceCode ::= '00000000'B

allSpeechTransmissionServices	TeleserviceCode ::= '00010000'B
telephony			TeleserviceCode ::= '00010001'B
emergencyCalls		TeleserviceCode ::= '00010010'B

allShortMessageServices	TeleserviceCode ::= '00100000'B
shortMessageMT-PP	TeleserviceCode ::= '00100001'B
shortMessageMO-PP	TeleserviceCode ::= '00100010'B

allFacsimileTransmissionServices	TeleserviceCode ::= '01100000'B
facsimileGroup3AndAlterSpeech	TeleserviceCode ::= '01100001'B
automaticFacsimileGroup3	TeleserviceCode ::= '01100010'B
facsimileGroup4	TeleserviceCode ::= '01100011'B

-- The following non-hierarchical Compound Teleservice Groups
-- are defined in TS 3GPP TS 22.030:
allDataTeleservices	TeleserviceCode ::= '01110000'B
	-- covers Teleservice Groups 'allFacsimileTransmissionServices'
	-- and 'allShortMessageServices'
allTeleservices-ExeptSMS	TeleserviceCode ::= '10000000'B
	-- covers Teleservice Groups 'allSpeechTransmissionServices' and
	-- 'allFacsimileTransmissionServices'
--
-- Compound Teleservice Group Codes are only used in call
-- independent supplementary service operations, i.e. they
-- are not used in InsertSubscriberData or in
-- DeleteSubscriberData messages.

allVoiceGroupCallServices	TeleserviceCode ::= '10010000'B
voiceGroupCall		TeleserviceCode ::= '10010001'B
voiceBroadcastCall	TeleserviceCode ::= '10010010'B

allPLMN-specificTS	TeleserviceCode ::= '11010000'B
plmn-specificTS-1	TeleserviceCode ::= '11010001'B
plmn-specificTS-2	TeleserviceCode ::= '11010010'B
plmn-specificTS-3	TeleserviceCode ::= '11010011'B
plmn-specificTS-4	TeleserviceCode ::= '11010100'B
plmn-specificTS-5	TeleserviceCode ::= '11010101'B
plmn-specificTS-6	TeleserviceCode ::= '11010110'B
plmn-specificTS-7	TeleserviceCode ::= '11010111'B
plmn-specificTS-8	TeleserviceCode ::= '11011000'B
plmn-specificTS-9	TeleserviceCode ::= '11011001'B
plmn-specificTS-A	TeleserviceCode ::= '11011010'B
plmn-specificTS-B	TeleserviceCode ::= '11011011'B
plmn-specificTS-C	TeleserviceCode ::= '11011100'B
plmn-specificTS-D	TeleserviceCode ::= '11011101'B
plmn-specificTS-E	TeleserviceCode ::= '11011110'B
plmn-specificTS-F	TeleserviceCode ::= '11011111'B

END
