/******************************************************************************
* Copyright (c) 2000-2019 Ericsson Telecom AB
* All rights reserved. This program and the accompanying materials
* are made available under the terms of the Eclipse Public License v2.0
* which accompanies this distribution, and is available at
* https://www.eclipse.org/org/documents/epl-2.0/EPL-2.0.html
*
* Contributors:
*   Roland Gecse - initial implementation and initial documentation
*   Akos Pernek
*   Antal Wuh.Hen.Chang
*   Attila Fulop
*   Balazs Barcsik
*   Bence Molnar
*   Csaba Koppany
*   David Juhasz
*   Eduard Czimbalmos
*   Elemer Lelik
*   Endre Kiss
*   Endre Kulcsar
*   Gabor Szalai
*   Gabor Tatarka
*   Gergely Futo
*   Istvan Sandor
*   Krisztian Pandi
*   Kulcsár Endre
*   Laszlo Tamas Zeke
*   Norbert Pinter
*   Roland Gecse
*   Tibor Bende
*   Tibor Szabo
*   Timea Moder
*   Zoltan Medve
*   Zsolt Nandor Torok
*   Zsolt Szalai
******************************************************************************/
//
//  File:               SyInterface_3GPP_TS29219_b30.ddf
//  Description:        DDF for Sy Interface according to 3GPP 29.219 v11.3.0
//  Rev:                R55A
//  Prodnr:             CNL 113 462
///////////////////////////////////////////////

// APPLICATION-NAME: Sy
// APPLICATION-REVISION: v11_3_0

// AVP implementations according to: 
// 3GPP 29.219 v11.3.0 - Sy Interface based on the Diameter PROTOCOL
//
//
//

// 3GPP 29.219 v11.3.0  5.6.1
type enumerated Command_Code 
{
  Session_Termination          (275),
  ThreeGPP_Spending_Limit               (8388635),
  ThreeGPP_Spending_Status_Notification (8388636)
}

// 3GPP 29.219 v11.3.0
// AVP: Policy-Counter-Identifier (2901) 3GPP (10415)
// 5.3.1
type AVP_UTF8String Policy_Counter_Identifier;

// 3GPP 29.219 v11.3.0
// AVP: Policy-Counter-Status (2902) 3GPP (10415)
// 5.3.2
type AVP_UTF8String Policy_Counter_Status;

// 3GPP 29.219 v11.3.0
// AVP: Policy-Counter-Status-Report (2903) 3GPP (10415)
// 5.3.3
type AVP_Grouped Policy_Counter_Status_Report;


// 3GPP 29.219 v11.3.0
// AVP: SL-Request-Type (2904) 3GPP (10415)
// 5.3.4
type enumerated SL_Request_Type
{
  INITIAL_REQUEST (0),
  INTERMEDIATE_REQUEST (1)
}

