/******************************************************************************
* Copyright (c) 2000-2019 Ericsson Telecom AB
* All rights reserved. This program and the accompanying materials
* are made available under the terms of the Eclipse Public License v2.0
* which accompanies this distribution, and is available at
* https://www.eclipse.org/org/documents/epl-2.0/EPL-2.0.html
*
* Contributors:
*   Roland Gecse - initial implementation and initial documentation
*   Akos Pernek
*   Antal Wuh.Hen.Chang
*   Attila Fulop
*   Balazs Barcsik
*   Bence Molnar
*   Csaba Koppany
*   David Juhasz
*   Eduard Czimbalmos
*   Elemer Lelik
*   Endre Kiss
*   Endre Kulcsar
*   Gabor Szalai
*   Gabor Tatarka
*   Gergely Futo
*   Istvan Sandor
*   Krisztian Pandi
*   Kulcsár Endre
*   Laszlo Tamas Zeke
*   Norbert Pinter
*   Roland Gecse
*   Tibor Bende
*   Tibor Szabo
*   Timea Moder
*   Zoltan Medve
*   Zsolt Nandor Torok
*   Zsolt Szalai
******************************************************************************/
//
//  File:               AAAInterface_3GPP_TS29273_840.ddf
//  Description:        DDF for EPS AAA according to 3GPP TS 29.273 V8.4.0
//  Rev:                R55A
//  Prodnr:             CNL 113 462
///////////////////////////////////////////////


// APPLICATION-NAME: AAA
// APPLICATION-REVISION: V8_4_0

// AVP implementations according to: 
// 3GPP TS 29.273 V8.4.0 - EPS AAA interfaces based on the Diameter protocol
// Statement of Compiance  X/174 02-AXB 250 20 Uen PA2

// Dependant applications
// IETF RFC 3588   - Diameter Base Protocol
// IETF RFC 4005   - Diameter Network Access Server Application

// 3GPP TS 32.273 V8.4.0  9.2.2
type enumerated Command_Code {  
  AA                    (265),
  Session_Termination   (275), 
  Abort_Session         (274)  
}

// 3GPP 29.273 V8.4.0
// AVP: MIP6-Agent-Info (486)
// 9.2.3.2.2
type AVP_Grouped MIP6_Agent_Info

// 3GPP 29.273 V8.4.0
// AVP: MIP6-Feature-Vector (124)
// 9.2.3.2.3
type AVP_Unsigned64 MIP6_Feature_Vector
