Faraday Technology FTWDT010 watchdog

This is an IP part from Faraday Technology found in the Gemini
SoCs and others.

Required properties:
- compatible : must be one of
  "faraday,ftwdt010"
  "cortina,gemini-watchdog", "faraday,ftwdt010"
- reg : shall contain base register location and length
- interrupts : shall contain the interrupt for the watchdog

Optional properties:
- timeout-sec : the default watchdog timeout in seconds.

Example:

watchdog@41000000 {
	compatible = "faraday,ftwdt010";
	reg = <0x41000000 0x1000>;
	interrupts = <3 IRQ_TYPE_LEVEL_HIGH>;
};
