What:		/sys/bus/counter/devices/counterX/countY/prescaler_available
KernelVersion:	5.2
Contact:	linux-iio@vger.kernel.org
Description:
		Discrete set of available values for the respective Count Y
		configuration are listed in this file. Values are delimited by
		newline characters.

What:		/sys/bus/counter/devices/counterX/countY/prescaler
KernelVersion:	5.2
Contact:	linux-iio@vger.kernel.org
Description:
		Configure the prescaler value associated with Count Y.
		On the FlexTimer, the counter clock source passes through a
		prescaler (i.e. a counter). This acts like a clock
		divider.
