Ralink Watchdog Timers

Required properties:
- compatible: must be "mediatek,mt7621-wdt"
- reg: physical base address of the controller and length of the register range

Example:

	watchdog@100 {
		compatible = "mediatek,mt7621-wdt";
		reg = <0x100 0x10>;
	};
