What:		/sys/bus/iio/devices/iio:deviceX/in_accel_x_calibbias
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_y_calibbias
What:		/sys/bus/iio/devices/iio:deviceX/in_accel_z_calibbias
What:		/sys/bus/iio/devices/iio:deviceX/in_anglvel_x_calibbias
What:		/sys/bus/iio/devices/iio:deviceX/in_anglvel_y_calibbias
What:		/sys/bus/iio/devices/iio:deviceX/in_anglvel_z_calibbias
KernelVersion:  5.8
Contact:        linux-iio@vger.kernel.org
Description:
		Hardware applied calibration offset (assumed to fix production
		inaccuracies). Values represent a real physical offset expressed
		in SI units (m/s^2 for accelerometer and rad/s for gyroscope).

What:		/sys/bus/iio/devices/iio:deviceX/in_accel_calibbias_available
What:		/sys/bus/iio/devices/iio:deviceX/in_anglvel_calibbias_available
KernelVersion:  5.8
Contact:        linux-iio@vger.kernel.org
Description:
		Range of available values for hardware offset. Values in SI
		units (m/s^2 for accelerometer and rad/s for gyroscope).
