.. SPDX-License-Identifier: GFDL-1.1-no-invariants-or-later

.. _V4L2-PIX-FMT-NV24:
.. _V4L2-PIX-FMT-NV42:

******************************************************
V4L2_PIX_FMT_NV24 ('NV24'), V4L2_PIX_FMT_NV42 ('NV42')
******************************************************

V4L2_PIX_FMT_NV42
Formats with full horizontal and vertical chroma resolutions, also known
as YUV 4:4:4. One luminance and one chrominance plane with alternating
chroma samples as opposed to ``V4L2_PIX_FMT_YVU420``


Description
===========

These are two-plane versions of the YUV 4:4:4 format. The three
components are separated into two sub-images or planes. The Y plane is
first, with each Y sample stored in one byte per pixel. For
``V4L2_PIX_FMT_NV24``, a combined CbCr plane immediately follows the Y
plane in memory. The CbCr plane has the same width and height, in
pixels, as the Y plane (and the image). Each line contains one CbCr pair
per pixel, with each Cb and Cr sample stored in one byte.
``V4L2_PIX_FMT_NV42`` is the same except that the Cb and Cr samples are
swapped, the CrCb plane starts with a Cr sample.

If the Y plane has pad bytes after each row, then the CbCr plane has
twice as many pad bytes after its rows.

**Byte Order.**
Each cell is one byte.


.. flat-table::
    :header-rows:  0
    :stub-columns: 0

    * - start + 0:
      - Y'\ :sub:`00`
      - Y'\ :sub:`01`
      - Y'\ :sub:`02`
      - Y'\ :sub:`03`
    * - start + 4:
      - Y'\ :sub:`10`
      - Y'\ :sub:`11`
      - Y'\ :sub:`12`
      - Y'\ :sub:`13`
    * - start + 8:
      - Y'\ :sub:`20`
      - Y'\ :sub:`21`
      - Y'\ :sub:`22`
      - Y'\ :sub:`23`
    * - start + 12:
      - Y'\ :sub:`30`
      - Y'\ :sub:`31`
      - Y'\ :sub:`32`
      - Y'\ :sub:`33`
    * - start + 16:
      - Cb\ :sub:`00`
      - Cr\ :sub:`00`
      - Cb\ :sub:`01`
      - Cr\ :sub:`01`
      - Cb\ :sub:`02`
      - Cr\ :sub:`02`
      - Cb\ :sub:`03`
      - Cr\ :sub:`03`
    * - start + 24:
      - Cb\ :sub:`10`
      - Cr\ :sub:`10`
      - Cb\ :sub:`11`
      - Cr\ :sub:`11`
      - Cb\ :sub:`12`
      - Cr\ :sub:`12`
      - Cb\ :sub:`13`
      - Cr\ :sub:`13`
    * - start + 32:
      - Cb\ :sub:`20`
      - Cr\ :sub:`20`
      - Cb\ :sub:`21`
      - Cr\ :sub:`21`
      - Cb\ :sub:`22`
      - Cr\ :sub:`22`
      - Cb\ :sub:`23`
      - Cr\ :sub:`23`
    * - start + 40:
      - Cb\ :sub:`30`
      - Cr\ :sub:`30`
      - Cb\ :sub:`31`
      - Cr\ :sub:`31`
      - Cb\ :sub:`32`
      - Cr\ :sub:`32`
      - Cb\ :sub:`33`
      - Cr\ :sub:`33`
