Marvell Bluetooth Chips
-----------------------

This documents the binding structure and common properties for serial
attached Marvell Bluetooth devices. The following chips are included in
this binding:

* Marvell 88W8897 Bluetooth devices

Required properties:
 - compatible: should be:
    "mrvl,88w8897"

Optional properties:
None so far

Example:

&serial0 {
	compatible = "ns16550a";
	...
	bluetooth {
		compatible = "mrvl,88w8897";
	};
};
