.. SPDX-License-Identifier: GFDL-1.1-no-invariants-or-later

.. _V4L2-PIX-FMT-SRGGB8:
.. _v4l2-pix-fmt-sbggr8:
.. _v4l2-pix-fmt-sgbrg8:
.. _v4l2-pix-fmt-sgrbg8:

***************************************************************************************************************************
V4L2_PIX_FMT_SRGGB8 ('RGGB'), V4L2_PIX_FMT_SGRBG8 ('GRBG'), V4L2_PIX_FMT_SGBRG8 ('GBRG'), V4L2_PIX_FMT_SBGGR8 ('BA81'),
***************************************************************************************************************************


8-bit Bayer formats


Description
===========

These four pixel formats are raw sRGB / Bayer formats with 8 bits per
sample. Each sample is stored in a byte. Each n-pixel row contains n/2
green samples and n/2 blue or red samples, with alternating red and
blue rows. They are conventionally described as GRGR... BGBG...,
RGRG... GBGB..., etc. Below is an example of a small V4L2_PIX_FMT_SBGGR8 image:

**Byte Order.**
Each cell is one byte.




.. flat-table::
    :header-rows:  0
    :stub-columns: 0

    * - start + 0:
      - B\ :sub:`00`
      - G\ :sub:`01`
      - B\ :sub:`02`
      - G\ :sub:`03`
    * - start + 4:
      - G\ :sub:`10`
      - R\ :sub:`11`
      - G\ :sub:`12`
      - R\ :sub:`13`
    * - start + 8:
      - B\ :sub:`20`
      - G\ :sub:`21`
      - B\ :sub:`22`
      - G\ :sub:`23`
    * - start + 12:
      - G\ :sub:`30`
      - R\ :sub:`31`
      - G\ :sub:`32`
      - R\ :sub:`33`
