Oxford Semiconductor OXNAS SoCs Family device tree bindings
-------------------------------------------

Boards with the OX810SE SoC shall have the following properties:
  Required root node property:
    compatible: "oxsemi,ox810se"

Boards with the OX820 SoC shall have the following properties:
  Required root node property:
    compatible: "oxsemi,ox820"

Board compatible values:
  - "wd,mbwe" (OX810SE)
  - "cloudengines,pogoplugv3" (OX820)
