\doxysection{src/l1/tch3.c File Reference}
\label{tch3_8c}\index{src/l1/tch3.c@{src/l1/tch3.c}}


Osmocom GMR-\/1 TCH3 channel coding implementation.  


{\ttfamily \#include $<$stdint.\+h$>$}\newline
{\ttfamily \#include $<$string.\+h$>$}\newline
{\ttfamily \#include $<$osmocom/core/bits.\+h$>$}\newline
{\ttfamily \#include $<$osmocom/core/conv.\+h$>$}\newline
{\ttfamily \#include $<$osmocom/gmr1/l1/conv.\+h$>$}\newline
{\ttfamily \#include $<$osmocom/gmr1/l1/punct.\+h$>$}\newline
{\ttfamily \#include $<$osmocom/gmr1/l1/scramb.\+h$>$}\newline
\doxysubsection*{Functions}
\begin{DoxyCompactItemize}
\item 
void \textbf{ gmr1\+\_\+tch3\+\_\+encode} (ubit\+\_\+t $\ast$bits\+\_\+e, const uint8\+\_\+t $\ast$frame0, const uint8\+\_\+t $\ast$frame1, const ubit\+\_\+t $\ast$bits\+\_\+s, const ubit\+\_\+t $\ast$ciph, int m)
\begin{DoxyCompactList}\small\item\em Stateless GMR-\/1 TCH3 channel coder. \end{DoxyCompactList}\item 
void \textbf{ gmr1\+\_\+tch3\+\_\+decode} (uint8\+\_\+t $\ast$frame0, uint8\+\_\+t $\ast$frame1, ubit\+\_\+t $\ast$bits\+\_\+s, const sbit\+\_\+t $\ast$bits\+\_\+e, const ubit\+\_\+t $\ast$ciph, int m, int $\ast$conv0\+\_\+rv, int $\ast$conv1\+\_\+rv)
\begin{DoxyCompactList}\small\item\em Stateless GMR-\/1 TCH3 channel decoder. \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
Osmocom GMR-\/1 TCH3 channel coding implementation. 

