libosmodsp 0.4.0.12-f6f4 Osmocom DSP library

Data Structures | Functions | Variables
iqbal.c File Reference
IQ balance utilities

IQ balance utils implementation. More...

## Data Structures
struct | _iqbal_estimate_state
| Cache for _osmo_iqbal_estimate when doing lots of calls. More...
struct | _iqbal_state
| Internal state structure for the IQ balance optimization algorithm. More...

## Functions
void | osmo_iqbal_fix (float complex *out, float complex *in, unsigned int len, float mag, float phase)
| Apply IQ balance correction to a given complex buffer. More...
struct osmo_cxvec * | osmo_iqbal_cxvec_fix (const struct osmo_cxvec *in, float mag, float phase, struct osmo_cxvec *out)
| Apply IQ balance correction to a given complex vector. More...
static void | _osmo_iqbal_estimate_release (struct _iqbal_estimate_state *state)
| Release a cache object created by _osmo_iqbal_estimate.
static float | _osmo_iqbal_estimate (const float complex *data, int fft_size, int fft_count, struct _iqbal_estimate_state **state_p)
| Objectively estimate IQ balance in a given complex buffer. More...
float | osmo_iqbal_estimate (const float complex *data, int fft_size, int fft_count)
| Objectively estimate IQ balance in a given complex buffer. More...
float | osmo_iqbal_cxvec_estimate (const struct osmo_cxvec *sig, int fft_size, int fft_count)
| Objectively estimate IQ balance in a given complex vector. More...
static float | _iqbal_objfn_value (struct _iqbal_state *state, float x[2])
| Optimization objective function - Value. More...
static void | _iqbal_objfn_gradient (struct _iqbal_state *state, float x[2], float v, float grad[2])
| Optimization objective function - Gradient estimation. More...
static float | _iqbal_objfn_val_gradient (struct _iqbal_state *state, float x[2], float grad[2])
| Optimization objective function - Value & Gradient estimation. More...
int | osmo_iqbal_cxvec_optimize (const struct osmo_cxvec *sig, float *mag, float *phase, const struct osmo_iqbal_opts *opts)
| Finds the best IQ balance correction parameters for a given signal. More...

## Variables
const struct osmo_iqbal_opts | osmo_iqbal_default_opts
| Default values for the optimization algorithm. More...

## Detailed Description

IQ balance utils implementation.

The actual algorithm used for estimation of the imbalance and its optimization is inspired by the IQ balancer of SDR# by Youssef Touil and described here :

http://sdrsharp.com/index.php/automatic-iq-correction-algorithm

The main differences are:

- Objective function uses complex correlation of left/right side of FFT
- Optimization based on steepest gradient with dynamic step size