<vtydoc xmlns='urn:osmocom:xml:libosmocore:vty:doc:1.0'>
  <node id='_common_cmds_'>
    <name>Common Commands</name>
    <description>These commands are available on all VTY nodes. They are listed here only once, to unclutter the VTY reference.</description>
    <command id='help'>
      <params>
        <param name='help' doc='Description of the interactive help system' />
      </params>
    </command>
    <command id='list [with-flags]'>
      <params>
        <param name='list' doc='Print command list' />
        <param name='[with-flags]' doc='Also print the VTY attribute flags' />
      </params>
    </command>
    <command id='show vty-attributes'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='vty-attributes' doc='List of VTY attributes' />
      </params>
    </command>
    <command id='show vty-attributes (application|library|global)'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='vty-attributes' doc='List of VTY attributes' />
        <param name='application' doc='Application specific attributes only' />
        <param name='library' doc='Library specific attributes only' />
        <param name='global' doc='Global attributes only' />
      </params>
    </command>
    <command id='write terminal'>
      <params>
        <param name='write' doc='Write running configuration to memory, network, or terminal' />
        <param name='terminal' doc='Write to terminal' />
      </params>
    </command>
    <command id='write file [PATH]'>
      <params>
        <param name='write' doc='Write running configuration to memory, network, or terminal' />
        <param name='file' doc='Write to configuration file' />
        <param name='[PATH]' doc='Set file path to store the config, or replace if already exists' />
      </params>
    </command>
    <command id='write memory'>
      <params>
        <param name='write' doc='Write running configuration to memory, network, or terminal' />
        <param name='memory' doc='Write configuration to the file (same as write file)' />
      </params>
    </command>
    <command id='write'>
      <params>
        <param name='write' doc='Write running configuration to memory, network, or terminal' />
      </params>
    </command>
    <command id='show running-config'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='running-config' doc='running configuration' />
      </params>
    </command>
    <command id='exit'>
      <params>
        <param name='exit' doc='Exit current mode and down to previous mode' />
      </params>
    </command>
    <command id='end'>
      <params>
        <param name='end' doc='End current mode and change to enable mode.' />
      </params>
    </command>
  </node>
  <node id='view'>
    <name>view</name>
    <command id='show version'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='version' doc='Displays program version' />
      </params>
    </command>
    <command id='show online-help'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='online-help' doc='Online help' />
      </params>
    </command>
    <command id='enable'>
      <params>
        <param name='enable' doc='Turn on privileged mode command' />
      </params>
    </command>
    <command id='terminal length &lt;0-512&gt;'>
      <params>
        <param name='terminal' doc='Set terminal line parameters' />
        <param name='length' doc='Set number of lines on a screen' />
        <param name='&lt;0-512&gt;' doc='Number of lines on screen (0 for no pausing)' />
      </params>
    </command>
    <command id='terminal no length'>
      <params>
        <param name='terminal' doc='Set terminal line parameters' />
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='length' doc='Set number of lines on a screen' />
      </params>
    </command>
    <command id='who'>
      <params>
        <param name='who' doc='Display who is on vty' />
      </params>
    </command>
    <command id='show history'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='history' doc='Display the session command history' />
      </params>
    </command>
    <command id='logging enable'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='enable' doc='Enables logging to this vty' />
      </params>
    </command>
    <command id='logging disable'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='disable' doc='Disables logging to this vty' />
      </params>
    </command>
    <command id='logging filter all (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='filter' doc='Filter log messages' />
        <param name='all' doc='Do you want to log all messages?' />
        <param name='0' doc='Only print messages matched by other filters' />
        <param name='1' doc='Bypass filter and print all messages' />
      </params>
    </command>
    <command id='logging color (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='color' doc='Configure color-printing for log messages' />
        <param name='0' doc='Don&apos;t use color for printing messages' />
        <param name='1' doc='Use color for printing messages' />
      </params>
    </command>
    <command id='logging timestamp (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='timestamp' doc='Configure log message timestamping' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with current timestamp' />
      </params>
    </command>
    <command id='logging print extended-timestamp (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='extended-timestamp' doc='Configure log message timestamping' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with current timestamp with YYYYMMDDhhmmssnnn' />
      </params>
    </command>
    <command id='logging print category (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='category' doc='Configure log message' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with category/subsystem name' />
      </params>
    </command>
    <command id='logging print category-hex (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='category-hex' doc='Configure log message' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with category/subsystem nr in hex (&apos;&lt;000b&gt;&apos;)' />
      </params>
    </command>
    <command id='logging print level (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='level' doc='Configure log message' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with the log level name' />
      </params>
    </command>
    <command id='logging print file (0|1|basename) [last]'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='file' doc='Configure log message' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with the source file and line' />
        <param name='basename' doc='Prefix each log message with the source file&apos;s basename (strip leading paths) and line' />
        <param name='[last]' doc='Log source file info at the end of a log line. If omitted, log source file info just before the log text.' />
      </params>
    </command>
    <command id='logging set-log-mask MASK'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='set-log-mask' doc='Set the logmask of this logging target' />
        <param name='MASK' doc='List of logging categories to log, e.g. &apos;abc:mno:xyz&apos;. Available log categories depend on the specific application, refer to the &apos;logging level&apos; command. Optionally add individual log levels like &apos;abc,1:mno,3:xyz,5&apos;, where the level numbers are LOGL_DEBUG=1 LOGL_INFO=3 LOGL_NOTICE=5 LOGL_ERROR=7 LOGL_FATAL=8' />
      </params>
    </command>
    <command id='logging level (smlc|ref|lb|lcs|lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns) (debug|info|notice|error|fatal)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='level' doc='Set the log level for a specified category' />
        <param name='smlc' doc='Serving Mobile Location Center' />
        <param name='ref' doc='Reference Counting' />
        <param name='lb' doc='Lb interface' />
        <param name='lcs' doc='Location Services' />
        <param name='lglobal' doc='Library-internal global log family' />
        <param name='llapd' doc='LAPD in libosmogsm' />
        <param name='linp' doc='A-bis Intput Subsystem' />
        <param name='lmux' doc='A-bis B-Subchannel TRAU Frame Multiplex' />
        <param name='lmi' doc='A-bis Input Driver for Signalling' />
        <param name='lmib' doc='A-bis Input Driver for B-Channels (voice)' />
        <param name='lsms' doc='Layer3 Short Message Service (SMS)' />
        <param name='lctrl' doc='Control Interface' />
        <param name='lgtp' doc='GPRS GTP library' />
        <param name='lstats' doc='Statistics messages and logging' />
        <param name='lgsup' doc='Generic Subscriber Update Protocol' />
        <param name='loap' doc='Osmocom Authentication Protocol' />
        <param name='lss7' doc='libosmo-sigtran Signalling System 7' />
        <param name='lsccp' doc='libosmo-sigtran SCCP Implementation' />
        <param name='lsua' doc='libosmo-sigtran SCCP User Adaptation' />
        <param name='lm3ua' doc='libosmo-sigtran MTP3 User Adaptation' />
        <param name='lmgcp' doc='libosmo-mgcp Media Gateway Control Protocol' />
        <param name='ljibuf' doc='libosmo-netif Jitter Buffer' />
        <param name='lrspro' doc='Remote SIM protocol' />
        <param name='lns' doc='GPRS NS layer' />
        <param name='debug' doc='Log debug messages and higher levels' />
        <param name='info' doc='Log informational messages and higher levels' />
        <param name='notice' doc='Log noticeable messages and higher levels' />
        <param name='error' doc='Log error messages and higher levels' />
        <param name='fatal' doc='Log only fatal messages' />
      </params>
    </command>
    <command id='logging level set-all (debug|info|notice|error|fatal)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='level' doc='Set the log level for a specified category' />
        <param name='set-all' doc='Once-off set all categories to the given log level. There is no single command to take back these changes -- each category is set to the given level, period.' />
        <param name='debug' doc='Log debug messages and higher levels' />
        <param name='info' doc='Log informational messages and higher levels' />
        <param name='notice' doc='Log noticeable messages and higher levels' />
        <param name='error' doc='Log error messages and higher levels' />
        <param name='fatal' doc='Log only fatal messages' />
      </params>
    </command>
    <command id='logging level force-all (debug|info|notice|error|fatal)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='level' doc='Set the log level for a specified category' />
        <param name='force-all' doc='Globally force all logging categories to a specific level. This is released by the &apos;no logging level force-all&apos; command. Note: any &apos;logging level &lt;category&gt; &lt;level&gt;&apos; commands will have no visible effect after this, until the forced level is released.' />
        <param name='debug' doc='Log debug messages and higher levels' />
        <param name='info' doc='Log informational messages and higher levels' />
        <param name='notice' doc='Log noticeable messages and higher levels' />
        <param name='error' doc='Log error messages and higher levels' />
        <param name='fatal' doc='Log only fatal messages' />
      </params>
    </command>
    <command id='no logging level force-all'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='logging' doc='Configure logging' />
        <param name='level' doc='Set the log level for a specified category' />
        <param name='force-all' doc='Release any globally forced log level set with &apos;logging level force-all &lt;level&gt;&apos;' />
      </params>
    </command>
    <command id='logp (smlc|ref|lb|lcs|lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns) (debug|info|notice|error|fatal) .LOGMESSAGE'>
      <params>
        <param name='logp' doc='Print a message on all log outputs; useful for placing markers in test logs' />
        <param name='smlc' doc='Serving Mobile Location Center' />
        <param name='ref' doc='Reference Counting' />
        <param name='lb' doc='Lb interface' />
        <param name='lcs' doc='Location Services' />
        <param name='lglobal' doc='Library-internal global log family' />
        <param name='llapd' doc='LAPD in libosmogsm' />
        <param name='linp' doc='A-bis Intput Subsystem' />
        <param name='lmux' doc='A-bis B-Subchannel TRAU Frame Multiplex' />
        <param name='lmi' doc='A-bis Input Driver for Signalling' />
        <param name='lmib' doc='A-bis Input Driver for B-Channels (voice)' />
        <param name='lsms' doc='Layer3 Short Message Service (SMS)' />
        <param name='lctrl' doc='Control Interface' />
        <param name='lgtp' doc='GPRS GTP library' />
        <param name='lstats' doc='Statistics messages and logging' />
        <param name='lgsup' doc='Generic Subscriber Update Protocol' />
        <param name='loap' doc='Osmocom Authentication Protocol' />
        <param name='lss7' doc='libosmo-sigtran Signalling System 7' />
        <param name='lsccp' doc='libosmo-sigtran SCCP Implementation' />
        <param name='lsua' doc='libosmo-sigtran SCCP User Adaptation' />
        <param name='lm3ua' doc='libosmo-sigtran MTP3 User Adaptation' />
        <param name='lmgcp' doc='libosmo-mgcp Media Gateway Control Protocol' />
        <param name='ljibuf' doc='libosmo-netif Jitter Buffer' />
        <param name='lrspro' doc='Remote SIM protocol' />
        <param name='lns' doc='GPRS NS layer' />
        <param name='debug' doc='Log debug messages and higher levels' />
        <param name='info' doc='Log informational messages and higher levels' />
        <param name='notice' doc='Log noticeable messages and higher levels' />
        <param name='error' doc='Log error messages and higher levels' />
        <param name='fatal' doc='Log only fatal messages' />
        <param name='.LOGMESSAGE' doc='Arbitrary message to log on given category and log level' />
      </params>
    </command>
    <command id='show logging vty'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='logging' doc='Show current logging configuration' />
        <param name='vty' doc='Show current logging configuration for this vty' />
      </params>
    </command>
    <command id='show alarms'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='alarms' doc='Show current logging configuration' />
      </params>
    </command>
    <command id='show talloc-context (application|all) (full|brief|DEPTH)'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='talloc-context' doc='Show talloc memory hierarchy' />
        <param name='application' doc='Application&apos;s context' />
        <param name='all' doc='All contexts, if NULL-context tracking is enabled' />
        <param name='full' doc='Display a full talloc memory hierarchy' />
        <param name='brief' doc='Display a brief talloc memory hierarchy' />
        <param name='DEPTH' doc='Specify required maximal depth value' />
      </params>
    </command>
    <command id='show talloc-context (application|all) (full|brief|DEPTH) tree ADDRESS'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='talloc-context' doc='Show talloc memory hierarchy' />
        <param name='application' doc='Application&apos;s context' />
        <param name='all' doc='All contexts, if NULL-context tracking is enabled' />
        <param name='full' doc='Display a full talloc memory hierarchy' />
        <param name='brief' doc='Display a brief talloc memory hierarchy' />
        <param name='DEPTH' doc='Specify required maximal depth value' />
        <param name='tree' doc='Display only a specific memory chunk' />
        <param name='ADDRESS' doc='Chunk address (e.g. 0xdeadbeef)' />
      </params>
    </command>
    <command id='show talloc-context (application|all) (full|brief|DEPTH) filter REGEXP'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='talloc-context' doc='Show talloc memory hierarchy' />
        <param name='application' doc='Application&apos;s context' />
        <param name='all' doc='All contexts, if NULL-context tracking is enabled' />
        <param name='full' doc='Display a full talloc memory hierarchy' />
        <param name='brief' doc='Display a brief talloc memory hierarchy' />
        <param name='DEPTH' doc='Specify required maximal depth value' />
        <param name='filter' doc='Filter chunks using regular expression' />
        <param name='REGEXP' doc='Regular expression' />
      </params>
    </command>
    <command id='show cells'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cells' doc='Show configured cell locations' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; users'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='users' doc='User Table' />
      </params>
    </command>
    <command id='show cs7 (sua|m3ua|ipa) [&lt;0-65534&gt;]'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='sua' doc='SCCP User Adaptation' />
        <param name='m3ua' doc='MTP3 User Adaptation' />
        <param name='ipa' doc='IPA Multiplex (SCCP Lite)' />
        <param name='[&lt;0-65534&gt;]' doc='Port Number' />
      </params>
    </command>
    <command id='show cs7 config'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='config' doc='Currently running cs7 configuration' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; asp'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='asp' doc='Application Server Process (ASP)' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; as (active|all|m3ua|sua)'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='as' doc='Application Server (AS)' />
        <param name='active' doc='Display all active ASs' />
        <param name='all' doc='Display all ASs (default)' />
        <param name='m3ua' doc='Display all m3ua ASs' />
        <param name='sua' doc='Display all SUA ASs' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; sccp addressbook'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='sccp' doc='Signalling Connection Control Part' />
        <param name='addressbook' doc='List all SCCP addressbook entries' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; sccp users'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='sccp' doc='Signalling Connection Control Part' />
        <param name='users' doc='Show List of SCCP Users registered' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; sccp ssn &lt;0-65535&gt;'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='sccp' doc='Signalling Connection Control Part' />
        <param name='ssn' doc='Find an SCCP User registered for the given SSN' />
        <param name='&lt;0-65535&gt;' doc='Subsystem Number (SSN)' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; sccp connections'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='sccp' doc='Signalling Connection Control Part' />
        <param name='connections' doc='Show List of active SCCP connections' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; sccp timers'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='sccp' doc='Signaling Connection Control Part' />
        <param name='timers' doc='Show List of SCCP timers' />
      </params>
    </command>
  </node>
  <node id='enable'>
    <name>enable</name>
    <command id='disable'>
      <params>
        <param name='disable' doc='Turn off privileged mode command' />
      </params>
    </command>
    <command id='configure terminal'>
      <params>
        <param name='configure' doc='Configuration from vty interface' />
        <param name='terminal' doc='Configuration terminal' />
      </params>
    </command>
    <command id='copy running-config startup-config'>
      <params>
        <param name='copy' doc='Copy configuration' />
        <param name='running-config' doc='Copy running config to... ' />
        <param name='startup-config' doc='Copy running config to startup config (same as write file)' />
      </params>
    </command>
    <command id='show startup-config'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='startup-config' doc='Contentes of startup configuration' />
      </params>
    </command>
    <command id='show version'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='version' doc='Displays program version' />
      </params>
    </command>
    <command id='show online-help'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='online-help' doc='Online help' />
      </params>
    </command>
    <command id='terminal length &lt;0-512&gt;'>
      <params>
        <param name='terminal' doc='Set terminal line parameters' />
        <param name='length' doc='Set number of lines on a screen' />
        <param name='&lt;0-512&gt;' doc='Number of lines on screen (0 for no pausing)' />
      </params>
    </command>
    <command id='terminal no length'>
      <params>
        <param name='terminal' doc='Set terminal line parameters' />
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='length' doc='Set number of lines on a screen' />
      </params>
    </command>
    <command id='who'>
      <params>
        <param name='who' doc='Display who is on vty' />
      </params>
    </command>
    <command id='show history'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='history' doc='Display the session command history' />
      </params>
    </command>
    <command id='terminal monitor'>
      <params>
        <param name='terminal' doc='Set terminal line parameters' />
        <param name='monitor' doc='Copy debug output to the current terminal line' />
      </params>
    </command>
    <command id='terminal no monitor'>
      <params>
        <param name='terminal' doc='Set terminal line parameters' />
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='monitor' doc='Copy debug output to the current terminal line' />
      </params>
    </command>
    <command id='logging enable'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='enable' doc='Enables logging to this vty' />
      </params>
    </command>
    <command id='logging disable'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='disable' doc='Disables logging to this vty' />
      </params>
    </command>
    <command id='logging filter all (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='filter' doc='Filter log messages' />
        <param name='all' doc='Do you want to log all messages?' />
        <param name='0' doc='Only print messages matched by other filters' />
        <param name='1' doc='Bypass filter and print all messages' />
      </params>
    </command>
    <command id='logging color (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='color' doc='Configure color-printing for log messages' />
        <param name='0' doc='Don&apos;t use color for printing messages' />
        <param name='1' doc='Use color for printing messages' />
      </params>
    </command>
    <command id='logging timestamp (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='timestamp' doc='Configure log message timestamping' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with current timestamp' />
      </params>
    </command>
    <command id='logging print extended-timestamp (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='extended-timestamp' doc='Configure log message timestamping' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with current timestamp with YYYYMMDDhhmmssnnn' />
      </params>
    </command>
    <command id='logging print category (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='category' doc='Configure log message' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with category/subsystem name' />
      </params>
    </command>
    <command id='logging print category-hex (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='category-hex' doc='Configure log message' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with category/subsystem nr in hex (&apos;&lt;000b&gt;&apos;)' />
      </params>
    </command>
    <command id='logging print level (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='level' doc='Configure log message' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with the log level name' />
      </params>
    </command>
    <command id='logging print file (0|1|basename) [last]'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='file' doc='Configure log message' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with the source file and line' />
        <param name='basename' doc='Prefix each log message with the source file&apos;s basename (strip leading paths) and line' />
        <param name='[last]' doc='Log source file info at the end of a log line. If omitted, log source file info just before the log text.' />
      </params>
    </command>
    <command id='logging set-log-mask MASK'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='set-log-mask' doc='Set the logmask of this logging target' />
        <param name='MASK' doc='List of logging categories to log, e.g. &apos;abc:mno:xyz&apos;. Available log categories depend on the specific application, refer to the &apos;logging level&apos; command. Optionally add individual log levels like &apos;abc,1:mno,3:xyz,5&apos;, where the level numbers are LOGL_DEBUG=1 LOGL_INFO=3 LOGL_NOTICE=5 LOGL_ERROR=7 LOGL_FATAL=8' />
      </params>
    </command>
    <command id='logging level (smlc|ref|lb|lcs|lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns) (debug|info|notice|error|fatal)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='level' doc='Set the log level for a specified category' />
        <param name='smlc' doc='Serving Mobile Location Center' />
        <param name='ref' doc='Reference Counting' />
        <param name='lb' doc='Lb interface' />
        <param name='lcs' doc='Location Services' />
        <param name='lglobal' doc='Library-internal global log family' />
        <param name='llapd' doc='LAPD in libosmogsm' />
        <param name='linp' doc='A-bis Intput Subsystem' />
        <param name='lmux' doc='A-bis B-Subchannel TRAU Frame Multiplex' />
        <param name='lmi' doc='A-bis Input Driver for Signalling' />
        <param name='lmib' doc='A-bis Input Driver for B-Channels (voice)' />
        <param name='lsms' doc='Layer3 Short Message Service (SMS)' />
        <param name='lctrl' doc='Control Interface' />
        <param name='lgtp' doc='GPRS GTP library' />
        <param name='lstats' doc='Statistics messages and logging' />
        <param name='lgsup' doc='Generic Subscriber Update Protocol' />
        <param name='loap' doc='Osmocom Authentication Protocol' />
        <param name='lss7' doc='libosmo-sigtran Signalling System 7' />
        <param name='lsccp' doc='libosmo-sigtran SCCP Implementation' />
        <param name='lsua' doc='libosmo-sigtran SCCP User Adaptation' />
        <param name='lm3ua' doc='libosmo-sigtran MTP3 User Adaptation' />
        <param name='lmgcp' doc='libosmo-mgcp Media Gateway Control Protocol' />
        <param name='ljibuf' doc='libosmo-netif Jitter Buffer' />
        <param name='lrspro' doc='Remote SIM protocol' />
        <param name='lns' doc='GPRS NS layer' />
        <param name='debug' doc='Log debug messages and higher levels' />
        <param name='info' doc='Log informational messages and higher levels' />
        <param name='notice' doc='Log noticeable messages and higher levels' />
        <param name='error' doc='Log error messages and higher levels' />
        <param name='fatal' doc='Log only fatal messages' />
      </params>
    </command>
    <command id='logging level set-all (debug|info|notice|error|fatal)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='level' doc='Set the log level for a specified category' />
        <param name='set-all' doc='Once-off set all categories to the given log level. There is no single command to take back these changes -- each category is set to the given level, period.' />
        <param name='debug' doc='Log debug messages and higher levels' />
        <param name='info' doc='Log informational messages and higher levels' />
        <param name='notice' doc='Log noticeable messages and higher levels' />
        <param name='error' doc='Log error messages and higher levels' />
        <param name='fatal' doc='Log only fatal messages' />
      </params>
    </command>
    <command id='logging level force-all (debug|info|notice|error|fatal)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='level' doc='Set the log level for a specified category' />
        <param name='force-all' doc='Globally force all logging categories to a specific level. This is released by the &apos;no logging level force-all&apos; command. Note: any &apos;logging level &lt;category&gt; &lt;level&gt;&apos; commands will have no visible effect after this, until the forced level is released.' />
        <param name='debug' doc='Log debug messages and higher levels' />
        <param name='info' doc='Log informational messages and higher levels' />
        <param name='notice' doc='Log noticeable messages and higher levels' />
        <param name='error' doc='Log error messages and higher levels' />
        <param name='fatal' doc='Log only fatal messages' />
      </params>
    </command>
    <command id='no logging level force-all'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='logging' doc='Configure logging' />
        <param name='level' doc='Set the log level for a specified category' />
        <param name='force-all' doc='Release any globally forced log level set with &apos;logging level force-all &lt;level&gt;&apos;' />
      </params>
    </command>
    <command id='logp (smlc|ref|lb|lcs|lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns) (debug|info|notice|error|fatal) .LOGMESSAGE'>
      <params>
        <param name='logp' doc='Print a message on all log outputs; useful for placing markers in test logs' />
        <param name='smlc' doc='Serving Mobile Location Center' />
        <param name='ref' doc='Reference Counting' />
        <param name='lb' doc='Lb interface' />
        <param name='lcs' doc='Location Services' />
        <param name='lglobal' doc='Library-internal global log family' />
        <param name='llapd' doc='LAPD in libosmogsm' />
        <param name='linp' doc='A-bis Intput Subsystem' />
        <param name='lmux' doc='A-bis B-Subchannel TRAU Frame Multiplex' />
        <param name='lmi' doc='A-bis Input Driver for Signalling' />
        <param name='lmib' doc='A-bis Input Driver for B-Channels (voice)' />
        <param name='lsms' doc='Layer3 Short Message Service (SMS)' />
        <param name='lctrl' doc='Control Interface' />
        <param name='lgtp' doc='GPRS GTP library' />
        <param name='lstats' doc='Statistics messages and logging' />
        <param name='lgsup' doc='Generic Subscriber Update Protocol' />
        <param name='loap' doc='Osmocom Authentication Protocol' />
        <param name='lss7' doc='libosmo-sigtran Signalling System 7' />
        <param name='lsccp' doc='libosmo-sigtran SCCP Implementation' />
        <param name='lsua' doc='libosmo-sigtran SCCP User Adaptation' />
        <param name='lm3ua' doc='libosmo-sigtran MTP3 User Adaptation' />
        <param name='lmgcp' doc='libosmo-mgcp Media Gateway Control Protocol' />
        <param name='ljibuf' doc='libosmo-netif Jitter Buffer' />
        <param name='lrspro' doc='Remote SIM protocol' />
        <param name='lns' doc='GPRS NS layer' />
        <param name='debug' doc='Log debug messages and higher levels' />
        <param name='info' doc='Log informational messages and higher levels' />
        <param name='notice' doc='Log noticeable messages and higher levels' />
        <param name='error' doc='Log error messages and higher levels' />
        <param name='fatal' doc='Log only fatal messages' />
        <param name='.LOGMESSAGE' doc='Arbitrary message to log on given category and log level' />
      </params>
    </command>
    <command id='show logging vty'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='logging' doc='Show current logging configuration' />
        <param name='vty' doc='Show current logging configuration for this vty' />
      </params>
    </command>
    <command id='show alarms'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='alarms' doc='Show current logging configuration' />
      </params>
    </command>
    <command id='show talloc-context (application|all) (full|brief|DEPTH)'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='talloc-context' doc='Show talloc memory hierarchy' />
        <param name='application' doc='Application&apos;s context' />
        <param name='all' doc='All contexts, if NULL-context tracking is enabled' />
        <param name='full' doc='Display a full talloc memory hierarchy' />
        <param name='brief' doc='Display a brief talloc memory hierarchy' />
        <param name='DEPTH' doc='Specify required maximal depth value' />
      </params>
    </command>
    <command id='show talloc-context (application|all) (full|brief|DEPTH) tree ADDRESS'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='talloc-context' doc='Show talloc memory hierarchy' />
        <param name='application' doc='Application&apos;s context' />
        <param name='all' doc='All contexts, if NULL-context tracking is enabled' />
        <param name='full' doc='Display a full talloc memory hierarchy' />
        <param name='brief' doc='Display a brief talloc memory hierarchy' />
        <param name='DEPTH' doc='Specify required maximal depth value' />
        <param name='tree' doc='Display only a specific memory chunk' />
        <param name='ADDRESS' doc='Chunk address (e.g. 0xdeadbeef)' />
      </params>
    </command>
    <command id='show talloc-context (application|all) (full|brief|DEPTH) filter REGEXP'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='talloc-context' doc='Show talloc memory hierarchy' />
        <param name='application' doc='Application&apos;s context' />
        <param name='all' doc='All contexts, if NULL-context tracking is enabled' />
        <param name='full' doc='Display a full talloc memory hierarchy' />
        <param name='brief' doc='Display a brief talloc memory hierarchy' />
        <param name='DEPTH' doc='Specify required maximal depth value' />
        <param name='filter' doc='Filter chunks using regular expression' />
        <param name='REGEXP' doc='Regular expression' />
      </params>
    </command>
    <command id='show cells'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cells' doc='Show configured cell locations' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; users'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='users' doc='User Table' />
      </params>
    </command>
    <command id='show cs7 (sua|m3ua|ipa) [&lt;0-65534&gt;]'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='sua' doc='SCCP User Adaptation' />
        <param name='m3ua' doc='MTP3 User Adaptation' />
        <param name='ipa' doc='IPA Multiplex (SCCP Lite)' />
        <param name='[&lt;0-65534&gt;]' doc='Port Number' />
      </params>
    </command>
    <command id='show cs7 config'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='config' doc='Currently running cs7 configuration' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; asp'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='asp' doc='Application Server Process (ASP)' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; as (active|all|m3ua|sua)'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='as' doc='Application Server (AS)' />
        <param name='active' doc='Display all active ASs' />
        <param name='all' doc='Display all ASs (default)' />
        <param name='m3ua' doc='Display all m3ua ASs' />
        <param name='sua' doc='Display all SUA ASs' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; sccp addressbook'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='sccp' doc='Signalling Connection Control Part' />
        <param name='addressbook' doc='List all SCCP addressbook entries' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; sccp users'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='sccp' doc='Signalling Connection Control Part' />
        <param name='users' doc='Show List of SCCP Users registered' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; sccp ssn &lt;0-65535&gt;'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='sccp' doc='Signalling Connection Control Part' />
        <param name='ssn' doc='Find an SCCP User registered for the given SSN' />
        <param name='&lt;0-65535&gt;' doc='Subsystem Number (SSN)' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; sccp connections'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='sccp' doc='Signalling Connection Control Part' />
        <param name='connections' doc='Show List of active SCCP connections' />
      </params>
    </command>
    <command id='show cs7 instance &lt;0-15&gt; sccp timers'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='An instance of the SS7 stack' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
        <param name='sccp' doc='Signaling Connection Control Part' />
        <param name='timers' doc='Show List of SCCP timers' />
      </params>
    </command>
  </node>
  <node id='config'>
    <name>config</name>
    <command id='hostname WORD'>
      <params>
        <param name='hostname' doc='Set system&apos;s network name' />
        <param name='WORD' doc='This system&apos;s network name' />
      </params>
    </command>
    <command id='no hostname [HOSTNAME]'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='hostname' doc='Reset system&apos;s network name' />
        <param name='[HOSTNAME]' doc='Host name of this router' />
      </params>
    </command>
    <command id='password (8|) WORD'>
      <params>
        <param name='password' doc='Assign the terminal connection password' />
        <param name='8' doc='Specifies a HIDDEN password will follow' />
        <param name='' doc='dummy string ' />
        <param name='WORD' doc='The HIDDEN line password string' />
      </params>
    </command>
    <command id='password LINE'>
      <params>
        <param name='password' doc='Assign the terminal connection password' />
        <param name='LINE' doc='The UNENCRYPTED (cleartext) line password' />
      </params>
    </command>
    <command id='enable password (8|) WORD'>
      <params>
        <param name='enable' doc='Modify enable password parameters' />
        <param name='password' doc='Assign the privileged level password' />
        <param name='8' doc='Specifies a HIDDEN password will follow' />
        <param name='' doc='dummy string ' />
        <param name='WORD' doc='The HIDDEN &apos;enable&apos; password string' />
      </params>
    </command>
    <command id='enable password LINE'>
      <params>
        <param name='enable' doc='Modify enable password parameters' />
        <param name='password' doc='Assign the privileged level password' />
        <param name='LINE' doc='The UNENCRYPTED (cleartext) &apos;enable&apos; password' />
      </params>
    </command>
    <command id='no enable password'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='enable' doc='Modify enable password parameters' />
        <param name='password' doc='Assign the privileged level password' />
      </params>
    </command>
    <command id='banner motd default'>
      <params>
        <param name='banner' doc='Set banner string' />
        <param name='motd' doc='Strings for motd' />
        <param name='default' doc='Default string' />
      </params>
    </command>
    <command id='banner motd file [FILE]'>
      <params>
        <param name='banner' doc='Set banner' />
        <param name='motd' doc='Banner for motd' />
        <param name='file' doc='Banner from a file' />
        <param name='[FILE]' doc='Filename' />
      </params>
    </command>
    <command id='no banner motd'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='banner' doc='Set banner string' />
        <param name='motd' doc='Strings for motd' />
      </params>
    </command>
    <command id='service terminal-length &lt;0-512&gt;'>
      <params>
        <param name='service' doc='Set up miscellaneous service' />
        <param name='terminal-length' doc='System wide terminal length configuration' />
        <param name='&lt;0-512&gt;' doc='Number of lines of VTY (0 means no line control)' />
      </params>
    </command>
    <command id='no service terminal-length [&lt;0-512&gt;]'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='service' doc='Set up miscellaneous service' />
        <param name='terminal-length' doc='System wide terminal length configuration' />
        <param name='[&lt;0-512&gt;]' doc='Number of lines of VTY (0 means no line control)' />
      </params>
    </command>
    <command id='line vty'>
      <params>
        <param name='line' doc='Configure a terminal line' />
        <param name='vty' doc='Virtual terminal' />
      </params>
    </command>
    <command id='service advanced-vty'>
      <params>
        <param name='service' doc='Set up miscellaneous service' />
        <param name='advanced-vty' doc='Enable advanced mode vty interface' />
      </params>
    </command>
    <command id='no service advanced-vty'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='service' doc='Set up miscellaneous service' />
        <param name='advanced-vty' doc='Enable advanced mode vty interface' />
      </params>
    </command>
    <command id='show history'>
      <params>
        <param name='show' doc='Show running system information' />
        <param name='history' doc='Display the session command history' />
      </params>
    </command>
    <command id='log stderr [blocking-io]'>
      <params>
        <param name='log' doc='Configure logging sub-system' />
        <param name='stderr' doc='Logging via STDERR of the process' />
        <param name='[blocking-io]' doc='Use blocking, synchronous I/O' />
      </params>
    </command>
    <command id='no log stderr'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='log' doc='Configure logging sub-system' />
        <param name='stderr' doc='Logging via STDERR of the process' />
      </params>
    </command>
    <command id='log file FILENAME [blocking-io]'>
      <params>
        <param name='log' doc='Configure logging sub-system' />
        <param name='file' doc='Logging to text file' />
        <param name='FILENAME' doc='Filename' />
        <param name='[blocking-io]' doc='Use blocking, synchronous I/O' />
      </params>
    </command>
    <command id='no log file FILENAME'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='log' doc='Configure logging sub-system' />
        <param name='file' doc='Logging to text file' />
        <param name='FILENAME' doc='Filename' />
      </params>
    </command>
    <command id='log alarms &lt;2-32700&gt;'>
      <params>
        <param name='log' doc='Configure logging sub-system' />
        <param name='alarms' doc='Logging alarms to osmo_strrb' />
        <param name='&lt;2-32700&gt;' doc='Maximum number of messages to log' />
      </params>
    </command>
    <command id='no log alarms'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='log' doc='Configure logging sub-system' />
        <param name='alarms' doc='Logging alarms to osmo_strrb' />
      </params>
    </command>
    <command id='log syslog (authpriv|cron|daemon|ftp|lpr|mail|news|user|uucp)'>
      <params>
        <param name='log' doc='Configure logging sub-system' />
        <param name='syslog' doc='Logging via syslog' />
        <param name='authpriv' doc='Security/authorization messages facility' />
        <param name='cron' doc='Clock daemon (cron/at) facility' />
        <param name='daemon' doc='General system daemon facility' />
        <param name='ftp' doc='Ftp daemon facility' />
        <param name='lpr' doc='Line printer facility' />
        <param name='mail' doc='Mail facility' />
        <param name='news' doc='News facility' />
        <param name='user' doc='Generic facility' />
        <param name='uucp' doc='UUCP facility' />
      </params>
    </command>
    <command id='log syslog local &lt;0-7&gt;'>
      <params>
        <param name='log' doc='Configure logging sub-system' />
        <param name='syslog' doc='Logging via syslog' />
        <param name='local' doc='Syslog LOCAL facility' />
        <param name='&lt;0-7&gt;' doc='Local facility number' />
      </params>
    </command>
    <command id='no log syslog'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='log' doc='Configure logging sub-system' />
        <param name='syslog' doc='Logging via syslog' />
      </params>
    </command>
    <command id='log systemd-journal [raw]'>
      <params>
        <param name='log' doc='Configure logging sub-system' />
        <param name='systemd-journal' doc='Logging to systemd-journal' />
        <param name='[raw]' doc='Offload rendering of the meta information (location, category) to systemd' />
      </params>
    </command>
    <command id='no log systemd-journal'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='log' doc='Configure logging sub-system' />
        <param name='systemd-journal' doc='Logging to systemd-journal' />
      </params>
    </command>
    <command id='log gsmtap [HOSTNAME]'>
      <params>
        <param name='log' doc='Configure logging sub-system' />
        <param name='gsmtap' doc='Logging via GSMTAP' />
        <param name='[HOSTNAME]' doc='Host name to send the GSMTAP logging to (UDP port 4729)' />
      </params>
    </command>
    <command id='ctrl'>
      <params>
        <param name='ctrl' doc='Configure the Control Interface' />
      </params>
    </command>
    <command id='cells'>
      <params>
        <param name='cells' doc='Configure cell locations' />
      </params>
    </command>
    <command id='cs7 instance &lt;0-15&gt;'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='cs7' doc='ITU-T Signaling System 7' />
        <param name='instance' doc='Configure a SS7 Instance' />
        <param name='&lt;0-15&gt;' doc='An instance of the SS7 stack' />
      </params>
    </command>
  </node>
  <node id='config-log'>
    <name>config-log</name>
    <command id='logging filter all (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='filter' doc='Filter log messages' />
        <param name='all' doc='Do you want to log all messages?' />
        <param name='0' doc='Only print messages matched by other filters' />
        <param name='1' doc='Bypass filter and print all messages' />
      </params>
    </command>
    <command id='logging color (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='color' doc='Configure color-printing for log messages' />
        <param name='0' doc='Don&apos;t use color for printing messages' />
        <param name='1' doc='Use color for printing messages' />
      </params>
    </command>
    <command id='logging timestamp (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='timestamp' doc='Configure log message timestamping' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with current timestamp' />
      </params>
    </command>
    <command id='logging print extended-timestamp (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='extended-timestamp' doc='Configure log message timestamping' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with current timestamp with YYYYMMDDhhmmssnnn' />
      </params>
    </command>
    <command id='logging print category (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='category' doc='Configure log message' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with category/subsystem name' />
      </params>
    </command>
    <command id='logging print category-hex (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='category-hex' doc='Configure log message' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with category/subsystem nr in hex (&apos;&lt;000b&gt;&apos;)' />
      </params>
    </command>
    <command id='logging print level (0|1)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='level' doc='Configure log message' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with the log level name' />
      </params>
    </command>
    <command id='logging print file (0|1|basename) [last]'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='print' doc='Log output settings' />
        <param name='file' doc='Configure log message' />
        <param name='0' doc='Don&apos;t prefix each log message' />
        <param name='1' doc='Prefix each log message with the source file and line' />
        <param name='basename' doc='Prefix each log message with the source file&apos;s basename (strip leading paths) and line' />
        <param name='[last]' doc='Log source file info at the end of a log line. If omitted, log source file info just before the log text.' />
      </params>
    </command>
    <command id='logging level (smlc|ref|lb|lcs|lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns) (debug|info|notice|error|fatal)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='level' doc='Set the log level for a specified category' />
        <param name='smlc' doc='Serving Mobile Location Center' />
        <param name='ref' doc='Reference Counting' />
        <param name='lb' doc='Lb interface' />
        <param name='lcs' doc='Location Services' />
        <param name='lglobal' doc='Library-internal global log family' />
        <param name='llapd' doc='LAPD in libosmogsm' />
        <param name='linp' doc='A-bis Intput Subsystem' />
        <param name='lmux' doc='A-bis B-Subchannel TRAU Frame Multiplex' />
        <param name='lmi' doc='A-bis Input Driver for Signalling' />
        <param name='lmib' doc='A-bis Input Driver for B-Channels (voice)' />
        <param name='lsms' doc='Layer3 Short Message Service (SMS)' />
        <param name='lctrl' doc='Control Interface' />
        <param name='lgtp' doc='GPRS GTP library' />
        <param name='lstats' doc='Statistics messages and logging' />
        <param name='lgsup' doc='Generic Subscriber Update Protocol' />
        <param name='loap' doc='Osmocom Authentication Protocol' />
        <param name='lss7' doc='libosmo-sigtran Signalling System 7' />
        <param name='lsccp' doc='libosmo-sigtran SCCP Implementation' />
        <param name='lsua' doc='libosmo-sigtran SCCP User Adaptation' />
        <param name='lm3ua' doc='libosmo-sigtran MTP3 User Adaptation' />
        <param name='lmgcp' doc='libosmo-mgcp Media Gateway Control Protocol' />
        <param name='ljibuf' doc='libosmo-netif Jitter Buffer' />
        <param name='lrspro' doc='Remote SIM protocol' />
        <param name='lns' doc='GPRS NS layer' />
        <param name='debug' doc='Log debug messages and higher levels' />
        <param name='info' doc='Log informational messages and higher levels' />
        <param name='notice' doc='Log noticeable messages and higher levels' />
        <param name='error' doc='Log error messages and higher levels' />
        <param name='fatal' doc='Log only fatal messages' />
      </params>
    </command>
    <command id='logging level set-all (debug|info|notice|error|fatal)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='level' doc='Set the log level for a specified category' />
        <param name='set-all' doc='Once-off set all categories to the given log level. There is no single command to take back these changes -- each category is set to the given level, period.' />
        <param name='debug' doc='Log debug messages and higher levels' />
        <param name='info' doc='Log informational messages and higher levels' />
        <param name='notice' doc='Log noticeable messages and higher levels' />
        <param name='error' doc='Log error messages and higher levels' />
        <param name='fatal' doc='Log only fatal messages' />
      </params>
    </command>
    <command id='logging level force-all (debug|info|notice|error|fatal)'>
      <params>
        <param name='logging' doc='Configure logging' />
        <param name='level' doc='Set the log level for a specified category' />
        <param name='force-all' doc='Globally force all logging categories to a specific level. This is released by the &apos;no logging level force-all&apos; command. Note: any &apos;logging level &lt;category&gt; &lt;level&gt;&apos; commands will have no visible effect after this, until the forced level is released.' />
        <param name='debug' doc='Log debug messages and higher levels' />
        <param name='info' doc='Log informational messages and higher levels' />
        <param name='notice' doc='Log noticeable messages and higher levels' />
        <param name='error' doc='Log error messages and higher levels' />
        <param name='fatal' doc='Log only fatal messages' />
      </params>
    </command>
    <command id='no logging level force-all'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='logging' doc='Configure logging' />
        <param name='level' doc='Set the log level for a specified category' />
        <param name='force-all' doc='Release any globally forced log level set with &apos;logging level force-all &lt;level&gt;&apos;' />
      </params>
    </command>
  </node>
  <node id='config-line'>
    <name>config-line</name>
    <command id='login'>
      <params>
        <param name='login' doc='Enable password checking' />
      </params>
    </command>
    <command id='no login'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='login' doc='Enable password checking' />
      </params>
    </command>
    <command id='bind A.B.C.D [&lt;0-65535&gt;]'>
      <params>
        <param name='bind' doc='Accept VTY telnet connections on local interface' />
        <param name='A.B.C.D' doc='Local interface IP address (default: 127.0.0.1)' />
        <param name='[&lt;0-65535&gt;]' doc='Local TCP port number' />
      </params>
    </command>
  </node>
  <node id='config-ctrl'>
    <name>config-ctrl</name>
    <command id='bind A.B.C.D'>
      <params>
        <param name='bind' doc='Set bind address to listen for Control connections' />
        <param name='A.B.C.D' doc='Local IP address (default 127.0.0.1)' />
      </params>
    </command>
  </node>
  <node id='config-cs7'>
    <name>config-cs7</name>
    <command id='description .TEXT'>
      <params>
        <param name='description' doc='Save human-readable description of the object' />
        <param name='.TEXT' doc='Text until the end of the line' />
      </params>
    </command>
    <command id='network-indicator (international | national | reserved | spare)'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='network-indicator' doc='Configure the Network Indicator' />
        <param name='international' doc='International Network' />
        <param name='national' doc='National Network' />
        <param name='reserved' doc='Reserved Network' />
        <param name='spare' doc='Spare Network' />
      </params>
    </command>
    <command id='point-code POINT_CODE'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='point-code' doc='Configure the local Point Code' />
        <param name='POINT_CODE' doc='Point Code' />
      </params>
    </command>
    <command id='point-code format &lt;1-24&gt; [&lt;1-23&gt;] [&lt;1-22&gt;]'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='point-code' doc='Point Code' />
        <param name='format' doc='Configure Point Code Format' />
        <param name='&lt;1-24&gt;' doc='Length of first PC component' />
        <param name='[&lt;1-23&gt;]' doc='Length of second PC component' />
        <param name='[&lt;1-22&gt;]' doc='Length of third PC component' />
      </params>
    </command>
    <command id='point-code format default'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='point-code' doc='Point Code' />
        <param name='format' doc='Configure Point Code Format' />
        <param name='default' doc='Default Point Code Format (3.8.3)' />
      </params>
    </command>
    <command id='point-code delimiter (default|dash)'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='point-code' doc='Point Code' />
        <param name='delimiter' doc='Configure Point Code Delimiter' />
        <param name='default' doc='Use dot as delimiter' />
        <param name='dash' doc='User dash as delimiter' />
      </params>
    </command>
    <command id='xua rkm routing-key-allocation (static-only|dynamic-permitted)'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='xua' doc='SIGTRAN xxxUA related' />
        <param name='rkm' doc='Routing Key Management' />
        <param name='routing-key-allocation' doc='Routing Key Management Allocation Policy' />
        <param name='static-only' doc='Only static (pre-confgured) Routing Keys permitted' />
        <param name='dynamic-permitted' doc='Dynamically allocate Routing Keys for what ASPs request' />
      </params>
    </command>
    <command id='asp NAME &lt;0-65535&gt; &lt;0-65535&gt; (sua|m3ua|ipa)'>
      <attributes scope='global'>
        <attribute doc='This command applies on VTY node exit' flag='@' />
      </attributes>
      <params>
        <param name='asp' doc='Configure Application Server Process' />
        <param name='NAME' doc='Name of ASP' />
        <param name='&lt;0-65535&gt;' doc='Remote SCTP port number' />
        <param name='&lt;0-65535&gt;' doc='Local SCTP port number' />
        <param name='sua' doc='SCCP User Adaptation' />
        <param name='m3ua' doc='MTP3 User Adaptation' />
        <param name='ipa' doc='IPA Multiplex (SCCP Lite)' />
      </params>
    </command>
    <command id='no asp NAME'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='asp' doc='Disable Application Server Process' />
        <param name='NAME' doc='Name of ASP' />
      </params>
    </command>
    <command id='as NAME (sua|m3ua|ipa)'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='as' doc='Configure an Application Server' />
        <param name='NAME' doc='Name of the Application Server' />
        <param name='sua' doc='SCCP User Adaptation' />
        <param name='m3ua' doc='MTP3 User Adaptation' />
        <param name='ipa' doc='IPA Multiplex (SCCP Lite)' />
      </params>
    </command>
    <command id='no as NAME'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='as' doc='Disable Application Server' />
        <param name='NAME' doc='Name of AS' />
      </params>
    </command>
    <command id='sccp-address NAME'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='sccp-address' doc='Create/Modify an SCCP addressbook entry' />
        <param name='NAME' doc='Name of the SCCP Address' />
      </params>
    </command>
    <command id='no sccp-address NAME'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='sccp-address' doc='Delete an SCCP addressbook entry' />
        <param name='NAME' doc='Name of the SCCP Address' />
      </params>
    </command>
    <command id='sccp-timer (conn_est|ias|iar|rel|repeat_rel|int|guard|reset|reassembly) &lt;1-999999&gt;'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='sccp-timer' doc='Configure SCCP timer values, see ITU-T Q.714' />
        <param name='conn_est' doc='Waiting for connection confirm message, 1 to 2 minutes (default: 60)' />
        <param name='ias' doc='Send keep-alive: on an idle connection, delay before sending an Idle Timer message, 5 to 10 minutes (default: 420)' />
        <param name='iar' doc='Receive keep-alive: on an idle connection, delay until considering a connection as stale, 11 to 21 minutes (default: 900)' />
        <param name='rel' doc='Waiting for release complete message, 10 to 20 seconds (default: 10)' />
        <param name='repeat_rel' doc='Waiting for release complete message; or to repeat sending released message after the initial expiry, 10 to 20 seconds (default: 10)' />
        <param name='int' doc='Waiting for release complete message; or to release connection resources, freeze the LRN and alert a maintenance function after the initial expiry, extending to 1 minute (default: 60)' />
        <param name='guard' doc='Waiting to resume normal procedure for temporary connection sections during the restart procedure, 23 to 25 minutes (default: 1380)' />
        <param name='reset' doc='Waiting to release temporary connection section or alert maintenance function after reset request message is sent, 10 to 20 seconds (default: 10)' />
        <param name='reassembly' doc='Waiting to receive all the segments of the remaining segments, single segmented message after receiving the first segment, 10 to 20 seconds (default: 10)' />
        <param name='&lt;1-999999&gt;' doc='Timer value, in seconds' />
      </params>
    </command>
  </node>
  <node id='config-cs7-as'>
    <name>config-cs7-as</name>
    <command id='description .TEXT'>
      <params>
        <param name='description' doc='Save human-readable description of the object' />
        <param name='.TEXT' doc='Text until the end of the line' />
      </params>
    </command>
    <command id='asp NAME'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='asp' doc='Specify that a given ASP is part of this AS' />
        <param name='NAME' doc='Name of ASP to be added to AS' />
      </params>
    </command>
    <command id='no asp NAME'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='asp' doc='Specify ASP to be removed from this AS' />
        <param name='NAME' doc='Name of ASP to be removed' />
      </params>
    </command>
    <command id='traffic-mode (broadcast | loadshare | roundrobin | override)'>
      <params>
        <param name='traffic-mode' doc='Specifies traffic mode of operation of the ASP within the AS' />
        <param name='broadcast' doc='Broadcast to all ASP within AS' />
        <param name='loadshare' doc='Share Load among all ASP within AS' />
        <param name='roundrobin' doc='Round-Robin between all ASP within AS' />
        <param name='override' doc='Override' />
      </params>
    </command>
    <command id='no traffic-mode'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='traffic-mode' doc='Remove explicit traffic mode of operation of this AS' />
      </params>
    </command>
    <command id='recovery-timeout &lt;1-2000&gt;'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='recovery-timeout' doc='Specifies the recovery timeout value in milliseconds' />
        <param name='&lt;1-2000&gt;' doc='Recovery Timeout in Milliseconds' />
      </params>
    </command>
    <command id='qos-class &lt;0-255&gt;'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='qos-class' doc='Specity QoS Class of AS' />
        <param name='&lt;0-255&gt;' doc='QoS Class of AS' />
      </params>
    </command>
    <command id='routing-key RCONTEXT DPC'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='routing-key' doc='Define a routing key' />
        <param name='RCONTEXT' doc='Routing context number' />
        <param name='DPC' doc='Destination Point Code' />
      </params>
    </command>
    <command id='routing-key RCONTEXT DPC si (aal2|bicc|b-isup|h248|isup|sat-isup|sccp|tup)'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='routing-key' doc='Define a routing key' />
        <param name='RCONTEXT' doc='Routing context number' />
        <param name='DPC' doc='Destination Point Code' />
        <param name='si' doc='Match on Service Indicator' />
        <param name='aal2' doc='ATM Adaption Layer 2' />
        <param name='bicc' doc='Bearer Independent Call Control' />
        <param name='b-isup' doc='Broadband ISDN User Part' />
        <param name='h248' doc='H.248' />
        <param name='isup' doc='ISDN User Part' />
        <param name='sat-isup' doc='Sattelite ISDN User Part' />
        <param name='sccp' doc='Signalling Connection Control Part' />
        <param name='tup' doc='Telephony User Part' />
      </params>
    </command>
    <command id='routing-key RCONTEXT DPC ssn SSN'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='routing-key' doc='Define a routing key' />
        <param name='RCONTEXT' doc='Routing context number' />
        <param name='DPC' doc='Destination Point Code' />
        <param name='ssn' doc='Match on Sub-System Number' />
        <param name='SSN' doc='Sub-System Number to match on' />
      </params>
    </command>
    <command id='routing-key RCONTEXT DPC si (aal2|bicc|b-isup|h248|isup|sat-isup|sccp|tup) ssn SSN'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='routing-key' doc='Define a routing key' />
        <param name='RCONTEXT' doc='Routing context number' />
        <param name='DPC' doc='Destination Point Code' />
        <param name='si' doc='Match on Service Indicator' />
        <param name='aal2' doc='ATM Adaption Layer 2' />
        <param name='bicc' doc='Bearer Independent Call Control' />
        <param name='b-isup' doc='Broadband ISDN User Part' />
        <param name='h248' doc='H.248' />
        <param name='isup' doc='ISDN User Part' />
        <param name='sat-isup' doc='Sattelite ISDN User Part' />
        <param name='sccp' doc='Signalling Connection Control Part' />
        <param name='tup' doc='Telephony User Part' />
        <param name='ssn' doc='Match on Sub-System Number' />
        <param name='SSN' doc='Sub-System Number to match on' />
      </params>
    </command>
    <command id='point-code override dpc PC'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='point-code' doc='Point Code Specific Features' />
        <param name='override' doc='Override (force) a point-code to hard-coded value' />
        <param name='dpc' doc='Override Source Point Code' />
        <param name='PC' doc='Override Destination Point Code' />
      </params>
    </command>
    <command id='point-code override patch-sccp (disabled|both)'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='point-code' doc='Point Code Specific Features' />
        <param name='override' doc='Override (force) a point-code to hard-coded value' />
        <param name='patch-sccp' doc='Patch point code values into SCCP called/calling address' />
        <param name='disabled' doc='Don&apos;t patch any point codes into SCCP called/calling address' />
        <param name='both' doc='Patch both origin and destination point codes into SCCP called/calling address' />
      </params>
    </command>
  </node>
  <node id='config-cs7-asp'>
    <name>config-cs7-asp</name>
    <command id='description .TEXT'>
      <params>
        <param name='description' doc='Save human-readable description of the object' />
        <param name='.TEXT' doc='Text until the end of the line' />
      </params>
    </command>
    <command id='remote-ip (A.B.C.D|X:X::X:X)'>
      <attributes scope='global'>
        <attribute doc='This command applies on VTY node exit' flag='@' />
      </attributes>
      <params>
        <param name='remote-ip' doc='Specify Remote IP Address of ASP' />
        <param name='A.B.C.D' doc='Remote IPv4 Address of ASP' />
        <param name='X:X::X:X' doc='Remote IPv6 Address of ASP' />
      </params>
    </command>
    <command id='local-ip (A.B.C.D|X:X::X:X)'>
      <attributes scope='global'>
        <attribute doc='This command applies on VTY node exit' flag='@' />
      </attributes>
      <params>
        <param name='local-ip' doc='Specify Local IP Address from which to contact ASP' />
        <param name='A.B.C.D' doc='Local IPv4 Address from which to contact of ASP' />
        <param name='X:X::X:X' doc='Local IPv6 Address from which to contact of ASP' />
      </params>
    </command>
    <command id='qos-class &lt;0-255&gt;'>
      <attributes scope='global'>
        <attribute doc='This command applies on VTY node exit' flag='@' />
      </attributes>
      <params>
        <param name='qos-class' doc='Specify QoS Class of ASP' />
        <param name='&lt;0-255&gt;' doc='QoS Class of ASP' />
      </params>
    </command>
    <command id='role (sg|asp|ipsp)'>
      <attributes scope='global'>
        <attribute doc='This command applies on VTY node exit' flag='@' />
      </attributes>
      <params>
        <param name='role' doc='Specify the xUA role for this ASP' />
        <param name='sg' doc='SG (Signaling Gateway)' />
        <param name='asp' doc='ASP (Application Server Process)' />
        <param name='ipsp' doc='IPSP (IP Signalling Point)' />
      </params>
    </command>
    <command id='sctp-role (client|server)'>
      <attributes scope='global'>
        <attribute doc='This command applies on VTY node exit' flag='@' />
      </attributes>
      <params>
        <param name='sctp-role' doc='Specify the SCTP role for this ASP' />
        <param name='client' doc='Operate as SCTP client; connect to a server' />
        <param name='server' doc='Operate as SCTP server; wait for client connections' />
      </params>
    </command>
    <command id='block'>
      <attributes scope='global'>
        <attribute doc='This command applies on VTY node exit' flag='@' />
      </attributes>
      <params>
        <param name='block' doc='Allows a SCTP Association with ASP, but doesn&apos;t let it become active' />
      </params>
    </command>
    <command id='shutdown'>
      <attributes scope='global'>
        <attribute doc='This command applies on VTY node exit' flag='@' />
      </attributes>
      <params>
        <param name='shutdown' doc='Terminates SCTP association; New associations will be rejected' />
      </params>
    </command>
  </node>
  <node id='config-cs7-sccpaddr'>
    <name>config-cs7-sccpaddr</name>
    <command id='no point-code'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='point-code' doc='Remove point-code Number' />
      </params>
    </command>
    <command id='no subsystem-number'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='subsystem-number' doc='Remove Subsystem Number' />
      </params>
    </command>
    <command id='no global-title'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='global-title' doc='Remove Global Title' />
      </params>
    </command>
    <command id='routing-indicator (GT|PC|IP)'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='routing-indicator' doc='Add Routing Indicator' />
        <param name='GT' doc='by global-title' />
        <param name='PC' doc='by point-code' />
        <param name='IP' doc='by ip-address' />
      </params>
    </command>
    <command id='point-code POINT_CODE'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='point-code' doc='Add point-code Number' />
        <param name='POINT_CODE' doc='PC' />
      </params>
    </command>
    <command id='subsystem-number &lt;0-4294967295&gt;'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='subsystem-number' doc='Add Subsystem Number' />
        <param name='&lt;0-4294967295&gt;' doc='SSN' />
      </params>
    </command>
    <command id='global-title'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='global-title' doc='Add/Modify Global Title' />
      </params>
    </command>
  </node>
  <node id='config-cs7-sccpaddr-gt'>
    <name>config-cs7-sccpaddr-gt</name>
    <command id='global-title-indicator &lt;0-15&gt;'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='global-title-indicator' doc='Set Global Title Indicator' />
        <param name='&lt;0-15&gt;' doc='GTI' />
      </params>
    </command>
    <command id='translation-type &lt;0-255&gt;'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='translation-type' doc='Set Global Title Translation Type' />
        <param name='&lt;0-255&gt;' doc='TT' />
      </params>
    </command>
    <command id='numbering-plan-indicator &lt;0-15&gt;'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='numbering-plan-indicator' doc='Set Global Title Numbering Plan Indicator' />
        <param name='&lt;0-15&gt;' doc='NPI' />
      </params>
    </command>
    <command id='nature-of-address-indicator &lt;0-127&gt;'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='nature-of-address-indicator' doc='Set Global Title Nature of Address Indicator' />
        <param name='&lt;0-127&gt;' doc='NAI' />
      </params>
    </command>
    <command id='digits DIGITS'>
      <attributes scope='global'>
        <attribute doc='This command applies immediately' flag='!' />
      </attributes>
      <params>
        <param name='digits' doc='Set Global Title Digits' />
        <param name='DIGITS' doc='Number digits' />
      </params>
    </command>
  </node>
  <node id='config-cells'>
    <name>config-cells</name>
    <command id='lac-ci &lt;0-65535&gt; &lt;0-65535&gt; lat LATITUDE lon LONGITUDE'>
      <params>
        <param name='lac-ci' doc='Cell location by LAC and CI' />
        <param name='&lt;0-65535&gt;' doc='LAC' />
        <param name='&lt;0-65535&gt;' doc='CI' />
        <param name='lat' doc='Global latitute coordinate' />
        <param name='LATITUDE' doc='Latitude floating-point number, -90.0 (S) to 90.0 (N)' />
        <param name='lon' doc='Global longitude coordinate' />
        <param name='LONGITUDE' doc='Longitude as floating-point number, -180.0 (W) to 180.0 (E)' />
      </params>
    </command>
    <command id='no lac-ci &lt;0-65535&gt; &lt;0-65535&gt;'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='lac-ci' doc='Remove Cell location by LAC and CI' />
        <param name='&lt;0-65535&gt;' doc='LAC' />
        <param name='&lt;0-65535&gt;' doc='CI' />
      </params>
    </command>
    <command id='cgi &lt;0-999&gt; &lt;0-999&gt; &lt;0-65535&gt; &lt;0-65535&gt; lat LATITUDE lon LONGITUDE'>
      <params>
        <param name='cgi' doc='Cell location by Cell-Global ID' />
        <param name='&lt;0-999&gt;' doc='MCC' />
        <param name='&lt;0-999&gt;' doc='MNC' />
        <param name='&lt;0-65535&gt;' doc='LAC' />
        <param name='&lt;0-65535&gt;' doc='CI' />
        <param name='lat' doc='Global latitute coordinate' />
        <param name='LATITUDE' doc='Latitude floating-point number, -90.0 (S) to 90.0 (N)' />
        <param name='lon' doc='Global longitude coordinate' />
        <param name='LONGITUDE' doc='Longitude as floating-point number, -180.0 (W) to 180.0 (E)' />
      </params>
    </command>
    <command id='no cgi &lt;0-999&gt; &lt;0-999&gt; &lt;0-65535&gt; &lt;0-65535&gt;'>
      <params>
        <param name='no' doc='Negate a command or set its defaults' />
        <param name='cgi' doc='Remove Cell location by Cell-Global ID' />
        <param name='&lt;0-999&gt;' doc='MCC' />
        <param name='&lt;0-999&gt;' doc='MNC' />
        <param name='&lt;0-65535&gt;' doc='LAC' />
        <param name='&lt;0-65535&gt;' doc='CI' />
      </params>
    </command>
  </node>
</vtydoc>
