09:32:47.725780 13891 C5G_Tests.ttcn:629 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-start.sh C5G_Tests.TC_ue_service_request_cm_idle_unknown_sess_active'.
09:32:48.771415 13891 C5G_Tests.ttcn:629 External command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-start.sh C5G_Tests.TC_ue_service_request_cm_idle_unknown_sess_active' was executed successfully (exit status: 0).
09:32:48.771677 13891 C5G_Tests.ttcn:629 Test case TC_ue_service_request_cm_idle_unknown_sess_active started.
09:32:48.771752 13891 C5G_Tests.ttcn:629 Initializing variables, timers and ports of component type C5G_Tests.MTC_CT inside testcase TC_ue_service_request_cm_idle_unknown_sess_active.
09:32:48.771859 13891 C5G_Tests.ttcn:629 Port NGAP_UNIT[0] was started.
09:32:48.771913 13891 C5G_Tests.ttcn:629 Port NGAP_UNIT[1] was started.
09:32:48.771960 13891 C5G_Tests.ttcn:629 Port NGAP_PROC[0] was started.
09:32:48.772006 13891 C5G_Tests.ttcn:629 Port NGAP_PROC[1] was started.
09:32:48.772052 13891 C5G_Tests.ttcn:629 Port TEID0 was started.
09:32:48.772098 13891 C5G_Tests.ttcn:629 Component type C5G_Tests.MTC_CT was initialized.
09:32:48.772150 13891 C5G_Tests.ttcn:197 Start timer g_Tguard: 30 s
09:32:48.772211 13891 C5G_Tests.ttcn:198 Altstep as_Tguard was activated as default, id 1
09:32:48.772267 13891 C5G_Tests.ttcn:189 Creating new PTC with component type GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM.
09:32:48.781602 18648 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:32:48.781819 18648 - TTCN-3 Parallel Test Component started on 6eab31b835ad. Component reference: GTP1U_EM(837), component type: GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM. Version: 11.1.0.
09:32:48.781894 18648 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:32:48.782037 18648 - Connected to MC.
09:32:48.782101 18648 - Initializing variables, timers and ports of component type GTPv1U_Emulation.GTPv1U_Emulation_CT inside testcase TC_ue_service_request_cm_idle_unknown_sess_active.
09:32:48.782287 13891 C5G_Tests.ttcn:189 PTC was created. Component reference: 837, alive: no, type: GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM.
09:32:48.782348 13891 C5G_Tests.ttcn:190 Mapping port GTP1U_EM(837):GTP1U to system:GTP1U.
09:32:48.785794 18648 - Port GTP1U was started.
09:32:48.785890 18648 - Port TEID0 was started.
09:32:48.785937 18648 - Port CLIENT was started.
09:32:48.785983 18648 - Port CLIENT_PROC was started.
09:32:48.786028 18648 - Port UECUPS was started.
09:32:48.786072 18648 - Component type GTPv1U_Emulation.GTPv1U_Emulation_CT was initialized.
09:32:48.786213 18648 - Port GTP1U was mapped to system:GTP1U.
09:32:48.786475 13891 C5G_Tests.ttcn:190 Map operation of GTP1U_EM(837):GTP1U to system:GTP1U finished.
09:32:48.786536 13891 C5G_Tests.ttcn:191 Connecting ports GTP1U_EM(837):TEID0 and mtc:TEID0.
09:32:48.787231 13891 C5G_Tests.ttcn:191 Port TEID0 is waiting for connection from GTP1U_EM(837):TEID0 on UNIX pathname /tmp/ttcn3-portconn-8c6ca674.
09:32:48.787424 18648 - Port TEID0 has established the connection with mtc:TEID0 using transport type UNIX.
09:32:48.787540 13891 C5G_Tests.ttcn:191 Port TEID0 has accepted the connection from GTP1U_EM(837):TEID0.
09:32:48.787637 13891 C5G_Tests.ttcn:191 Connect operation on GTP1U_EM(837):TEID0 and mtc:TEID0 finished.
09:32:48.787711 13891 C5G_Tests.ttcn:192 Starting function main({
    gtpu_bind_ip := omit,
    gtpu_bind_port := omit,
    use_gtpu_daemon := true
}) on component GTP1U_EM(837).
09:32:48.787963 13891 C5G_Tests.ttcn:192 Function was started.
09:32:48.788226 13891 C5G_Tests.ttcn:167 Creating new PTC with component type NGAP_Emulation.NGAP_Emulation_CT, component name: TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0.
09:32:48.788326 18648 - Starting function main({
    gtpu_bind_ip := omit,
    gtpu_bind_port := omit,
    use_gtpu_daemon := true
}).
09:32:48.789190 18648 Osmocom_Types.ttcn:65 Random number generator was initialized with seed 185.789182: srand48(520105935).
09:32:48.789287 18648 Osmocom_Types.ttcn:65 Function rnd() returned 0.119503.
09:32:48.789517 18648 Osmocom_Types.ttcn:65 Function rnd() returned 0.947438.
09:32:48.790010 18648 GTPv1U_Emulation.ttcnpp:239 Mapping port GTP1U_EM(837):UECUPS to system:UECUPS.
09:32:48.790339 18648 GTPv1U_Emulation.ttcnpp:239 Port UECUPS was mapped to system:UECUPS.
09:32:48.790720 18648 GTPv1U_Emulation.ttcnpp:239 Map operation of GTP1U_EM(837):UECUPS to system:UECUPS finished.
09:32:48.792201 18648 GTPv1U_Emulation.ttcnpp:240 entering f__IPL4__PROVIDER__connect: :-1 -> 127.0.0.20:4268 / SCTP
09:32:48.793275 18648 GTPv1U_Emulation.ttcnpp:240 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
09:32:48.796840 18648 GTPv1U_Emulation.ttcnpp:214 Sent on UECUPS to system @UECUPS_CodecPort.UECUPS_Send : {
    connId := 1,
    msg := {
        reset_all_state := { }
    }
}
09:32:48.797026 18649 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:32:48.797208 18648 UECUPS_CodecPort.ttcn:56 f_enc_PDU_UECUPS(): Encoding @UECUPS_Types.PDU_UECUPS: {
    reset_all_state := { }
}
09:32:48.797294 18649 - TTCN-3 Parallel Test Component started on 6eab31b835ad. Component reference: TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838), component type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0. Version: 11.1.0.
09:32:48.797404 18649 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:32:48.797499 18648 UECUPS_CodecPort.ttcn:56 f_enc_PDU_UECUPS(): Stream after encoding: '7B2272657365745F616C6C5F7374617465223A7B7D7D'O ("{\"reset_all_state\":{}}")
09:32:48.797617 18649 - Connected to MC.
09:32:48.797677 18649 - Initializing variables, timers and ports of component type NGAP_Emulation.NGAP_Emulation_CT inside testcase TC_ue_service_request_cm_idle_unknown_sess_active.
09:32:48.797798 18648 GTPv1U_Emulation.ttcnpp:214 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := <unbound>,
    msg := '7B2272657365745F616C6C5F7374617465223A7B7D7D'O ("{\"reset_all_state\":{}}")
}
09:32:48.797901 13891 C5G_Tests.ttcn:167 PTC was created. Component reference: 838, alive: no, type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0.
09:32:48.798008 13891 C5G_Tests.ttcn:168 Mapping port TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP to system:NGAP_CODEC_PT.
09:32:48.798304 18648 GTPv1U_Emulation.ttcnpp:215 Start timer T: 30 s
09:32:48.799265 18648 GTPv1U_Emulation.ttcnpp:216 Message enqueued on UECUPS from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:32:48.799520 18648 GTPv1U_Emulation.ttcnpp:217 Matching on port UECUPS failed: Type of the first message in the queue is not @UECUPS_CodecPort.UECUPS_RecvFrom.
09:32:48.799717 18648 GTPv1U_Emulation.ttcnpp:218 Matching on port UECUPS succeeded:  matched
09:32:48.799800 18648 GTPv1U_Emulation.ttcnpp:218 Receive operation on port UECUPS succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:32:48.799853 18648 GTPv1U_Emulation.ttcnpp:218 Message with id 1 was extracted from the queue of UECUPS.
09:32:48.800066 18648 GTPv1U_Emulation.ttcnpp:216 Message enqueued on UECUPS from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    proto := {
        sctp := {
            sinfo_stream := 0,
            sinfo_ppid := 0,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '7B2272657365745F616C6C5F73746174655F726573223A207B22726573756C74223A20224F4B227D7D'O ("{\"reset_all_state_res\": {\"result\": \"OK\"}}")
} id 2
09:32:48.800169 18648 UECUPS_CodecPort.ttcn:50 f_dec_PDU_UECUPS(): Stream before decoding: '7B2272657365745F616C6C5F73746174655F726573223A207B22726573756C74223A20224F4B227D7D'O ("{\"reset_all_state_res\": {\"result\": \"OK\"}}")
09:32:48.800414 18648 UECUPS_CodecPort.ttcn:50 f_dec_PDU_UECUPS(): Decoded @UECUPS_Types.PDU_UECUPS: {
    reset_all_state_res := {
        result := OK (1)
    }
}
09:32:48.800521 18648 GTPv1U_Emulation.ttcnpp:216 Incoming message was mapped to @UECUPS_CodecPort.UECUPS_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    msg := {
        reset_all_state_res := {
            result := OK (1)
        }
    }
} id 2
09:32:48.800666 18648 GTPv1U_Emulation.ttcnpp:217 Matching on port UECUPS succeeded:  matched
09:32:48.800708 18648 GTPv1U_Emulation.ttcnpp:217 Receive operation on port UECUPS succeeded, message from system(): @UECUPS_CodecPort.UECUPS_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    msg := {
        reset_all_state_res := {
            result := OK (1)
        }
    }
} id 2
09:32:48.800726 18649 - Port NGAP was started.
09:32:48.800745 18648 GTPv1U_Emulation.ttcnpp:217 Message with id 2 was extracted from the queue of UECUPS.
09:32:48.800809 18649 - Port NGAP_CLIENT was started.
09:32:48.800845 18649 - Port NGAP_PROC was started.
09:32:48.800851 18648 GTPv1U_Emulation.ttcnpp:250 Altstep as_uecups_ind was activated as default, id 1
09:32:48.800880 18649 - Port NGAP_UNIT was started.
09:32:48.800914 18649 - Component type NGAP_Emulation.NGAP_Emulation_CT was initialized.
09:32:48.801001 18649 - Port NGAP was mapped to system:NGAP_CODEC_PT.
09:32:48.801215 13891 C5G_Tests.ttcn:168 Map operation of TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP to system:NGAP_CODEC_PT finished.
09:32:48.801263 13891 C5G_Tests.ttcn:169 Connecting ports TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_PROC and mtc:NGAP_PROC[0].
09:32:48.801677 13891 C5G_Tests.ttcn:169 Port NGAP_PROC[0] is waiting for connection from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-bf54f519.
09:32:48.801829 18649 - Port NGAP_PROC has established the connection with mtc:NGAP_PROC[0] using transport type UNIX.
09:32:48.801897 13891 C5G_Tests.ttcn:169 Port NGAP_PROC[0] has accepted the connection from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_PROC.
09:32:48.801985 13891 C5G_Tests.ttcn:169 Connect operation on TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_PROC and mtc:NGAP_PROC[0] finished.
09:32:48.802017 13891 C5G_Tests.ttcn:170 Connecting ports TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_UNIT and mtc:NGAP_UNIT[0].
09:32:48.802289 13891 C5G_Tests.ttcn:170 Port NGAP_UNIT[0] is waiting for connection from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_UNIT on UNIX pathname /tmp/ttcn3-portconn-ae4dec08.
09:32:48.802357 18649 - Port NGAP_UNIT has established the connection with mtc:NGAP_UNIT[0] using transport type UNIX.
09:32:48.802427 13891 C5G_Tests.ttcn:170 Port NGAP_UNIT[0] has accepted the connection from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_UNIT.
09:32:48.802479 13891 C5G_Tests.ttcn:170 Connect operation on TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_UNIT and mtc:NGAP_UNIT[0] finished.
09:32:48.802512 13891 C5G_Tests.ttcn:171 Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50000,
    role := NG_NAS_ROLE_UE (0)
}, "TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0") on component TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838).
09:32:48.802639 13891 C5G_Tests.ttcn:171 Function was started.
09:32:48.802826 18649 - Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50000,
    role := NG_NAS_ROLE_UE (0)
}, "TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0").
09:32:48.804370 18649 NGAP_Emulation.ttcn:501 Mapping port TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP to system:NGAP_CODEC_PT.
09:32:48.804476 18649 NGAP_Emulation.ttcn:501 Map operation of TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP to system:NGAP_CODEC_PT finished.
09:32:48.804987 18649 NGAP_Emulation.ttcn:506 entering f__IPL4__PROVIDER__connect: 127.0.0.202:50000 -> 127.0.0.5:38412 / SCTP
09:32:48.805333 18649 NGAP_Emulation.ttcn:506 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
09:32:48.806564 18649 NGAP_Emulation.ttcn:518 Sent on NGAP_UNIT to mtc @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
}
09:32:48.806741 13891 C5G_Tests.ttcn:172 Message enqueued on NGAP_UNIT[0] from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
09:32:48.806815 13891 C5G_Tests.ttcn:172 Matching on port NGAP_UNIT[0] succeeded:  matched
09:32:48.806860 13891 C5G_Tests.ttcn:172 Receive operation on port NGAP_UNIT[0] succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838): @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
09:32:48.806902 13891 C5G_Tests.ttcn:172 Message with id 1 was extracted from the queue of NGAP_UNIT[0].
09:32:48.807032 13891 C5G_Tests.ttcn:167 Creating new PTC with component type NGAP_Emulation.NGAP_Emulation_CT, component name: TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1.
09:32:48.809543 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:32:48.809694 18649 NGAP_Emulation.ttcn:624 Matching on port NGAP failed: Type of the first message in the queue is not @NGAP_CodecPort.NGAP_RecvFrom.
09:32:48.809765 18649 NGAP_Emulation.ttcn:676 Matching on port NGAP succeeded:  matched
09:32:48.809795 18649 NGAP_Emulation.ttcn:676 Receive operation on port NGAP succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:32:48.809813 18649 NGAP_Emulation.ttcn:676 Message with id 1 was extracted from the queue of NGAP.
09:32:48.810505 18650 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:32:48.810573 18650 - TTCN-3 Parallel Test Component started on 6eab31b835ad. Component reference: TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839), component type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1. Version: 11.1.0.
09:32:48.810601 18650 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:32:48.810664 18650 - Connected to MC.
09:32:48.810680 18650 - Initializing variables, timers and ports of component type NGAP_Emulation.NGAP_Emulation_CT inside testcase TC_ue_service_request_cm_idle_unknown_sess_active.
09:32:48.810729 13891 C5G_Tests.ttcn:167 PTC was created. Component reference: 839, alive: no, type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1.
09:32:48.810749 13891 C5G_Tests.ttcn:168 Mapping port TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP to system:NGAP_CODEC_PT.
09:32:48.811867 18650 - Port NGAP was started.
09:32:48.811897 18650 - Port NGAP_CLIENT was started.
09:32:48.811911 18650 - Port NGAP_PROC was started.
09:32:48.811924 18650 - Port NGAP_UNIT was started.
09:32:48.811937 18650 - Component type NGAP_Emulation.NGAP_Emulation_CT was initialized.
09:32:48.811976 18650 - Port NGAP was mapped to system:NGAP_CODEC_PT.
09:32:48.812017 13891 C5G_Tests.ttcn:168 Map operation of TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP to system:NGAP_CODEC_PT finished.
09:32:48.812035 13891 C5G_Tests.ttcn:169 Connecting ports TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP_PROC and mtc:NGAP_PROC[1].
09:32:48.812192 13891 C5G_Tests.ttcn:169 Port NGAP_PROC[1] is waiting for connection from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-be55f519.
09:32:48.812227 18650 - Port NGAP_PROC has established the connection with mtc:NGAP_PROC[1] using transport type UNIX.
09:32:48.812260 13891 C5G_Tests.ttcn:169 Port NGAP_PROC[1] has accepted the connection from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP_PROC.
09:32:48.812279 13891 C5G_Tests.ttcn:169 Connect operation on TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP_PROC and mtc:NGAP_PROC[1] finished.
09:32:48.812294 13891 C5G_Tests.ttcn:170 Connecting ports TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP_UNIT and mtc:NGAP_UNIT[1].
09:32:48.812417 13891 C5G_Tests.ttcn:170 Port NGAP_UNIT[1] is waiting for connection from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP_UNIT on UNIX pathname /tmp/ttcn3-portconn-af4cec08.
09:32:48.812447 18650 - Port NGAP_UNIT has established the connection with mtc:NGAP_UNIT[1] using transport type UNIX.
09:32:48.812483 13891 C5G_Tests.ttcn:170 Port NGAP_UNIT[1] has accepted the connection from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP_UNIT.
09:32:48.812531 13891 C5G_Tests.ttcn:170 Connect operation on TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP_UNIT and mtc:NGAP_UNIT[1] finished.
09:32:48.812545 13891 C5G_Tests.ttcn:171 Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50001,
    role := NG_NAS_ROLE_UE (0)
}, "TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1") on component TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839).
09:32:48.812594 13891 C5G_Tests.ttcn:171 Function was started.
09:32:48.812671 18650 - Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50001,
    role := NG_NAS_ROLE_UE (0)
}, "TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1").
09:32:48.813310 18650 NGAP_Emulation.ttcn:501 Mapping port TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP to system:NGAP_CODEC_PT.
09:32:48.813351 18650 NGAP_Emulation.ttcn:501 Map operation of TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP to system:NGAP_CODEC_PT finished.
09:32:48.813628 18650 NGAP_Emulation.ttcn:506 entering f__IPL4__PROVIDER__connect: 127.0.0.202:50001 -> 127.0.0.5:38412 / SCTP
09:32:48.813818 18650 NGAP_Emulation.ttcn:506 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
09:32:48.814646 18650 NGAP_Emulation.ttcn:518 Sent on NGAP_UNIT to mtc @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
}
09:32:48.814723 13891 C5G_Tests.ttcn:172 Message enqueued on NGAP_UNIT[1] from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839) @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
09:32:48.814749 13891 C5G_Tests.ttcn:172 Matching on port NGAP_UNIT[1] succeeded:  matched
09:32:48.814767 13891 C5G_Tests.ttcn:172 Receive operation on port NGAP_UNIT[1] succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839): @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
09:32:48.814784 13891 C5G_Tests.ttcn:172 Message with id 1 was extracted from the queue of NGAP_UNIT[1].
09:32:48.815015 13891 C5G_Tests.ttcn:287 Sent on NGAP_UNIT[0] to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
}
09:32:48.815055 13891 C5G_Tests.ttcn:288 Start timer T: 5 s
09:32:48.816416 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP_UNIT from mtc @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
} id 1
09:32:48.816653 18649 NGAP_Emulation.ttcn:618 Matching on port NGAP_UNIT succeeded:  matched
09:32:48.816689 18649 NGAP_Emulation.ttcn:618 Receive operation on port NGAP_UNIT succeeded, message from mtc: @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
} id 1
09:32:48.816708 18649 NGAP_Emulation.ttcn:618 Message with id 1 was extracted from the queue of NGAP_UNIT.
09:32:48.816979 18650 NGAP_Emulation.ttcn:535 Message enqueued on NGAP from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:32:48.817098 18650 NGAP_Emulation.ttcn:624 Matching on port NGAP failed: Type of the first message in the queue is not @NGAP_CodecPort.NGAP_RecvFrom.
09:32:48.817152 18650 NGAP_Emulation.ttcn:676 Matching on port NGAP succeeded:  matched
09:32:48.817177 18650 NGAP_Emulation.ttcn:676 Receive operation on port NGAP succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:32:48.817192 18650 NGAP_Emulation.ttcn:676 Message with id 1 was extracted from the queue of NGAP.
09:32:48.818337 18649 NGAP_Emulation.ttcn:620 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupRequest := {
                    protocolIEs := {
                        {
                            id := 27,
                            criticality := reject (0),
                            value_ := {
                                globalRANNodeID := {
                                    globalGNB_ID := {
                                        pLMNIdentity := '99F907'O,
                                        gNB_ID := {
                                            gNB_ID := '0000000000000000000000'B
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 102,
                            criticality := reject (0),
                            value_ := {
                                supportedTAList := {
                                    {
                                        tAC := '000001'O,
                                        broadcastPLMNList := {
                                            {
                                                pLMNIdentity := '99F907'O,
                                                tAISliceSupportList := {
                                                    {
                                                        s_NSSAI := {
                                                            sST := '01'O,
                                                            sD := omit,
                                                            iE_Extensions := omit
                                                        },
                                                        iE_Extensions := omit
                                                    }
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 21,
                            criticality := ignore (1),
                            value_ := {
                                pagingDRX := v32 (0)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:32:48.818851 18649 NGAP_Emulation.ttcn:620 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '00150025000003001B00080099F907000000000066000D00000000010099F907000000080015400100'O
}
09:32:48.819232 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 0,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '201500320000040001000E05806F70656E3567732D616D663000600008000099F90702004000564001FF005000080099F90700000008'O
} id 2
09:32:48.820308 18649 NGAP_Emulation.ttcn:535 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        successfulOutcome := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupResponse := {
                    protocolIEs := {
                        {
                            id := 1,
                            criticality := reject (0),
                            value_ := {
                                aMFName := "open5gs-amf0"
                            }
                        },
                        {
                            id := 96,
                            criticality := reject (0),
                            value_ := {
                                servedGUAMIList := {
                                    {
                                        gUAMI := {
                                            pLMNIdentity := '99F907'O,
                                            aMFRegionID := '00000010'B,
                                            aMFSetID := '0000000001'B,
                                            aMFPointer := '000000'B,
                                            iE_Extensions := omit
                                        },
                                        backupAMFName := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 86,
                            criticality := ignore (1),
                            value_ := {
                                relativeAMFCapacity := 255
                            }
                        },
                        {
                            id := 80,
                            criticality := reject (0),
                            value_ := {
                                pLMNSupportList := {
                                    {
                                        pLMNIdentity := '99F907'O,
                                        sliceSupportList := {
                                            {
                                                s_NSSAI := {
                                                    sST := '01'O,
                                                    sD := omit,
                                                    iE_Extensions := omit
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:32:48.820443 18649 NGAP_Emulation.ttcn:624 Matching on port NGAP succeeded:  matched
09:32:48.820476 18649 NGAP_Emulation.ttcn:624 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        successfulOutcome := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupResponse := {
                    protocolIEs := {
                        {
                            id := 1,
                            criticality := reject (0),
                            value_ := {
                                aMFName := "open5gs-amf0"
                            }
                        },
                        {
                            id := 96,
                            criticality := reject (0),
                            value_ := {
                                servedGUAMIList := {
                                    {
                                        gUAMI := {
                                            pLMNIdentity := '99F907'O,
                                            aMFRegionID := '00000010'B,
                                            aMFSetID := '0000000001'B,
                                            aMFPointer := '000000'B,
                                            iE_Extensions := omit
                                        },
                                        backupAMFName := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 86,
                            criticality := ignore (1),
                            value_ := {
                                relativeAMFCapacity := 255
                            }
                        },
                        {
                            id := 80,
                            criticality := reject (0),
                            value_ := {
                                pLMNSupportList := {
                                    {
                                        pLMNIdentity := '99F907'O,
                                        sliceSupportList := {
                                            {
                                                s_NSSAI := {
                                                    sST := '01'O,
                                                    sD := omit,
                                                    iE_Extensions := omit
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:32:48.820502 18649 NGAP_Emulation.ttcn:624 Message with id 2 was extracted from the queue of NGAP.
09:32:48.820601 18649 C5G_Tests.ttcn:134 Sent on NGAP_UNIT to mtc @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:32:48.820883 13891 C5G_Tests.ttcn:289 Message enqueued on NGAP_UNIT[0] from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:32:48.820913 13891 C5G_Tests.ttcn:290 Matching on port NGAP_UNIT[0] succeeded:  matched
09:32:48.820931 13891 C5G_Tests.ttcn:290 Receive operation on port NGAP_UNIT[0] succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838): @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:32:48.820949 13891 C5G_Tests.ttcn:290 Message with id 2 was extracted from the queue of NGAP_UNIT[0].
09:32:48.820962 13891 C5G_Tests.ttcn:291 setverdict(pass): none -> pass
09:32:48.821004 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.153192.
09:32:48.821020 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.776049.
09:32:48.821033 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.766831.
09:32:48.821046 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.490418.
09:32:48.821058 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.145952.
09:32:48.821083 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.351824.
09:32:48.821097 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.046593.
09:32:48.821113 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.973869.
09:32:48.821125 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.383942.
09:32:48.821137 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.577333.
09:32:48.821150 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.021109.
09:32:48.821161 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.217076.
09:32:48.821173 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.046622.
09:32:48.821186 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.417424.
09:32:48.821198 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.124955.
09:32:48.821210 13891 Osmocom_Types.ttcn:65 Function rnd() returned 0.467827.
09:32:48.821258 13891 C5G_Tests.ttcn:223 Creating new PTC with component type ConnHdlr.ConnHdlr, component name: TC_ue_service_request_cm_idle_unknown_sess_active0.
09:32:48.824309 18651 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:32:48.824388 18651 - TTCN-3 Parallel Test Component started on 6eab31b835ad. Component reference: TC_ue_service_request_cm_idle_unknown_sess_active0(840), component type: ConnHdlr.ConnHdlr, component name: TC_ue_service_request_cm_idle_unknown_sess_active0. Version: 11.1.0.
09:32:48.824415 18651 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:32:48.824484 18651 - Connected to MC.
09:32:48.824509 18651 - Initializing variables, timers and ports of component type ConnHdlr.ConnHdlr inside testcase TC_ue_service_request_cm_idle_unknown_sess_active.
09:32:48.824528 13891 C5G_Tests.ttcn:223 PTC was created. Component reference: 840, alive: no, type: ConnHdlr.ConnHdlr, component name: TC_ue_service_request_cm_idle_unknown_sess_active0.
09:32:48.824554 13891 C5G_Tests.ttcn:225 Connecting ports TC_ue_service_request_cm_idle_unknown_sess_active0(840):NGAP and TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_CLIENT.
09:32:48.824781 18649 NGAP_Emulation.ttcn:535 Port NGAP_CLIENT is waiting for connection from TC_ue_service_request_cm_idle_unknown_sess_active0(840):NGAP on UNIX pathname /tmp/ttcn3-portconn-6c00a217.
09:32:48.826219 18651 - Port NGAP was started.
09:32:48.826257 18651 - Port NGAP_PROC was started.
09:32:48.826277 18651 - Port GTP1U[0] was started.
09:32:48.826296 18651 - Port GTP1U[1] was started.
09:32:48.826315 18651 - Port GTP1U[2] was started.
09:32:48.826333 18651 - Port GTP1U[3] was started.
09:32:48.826352 18651 - Port GTP1U_PROC[0] was started.
09:32:48.826371 18651 - Port GTP1U_PROC[1] was started.
09:32:48.826390 18651 - Port GTP1U_PROC[2] was started.
09:32:48.826408 18651 - Port GTP1U_PROC[3] was started.
09:32:48.826427 18651 - Port COORD was started.
09:32:48.826446 18651 - Component type ConnHdlr.ConnHdlr was initialized.
09:32:48.826508 18651 - Port NGAP has established the connection with TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_CLIENT using transport type UNIX.
09:32:48.826571 18649 NGAP_Emulation.ttcn:535 Port NGAP_CLIENT has accepted the connection from TC_ue_service_request_cm_idle_unknown_sess_active0(840):NGAP.
09:32:48.826591 13891 C5G_Tests.ttcn:225 Connect operation on TC_ue_service_request_cm_idle_unknown_sess_active0(840):NGAP and TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_CLIENT finished.
09:32:48.826616 13891 C5G_Tests.ttcn:226 Connecting ports TC_ue_service_request_cm_idle_unknown_sess_active0(840):NGAP_PROC and TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_PROC.
09:32:48.826817 18649 NGAP_Emulation.ttcn:535 Port NGAP_PROC is waiting for connection from TC_ue_service_request_cm_idle_unknown_sess_active0(840):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-761aad5e.
09:32:48.826858 18651 - Port NGAP_PROC has established the connection with TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_PROC using transport type UNIX.
09:32:48.826926 18649 NGAP_Emulation.ttcn:535 Port NGAP_PROC has accepted the connection from TC_ue_service_request_cm_idle_unknown_sess_active0(840):NGAP_PROC.
09:32:48.826943 13891 C5G_Tests.ttcn:226 Connect operation on TC_ue_service_request_cm_idle_unknown_sess_active0(840):NGAP_PROC and TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_PROC finished.
09:32:48.826967 13891 C5G_Tests.ttcn:229 Connecting ports TC_ue_service_request_cm_idle_unknown_sess_active0(840):GTP1U[0] and GTP1U_EM(837):CLIENT.
09:32:48.827168 18648 GTPv1U_Emulation.ttcnpp:297 Port CLIENT is waiting for connection from TC_ue_service_request_cm_idle_unknown_sess_active0(840):GTP1U[0] on UNIX pathname /tmp/ttcn3-portconn-6d58d171.
09:32:48.827206 18651 - Port GTP1U[0] has established the connection with GTP1U_EM(837):CLIENT using transport type UNIX.
09:32:48.827299 18648 GTPv1U_Emulation.ttcnpp:297 Port CLIENT has accepted the connection from TC_ue_service_request_cm_idle_unknown_sess_active0(840):GTP1U[0].
09:32:48.827332 13891 C5G_Tests.ttcn:229 Connect operation on TC_ue_service_request_cm_idle_unknown_sess_active0(840):GTP1U[0] and GTP1U_EM(837):CLIENT finished.
09:32:48.827357 13891 C5G_Tests.ttcn:230 Connecting ports TC_ue_service_request_cm_idle_unknown_sess_active0(840):GTP1U_PROC[0] and GTP1U_EM(837):CLIENT_PROC.
09:32:48.827562 18648 GTPv1U_Emulation.ttcnpp:297 Port CLIENT_PROC is waiting for connection from TC_ue_service_request_cm_idle_unknown_sess_active0(840):GTP1U_PROC[0] on UNIX pathname /tmp/ttcn3-portconn-2f03a51c.
09:32:48.827610 18651 - Port GTP1U_PROC[0] has established the connection with GTP1U_EM(837):CLIENT_PROC using transport type UNIX.
09:32:48.827670 18648 GTPv1U_Emulation.ttcnpp:297 Port CLIENT_PROC has accepted the connection from TC_ue_service_request_cm_idle_unknown_sess_active0(840):GTP1U_PROC[0].
09:32:48.827698 13891 C5G_Tests.ttcn:230 Connect operation on TC_ue_service_request_cm_idle_unknown_sess_active0(840):GTP1U_PROC[0] and GTP1U_EM(837):CLIENT_PROC finished.
09:32:48.827725 13891 C5G_Tests.ttcn:237 Starting function f_init_handler(refers(C5G_Tests.f_TC_ue_service_request_cm_idle_unknown_sess_active), {
    ngran_pars := {
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000000'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000000'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        },
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000001'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000001'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        }
    },
    ue_pars := {
        idx := 0,
        imsi := '999700000000000'H,
        imeisv := '1774130935020414'H,
        usim_key := '762A2206FE0B4151ACE403C86A11E479'O,
        usim_opc := '3C6E0B8A9C15224A8228B9A98CA1531D'O,
        apn := "internet",
        ran_id := 0,
        amf_id := omit,
        guti := omit,
        pti := '00'O,
        sess_pars := {
            id := 1,
            run_prog_pars := {
                run_as_user := "root",
                log_path_prefix := "./run_prog",
                tun_netns_name := "tun0",
                tun_dev_name := "tun0",
                ping_hostname := "10.45.0.1"
            },
            ran_gtpu_ip := "127.0.0.20",
            ran_gtpu_teid := '00000001'O,
            cn_gtpu_ip := omit,
            cn_gtpu_teid := omit,
            qos_rules := omit,
            ue_ip4 := omit,
            ue_ip6 := omit,
            ipv6_interface_id := omit
        }
    },
    c5g_idx := 0,
    kset_id := {
        iei := omit,
        tsc := '0'B,
        nasKeySetId := '111'B
    },
    exp_CoreNetworkAssistanceInformationForInactive := false
}) on component TC_ue_service_request_cm_idle_unknown_sess_active0(840).
09:32:48.827875 13891 C5G_Tests.ttcn:237 Function was started.
09:32:48.829227 18651 - Starting function f_init_handler(refers(C5G_Tests.f_TC_ue_service_request_cm_idle_unknown_sess_active), {
    ngran_pars := {
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000000'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000000'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        },
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000001'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000001'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        }
    },
    ue_pars := {
        idx := 0,
        imsi := '999700000000000'H,
        imeisv := '1774130935020414'H,
        usim_key := '762A2206FE0B4151ACE403C86A11E479'O,
        usim_opc := '3C6E0B8A9C15224A8228B9A98CA1531D'O,
        apn := "internet",
        ran_id := 0,
        amf_id := omit,
        guti := omit,
        pti := '00'O,
        sess_pars := {
            id := 1,
            run_prog_pars := {
                run_as_user := "root",
                log_path_prefix := "./run_prog",
                tun_netns_name := "tun0",
                tun_dev_name := "tun0",
                ping_hostname := "10.45.0.1"
            },
            ran_gtpu_ip := "127.0.0.20",
            ran_gtpu_teid := '00000001'O,
            cn_gtpu_ip := omit,
            cn_gtpu_teid := omit,
            qos_rules := omit,
            ue_ip4 := omit,
            ue_ip6 := omit,
            ipv6_interface_id := omit
        }
    },
    c5g_idx := 0,
    kset_id := {
        iei := omit,
        tsc := '0'B,
        nasKeySetId := '111'B
    },
    exp_CoreNetworkAssistanceInformationForInactive := false
}).
09:32:48.834418 18651 ConnHdlr.ttcn:807 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '111'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '001'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000D'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '001'B,
            otherDigits := '99F907214300010000000000'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:32:48.835333 18651 ConnHdlr.ttcn:807 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004179000D0199F9072143000100000000002E028040'O
09:32:48.839863 18651 ConnHdlr.ttcn:812 Sent on NGAP to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
}
09:32:48.840740 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP_CLIENT from TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 1
09:32:48.840811 18649 NGAP_Emulation.ttcn:537 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.840832 18649 NGAP_Emulation.ttcn:543 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.840848 18649 NGAP_Emulation.ttcn:549 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.840870 18649 NGAP_Emulation.ttcn:556 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.841076 18649 NGAP_Emulation.ttcn:563 Matching on port NGAP_CLIENT succeeded:  matched
09:32:48.841109 18649 NGAP_Emulation.ttcn:563 Receive operation on port NGAP_CLIENT succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active0(840): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 1
09:32:48.841131 18649 NGAP_Emulation.ttcn:563 Message with id 1 was extracted from the queue of NGAP_CLIENT.
09:32:48.842528 18649 NGAP_Emulation.ttcn:569 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 15,
            criticality := ignore (1),
            value_ := {
                initialUEMessage := {
                    protocolIEs := {
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := reject (0),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 90,
                            criticality := ignore (1),
                            value_ := {
                                rRCEstablishmentCause := mo_Signalling (3)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:32:48.842791 18649 NGAP_Emulation.ttcn:569 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '000F403D00000400550002000000260018177E004179000D0199F9072143000100000000002E0280400079000F4099F907000000000099F907000001005A400118'O
}
09:32:48.848732 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '0004403F000003000A000320030D0055000200000026002B2A7E00560302000021F1ADAC74FCAB618E5BAF78C76FDF31B220106EB1B1F6042380005DEB80DAE98BACAF'O
} id 3
09:32:48.849465 18649 NGAP_Emulation.ttcn:535 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E00560302000021F1ADAC74FCAB618E5BAF78C76FDF31B220106EB1B1F6042380005DEB80DAE98BACAF'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 3
09:32:48.849692 18649 NGAP_Emulation.ttcn:624 Matching on port NGAP succeeded:  matched
09:32:48.849762 18649 NGAP_Emulation.ttcn:624 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E00560302000021F1ADAC74FCAB618E5BAF78C76FDF31B220106EB1B1F6042380005DEB80DAE98BACAF'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 3
09:32:48.849820 18649 NGAP_Emulation.ttcn:624 Message with id 3 was extracted from the queue of NGAP.
09:32:48.850303 18649 NGAP_Emulation.ttcn:646 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E00560302000021F1ADAC74FCAB618E5BAF78C76FDF31B220106EB1B1F6042380005DEB80DAE98BACAF'O
09:32:48.851771 18649 NGAP_Emulation.ttcn:646 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '11110001101011011010110001110100111111001010101101100001100011100101101110101111011110001100011101101111110111110011000110110010'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '01101110101100011011000111110110000001000010001110000000000000000101110111101011100000001101101011101001100010111010110010101111'B
        },
        eapMessage := omit
    }
}
09:32:48.852411 18649 NGAP_Emulation.ttcn:656 Sent on NGAP_CLIENT to TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '11110001101011011010110001110100111111001010101101100001100011100101101110101111011110001100011101101111110111110011000110110010'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '01101110101100011011000111110110000001000010001110000000000000000101110111101011100000001101101011101001100010111010110010101111'B
        },
        eapMessage := omit
    }
}
09:32:48.852968 18651 ConnHdlr.ttcn:824 Message enqueued on NGAP from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '11110001101011011010110001110100111111001010101101100001100011100101101110101111011110001100011101101111110111110011000110110010'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '01101110101100011011000111110110000001000010001110000000000000000101110111101011100000001101101011101001100010111010110010101111'B
        },
        eapMessage := omit
    }
} id 1
09:32:48.853385 18651 ConnHdlr.ttcn:272 Matching on port NGAP succeeded:  matched
09:32:48.853468 18651 ConnHdlr.ttcn:272 Receive operation on port NGAP succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '11110001101011011010110001110100111111001010101101100001100011100101101110101111011110001100011101101111110111110011000110110010'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '01101110101100011011000111110110000001000010001110000000000000000101110111101011100000001101101011101001100010111010110010101111'B
        },
        eapMessage := omit
    }
} id 1
09:32:48.853532 18651 ConnHdlr.ttcn:272 Message with id 1 was extracted from the queue of NGAP.
09:32:48.857294 18651 ConnHdlr.ttcn:317 Sent on NGAP to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := 'F9570E12F157A1BD08D2152D99191BF848C2F25D2D8DFF38AE3FB678DFDE6FAF'O,
        k_nas_enc := 'FE33303B3B899EC49EB182EE6EC36E468F65755F29D4AC03EA8DCE7767C1A972'O
    }
}
09:32:48.857521 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP_CLIENT from TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := 'F9570E12F157A1BD08D2152D99191BF848C2F25D2D8DFF38AE3FB678DFDE6FAF'O,
        k_nas_enc := 'FE33303B3B899EC49EB182EE6EC36E468F65755F29D4AC03EA8DCE7767C1A972'O
    }
} id 2
09:32:48.857636 18651 ConnHdlr.ttcn:321 Sent on NGAP to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '00101100110101101111101111111000000010111101011100010001110101011110111110111011111111101001110100001011100110011101100011001111'B
        },
        eapMessage := omit
    }
}
09:32:48.857638 18649 NGAP_Emulation.ttcn:537 Matching on port NGAP_CLIENT succeeded:  matched
09:32:48.857680 18649 NGAP_Emulation.ttcn:537 Receive operation on port NGAP_CLIENT succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active0(840): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := 'F9570E12F157A1BD08D2152D99191BF848C2F25D2D8DFF38AE3FB678DFDE6FAF'O,
        k_nas_enc := 'FE33303B3B899EC49EB182EE6EC36E468F65755F29D4AC03EA8DCE7767C1A972'O
    }
} id 2
09:32:48.857712 18649 NGAP_Emulation.ttcn:537 Message with id 2 was extracted from the queue of NGAP_CLIENT.
09:32:48.858055 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP_CLIENT from TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '00101100110101101111101111111000000010111101011100010001110101011110111110111011111111101001110100001011100110011101100011001111'B
        },
        eapMessage := omit
    }
} id 3
09:32:48.858224 18649 NGAP_Emulation.ttcn:537 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.858256 18649 NGAP_Emulation.ttcn:543 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.858291 18649 NGAP_Emulation.ttcn:549 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.858315 18649 NGAP_Emulation.ttcn:556 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.858349 18649 NGAP_Emulation.ttcn:563 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.858385 18649 NGAP_Emulation.ttcn:572 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.858420 18649 NGAP_Emulation.ttcn:581 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.858453 18649 NGAP_Emulation.ttcn:589 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.858529 18649 NGAP_Emulation.ttcn:598 Matching on port NGAP_CLIENT succeeded:  matched
09:32:48.858570 18649 NGAP_Emulation.ttcn:598 Receive operation on port NGAP_CLIENT succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active0(840): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '00101100110101101111101111111000000010111101011100010001110101011110111110111011111111101001110100001011100110011101100011001111'B
        },
        eapMessage := omit
    }
} id 3
09:32:48.858603 18649 NGAP_Emulation.ttcn:598 Message with id 3 was extracted from the queue of NGAP_CLIENT.
09:32:48.858704 18649 NGAP_Emulation.ttcn:602 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '00101100110101101111101111111000000010111101011100010001110101011110111110111011111111101001110100001011100110011101100011001111'B
        },
        eapMessage := omit
    }
}
09:32:48.859020 18649 NGAP_Emulation.ttcn:602 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E00572D102CD6FBF80BD711D5EFBBFE9D0B99D8CF'O
09:32:48.860103 18649 NGAP_Emulation.ttcn:603 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E00572D102CD6FBF80BD711D5EFBBFE9D0B99D8CF'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:32:48.860280 18649 NGAP_Emulation.ttcn:603 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E403D000004000A000320030D00550002000000260016157E00572D102CD6FBF80BD711D5EFBBFE9D0B99D8CF0079400F4099F907000000000099F907000001'O
}
09:32:48.867305 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044028000003000A000320030D00550002000000260014137E03C73F9F4E007E005D0103028040E1360102'O
} id 4
09:32:48.867526 18649 NGAP_Emulation.ttcn:535 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E03C73F9F4E007E005D0103028040E1360102'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 4
09:32:48.867782 18649 NGAP_Emulation.ttcn:624 Matching on port NGAP succeeded:  matched
09:32:48.867852 18649 NGAP_Emulation.ttcn:624 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E03C73F9F4E007E005D0103028040E1360102'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 4
09:32:48.867898 18649 NGAP_Emulation.ttcn:624 Message with id 4 was extracted from the queue of NGAP.
09:32:48.867958 18649 NGAP_Emulation.ttcn:646 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E03C73F9F4E007E005D0103028040E1360102'O
09:32:48.868051 18649 NGAP_Emulation.ttcn:646 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0011'B,
        messageAuthenticationCode := 'C73F9F4E'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E005D0103028040E1360102'O
    }
}
09:32:48.869671 18649 NG_CryptoFunctions.ttcn:242 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E005D0103028040E1360102'O
09:32:48.870062 18649 NG_CryptoFunctions.ttcn:242 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
}
09:32:48.870443 18649 NGAP_Emulation.ttcn:656 Sent on NGAP_CLIENT to TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
}
09:32:48.870815 18651 ConnHdlr.ttcn:825 Message enqueued on NGAP from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
} id 2
09:32:48.871162 18651 ConnHdlr.ttcn:333 Matching on port NGAP succeeded:  matched
09:32:48.871232 18651 ConnHdlr.ttcn:333 Receive operation on port NGAP succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
} id 2
09:32:48.871273 18651 ConnHdlr.ttcn:333 Message with id 2 was extracted from the queue of NGAP.
09:32:48.871353 18651 ConnHdlr.ttcn:338 Sent on NGAP to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
}
09:32:48.871429 18651 ConnHdlr.ttcn:343 Sent on NGAP to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
}
09:32:48.871451 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP_CLIENT from TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} id 4
09:32:48.871565 18649 NGAP_Emulation.ttcn:537 Matching on port NGAP_CLIENT {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} with {
    set_nas_keys := ?
} unmatched: First message in the queue does not match the template: 
09:32:48.871613 18649 NGAP_Emulation.ttcn:543 Matching on port NGAP_CLIENT {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} with {
    reset_nas_counts := ?
} unmatched: First message in the queue does not match the template: 
09:32:48.871655 18649 NGAP_Emulation.ttcn:549 Matching on port NGAP_CLIENT succeeded:  matched
09:32:48.871713 18649 NGAP_Emulation.ttcn:549 Receive operation on port NGAP_CLIENT succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active0(840): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} id 4
09:32:48.871720 18651 ConnHdlr.ttcn:353 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '001'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000D'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '001'B,
            otherDigits := '99F907214300010000000000'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:32:48.871748 18649 NGAP_Emulation.ttcn:549 Message with id 4 was extracted from the queue of NGAP_CLIENT.
09:32:48.871871 18651 ConnHdlr.ttcn:353 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004139000D0199F9072143000100000000002E028040'O
09:32:48.871900 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP_CLIENT from TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} id 5
09:32:48.871944 18649 NGAP_Emulation.ttcn:537 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    set_nas_keys := ?
} unmatched: First message in the queue does not match the template: 
09:32:48.871978 18649 NGAP_Emulation.ttcn:543 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    reset_nas_counts := ?
} unmatched: First message in the queue does not match the template: 
09:32:48.872049 18649 NGAP_Emulation.ttcn:549 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    set_nas_alg_int := ?
} unmatched: First message in the queue does not match the template: 
09:32:48.872091 18649 NGAP_Emulation.ttcn:556 Matching on port NGAP_CLIENT succeeded:  matched
09:32:48.872122 18649 NGAP_Emulation.ttcn:556 Receive operation on port NGAP_CLIENT succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active0(840): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} id 5
09:32:48.872154 18649 NGAP_Emulation.ttcn:556 Message with id 5 was extracted from the queue of NGAP_CLIENT.
09:32:48.872157 18651 ConnHdlr.ttcn:354 Sent on NGAP to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '1774130935020414'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004139000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
}
09:32:48.872375 18651 NGAP_Emulation.ttcn:802 Called on NGAP_PROC to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NGAP_Emulation.NGAPEM_obtain_amf_id : { }
09:32:48.872479 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP_CLIENT from TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '1774130935020414'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004139000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
} id 6
09:32:48.872592 18649 NGAP_Emulation.ttcn:537 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.872625 18649 NGAP_Emulation.ttcn:543 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.872654 18649 NGAP_Emulation.ttcn:549 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.872681 18649 NGAP_Emulation.ttcn:556 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.872718 18649 NGAP_Emulation.ttcn:563 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.872758 18649 NGAP_Emulation.ttcn:572 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.872797 18649 NGAP_Emulation.ttcn:581 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.872834 18649 NGAP_Emulation.ttcn:589 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.872872 18649 NGAP_Emulation.ttcn:598 Matching on port NGAP_CLIENT succeeded:  matched
09:32:48.872916 18649 NGAP_Emulation.ttcn:598 Receive operation on port NGAP_CLIENT succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active0(840): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '1774130935020414'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004139000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
} id 6
09:32:48.872948 18649 NGAP_Emulation.ttcn:598 Message with id 6 was extracted from the queue of NGAP_CLIENT.
09:32:48.873024 18649 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '1774130935020414'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004139000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
}
09:32:48.873170 18649 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E005E7700090517741309350204147100177E004139000D0199F9072143000100000000002E028040'O
09:32:48.874169 18649 NGAP_Emulation.ttcn:602 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0100'B,
        messageAuthenticationCode := '216F9505'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E005E7700090517741309350204147100177E004139000D0199F9072143000100000000002E028040'O
    }
}
09:32:48.874217 18649 NGAP_Emulation.ttcn:602 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E04216F9505007E005E7700090517741309350204147100177E004139000D0199F9072143000100000000002E028040'O
09:32:48.874346 18649 NGAP_Emulation.ttcn:603 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E04216F9505007E005E7700090517741309350204147100177E004139000D0199F9072143000100000000002E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:32:48.874432 18649 NGAP_Emulation.ttcn:603 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4058000004000A000320030D00550002000000260031307E04216F9505007E005E7700090517741309350204147100177E004139000D0199F9072143000100000000002E0280400079400F4099F907000000000099F907000001'O
}
09:32:48.874637 18649 NGAP_Emulation.ttcn:535 Call enqueued on NGAP_PROC from TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } id 1
09:32:48.874715 18649 NGAP_Emulation.ttcn:678 Matching on port NGAP_PROC failed: The first entity in the queue is not a call for signature @NGAP_Emulation.NGAPEM_register.
09:32:48.874744 18649 NGAP_Emulation.ttcn:682 Matching on port NGAP_PROC failed: The first entity in the queue is not a call for signature @NGAP_Emulation.NGAPEM_register_proc.
09:32:48.874776 18649 NGAP_Emulation.ttcn:686 Matching on port NGAP_PROC succeeded: { } with { } matched
09:32:48.874838 18649 NGAP_Emulation.ttcn:686 Getcall operation on port NGAP_PROC succeeded, call from TC_ue_service_request_cm_idle_unknown_sess_active0(840): @NGAP_Emulation.NGAPEM_obtain_amf_id : { } id 1
09:32:48.874867 18649 NGAP_Emulation.ttcn:686 Operation with id 1 was extracted from the queue of NGAP_PROC.
09:32:48.874912 18649 NGAP_Emulation.ttcn:689 Replied on NGAP_PROC to TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 781
09:32:48.875021 18651 NGAP_Emulation.ttcn:802 Reply enqueued on NGAP_PROC from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 781 id 1
09:32:48.875092 18651 NGAP_Emulation.ttcn:803 Matching on port NGAP_PROC succeeded: { } with { } matched value 781 with ? matched
09:32:48.875163 18651 NGAP_Emulation.ttcn:803 Getreply operation on port NGAP_PROC succeeded, reply from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838): @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 781 id 1
09:32:48.875193 18651 NGAP_Emulation.ttcn:803 Operation with id 1 was extracted from the queue of NGAP_PROC.
09:32:48.889354 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044057000005000A000320030D0055000200000026002F2E7E02406BECB4017E0042010177000BF299F907020040C000028454074099F90700000115020101210201005E0192006E400A0C3B9ACA00303B9ACA00000000020001'O
} id 5
09:32:48.890547 18649 NGAP_Emulation.ttcn:535 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02406BECB4017E0042010177000BF299F907020040C000028454074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 110,
                            criticality := ignore (1),
                            value_ := {
                                uEAggregateMaximumBitRate := {
                                    uEAggregateMaximumBitRateDL := 1000000000,
                                    uEAggregateMaximumBitRateUL := 1000000000,
                                    iE_Extensions := omit
                                }
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 5
09:32:48.890822 18649 NGAP_Emulation.ttcn:624 Matching on port NGAP succeeded:  matched
09:32:48.890913 18649 NGAP_Emulation.ttcn:624 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02406BECB4017E0042010177000BF299F907020040C000028454074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 110,
                            criticality := ignore (1),
                            value_ := {
                                uEAggregateMaximumBitRate := {
                                    uEAggregateMaximumBitRateDL := 1000000000,
                                    uEAggregateMaximumBitRateUL := 1000000000,
                                    iE_Extensions := omit
                                }
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 5
09:32:48.890967 18649 NGAP_Emulation.ttcn:624 Message with id 5 was extracted from the queue of NGAP.
09:32:48.891034 18649 NGAP_Emulation.ttcn:646 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E02406BECB4017E0042010177000BF299F907020040C000028454074099F90700000115020101210201005E0192'O
09:32:48.891108 18649 NGAP_Emulation.ttcn:646 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '406BECB4'O,
        sequenceNumber := '01'O,
        plainNASMessage := '7E0042010177000BF299F907020040C000028454074099F90700000115020101210201005E0192'O
    }
}
09:32:48.892537 18649 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0042010177000BF299F907020040C000028454074099F90700000115020101210201005E0192'O
09:32:48.894071 18649 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000284'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:32:48.895285 18649 NGAP_Emulation.ttcn:656 Sent on NGAP_CLIENT to TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000284'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:32:48.896380 18651 ConnHdlr.ttcn:830 Message enqueued on NGAP from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000284'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 3
09:32:48.897257 18651 ConnHdlr.ttcn:830 Matching on port NGAP succeeded:  matched
09:32:48.897375 18651 ConnHdlr.ttcn:830 Receive operation on port NGAP succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000284'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 3
09:32:48.897446 18651 ConnHdlr.ttcn:830 Message with id 3 was extracted from the queue of NGAP.
09:32:48.897607 18651 ConnHdlr.ttcn:832 Sent on NGAP to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:32:48.897750 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP_CLIENT from TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 7
09:32:48.897853 18649 NGAP_Emulation.ttcn:537 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.897896 18649 NGAP_Emulation.ttcn:543 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.897936 18649 NGAP_Emulation.ttcn:549 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.897974 18649 NGAP_Emulation.ttcn:556 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.898025 18649 NGAP_Emulation.ttcn:563 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.898086 18649 NGAP_Emulation.ttcn:572 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.898142 18649 NGAP_Emulation.ttcn:581 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.898195 18649 NGAP_Emulation.ttcn:589 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.898243 18649 NGAP_Emulation.ttcn:598 Matching on port NGAP_CLIENT succeeded:  matched
09:32:48.898291 18649 NGAP_Emulation.ttcn:598 Receive operation on port NGAP_CLIENT succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active0(840): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 7
09:32:48.898338 18649 NGAP_Emulation.ttcn:598 Message with id 7 was extracted from the queue of NGAP_CLIENT.
09:32:48.898410 18649 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:32:48.898504 18649 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0043'O
09:32:48.899542 18649 NGAP_Emulation.ttcn:602 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '1F1B15B4'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0043'O
    }
}
09:32:48.899605 18649 NGAP_Emulation.ttcn:602 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E021F1B15B4007E0043'O
09:32:48.899809 18649 NGAP_Emulation.ttcn:603 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E021F1B15B4007E0043'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:32:48.899935 18649 NGAP_Emulation.ttcn:603 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4032000004000A000320030D0055000200000026000B0A7E021F1B15B4007E00430079400F4099F907000000000099F907000001'O
}
09:32:48.901731 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044048000003000A000320030D00550002000000260034337E02682447D4027E0054430F90004F00700065006E003500470053450990004E00650078007446004762402190238400490100'O
} id 6
09:32:48.901882 18649 NGAP_Emulation.ttcn:535 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02682447D4027E0054430F90004F00700065006E003500470053450990004E00650078007446004762402190238400490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 6
09:32:48.901997 18649 NGAP_Emulation.ttcn:624 Matching on port NGAP succeeded:  matched
09:32:48.902057 18649 NGAP_Emulation.ttcn:624 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02682447D4027E0054430F90004F00700065006E003500470053450990004E00650078007446004762402190238400490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 6
09:32:48.902101 18649 NGAP_Emulation.ttcn:624 Message with id 6 was extracted from the queue of NGAP.
09:32:48.902163 18649 NGAP_Emulation.ttcn:646 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E02682447D4027E0054430F90004F00700065006E003500470053450990004E00650078007446004762402190238400490100'O
09:32:48.902225 18649 NGAP_Emulation.ttcn:646 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '682447D4'O,
        sequenceNumber := '02'O,
        plainNASMessage := '7E0054430F90004F00700065006E003500470053450990004E00650078007446004762402190238400490100'O
    }
}
09:32:48.903329 18649 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0054430F90004F00700065006E003500470053450990004E00650078007446004762402190238400490100'O
09:32:48.903764 18649 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '62'O ("b"),
            month := '40'O ("@"),
            day := '21'O ("!"),
            hour := '90'O,
            minute := '23'O ("#"),
            second := '84'O,
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:32:48.904152 18649 NGAP_Emulation.ttcn:656 Sent on NGAP_CLIENT to TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '62'O ("b"),
            month := '40'O ("@"),
            day := '21'O ("!"),
            hour := '90'O,
            minute := '23'O ("#"),
            second := '84'O,
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:32:48.904439 18651 ConnHdlr.ttcn:834 Message enqueued on NGAP from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '62'O ("b"),
            month := '40'O ("@"),
            day := '21'O ("!"),
            hour := '90'O,
            minute := '23'O ("#"),
            second := '84'O,
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 4
09:32:48.904765 18651 ConnHdlr.ttcn:362 Matching on port NGAP succeeded:  matched
09:32:48.904825 18651 ConnHdlr.ttcn:362 Receive operation on port NGAP succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '62'O ("b"),
            month := '40'O ("@"),
            day := '21'O ("!"),
            hour := '90'O,
            minute := '23'O ("#"),
            second := '84'O,
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 4
09:32:48.904869 18651 ConnHdlr.ttcn:362 Message with id 4 was extracted from the queue of NGAP.
09:32:48.904940 18651 ConnHdlr.ttcn:363 Sent on NGAP to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:32:48.905024 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP_CLIENT from TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 8
09:32:48.905089 18649 NGAP_Emulation.ttcn:537 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.905118 18649 NGAP_Emulation.ttcn:543 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.905145 18649 NGAP_Emulation.ttcn:549 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.905171 18649 NGAP_Emulation.ttcn:556 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.905205 18649 NGAP_Emulation.ttcn:563 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.905242 18649 NGAP_Emulation.ttcn:572 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.905279 18649 NGAP_Emulation.ttcn:581 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.905314 18649 NGAP_Emulation.ttcn:589 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:48.905346 18649 NGAP_Emulation.ttcn:598 Matching on port NGAP_CLIENT succeeded:  matched
09:32:48.905381 18649 NGAP_Emulation.ttcn:598 Receive operation on port NGAP_CLIENT succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active0(840): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 8
09:32:48.905415 18649 NGAP_Emulation.ttcn:598 Message with id 8 was extracted from the queue of NGAP_CLIENT.
09:32:48.905464 18649 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:32:48.905483 18651 ConnHdlr.ttcn:895 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    service_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01001100'B,
        serviceType := '0000'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        s_TMSI := {
            iei := omit,
            iel := '0007'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '100'B,
            otherDigits := '0040C0000284'O
        },
        ulDataStatus := omit,
        pduSessionStatus := {
            iei := '50'O ("P"),
            iel := '02'O,
            psi0_7 := '00000010'B,
            psi8_15 := '00000000'B,
            spare := omit
        },
        allowedPDUSessionStatus := omit,
        nasMsg := omit,
        ueRequestType := omit,
        pagingRestrict := omit
    }
}
09:32:48.905517 18649 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0055'O
09:32:48.905613 18651 ConnHdlr.ttcn:895 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004C030007F40040C000028450020200'O
09:32:48.905717 18651 ConnHdlr.ttcn:904 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    service_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01001100'B,
        serviceType := '0000'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        s_TMSI := {
            iei := omit,
            iel := '0007'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '100'B,
            otherDigits := '0040C0000284'O
        },
        ulDataStatus := omit,
        pduSessionStatus := omit,
        allowedPDUSessionStatus := omit,
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004C030007F40040C000028450020200'O
        },
        ueRequestType := omit,
        pagingRestrict := omit
    }
}
09:32:48.905838 18651 ConnHdlr.ttcn:904 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004C030007F40040C00002847100117E004C030007F40040C000028450020200'O
09:32:48.906315 18649 NGAP_Emulation.ttcn:602 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '6D7F4D9C'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0055'O
    }
}
09:32:48.906356 18649 NGAP_Emulation.ttcn:602 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E026D7F4D9C007E0055'O
09:32:48.906482 18649 NGAP_Emulation.ttcn:603 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E026D7F4D9C007E0055'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:32:48.906575 18649 NGAP_Emulation.ttcn:603 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4032000004000A000320030D0055000200000026000B0A7E026D7F4D9C007E00550079400F4099F907000000000099F907000001'O
}
09:32:48.906999 18651 ConnHdlr.ttcn:915 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0001'B,
        messageAuthenticationCode := '81D1EA60'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E004C030007F40040C00002847100117E004C030007F40040C000028450020200'O
    }
}
09:32:48.907058 18651 ConnHdlr.ttcn:915 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0181D1EA60007E004C030007F40040C00002847100117E004C030007F40040C000028450020200'O
09:32:48.907260 18651 ConnHdlr.ttcn:920 Sent on NGAP to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E0181D1EA60007E004C030007F40040C00002847100117E004C030007F40040C000028450020200'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
}
09:32:48.907372 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP_CLIENT from TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E0181D1EA60007E004C030007F40040C00002847100117E004C030007F40040C000028450020200'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 9
09:32:48.907423 18649 NGAP_Emulation.ttcn:537 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.907448 18649 NGAP_Emulation.ttcn:543 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.907476 18649 NGAP_Emulation.ttcn:549 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.907501 18649 NGAP_Emulation.ttcn:556 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:48.907545 18649 NGAP_Emulation.ttcn:563 Matching on port NGAP_CLIENT succeeded:  matched
09:32:48.907586 18649 NGAP_Emulation.ttcn:563 Receive operation on port NGAP_CLIENT succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active0(840): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E0181D1EA60007E004C030007F40040C00002847100117E004C030007F40040C000028450020200'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 9
09:32:48.907619 18649 NGAP_Emulation.ttcn:563 Message with id 9 was extracted from the queue of NGAP_CLIENT.
09:32:48.907756 18649 NGAP_Emulation.ttcn:569 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 15,
            criticality := ignore (1),
            value_ := {
                initialUEMessage := {
                    protocolIEs := {
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0181D1EA60007E004C030007F40040C00002847100117E004C030007F40040C000028450020200'O
                            }
                        },
                        {
                            id := 121,
                            criticality := reject (0),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 90,
                            criticality := ignore (1),
                            value_ := {
                                rRCEstablishmentCause := mo_Signalling (3)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:32:48.907835 18649 NGAP_Emulation.ttcn:569 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '000F404E00000400550002000000260029287E0181D1EA60007E004C030007F40040C00002847100117E004C030007F40040C0000284500202000079000F4099F907000000000099F907000001005A400118'O
}
09:32:49.113619 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044023000003000A000320030D0055000200000026000F0E7E021A783FC6037E004E50020000'O
} id 7
09:32:49.114082 18649 NGAP_Emulation.ttcn:535 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E021A783FC6037E004E50020000'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
09:32:49.114547 18649 NGAP_Emulation.ttcn:624 Matching on port NGAP succeeded:  matched
09:32:49.114842 18649 NGAP_Emulation.ttcn:624 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E021A783FC6037E004E50020000'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
09:32:49.115009 18649 NGAP_Emulation.ttcn:624 Message with id 7 was extracted from the queue of NGAP.
09:32:49.115103 18649 NGAP_Emulation.ttcn:646 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E021A783FC6037E004E50020000'O
09:32:49.115184 18649 NGAP_Emulation.ttcn:646 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '1A783FC6'O,
        sequenceNumber := '03'O,
        plainNASMessage := '7E004E50020000'O
    }
}
09:32:49.116353 18649 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E004E50020000'O
09:32:49.116546 18649 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    service_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01001110'B,
        pduSessionStatus := {
            iei := '50'O ("P"),
            iel := '02'O,
            psi0_7 := '00000000'B,
            psi8_15 := '00000000'B,
            spare := omit
        },
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        eapMessage := omit,
        t3448 := omit,
        ngAddRequestResult := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit
    }
}
09:32:49.116792 18649 NGAP_Emulation.ttcn:656 Sent on NGAP_CLIENT to TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    service_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01001110'B,
        pduSessionStatus := {
            iei := '50'O ("P"),
            iel := '02'O,
            psi0_7 := '00000000'B,
            psi8_15 := '00000000'B,
            spare := omit
        },
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        eapMessage := omit,
        t3448 := omit,
        ngAddRequestResult := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit
    }
}
09:32:49.117045 18651 C5G_Tests.ttcn:626 Message enqueued on NGAP from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    service_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01001110'B,
        pduSessionStatus := {
            iei := '50'O ("P"),
            iel := '02'O,
            psi0_7 := '00000000'B,
            psi8_15 := '00000000'B,
            spare := omit
        },
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        eapMessage := omit,
        t3448 := omit,
        ngAddRequestResult := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit
    }
} id 5
09:32:49.117328 18651 C5G_Tests.ttcn:626 Matching on port NGAP succeeded:  matched
09:32:49.117401 18651 C5G_Tests.ttcn:626 Receive operation on port NGAP succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    service_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01001110'B,
        pduSessionStatus := {
            iei := '50'O ("P"),
            iel := '02'O,
            psi0_7 := '00000000'B,
            psi8_15 := '00000000'B,
            spare := omit
        },
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        eapMessage := omit,
        t3448 := omit,
        ngAddRequestResult := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit
    }
} id 5
09:32:49.117460 18651 C5G_Tests.ttcn:626 Message with id 5 was extracted from the queue of NGAP.
09:32:49.117912 18651 ConnHdlr.ttcn:973 Sent on NGAP to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000284'O
        }
    }
}
09:32:49.118135 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP_CLIENT from TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000284'O
        }
    }
} id 10
09:32:49.118313 18649 NGAP_Emulation.ttcn:537 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:49.118365 18649 NGAP_Emulation.ttcn:543 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:49.118409 18649 NGAP_Emulation.ttcn:549 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:49.119100 18649 NGAP_Emulation.ttcn:556 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:49.119176 18649 NGAP_Emulation.ttcn:563 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:49.119252 18649 NGAP_Emulation.ttcn:572 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:49.119326 18649 NGAP_Emulation.ttcn:581 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:49.119392 18649 NGAP_Emulation.ttcn:589 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:32:49.119468 18649 NGAP_Emulation.ttcn:598 Matching on port NGAP_CLIENT succeeded:  matched
09:32:49.119540 18649 NGAP_Emulation.ttcn:598 Receive operation on port NGAP_CLIENT succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active0(840): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000284'O
        }
    }
} id 10
09:32:49.119606 18649 NGAP_Emulation.ttcn:598 Message with id 10 was extracted from the queue of NGAP_CLIENT.
09:32:49.119718 18649 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000284'O
        }
    }
}
09:32:49.119873 18649 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004531000BF299F907020040C0000284'O
09:32:49.121365 18649 NGAP_Emulation.ttcn:602 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'D9287CC4'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E004531000BF299F907020040C0000284'O
    }
}
09:32:49.121443 18649 NGAP_Emulation.ttcn:602 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E02D9287CC4007E004531000BF299F907020040C0000284'O
09:32:49.121717 18649 NGAP_Emulation.ttcn:603 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02D9287CC4007E004531000BF299F907020040C0000284'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:32:49.121919 18649 NGAP_Emulation.ttcn:603 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4040000004000A000320030D00550002000000260019187E02D9287CC4007E004531000BF299F907020040C00002840079400F4099F907000000000099F907000001'O
}
09:32:49.136092 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '0004401F000003000A000320030D0055000200000026000B0A7E02BC1F3093047E0046'O
} id 8
09:32:49.136424 18649 NGAP_Emulation.ttcn:535 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02BC1F3093047E0046'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:32:49.136723 18649 NGAP_Emulation.ttcn:624 Matching on port NGAP succeeded:  matched
09:32:49.136815 18649 NGAP_Emulation.ttcn:624 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02BC1F3093047E0046'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:32:49.136887 18649 NGAP_Emulation.ttcn:624 Message with id 8 was extracted from the queue of NGAP.
09:32:49.136978 18649 NGAP_Emulation.ttcn:646 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E02BC1F3093047E0046'O
09:32:49.137065 18649 NGAP_Emulation.ttcn:646 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'BC1F3093'O,
        sequenceNumber := '04'O,
        plainNASMessage := '7E0046'O
    }
}
09:32:49.138496 18649 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0046'O
09:32:49.138622 18649 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
}
09:32:49.138739 18649 NGAP_Emulation.ttcn:656 Sent on NGAP_CLIENT to TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
}
09:32:49.138943 18651 ConnHdlr.ttcn:975 Message enqueued on NGAP from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
} id 6
09:32:49.139074 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '002900110000020072000502030D0000000F400148'O
} id 9
09:32:49.139117 18651 ConnHdlr.ttcn:975 Matching on port NGAP succeeded:  matched
09:32:49.139182 18651 ConnHdlr.ttcn:975 Receive operation on port NGAP succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
} id 6
09:32:49.139239 18651 ConnHdlr.ttcn:975 Message with id 6 was extracted from the queue of NGAP.
09:32:49.140378 18649 NGAP_Emulation.ttcn:535 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseCommand := {
                    protocolIEs := {
                        {
                            id := 114,
                            criticality := reject (0),
                            value_ := {
                                uE_NGAP_IDs := {
                                    uE_NGAP_ID_pair := {
                                        aMF_UE_NGAP_ID := 781,
                                        rAN_UE_NGAP_ID := 0,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 15,
                            criticality := ignore (1),
                            value_ := {
                                cause := {
                                    nas := deregister (2)
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 9
09:32:49.140565 18649 NGAP_Emulation.ttcn:624 Matching on port NGAP succeeded:  matched
09:32:49.140636 18649 NGAP_Emulation.ttcn:624 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseCommand := {
                    protocolIEs := {
                        {
                            id := 114,
                            criticality := reject (0),
                            value_ := {
                                uE_NGAP_IDs := {
                                    uE_NGAP_ID_pair := {
                                        aMF_UE_NGAP_ID := 781,
                                        rAN_UE_NGAP_ID := 0,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 15,
                            criticality := ignore (1),
                            value_ := {
                                cause := {
                                    nas := deregister (2)
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 9
09:32:49.140686 18649 NGAP_Emulation.ttcn:624 Message with id 9 was extracted from the queue of NGAP.
09:32:49.140877 18649 NGAP_Emulation.ttcn:663 Sent on NGAP_CLIENT to TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 781,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:32:49.142212 18651 ConnHdlr.ttcn:976 Message enqueued on NGAP from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 781,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
09:32:49.143030 18651 ConnHdlr.ttcn:989 Matching on port NGAP succeeded:  matched
09:32:49.143092 18651 ConnHdlr.ttcn:989 Receive operation on port NGAP succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 781,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
09:32:49.143145 18651 ConnHdlr.ttcn:989 Message with id 7 was extracted from the queue of NGAP.
09:32:49.145191 18651 ConnHdlr.ttcn:990 Sent on NGAP to TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 781
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:32:49.145607 18651 - Function f_init_handler finished. PTC terminates.
09:32:49.145663 18651 - Terminating component type ConnHdlr.ConnHdlr.
09:32:49.145704 18651 - Removing unterminated connection between port NGAP and TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_CLIENT.
09:32:49.145775 18651 - Port NGAP was stopped.
09:32:49.145814 18651 - Removing unterminated connection between port NGAP_PROC and TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_PROC.
09:32:49.145840 18649 NGAP_Emulation.ttcn:535 Message enqueued on NGAP_CLIENT from TC_ue_service_request_cm_idle_unknown_sess_active0(840) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 781
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 11
09:32:49.145869 18651 - Port NGAP_PROC was stopped.
09:32:49.145909 18651 - Removing unterminated connection between port GTP1U[0] and GTP1U_EM(837):CLIENT.
09:32:49.145958 18651 - Port GTP1U[0] was stopped.
09:32:49.145992 18651 - Port GTP1U[1] was stopped.
09:32:49.145998 18648 GTPv1U_Emulation.ttcnpp:297 Connection of port CLIENT to TC_ue_service_request_cm_idle_unknown_sess_active0(840):GTP1U[0] was closed unexpectedly by the peer.
09:32:49.146003 18649 NGAP_Emulation.ttcn:537 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:49.146027 18651 - Port GTP1U[2] was stopped.
09:32:49.146044 18649 NGAP_Emulation.ttcn:543 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:49.146068 18651 - Port GTP1U[3] was stopped.
09:32:49.146077 18649 NGAP_Emulation.ttcn:549 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:49.146095 18648 GTPv1U_Emulation.ttcnpp:297 Port CLIENT was disconnected from TC_ue_service_request_cm_idle_unknown_sess_active0(840):GTP1U[0].
09:32:49.146103 18651 - Removing unterminated connection between port GTP1U_PROC[0] and GTP1U_EM(837):CLIENT_PROC.
09:32:49.146112 18649 NGAP_Emulation.ttcn:556 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:32:49.146161 18651 - Port GTP1U_PROC[0] was stopped.
09:32:49.146226 18648 GTPv1U_Emulation.ttcnpp:297 Connection of port CLIENT_PROC to TC_ue_service_request_cm_idle_unknown_sess_active0(840):GTP1U_PROC[0] was closed unexpectedly by the peer.
09:32:49.146253 18651 - Port GTP1U_PROC[1] was stopped.
09:32:49.146265 18648 GTPv1U_Emulation.ttcnpp:297 Port CLIENT_PROC was disconnected from TC_ue_service_request_cm_idle_unknown_sess_active0(840):GTP1U_PROC[0].
09:32:49.146288 18651 - Port GTP1U_PROC[2] was stopped.
09:32:49.146323 18651 - Port GTP1U_PROC[3] was stopped.
09:32:49.146360 18651 - Port COORD was stopped.
09:32:49.146393 18651 - Component type ConnHdlr.ConnHdlr was shut down inside testcase TC_ue_service_request_cm_idle_unknown_sess_active.
09:32:49.146436 18651 - Final verdict of PTC: none
09:32:49.146567 13891 C5G_Tests.ttcn:636 PTC with component reference 840 is done.
09:32:49.146605 18649 NGAP_Emulation.ttcn:563 Matching on port NGAP_CLIENT {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 781
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} with {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := ?
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := ?
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := ?
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := ?
                        }
                    }
                }
            }
        }
    }
} unmatched: First message in the queue does not match the template: 
09:32:49.146615 18651 - Disconnected from MC.
09:32:49.146677 18651 - TTCN-3 Parallel Test Component finished.
09:32:49.146784 13891 C5G_Tests.ttcn:636 Terminating component type C5G_Tests.MTC_CT.
09:32:49.146869 18649 NGAP_Emulation.ttcn:572 Matching on port NGAP_CLIENT {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 781
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} with {
    initiatingMessage := {
        procedureCode := 25,
        criticality := reject (0),
        value_ := {
            pathSwitchRequest := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := ?
                        }
                    },
                    {
                        id := 100,
                        criticality := reject (0),
                        value_ := {
                            aMF_UE_NGAP_ID := ?
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := ?
                        }
                    },
                    {
                        id := 119,
                        criticality := ignore (1),
                        value_ := {
                            uESecurityCapabilities := ?
                        }
                    },
                    {
                        id := 76,
                        criticality := reject (0),
                        value_ := {
                            pDUSessionResourceToBeSwitchedDLList := ?
                        }
                    }
                }
            }
        }
    }
} unmatched: First message in the queue does not match the template: 
09:32:49.146885 13891 C5G_Tests.ttcn:636 Default with id 1 (altstep as_Tguard) was deactivated.
09:32:49.146973 13891 C5G_Tests.ttcn:636 Stop timer g_Tguard: 30 s
09:32:49.147060 13891 C5G_Tests.ttcn:636 Removing unterminated connection between port NGAP_UNIT[0] and TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_UNIT.
09:32:49.147210 13891 C5G_Tests.ttcn:636 Port NGAP_UNIT[0] was stopped.
09:32:49.147297 13891 C5G_Tests.ttcn:636 Removing unterminated connection between port NGAP_UNIT[1] and TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP_UNIT.
09:32:49.147306 18649 NGAP_Emulation.ttcn:581 Matching on port NGAP_CLIENT .successfulOutcome.procedureCode := 41 with 13 unmatched.successfulOutcome.value_{
    uEContextReleaseComplete := {
        protocolIEs := {
            {
                id := 10,
                criticality := ignore (1),
                value_ := {
                    aMF_UE_NGAP_ID := 781
                }
            },
            {
                id := 85,
                criticality := ignore (1),
                value_ := {
                    rAN_UE_NGAP_ID := 0
                }
            },
            {
                id := 121,
                criticality := ignore (1),
                value_ := {
                    userLocationInformation := {
                        userLocationInformationNR := {
                            nR_CGI := {
                                pLMNIdentity := '99F907'O,
                                nRCellIdentity := '000000000000000000000000000000000000'B,
                                iE_Extensions := omit
                            },
                            tAI := {
                                pLMNIdentity := '99F907'O,
                                tAC := '000001'O,
                                iE_Extensions := omit
                            },
                            timeStamp := omit,
                            iE_Extensions := omit
                        }
                    }
                }
            }
        }
    }
} with {
    handoverRequestAcknowledge := {
        protocolIEs := {
            {
                id := 10,
                criticality := ignore (1),
                value_ := {
                    aMF_UE_NGAP_ID := ?
                }
            },
            {
                id := 85,
                criticality := ignore (1),
                value_ := {
                    rAN_UE_NGAP_ID := ?
                }
            },
            {
                id := 53,
                criticality := ignore (1),
                value_ := {
                    pDUSessionResourceAdmittedList := ?
                }
            },
            {
                id := 106,
                criticality := reject (0),
                value_ := {
                    targetToSource_TransparentContainer := ?
                }
            }
        }
    }
} unmatched: First message in the queue does not match the template: 
09:32:49.147436 13891 C5G_Tests.ttcn:636 Port NGAP_UNIT[1] was stopped.
09:32:49.147483 18649 NGAP_Emulation.ttcn:589 Matching on port NGAP_CLIENT {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 781
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} with {
    initiatingMessage := {
        procedureCode := 11,
        criticality := ignore (1),
        value_ := {
            handoverNotify := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := reject (0),
                        value_ := {
                            aMF_UE_NGAP_ID := ?
                        }
                    },
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := ?
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := ?
                        }
                    }
                }
            }
        }
    }
} unmatched: First message in the queue does not match the template: 
09:32:49.147483 18650 NGAP_Emulation.ttcn:535 Connection of port NGAP_UNIT to mtc:NGAP_UNIT[1] was closed unexpectedly by the peer.
09:32:49.147528 13891 C5G_Tests.ttcn:636 Removing unterminated connection between port NGAP_PROC[0] and TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838):NGAP_PROC.
09:32:49.147552 18649 NGAP_Emulation.ttcn:598 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type.
09:32:49.147600 18649 NGAP_Emulation.ttcn:611 Matching on port NGAP_CLIENT succeeded:  matched
09:32:49.147609 18650 NGAP_Emulation.ttcn:535 Port NGAP_UNIT was disconnected from mtc:NGAP_UNIT[1].
09:32:49.147644 13891 C5G_Tests.ttcn:636 Port NGAP_PROC[0] was stopped.
09:32:49.147681 18649 NGAP_Emulation.ttcn:611 Receive operation on port NGAP_CLIENT succeeded, message from TC_ue_service_request_cm_idle_unknown_sess_active0(840): @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 781
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 11
09:32:49.147746 13891 C5G_Tests.ttcn:636 Removing unterminated connection between port NGAP_PROC[1] and TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839):NGAP_PROC.
09:32:49.147835 18649 NGAP_Emulation.ttcn:611 Message with id 11 was extracted from the queue of NGAP_CLIENT.
09:32:49.147891 13891 C5G_Tests.ttcn:636 Port NGAP_PROC[1] was stopped.
09:32:49.147964 18650 NGAP_Emulation.ttcn:535 Connection of port NGAP_PROC to mtc:NGAP_PROC[1] was closed unexpectedly by the peer.
09:32:49.148040 18650 NGAP_Emulation.ttcn:535 Port NGAP_PROC was disconnected from mtc:NGAP_PROC[1].
09:32:49.148046 13891 C5G_Tests.ttcn:636 Removing unterminated connection between port TEID0 and GTP1U_EM(837):TEID0.
09:32:49.148143 13891 C5G_Tests.ttcn:636 Port TEID0 was stopped.
09:32:49.148148 18648 GTPv1U_Emulation.ttcnpp:297 Connection of port TEID0 to mtc:TEID0 was closed unexpectedly by the peer.
09:32:49.148218 18648 GTPv1U_Emulation.ttcnpp:297 Port TEID0 was disconnected from mtc:TEID0.
09:32:49.148245 13891 C5G_Tests.ttcn:636 Component type C5G_Tests.MTC_CT was shut down inside testcase TC_ue_service_request_cm_idle_unknown_sess_active.
09:32:49.148317 13891 C5G_Tests.ttcn:636 Waiting for PTCs to finish.
09:32:49.148434 18648 GTPv1U_Emulation.ttcnpp:297 Kill was requested from MC.
09:32:49.148448 18650 NGAP_Emulation.ttcn:535 Kill was requested from MC.
09:32:49.148475 18648 GTPv1U_Emulation.ttcnpp:297 Terminating test component execution.
09:32:49.148485 18650 NGAP_Emulation.ttcn:535 Terminating test component execution.
09:32:49.148801 18649 NGAP_Emulation.ttcn:614 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        successfulOutcome := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseComplete := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := ignore (1),
                            value_ := {
                                aMF_UE_NGAP_ID := 781
                            }
                        },
                        {
                            id := 85,
                            criticality := ignore (1),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:32:49.149018 18649 NGAP_Emulation.ttcn:614 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '20290023000003000A400320030D0055400200000079400F4099F907000000000099F907000001'O
}
09:32:49.149100 18650 - Function main was stopped. PTC terminates.
09:32:49.149162 18648 - Function main was stopped. PTC terminates.
09:32:49.149191 18650 - Terminating component type NGAP_Emulation.NGAP_Emulation_CT.
09:32:49.149233 18650 - Removing unterminated mapping between port NGAP and system:NGAP_CODEC_PT.
09:32:49.149243 18648 - Terminating component type GTPv1U_Emulation.GTPv1U_Emulation_CT.
09:32:49.149314 18648 - Default with id 1 (altstep as_uecups_ind) was deactivated.
09:32:49.149362 18649 NGAP_Emulation.ttcn:535 Connection of port NGAP_CLIENT to TC_ue_service_request_cm_idle_unknown_sess_active0(840):NGAP was closed unexpectedly by the peer.
09:32:49.149373 18648 - Removing unterminated mapping between port GTP1U and system:GTP1U.
09:32:49.149415 18649 NGAP_Emulation.ttcn:535 Port NGAP_CLIENT was disconnected from TC_ue_service_request_cm_idle_unknown_sess_active0(840):NGAP.
09:32:49.149449 18648 - Port GTP1U was unmapped from system:GTP1U.
09:32:49.149477 18649 NGAP_Emulation.ttcn:535 Connection of port NGAP_PROC to TC_ue_service_request_cm_idle_unknown_sess_active0(840):NGAP_PROC was closed unexpectedly by the peer.
09:32:49.149491 18648 - Port GTP1U was stopped.
09:32:49.149544 18649 NGAP_Emulation.ttcn:535 Port NGAP_PROC was disconnected from TC_ue_service_request_cm_idle_unknown_sess_active0(840):NGAP_PROC.
09:32:49.149554 18648 - Port TEID0 was stopped.
09:32:49.149590 18648 - Port CLIENT was stopped.
09:32:49.149594 18649 NGAP_Emulation.ttcn:535 Connection of port NGAP_UNIT to mtc:NGAP_UNIT[0] was closed unexpectedly by the peer.
09:32:49.149662 18648 - Port CLIENT_PROC was stopped.
09:32:49.149668 18650 - Port NGAP was unmapped from system:NGAP_CODEC_PT.
09:32:49.149675 18649 NGAP_Emulation.ttcn:535 Port NGAP_UNIT was disconnected from mtc:NGAP_UNIT[0].
09:32:49.149697 18648 - Removing unterminated mapping between port UECUPS and system:UECUPS.
09:32:49.149732 18650 - Port NGAP was stopped.
09:32:49.149763 18649 NGAP_Emulation.ttcn:535 Connection of port NGAP_PROC to mtc:NGAP_PROC[0] was closed unexpectedly by the peer.
09:32:49.149776 18650 - Port NGAP_CLIENT was stopped.
09:32:49.149805 18649 NGAP_Emulation.ttcn:535 Port NGAP_PROC was disconnected from mtc:NGAP_PROC[0].
09:32:49.149812 18650 - Port NGAP_PROC was stopped.
09:32:49.149850 18650 - Port NGAP_UNIT was stopped.
09:32:49.149851 18649 NGAP_Emulation.ttcn:535 Kill was requested from MC.
09:32:49.149884 18650 - Component type NGAP_Emulation.NGAP_Emulation_CT was shut down inside testcase TC_ue_service_request_cm_idle_unknown_sess_active.
09:32:49.149898 18649 NGAP_Emulation.ttcn:535 Terminating test component execution.
09:32:49.149929 18650 - Final verdict of PTC: none
09:32:49.150067 18650 - Disconnected from MC.
09:32:49.150112 18650 - TTCN-3 Parallel Test Component finished.
09:32:49.150499 18649 - Function main was stopped. PTC terminates.
09:32:49.150618 18649 - Terminating component type NGAP_Emulation.NGAP_Emulation_CT.
09:32:49.150670 18649 - Removing unterminated mapping between port NGAP and system:NGAP_CODEC_PT.
09:32:49.150768 18648 - Port UECUPS was unmapped from system:UECUPS.
09:32:49.150940 18648 - Port UECUPS was stopped.
09:32:49.151021 18648 - Component type GTPv1U_Emulation.GTPv1U_Emulation_CT was shut down inside testcase TC_ue_service_request_cm_idle_unknown_sess_active.
09:32:49.151143 18649 - Port NGAP was unmapped from system:NGAP_CODEC_PT.
09:32:49.151144 18648 - Final verdict of PTC: none
09:32:49.151207 18649 - Port NGAP was stopped.
09:32:49.151267 18649 - Port NGAP_CLIENT was stopped.
09:32:49.151295 18649 - Port NGAP_PROC was stopped.
09:32:49.151324 18649 - Port NGAP_UNIT was stopped.
09:32:49.151329 18648 - Disconnected from MC.
09:32:49.151353 18649 - Component type NGAP_Emulation.NGAP_Emulation_CT was shut down inside testcase TC_ue_service_request_cm_idle_unknown_sess_active.
09:32:49.151386 18648 - TTCN-3 Parallel Test Component finished.
09:32:49.151391 18649 - Final verdict of PTC: none
09:32:49.151517 18649 - Disconnected from MC.
09:32:49.151550 18649 - TTCN-3 Parallel Test Component finished.
09:32:49.151558 13891 C5G_Tests.ttcn:636 Setting final verdict of the test case.
09:32:49.151649 13891 C5G_Tests.ttcn:636 Local verdict of MTC: pass
09:32:49.151741 13891 C5G_Tests.ttcn:636 Local verdict of PTC GTP1U_EM(837): none (pass -> pass)
09:32:49.151814 13891 C5G_Tests.ttcn:636 Local verdict of PTC TC_ue_service_request_cm_idle_unknown_sess_active-NGAP0(838): none (pass -> pass)
09:32:49.151923 13891 C5G_Tests.ttcn:636 Local verdict of PTC TC_ue_service_request_cm_idle_unknown_sess_active-NGAP1(839): none (pass -> pass)
09:32:49.151976 13891 C5G_Tests.ttcn:636 Local verdict of PTC TC_ue_service_request_cm_idle_unknown_sess_active0(840): none (pass -> pass)
09:32:49.152016 13891 C5G_Tests.ttcn:636 Test case TC_ue_service_request_cm_idle_unknown_sess_active finished. Verdict: pass
09:32:49.152059 13891 C5G_Tests.ttcn:636 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-stop.sh C5G_Tests.TC_ue_service_request_cm_idle_unknown_sess_active pass'.
09:32:51.205855 13891 C5G_Tests.ttcn:636 External command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-stop.sh C5G_Tests.TC_ue_service_request_cm_idle_unknown_sess_active pass' was executed successfully (exit status: 0).
09:32:51.205916 13891 C5G_Tests.ttcn:651 Switching to log file `C5G_Tests-TC_ue_service_request_cm_connected-6eab31b835ad-mtc-13891.log'
