03:25:56.683052 24 BTS_Tests.ttcn:7897 Starting external command `../ttcn3-tcpdump-start.sh BTS_Tests.TC_lapdm_selftest'.
03:25:57.692557 24 BTS_Tests.ttcn:7897 External command `../ttcn3-tcpdump-start.sh BTS_Tests.TC_lapdm_selftest' was executed successfully (exit status: 0).
03:25:57.692757 24 BTS_Tests.ttcn:7897 Test case TC_lapdm_selftest started.
03:25:57.692803 24 BTS_Tests.ttcn:7897 Initializing variables, timers and ports of component type BTS_Tests.test_CT inside testcase TC_lapdm_selftest.
03:25:57.692943 24 BTS_Tests.ttcn:7897 Port IPA_CTRL was started.
03:25:57.692972 24 BTS_Tests.ttcn:7897 Port RSL_CCHAN was started.
03:25:57.692992 24 BTS_Tests.ttcn:7897 Port L1CTL was started.
03:25:57.693012 24 BTS_Tests.ttcn:7897 Port BTS_TRXC was started.
03:25:57.693032 24 BTS_Tests.ttcn:7897 Port BTSVTY was started.
03:25:57.693051 24 BTS_Tests.ttcn:7897 Port BSCVTY was started.
03:25:57.693070 24 BTS_Tests.ttcn:7897 Port PCU was started.
03:25:57.693090 24 BTS_Tests.ttcn:7897 Component type BTS_Tests.test_CT was initialized.
03:25:57.693734 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Stream before decoding: '030301'O
03:25:57.694369 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Decoded @LAPDm_Types.LapdmFrameAB: { addr := { spare := '0'B, lpd := 0, sapi := 0, c_r := true, ea := true }, ctrl := { u := { u := '000'B, p_f := false, u2 := '00'B, spare := '11'B } }, len := 0, m := false, el := 1, payload := ''O, padding := ''O }
03:25:57.694740 24 BTS_Tests.ttcn:7884 "ui_s0_empty": matched
03:25:57.694795 24 BTS_Tests.ttcn:7885 setverdict(pass): none -> pass
03:25:57.694834 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Encoding @LAPDm_Types.LapdmFrame: { ab := { addr := { spare := '0'B, lpd := 0, sapi := 0, c_r := true, ea := true }, ctrl := { u := { u := '000'B, p_f := false, u2 := '00'B, spare := '11'B } }, len := 0, m := false, el := 1, payload := ''O, padding := ''O } }
03:25:57.695164 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Stream after encoding: '030301'O
03:25:57.695198 24 BTS_Tests.ttcn:7893 setverdict(pass): pass -> pass, component reason not changed
03:25:57.695300 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Stream before decoding: '0F0301'O
03:25:57.695336 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Decoded @LAPDm_Types.LapdmFrameAB: { addr := { spare := '0'B, lpd := 0, sapi := 3, c_r := true, ea := true }, ctrl := { u := { u := '000'B, p_f := false, u2 := '00'B, spare := '11'B } }, len := 0, m := false, el := 1, payload := ''O, padding := ''O }
03:25:57.695381 24 BTS_Tests.ttcn:7884 "ui_s3_empty": matched
03:25:57.695412 24 BTS_Tests.ttcn:7885 setverdict(pass): pass -> pass, component reason not changed
03:25:57.695440 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Encoding @LAPDm_Types.LapdmFrame: { ab := { addr := { spare := '0'B, lpd := 0, sapi := 3, c_r := true, ea := true }, ctrl := { u := { u := '000'B, p_f := false, u2 := '00'B, spare := '11'B } }, len := 0, m := false, el := 1, payload := ''O, padding := ''O } }
03:25:57.695492 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Stream after encoding: '0F0301'O
03:25:57.695515 24 BTS_Tests.ttcn:7893 setverdict(pass): pass -> pass, component reason not changed
03:25:57.695558 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Stream before decoding: '013F01'O
03:25:57.695586 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Decoded @LAPDm_Types.LapdmFrameAB: { addr := { spare := '0'B, lpd := 0, sapi := 0, c_r := false, ea := true }, ctrl := { u := { u := '001'B, p_f := true, u2 := '11'B, spare := '11'B } }, len := 0, m := false, el := 1, payload := ''O, padding := ''O }
03:25:57.695624 24 BTS_Tests.ttcn:7884 "sabm_s0_empty": matched
03:25:57.695653 24 BTS_Tests.ttcn:7885 setverdict(pass): pass -> pass, component reason not changed
03:25:57.695679 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Encoding @LAPDm_Types.LapdmFrame: { ab := { addr := { spare := '0'B, lpd := 0, sapi := 0, c_r := false, ea := true }, ctrl := { u := { u := '001'B, p_f := true, u2 := '11'B, spare := '11'B } }, len := 0, m := false, el := 1, payload := ''O, padding := ''O } }
03:25:57.695724 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Stream after encoding: '013F01'O
03:25:57.695746 24 BTS_Tests.ttcn:7893 setverdict(pass): pass -> pass, component reason not changed
03:25:57.695804 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Stream before decoding: '013F1123420815'O
03:25:57.695834 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Decoded @LAPDm_Types.LapdmFrameAB: { addr := { spare := '0'B, lpd := 0, sapi := 0, c_r := false, ea := true }, ctrl := { u := { u := '001'B, p_f := true, u2 := '11'B, spare := '11'B } }, len := 4, m := false, el := 1, payload := '23420815'O, padding := ''O }
03:25:57.695872 24 BTS_Tests.ttcn:7884 "sabm_s0_l3": matched
03:25:57.695900 24 BTS_Tests.ttcn:7885 setverdict(pass): pass -> pass, component reason not changed
03:25:57.695927 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Encoding @LAPDm_Types.LapdmFrame: { ab := { addr := { spare := '0'B, lpd := 0, sapi := 0, c_r := false, ea := true }, ctrl := { u := { u := '001'B, p_f := true, u2 := '11'B, spare := '11'B } }, len := 4, m := false, el := 1, payload := '23420815'O, padding := ''O } }
03:25:57.695972 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Stream after encoding: '013F1123420815'O
03:25:57.695996 24 BTS_Tests.ttcn:7893 setverdict(pass): pass -> pass, component reason not changed
03:25:57.696095 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Stream before decoding: '03E101'O
03:25:57.696135 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Decoded @LAPDm_Types.LapdmFrameAB: { addr := { spare := '0'B, lpd := 0, sapi := 0, c_r := true, ea := true }, ctrl := { s := { n_r := 7, p_f := false, s := '00'B, spare := '01'B } }, len := 0, m := false, el := 1, payload := ''O, padding := ''O }
03:25:57.696200 24 BTS_Tests.ttcn:7884 "rr_s0_7": matched
03:25:57.696230 24 BTS_Tests.ttcn:7885 setverdict(pass): pass -> pass, component reason not changed
03:25:57.696257 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Encoding @LAPDm_Types.LapdmFrame: { ab := { addr := { spare := '0'B, lpd := 0, sapi := 0, c_r := true, ea := true }, ctrl := { s := { n_r := 7, p_f := false, s := '00'B, spare := '01'B } }, len := 0, m := false, el := 1, payload := ''O, padding := ''O } }
03:25:57.696304 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Stream after encoding: '03E101'O
03:25:57.696326 24 BTS_Tests.ttcn:7893 setverdict(pass): pass -> pass, component reason not changed
03:25:57.696433 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Stream before decoding: '03000D063505'O
03:25:57.696476 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Decoded @LAPDm_Types.LapdmFrameAB: { addr := { spare := '0'B, lpd := 0, sapi := 0, c_r := true, ea := true }, ctrl := { i := { n_r := 0, p := false, n_s := 0, spare := '0'B } }, len := 3, m := false, el := 1, payload := '063505'O, padding := ''O }
03:25:57.696535 24 BTS_Tests.ttcn:7884 "I/0/0": matched
03:25:57.696569 24 BTS_Tests.ttcn:7885 setverdict(pass): pass -> pass, component reason not changed
03:25:57.696597 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Encoding @LAPDm_Types.LapdmFrame: { ab := { addr := { spare := '0'B, lpd := 0, sapi := 0, c_r := true, ea := true }, ctrl := { i := { n_r := 0, p := false, n_s := 0, spare := '0'B } }, len := 3, m := false, el := 1, payload := '063505'O, padding := ''O } }
03:25:57.696645 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Stream after encoding: '03000D063505'O
03:25:57.696668 24 BTS_Tests.ttcn:7893 setverdict(pass): pass -> pass, component reason not changed
03:25:57.696704 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Stream before decoding: '03E00D063505'O
03:25:57.696732 24 BTS_Tests.ttcn:7875 dec_LapdmFrameAB(): Decoded @LAPDm_Types.LapdmFrameAB: { addr := { spare := '0'B, lpd := 0, sapi := 0, c_r := true, ea := true }, ctrl := { i := { n_r := 7, p := false, n_s := 0, spare := '0'B } }, len := 3, m := false, el := 1, payload := '063505'O, padding := ''O }
03:25:57.696769 24 BTS_Tests.ttcn:7884 "I/7/0": matched
03:25:57.696799 24 BTS_Tests.ttcn:7885 setverdict(pass): pass -> pass, component reason not changed
03:25:57.696827 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Encoding @LAPDm_Types.LapdmFrame: { ab := { addr := { spare := '0'B, lpd := 0, sapi := 0, c_r := true, ea := true }, ctrl := { i := { n_r := 7, p := false, n_s := 0, spare := '0'B } }, len := 3, m := false, el := 1, payload := '063505'O, padding := ''O } }
03:25:57.696872 24 BTS_Tests.ttcn:7889 enc_LapdmFrame(): Stream after encoding: '03E00D063505'O
03:25:57.696905 24 BTS_Tests.ttcn:7893 setverdict(pass): pass -> pass, component reason not changed
03:25:57.696953 24 BTS_Tests.ttcn:7904 Terminating component type BTS_Tests.test_CT.
03:25:57.696981 24 BTS_Tests.ttcn:7904 Port IPA_CTRL was stopped.
03:25:57.697005 24 BTS_Tests.ttcn:7904 Port RSL_CCHAN was stopped.
03:25:57.697026 24 BTS_Tests.ttcn:7904 Port L1CTL was stopped.
03:25:57.697046 24 BTS_Tests.ttcn:7904 Port BTS_TRXC was stopped.
03:25:57.697066 24 BTS_Tests.ttcn:7904 Port BTSVTY was stopped.
03:25:57.697086 24 BTS_Tests.ttcn:7904 Port BSCVTY was stopped.
03:25:57.697105 24 BTS_Tests.ttcn:7904 Port PCU was stopped.
03:25:57.697125 24 BTS_Tests.ttcn:7904 Component type BTS_Tests.test_CT was shut down inside testcase TC_lapdm_selftest.
03:25:57.697151 24 BTS_Tests.ttcn:7904 Waiting for PTCs to finish.
03:25:57.697241 24 BTS_Tests.ttcn:7904 Setting final verdict of the test case.
03:25:57.697273 24 BTS_Tests.ttcn:7904 Local verdict of MTC: pass
03:25:57.697303 24 BTS_Tests.ttcn:7904 No PTCs were created.
03:25:57.697333 24 BTS_Tests.ttcn:7904 Test case TC_lapdm_selftest finished. Verdict: pass
03:25:57.697373 24 BTS_Tests.ttcn:7904 Starting external command `../ttcn3-tcpdump-stop.sh BTS_Tests.TC_lapdm_selftest pass'.
03:26:01.040644 24 BTS_Tests.ttcn:7904 External command `../ttcn3-tcpdump-stop.sh BTS_Tests.TC_lapdm_selftest pass' was executed successfully (exit status: 0).
03:26:01.040701 24 BTS_Tests.ttcn:8044 Switching to log file `BTS_Tests-TC_tch_sign_l2_fill_frame-a28ec9a6a10e-mtc-24.log'
