\doxysection{include/osmocom/gmr1/l1/rach.h File Reference}
\label{rach_8h}\index{include/osmocom/gmr1/l1/rach.h@{include/osmocom/gmr1/l1/rach.h}}


Osmocom GMR-\/1 RACH channel coding header.  


{\ttfamily \#include $<$stdint.\+h$>$}\newline
{\ttfamily \#include $<$osmocom/core/bits.\+h$>$}\newline
\doxysubsection*{Functions}
\begin{DoxyCompactItemize}
\item 
void \textbf{ gmr1\+\_\+rach\+\_\+encode} (ubit\+\_\+t $\ast$bits\+\_\+e, const uint8\+\_\+t $\ast$rach, uint8\+\_\+t sb\+\_\+mask)
\begin{DoxyCompactList}\small\item\em Stateless GMR-\/1 RACH channel coder. \end{DoxyCompactList}\item 
int \textbf{ gmr1\+\_\+rach\+\_\+decode} (uint8\+\_\+t $\ast$rach, const sbit\+\_\+t $\ast$bits\+\_\+e, uint8\+\_\+t sb\+\_\+mask, int $\ast$conv\+\_\+rv, int $\ast$crc\+\_\+rv)
\begin{DoxyCompactList}\small\item\em Stateless GMR-\/1 RACH channel decoder. \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
Osmocom GMR-\/1 RACH channel coding header. 

