===== test_gsm_authen
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000004620 LU-type=IMSI-ATTACH
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 001-868-1
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: rev=GSM net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000004620 id=901700000004620
DVLR New subscr, IMSI: 901700000004620
DVLR VLR subscr IMSI-901700000004620 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000004620 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000004026f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000004026f003222010585df1ae287f6e273dce07090d61320b21042d8b2c3e220861855fb81fc2a8000322201012aca96fb4ffdea5c985cbafa9b6e18b210420bde240220807fa7502e07e1c0003222010e7c03ba7cf0e2fde82b2dc4d63077d422104a29514ae2208e2b234f80788640003222010fa8f20b781b5881329d4fea26b1a3c5121045afc8d7222082392f14f709ae000032220100fd4cc8dbe8715d1f439e304edfd68dc2104bc8d1c5b2208da7cdd6bfe2d70000a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000004620) Received 5 auth tuples
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x1)
- sending GSM Auth Request for IMSI-901700000004620:GERAN-A:LU: tuple use_count=1 key_seq=0 auth_types=0x1 and...
- ...rand=585df1ae287f6e273dce07090d61320b
- ...expecting sres=2d8b2c3e
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- If the HLR were to send a GSUP _UPDATE_LOCATION_RESULT we'd still reject
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Event VLR_ULA_E_HLR_LU_RES not permitted
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends GSUP LU Req to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = 2d8b2c3e)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000004620) AUTH on GERAN received SRES/RES: 2d8b2c3e (4 bytes)
DVLR SUBSCR(IMSI-901700000004620) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000004026f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000004026f00804036470f10a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000004620 has MSISDN:46071
DMSC msub(IMSI-901700000004620:MSISDN-46071) VLR: update for IMSI=901700000004620 (MSISDN=46071)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
- sending LU Accept for IMSI-901700000004620:MSISDN-46071:GERAN-A:LU
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + attached: now used by 3 (active-conn,vlr_gsup_rx,attached)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU))
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Deferring: will deallocate with upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU))
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: - lu: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 4 (active-conn,vlr_gsup_rx,attached,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 5 (active-conn,vlr_gsup_rx,attached,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,vlr_gsup_rx,attached,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 3 (active-conn,vlr_gsup_rx,attached)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Deferring: will deallocate with upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Deallocated, including all deferred deallocations
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 2 (active-conn,attached)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
  bssap_clear_sent == 1
- LU was successful, and the conn has already been closed
  lu_result_sent == 1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DMSC msub(IMSI-901700000004620:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- after a while, a new conn sends a CM Service Request. VLR responds with Auth Req, 2nd auth vector
  MSC <--GERAN-A-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(IMSI-901700000004620:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=Short-Messaging-Service
DREF msc_a(IMSI-901700000004620:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_sms: now used by 2 (rx_from_ms,cm_service_sms)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000004620:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000004620:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=GSM net=GERAN Auth (no Ciph)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=1 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x1)
- sending GSM Auth Request for IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ: tuple use_count=1 key_seq=1 auth_types=0x1 and...
- ...rand=12aca96fb4ffdea5c985cbafa9b6e18b
- ...expecting sres=20bde240
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (cm_service_sms)
  cm_service_result_sent == 0
  auth_request_sent == 1
- needs auth, not yet accepted
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- MS sends Authen Response, VLR accepts with a CM Service Accept
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (cm_service_sms,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = 20bde240)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071) AUTH on GERAN received SRES/RES: 20bde240 (4 bytes)
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_CM_SERV_ACC
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_CM_SERV_ACC: 0521
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (cm_service_sms)
  cm_service_result_sent == 1
- Concluding CM Service Request
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - cm_service_sms: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
  bssap_clear_sent == 1
- all requests serviced, conn has been released
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 2
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000004620:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- an SMS is sent, MS is paged
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + test_gsm_authen: now used by 2 (attached,test_gsm_authen)
  llist_count(&vsub->cs.requests) == 0
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + SMS-receiver: now used by 3 (attached,test_gsm_authen,SMS-receiver)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + SMS: now used by 4 (attached,test_gsm_authen,SMS-receiver,SMS)
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071 callref-0x40000001 tid-0) New transaction
DLSMS SMC(0) instance created for network
DLSMS SMR(0) instance created for network.
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071 callref-0x40000001 tid-0) Going to send a MT SMS
DLSMS SMR(0) message SM-RL-DATA_REQ received in state IDLE
DLSMS SMR(0) TX SMS RP-DATA
DLSMS SMR(0) new RP state IDLE -> WAIT_FOR_RP_ACK
DLSMS SMC(0) message MNSMS-EST-REQ received in state IDLE
DLSMS SMC(0) new CP state IDLE -> MM_CONN_PENDING
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071 callref-0x40000001 tid-0) Initiating Paging due to MMSMS_EST_REQ
DPAG Paging: IMSI-901700000004620:MSISDN-46071 for MT-SMS: Starting paging
  paging request (SIGNALLING_LOW_PRIO) to IMSI-901700000004620:MSISDN-46071 on GERAN-A
  strcmp(paging_expecting_imsi, vsub->imsi) == 0
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + Paging: now used by 5 (attached,test_gsm_authen,SMS-receiver,SMS,Paging)
  llist_count(&vsub->cs.requests) == 1
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - test_gsm_authen: now used by 4 (attached,SMS-receiver,SMS,Paging)
  paging_sent == 1
- the subscriber and its pending request should remain
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + test_gsm_authen: now used by 5 (attached,SMS-receiver,SMS,Paging,test_gsm_authen)
  llist_count(&vsub->cs.requests) == 1
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - test_gsm_authen: now used by 4 (attached,SMS-receiver,SMS,Paging)
- MS replies with Paging Response, and VLR sends Auth Request with third key
  MSC <--GERAN-A-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: RR GSM48_MT_RR_PAG_RESP
DRR msc_a(IMSI-901700000004620:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Rx PAGING RESPONSE IMSI-901700000004620
DREF msc_a(IMSI-901700000004620:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: + paging-response: now used by 2 (rx_from_ms,paging-response)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000004620:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000004620:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: rev=GSM net=GERAN Auth (no Ciph)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 5 (attached,SMS-receiver,SMS,Paging,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + active-conn: now used by 6 (attached,SMS-receiver,SMS,Paging,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=2 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x1)
- sending GSM Auth Request for IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP: tuple use_count=1 key_seq=2 auth_types=0x1 and...
- ...rand=e7c03ba7cf0e2fde82b2dc4d63077d42
- ...expecting sres=a29514ae
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 5 (attached,SMS-receiver,SMS,Paging,active-conn)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (paging-response)
  auth_request_sent == 1
- needs auth, not yet accepted
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- MS sends Authen Response, VLR accepts and sends pending SMS
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (paging-response,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = a29514ae)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071) AUTH on GERAN received SRES/RES: a29514ae (4 bytes)
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DPAG Paging: IMSI-901700000004620:MSISDN-46071 for MT-SMS: Paging Response action (success)
DPAG Paging: IMSI-901700000004620:MSISDN-46071 for MT-SMS: Removing Paging Request
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071 callref-0x40000001 tid-0) mmsms_paging_cb(success)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + sms: now used by 3 (paging-response,rx_from_ms,sms)
DLSMS SMC(0) message MMSMS-EST-CNF received in state MM_CONN_PENDING
DLSMS SMC(0) send CP data
DLSMS SMC(0) new CP state MM_CONN_PENDING -> WAIT_CP_ACK
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x40000001 tid-0) sending CP message (trans=0)
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x40000001 tid-0) GSM4.11 TX 09 01 58 01 00 07 91 44 77 58 10 06 50 00 4c 00 05 80 64 70 f1 00 00 07 10 10 00 00 00 00 44 50 79 da 1e 1e e7 41 69 37 48 5e 9e a7 c9 65 37 3d 1d 66 83 c2 70 38 3b 3d 0e d3 d3 6f f7 1c 94 9e 83 c2 20 72 79 9e 96 87 c5 ec 32 a8 1d 96 af cb f4 b4 fb 0c 7a c3 e9 e9 b7 db 05 
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Sending DTAP: SMS SMS:0x01
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: SMS:0x01: 09015801000791447758100650004c0005806470f1000007101000000000445079da1e1ee7416937485e9ea7c965373d1d6683c270383b3d0ed3d36ff71c949e83c22072799e9687c5ec32a81d96afcbf4b4fb0c7ac3e9e9b7db05
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - Paging: now used by 4 (attached,SMS-receiver,SMS,active-conn)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - paging-response: now used by 2 (rx_from_ms,sms)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (sms)
  dtap_tx_confirmed == 1
- SMS was delivered, no requests pending for subscr
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + test_gsm_authen: now used by 5 (attached,SMS-receiver,SMS,active-conn,test_gsm_authen)
  llist_count(&vsub->cs.requests) == 0
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - test_gsm_authen: now used by 4 (attached,SMS-receiver,SMS,active-conn)
- conn is still open to wait for SMS ack dance
  llist_count(&msub_list) == 1
- MS replies with CP-ACK for received SMS
  MSC <--GERAN-A-- MS: SMS:0x04
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (sms,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: SMS SMS:0x04
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x40000001 tid-0) receiving SMS message SMS:0x04
DLSMS SMC(0) message MMSMS-DATA-IND (CP ACK) received in state WAIT_CP_ACK
DLSMS SMC(0) received CP-ACK
DLSMS SMC(0) new CP state WAIT_CP_ACK -> MM_ESTABLISHED
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (sms)
  llist_count(&msub_list) == 1
- MS also sends RP-ACK, MSC in turn sends CP-ACK for that
  MSC <--GERAN-A-- MS: SMS:0x01
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (sms,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: SMS SMS:0x01
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x40000001 tid-0) receiving SMS message SMS:0x01
DLSMS SMC(0) message MMSMS-DATA-IND (CP DATA) received in state MM_ESTABLISHED
DLSMS SMC(0) received CP-DATA
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x40000001 tid-0) sending CP message (trans=0)
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x40000001 tid-0) GSM4.11 TX 09 04 
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Sending DTAP: SMS SMS:0x04
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: SMS:0x04: 0904
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x40000001 tid-0) MNSMS-DATA/EST-IND
DLSMS SMR(0) message MNSMS-DATA-IND received in state WAIT_FOR_RP_ACK
DLSMS SMR(0) RX SMS RP-ACK
DLSMS SMR(0) new RP state WAIT_FOR_RP_ACK -> IDLE
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x40000001 tid-0) RX SMS RP-ACK (MO)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - SMS-receiver: now used by 3 (attached,SMS,active-conn)
DLSMS SMR(0) TX: MNSMS-REL-REQ
DLSMS SMC(0) message MNSMS-REL-REQ received in state MM_ESTABLISHED
DLSMS SMC(0) new CP state MM_ESTABLISHED -> IDLE
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x40000001 tid-0) Got MMSMS_REL_REQ, destroying transaction.
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x40000001 tid-0) Freeing transaction
DLSMS SMR(0) clearing SMR instance
DLSMS SMC(0) clearing instance
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - SMS: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - sms: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
  dtap_tx_confirmed == 1
  bssap_clear_sent == 1
- SMS is done, conn is gone
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP))
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msub(IMSI-901700000004620:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- subscriber detaches
  MSC <--GERAN-A-- MS: GSM48_MT_MM_IMSI_DETACH_IND
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_IMSI_DETACH_IND
DMM IMSI DETACH INDICATION: IMSI-901700000004620
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + gsm48_rx_mm_imsi_detach_ind: now used by 2 (attached,gsm48_rx_mm_imsi_detach_ind)
DMM IMSI DETACH for IMSI-901700000004620:MSISDN-46071
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + active-conn: now used by 3 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn)
GSUP --> HLR: OSMO_GSUP_MSGT_PURGE_MS_REQUEST: 0c010809710000004026f02801020a0101
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - attached: now used by 2 (gsm48_rx_mm_imsi_detach_ind,active-conn)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - gsm48_rx_mm_imsi_detach_ind: now used by 1 (active-conn)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_CN_CLOSE
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: Releasing: msc_a use is 1 (rx_from_ms)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 2 (active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 2 (active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 2 (rx_from_ms,wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 1 (active-conn)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: - rx_from_ms: now used by 1 (wait-Clear-Complete)
  bssap_clear_sent == 1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASED}: max total use count was 2
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE)
DMSC msub(IMSI-901700000004620:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - active-conn: now used by 0 (-)
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071) freeing VLR subscr (max total use count was 6)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
===== test_gsm_authen: SUCCESS

===== test_gsm_authen_tmsi
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000004620 LU-type=IMSI-ATTACH
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 001-868-1
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: rev=GSM net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000004620 id=901700000004620
DVLR New subscr, IMSI: 901700000004620
DVLR VLR subscr IMSI-901700000004620 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000004620 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000004026f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000004026f003222010585df1ae287f6e273dce07090d61320b21042d8b2c3e220861855fb81fc2a8000322201012aca96fb4ffdea5c985cbafa9b6e18b210420bde240220807fa7502e07e1c0003222010e7c03ba7cf0e2fde82b2dc4d63077d422104a29514ae2208e2b234f80788640003222010fa8f20b781b5881329d4fea26b1a3c5121045afc8d7222082392f14f709ae000032220100fd4cc8dbe8715d1f439e304edfd68dc2104bc8d1c5b2208da7cdd6bfe2d70000a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000004620) Received 5 auth tuples
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x1)
- sending GSM Auth Request for IMSI-901700000004620:GERAN-A:LU: tuple use_count=1 key_seq=0 auth_types=0x1 and...
- ...rand=585df1ae287f6e273dce07090d61320b
- ...expecting sres=2d8b2c3e
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- If the HLR were to send a GSUP _UPDATE_LOCATION_RESULT we'd still reject
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Event VLR_ULA_E_HLR_LU_RES not permitted
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends GSUP LU Req to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = 2d8b2c3e)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000004620) AUTH on GERAN received SRES/RES: 2d8b2c3e (4 bytes)
DVLR SUBSCR(IMSI-901700000004620) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000004026f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000004026f00804036470f10a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000004620 has MSISDN:46071
DMSC msub(IMSI-901700000004620:MSISDN-46071) VLR: update for IMSI=901700000004620 (MSISDN=46071)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: lu_compl_vlr_new_tmsi()
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100) VLR: update for IMSI=901700000004620 (MSISDN=46071)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_TMSI_CNF
- sending LU Accept for IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU, with TMSI 0x03020100
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
- a LU Accept with a new TMSI was sent, waiting for TMSI Realloc Compl
  llist_count(&msub_list) == 1
  lu_result_sent == 1
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- even though the TMSI is not acked, we can already find the subscr with it
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100 + test_gsm_authen_tmsi: now used by 2 (active-conn,test_gsm_authen_tmsi)
  vsub != NULL == 1
  strcmp(vsub->imsi, imsi) == 0
  vsub->tmsi_new == 0x03020100
  vsub->tmsi == 0xffffffff
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100 - test_gsm_authen_tmsi: now used by 1 (active-conn)
- MS sends TMSI Realloc Complete
  MSC <--GERAN-A-- MS: GSM48_MT_MM_TMSI_REALL_COMPL
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_TMSI_REALL_COMPL
DMM msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: TMSI Reallocation Completed
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_NEW_TMSI_ACK
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: Received Event LU_COMPL_VLR_E_NEW_TMSI_ACK
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) VLR: update for IMSI=901700000004620 (MSISDN=46071)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + attached: now used by 2 (active-conn,attached)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: - lu: now used by 1 (rx_from_ms)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_DONE}: Deallocated
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,attached,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (active-conn,attached)
  bssap_clear_sent == 1
- LU was successful, and the conn has already been closed
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
- Subscriber has the new TMSI
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + test_gsm_authen_tmsi: now used by 2 (attached,test_gsm_authen_tmsi)
  vsub != NULL == 1
  strcmp(vsub->imsi, imsi) == 0
  vsub->tmsi_new == 0xffffffff
  vsub->tmsi == 0x03020100
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - test_gsm_authen_tmsi: now used by 1 (attached)


- after a while, a new conn sends a CM Service Request using above TMSI. VLR responds with Auth Req, 2nd auth vector
  MSC <--GERAN-A-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=Short-Messaging-Service
DREF msc_a(TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_sms: now used by 2 (rx_from_ms,cm_service_sms)
DVLR Process_Access_Request_VLR(TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=GSM net=GERAN Auth (no Ciph)
DVLR Process_Access_Request_VLR(TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=1 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x1)
- sending GSM Auth Request for IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ: tuple use_count=1 key_seq=1 auth_types=0x1 and...
- ...rand=12aca96fb4ffdea5c985cbafa9b6e18b
- ...expecting sres=20bde240
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (cm_service_sms)
  cm_service_result_sent == 0
  auth_request_sent == 1
- needs auth, not yet accepted
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- MS sends Authen Response, VLR accepts with a CM Service Accept
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (cm_service_sms,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = 20bde240)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) AUTH on GERAN received SRES/RES: 20bde240 (4 bytes)
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_CM_SERV_ACC
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_CM_SERV_ACC: 0521
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (cm_service_sms)
  cm_service_result_sent == 1
- Concluding CM Service Request
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - cm_service_sms: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
  bssap_clear_sent == 1
- all requests serviced, conn has been released
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 2
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- an SMS is sent, MS is paged
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + test_gsm_authen_tmsi: now used by 2 (attached,test_gsm_authen_tmsi)
  llist_count(&vsub->cs.requests) == 0
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + SMS-receiver: now used by 3 (attached,test_gsm_authen_tmsi,SMS-receiver)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + SMS: now used by 4 (attached,test_gsm_authen_tmsi,SMS-receiver,SMS)
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 callref-0x40000002 tid-0) New transaction
DLSMS SMC(0) instance created for network
DLSMS SMR(0) instance created for network.
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 callref-0x40000002 tid-0) Going to send a MT SMS
DLSMS SMR(0) message SM-RL-DATA_REQ received in state IDLE
DLSMS SMR(0) TX SMS RP-DATA
DLSMS SMR(0) new RP state IDLE -> WAIT_FOR_RP_ACK
DLSMS SMC(0) message MNSMS-EST-REQ received in state IDLE
DLSMS SMC(0) new CP state IDLE -> MM_CONN_PENDING
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 callref-0x40000002 tid-0) Initiating Paging due to MMSMS_EST_REQ
DPAG Paging: IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 for MT-SMS: Starting paging
  paging request (SIGNALLING_LOW_PRIO) to IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 on GERAN-A
  paging_expecting_tmsi == 0x03020100
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + Paging: now used by 5 (attached,test_gsm_authen_tmsi,SMS-receiver,SMS,Paging)
  llist_count(&vsub->cs.requests) == 1
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - test_gsm_authen_tmsi: now used by 4 (attached,SMS-receiver,SMS,Paging)
  paging_sent == 1
- the subscriber and its pending request should remain
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + test_gsm_authen_tmsi: now used by 5 (attached,SMS-receiver,SMS,Paging,test_gsm_authen_tmsi)
  llist_count(&vsub->cs.requests) == 1
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - test_gsm_authen_tmsi: now used by 4 (attached,SMS-receiver,SMS,Paging)
- MS replies with Paging Response using TMSI, and VLR sends Auth Request with third key
  MSC <--GERAN-A-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: RR GSM48_MT_RR_PAG_RESP
DRR msc_a(TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Rx PAGING RESPONSE TMSI-0x03020100
DREF msc_a(TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: + paging-response: now used by 2 (rx_from_ms,paging-response)
DVLR Process_Access_Request_VLR(TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: is child of msc_a(TMSI-0x03020100:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: rev=GSM net=GERAN Auth (no Ciph)
DVLR Process_Access_Request_VLR(TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + proc_arq_vlr_fn_init: now used by 5 (attached,SMS-receiver,SMS,Paging,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + active-conn: now used by 6 (attached,SMS-receiver,SMS,Paging,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=2 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x1)
- sending GSM Auth Request for IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP: tuple use_count=1 key_seq=2 auth_types=0x1 and...
- ...rand=e7c03ba7cf0e2fde82b2dc4d63077d42
- ...expecting sres=a29514ae
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - proc_arq_vlr_fn_init: now used by 5 (attached,SMS-receiver,SMS,Paging,active-conn)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (paging-response)
  auth_request_sent == 1
- needs auth, not yet accepted
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- MS sends Authen Response, VLR accepts and sends pending SMS
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (paging-response,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = a29514ae)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) AUTH on GERAN received SRES/RES: a29514ae (4 bytes)
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DPAG Paging: IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 for MT-SMS: Paging Response action (success)
DPAG Paging: IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 for MT-SMS: Removing Paging Request
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 callref-0x40000002 tid-0) mmsms_paging_cb(success)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + sms: now used by 3 (paging-response,rx_from_ms,sms)
DLSMS SMC(0) message MMSMS-EST-CNF received in state MM_CONN_PENDING
DLSMS SMC(0) send CP data
DLSMS SMC(0) new CP state MM_CONN_PENDING -> WAIT_CP_ACK
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP callref-0x40000002 tid-0) sending CP message (trans=0)
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP callref-0x40000002 tid-0) GSM4.11 TX 09 01 58 01 00 07 91 44 77 58 10 06 50 00 4c 00 05 80 64 70 f1 00 00 07 10 10 00 00 00 00 44 50 79 da 1e 1e e7 41 69 37 48 5e 9e a7 c9 65 37 3d 1d 66 83 c2 70 38 3b 3d 0e d3 d3 6f f7 1c 94 9e 83 c2 20 72 79 9e 96 87 c5 ec 32 a8 1d 96 af cb f4 b4 fb 0c 7a c3 e9 e9 b7 db 05 
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Sending DTAP: SMS SMS:0x01
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: SMS:0x01: 09015801000791447758100650004c0005806470f1000007101000000000445079da1e1ee7416937485e9ea7c965373d1d6683c270383b3d0ed3d36ff71c949e83c22072799e9687c5ec32a81d96afcbf4b4fb0c7ac3e9e9b7db05
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - Paging: now used by 4 (attached,SMS-receiver,SMS,active-conn)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - paging-response: now used by 2 (rx_from_ms,sms)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (sms)
  dtap_tx_confirmed == 1
- SMS was delivered, no requests pending for subscr
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + test_gsm_authen_tmsi: now used by 5 (attached,SMS-receiver,SMS,active-conn,test_gsm_authen_tmsi)
  llist_count(&vsub->cs.requests) == 0
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - test_gsm_authen_tmsi: now used by 4 (attached,SMS-receiver,SMS,active-conn)
- conn is still open to wait for SMS ack dance
  llist_count(&msub_list) == 1
- MS replies with CP-ACK for received SMS
  MSC <--GERAN-A-- MS: SMS:0x04
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (sms,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: SMS SMS:0x04
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP callref-0x40000002 tid-0) receiving SMS message SMS:0x04
DLSMS SMC(0) message MMSMS-DATA-IND (CP ACK) received in state WAIT_CP_ACK
DLSMS SMC(0) received CP-ACK
DLSMS SMC(0) new CP state WAIT_CP_ACK -> MM_ESTABLISHED
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (sms)
  llist_count(&msub_list) == 1
- MS also sends RP-ACK, MSC in turn sends CP-ACK for that
  MSC <--GERAN-A-- MS: SMS:0x01
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (sms,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: SMS SMS:0x01
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP callref-0x40000002 tid-0) receiving SMS message SMS:0x01
DLSMS SMC(0) message MMSMS-DATA-IND (CP DATA) received in state MM_ESTABLISHED
DLSMS SMC(0) received CP-DATA
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP callref-0x40000002 tid-0) sending CP message (trans=0)
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP callref-0x40000002 tid-0) GSM4.11 TX 09 04 
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Sending DTAP: SMS SMS:0x04
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: SMS:0x04: 0904
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP callref-0x40000002 tid-0) MNSMS-DATA/EST-IND
DLSMS SMR(0) message MNSMS-DATA-IND received in state WAIT_FOR_RP_ACK
DLSMS SMR(0) RX SMS RP-ACK
DLSMS SMR(0) new RP state WAIT_FOR_RP_ACK -> IDLE
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP callref-0x40000002 tid-0) RX SMS RP-ACK (MO)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - SMS-receiver: now used by 3 (attached,SMS,active-conn)
DLSMS SMR(0) TX: MNSMS-REL-REQ
DLSMS SMC(0) message MNSMS-REL-REQ received in state MM_ESTABLISHED
DLSMS SMC(0) new CP state MM_ESTABLISHED -> IDLE
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP callref-0x40000002 tid-0) Got MMSMS_REL_REQ, destroying transaction.
DLSMS trans(SMS IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP callref-0x40000002 tid-0) Freeing transaction
DLSMS SMR(0) clearing SMR instance
DLSMS SMC(0) clearing instance
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - SMS: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - sms: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
  dtap_tx_confirmed == 1
  bssap_clear_sent == 1
- SMS is done, conn is gone
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP))
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP)
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- subscriber sends LU Request, this time with the TMSI
- Location Update request causes an Auth Req to MS
  MSC <--GERAN-A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=TMSI-0x03020100 LU-type=IMSI-ATTACH
DMM msc_a(TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 001-868-1
DREF msc_a(TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_IDLE}: is child of msc_a(TMSI-0x03020100:GERAN-A:LU)
DVLR vlr_lu_fsm(TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_IDLE}: rev=GSM net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + _lu_fsm_associate_vsub: now used by 2 (attached,_lu_fsm_associate_vsub)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + active-conn: now used by 3 (attached,_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - _lu_fsm_associate_vsub: now used by 2 (attached,active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=3 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x1)
- sending GSM Auth Request for IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU: tuple use_count=1 key_seq=3 auth_types=0x1 and...
- ...rand=fa8f20b781b5881329d4fea26b1a3c51
- ...expecting sres=5afc8d72
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends GSUP LU Req to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = 5afc8d72)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) AUTH on GERAN received SRES/RES: 5afc8d72 (4 bytes)
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000004026f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
DVLR VLR_Authenticate(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000004026f00804036470f10a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + vlr_gsup_rx: now used by 3 (attached,active-conn,vlr_gsup_rx)
DVLR IMSI:901700000004620 has MSISDN:46071
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) VLR: update for IMSI=901700000004620 (MSISDN=46071)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - vlr_gsup_rx: now used by 2 (attached,active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + vlr_gsup_rx: now used by 3 (attached,active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: lu_compl_vlr_new_tmsi()
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504) VLR: update for IMSI=901700000004620 (MSISDN=46071)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_TMSI_CNF
- sending LU Accept for IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU, with TMSI 0x07060504
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504 - vlr_gsup_rx: now used by 2 (attached,active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
- a LU Accept with a new TMSI was sent, waiting for TMSI Realloc Compl
  llist_count(&msub_list) == 1
  lu_result_sent == 1
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- even though the TMSI is not acked, we can already find the subscr with it
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504 + test_gsm_authen_tmsi: now used by 3 (attached,active-conn,test_gsm_authen_tmsi)
  vsub != NULL == 1
  strcmp(vsub->imsi, imsi) == 0
  vsub->tmsi_new == 0x07060504
  vsub->tmsi == 0x03020100
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504 - test_gsm_authen_tmsi: now used by 2 (attached,active-conn)
- MS sends TMSI Realloc Complete
  MSC <--GERAN-A-- MS: GSM48_MT_MM_TMSI_REALL_COMPL
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_TMSI_REALL_COMPL
DMM msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: TMSI Reallocation Completed
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:TMSInew-0x07060504:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_NEW_TMSI_ACK
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: Received Event LU_COMPL_VLR_E_NEW_TMSI_ACK
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504) VLR: update for IMSI=901700000004620 (MSISDN=46071)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: - lu: now used by 1 (rx_from_ms)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){VLR_ULA_S_DONE}: Deallocated
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
  bssap_clear_sent == 1
- LU was successful, and the conn has already been closed
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU)
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
- subscriber has the new TMSI
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 + test_gsm_authen_tmsi: now used by 2 (attached,test_gsm_authen_tmsi)
  vsub != NULL == 1
  strcmp(vsub->imsi, imsi) == 0
  vsub->tmsi_new == 0xffffffff
  vsub->tmsi == 0x07060504
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 - test_gsm_authen_tmsi: now used by 1 (attached)


- subscriber detaches, using new TMSI
  MSC <--GERAN-A-- MS: GSM48_MT_MM_IMSI_DETACH_IND
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_IMSI_DETACH_IND
DMM IMSI DETACH INDICATION: TMSI-0x07060504
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 + gsm48_rx_mm_imsi_detach_ind: now used by 2 (attached,gsm48_rx_mm_imsi_detach_ind)
DMM IMSI DETACH for IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 + active-conn: now used by 3 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn)
GSUP --> HLR: OSMO_GSUP_MSGT_PURGE_MS_REQUEST: 0c010809710000004026f02801020a0101
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 - attached: now used by 2 (gsm48_rx_mm_imsi_detach_ind,active-conn)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 - gsm48_rx_mm_imsi_detach_ind: now used by 1 (active-conn)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_CN_CLOSE
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASING}: Releasing: msc_a use is 1 (rx_from_ms)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 + msc_a_fsm_releasing_onenter: now used by 2 (active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 + vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 - vlr_subscr_cancel_attach_fsm: now used by 2 (active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 2 (rx_from_ms,wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 - msc_a_fsm_releasing_onenter: now used by 1 (active-conn)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASING}: - rx_from_ms: now used by 1 (wait-Clear-Complete)
  bssap_clear_sent == 1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASED}: max total use count was 2
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE)
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504 - active-conn: now used by 0 (-)
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504) freeing VLR subscr (max total use count was 6)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x07060504:GERAN-A:NONE){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
===== test_gsm_authen_tmsi: SUCCESS

===== test_gsm_authen_imei
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000004620 LU-type=IMSI-ATTACH
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 001-868-1
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: rev=GSM net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000004620 id=901700000004620
DVLR New subscr, IMSI: 901700000004620
DVLR VLR subscr IMSI-901700000004620 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000004620 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000004026f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000004026f003222010585df1ae287f6e273dce07090d61320b21042d8b2c3e220861855fb81fc2a8000322201012aca96fb4ffdea5c985cbafa9b6e18b210420bde240220807fa7502e07e1c0003222010e7c03ba7cf0e2fde82b2dc4d63077d422104a29514ae2208e2b234f80788640003222010fa8f20b781b5881329d4fea26b1a3c5121045afc8d7222082392f14f709ae000032220100fd4cc8dbe8715d1f439e304edfd68dc2104bc8d1c5b2208da7cdd6bfe2d70000a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000004620) Received 5 auth tuples
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x1)
- sending GSM Auth Request for IMSI-901700000004620:GERAN-A:LU: tuple use_count=1 key_seq=0 auth_types=0x1 and...
- ...rand=585df1ae287f6e273dce07090d61320b
- ...expecting sres=2d8b2c3e
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- If the HLR were to send a GSUP _UPDATE_LOCATION_RESULT we'd still reject
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Event VLR_ULA_E_HLR_LU_RES not permitted
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends GSUP LU Req to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = 2d8b2c3e)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000004620) AUTH on GERAN received SRES/RES: 2d8b2c3e (4 bytes)
DVLR SUBSCR(IMSI-901700000004620) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000004026f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000004026f00804036470f10a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000004620 has MSISDN:46071
DMSC msub(IMSI-901700000004620:MSISDN-46071) VLR: update for IMSI=901700000004620 (MSISDN=46071)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT, and we send an ID Request for the IMEI to the MS
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_IMEI
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_ID_REQ
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_ID_REQ: 051802
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
- We will only do business when the IMEI is known
  llist_count(&msub_list) == 1
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + test_gsm_authen_imei: now used by 2 (active-conn,test_gsm_authen_imei)
  vsub->imei[0] == 0
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - test_gsm_authen_imei: now used by 1 (active-conn)
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- MS replies with an Identity Response, VLR sends the IMEI to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_ID_RESP
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_ID_RESP
DMM IDENTITY RESPONSE: IMEI-423423423423420
DVLR set IMEI on subscriber; IMSI=901700000004620 IMEI=42342342342342
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_ID_IMEI
GSUP --> HLR: OSMO_GSUP_MSGT_CHECK_IMEI_REQUEST: 30010809710000004026f0500807244332244332240a0101
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- HLR accepts the IMEI
<-- GSUP rx OSMO_GSUP_MSGT_CHECK_IMEI_RESULT: 32010809710000004026f05101000a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_HLR_IMEI_ACK
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_IMEI}: Received Event LU_COMPL_VLR_E_IMEI_CHECK_ACK
- sending LU Accept for IMSI-901700000004620:MSISDN-46071:GERAN-A:LU
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + attached: now used by 3 (active-conn,vlr_gsup_rx,attached)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_IMEI}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: - lu: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 4 (active-conn,vlr_gsup_rx,attached,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 5 (active-conn,vlr_gsup_rx,attached,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,vlr_gsup_rx,attached,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 3 (active-conn,vlr_gsup_rx,attached)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 2 (active-conn,attached)
<-- GSUP rx OSMO_GSUP_MSGT_CHECK_IMEI_RESULT: vlr_gsupc_read_cb() returns 0
  bssap_clear_sent == 1
- LU was successful, and the conn has already been closed
  lu_result_sent == 1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DMSC msub(IMSI-901700000004620:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
- Subscriber has the IMEI
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + test_gsm_authen_imei: now used by 2 (attached,test_gsm_authen_imei)
  strcmp(vsub->imei, "42342342342342") == 0
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - test_gsm_authen_imei: now used by 1 (attached)


- subscriber detaches
  MSC <--GERAN-A-- MS: GSM48_MT_MM_IMSI_DETACH_IND
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_IMSI_DETACH_IND
DMM IMSI DETACH INDICATION: IMSI-901700000004620
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + gsm48_rx_mm_imsi_detach_ind: now used by 2 (attached,gsm48_rx_mm_imsi_detach_ind)
DMM IMSI DETACH for IMSI-901700000004620:MSISDN-46071
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + active-conn: now used by 3 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn)
GSUP --> HLR: OSMO_GSUP_MSGT_PURGE_MS_REQUEST: 0c010809710000004026f02801020a0101
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - attached: now used by 2 (gsm48_rx_mm_imsi_detach_ind,active-conn)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - gsm48_rx_mm_imsi_detach_ind: now used by 1 (active-conn)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_CN_CLOSE
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: Releasing: msc_a use is 1 (rx_from_ms)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 2 (active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 2 (active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 2 (rx_from_ms,wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 1 (active-conn)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: - rx_from_ms: now used by 1 (wait-Clear-Complete)
  bssap_clear_sent == 1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASED}: max total use count was 2
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE)
DMSC msub(IMSI-901700000004620:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - active-conn: now used by 0 (-)
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071) freeing VLR subscr (max total use count was 5)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:NONE){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
===== test_gsm_authen_imei: SUCCESS

===== test_gsm_authen_imei_nack
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000004620 LU-type=IMSI-ATTACH
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 001-868-1
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: rev=GSM net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000004620 id=901700000004620
DVLR New subscr, IMSI: 901700000004620
DVLR VLR subscr IMSI-901700000004620 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000004620 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000004026f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000004026f003222010585df1ae287f6e273dce07090d61320b21042d8b2c3e220861855fb81fc2a8000322201012aca96fb4ffdea5c985cbafa9b6e18b210420bde240220807fa7502e07e1c0003222010e7c03ba7cf0e2fde82b2dc4d63077d422104a29514ae2208e2b234f80788640003222010fa8f20b781b5881329d4fea26b1a3c5121045afc8d7222082392f14f709ae000032220100fd4cc8dbe8715d1f439e304edfd68dc2104bc8d1c5b2208da7cdd6bfe2d70000a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000004620) Received 5 auth tuples
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x1)
- sending GSM Auth Request for IMSI-901700000004620:GERAN-A:LU: tuple use_count=1 key_seq=0 auth_types=0x1 and...
- ...rand=585df1ae287f6e273dce07090d61320b
- ...expecting sres=2d8b2c3e
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- If the HLR were to send a GSUP _UPDATE_LOCATION_RESULT we'd still reject
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Event VLR_ULA_E_HLR_LU_RES not permitted
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends GSUP LU Req to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = 2d8b2c3e)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000004620) AUTH on GERAN received SRES/RES: 2d8b2c3e (4 bytes)
DVLR SUBSCR(IMSI-901700000004620) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000004026f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000004026f00804036470f10a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000004620 has MSISDN:46071
DMSC msub(IMSI-901700000004620:MSISDN-46071) VLR: update for IMSI=901700000004620 (MSISDN=46071)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT, and we send an ID Request for the IMEI to the MS
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_IMEI
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_ID_REQ
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_ID_REQ: 051802
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
- We will only do business when the IMEI is known
  llist_count(&msub_list) == 1
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + test_gsm_authen_imei_nack: now used by 2 (active-conn,test_gsm_authen_imei_nack)
  vsub->imei[0] == 0
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - test_gsm_authen_imei_nack: now used by 1 (active-conn)
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- MS replies with an Identity Response, VLR sends the IMEI to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_ID_RESP
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_ID_RESP
DMM IDENTITY RESPONSE: IMEI-423423423423420
DVLR set IMEI on subscriber; IMSI=901700000004620 IMEI=42342342342342
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_ID_IMEI
GSUP --> HLR: OSMO_GSUP_MSGT_CHECK_IMEI_REQUEST: 30010809710000004026f0500807244332244332240a0101
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- HLR does not like the IMEI and sends NACK
<-- GSUP rx OSMO_GSUP_MSGT_CHECK_IMEI_RESULT: 32010809710000004026f05101010a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_HLR_IMEI_NACK
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_IMEI}: Received Event LU_COMPL_VLR_E_IMEI_CHECK_NACK
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_IMEI}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_FAILURE
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Deallocated
- sending LU Reject for IMSI-901700000004620:MSISDN-46071:GERAN-A:LU, cause 6
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_CN_CLOSE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - lu: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (active-conn,vlr_gsup_rx,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,vlr_gsup_rx,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,vlr_gsup_rx,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_CHECK_IMEI_RESULT: vlr_gsupc_read_cb() returns 0
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DMSC msub(IMSI-901700000004620:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - active-conn: now used by 0 (-)
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071) freeing VLR subscr (max total use count was 4)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
===== test_gsm_authen_imei_nack: SUCCESS

===== test_gsm_authen_imei_err
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000004620 LU-type=IMSI-ATTACH
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 001-868-1
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: rev=GSM net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000004620 id=901700000004620
DVLR New subscr, IMSI: 901700000004620
DVLR VLR subscr IMSI-901700000004620 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000004620 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000004026f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000004026f003222010585df1ae287f6e273dce07090d61320b21042d8b2c3e220861855fb81fc2a8000322201012aca96fb4ffdea5c985cbafa9b6e18b210420bde240220807fa7502e07e1c0003222010e7c03ba7cf0e2fde82b2dc4d63077d422104a29514ae2208e2b234f80788640003222010fa8f20b781b5881329d4fea26b1a3c5121045afc8d7222082392f14f709ae000032220100fd4cc8dbe8715d1f439e304edfd68dc2104bc8d1c5b2208da7cdd6bfe2d70000a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000004620) Received 5 auth tuples
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x1)
- sending GSM Auth Request for IMSI-901700000004620:GERAN-A:LU: tuple use_count=1 key_seq=0 auth_types=0x1 and...
- ...rand=585df1ae287f6e273dce07090d61320b
- ...expecting sres=2d8b2c3e
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- If the HLR were to send a GSUP _UPDATE_LOCATION_RESULT we'd still reject
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Event VLR_ULA_E_HLR_LU_RES not permitted
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends GSUP LU Req to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = 2d8b2c3e)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000004620) AUTH on GERAN received SRES/RES: 2d8b2c3e (4 bytes)
DVLR SUBSCR(IMSI-901700000004620) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000004026f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000004026f00804036470f10a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000004620 has MSISDN:46071
DMSC msub(IMSI-901700000004620:MSISDN-46071) VLR: update for IMSI=901700000004620 (MSISDN=46071)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT, and we send an ID Request for the IMEI to the MS
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_IMEI
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_ID_REQ
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_ID_REQ: 051802
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
- We will only do business when the IMEI is known
  llist_count(&msub_list) == 1
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + test_gsm_authen_imei_err: now used by 2 (active-conn,test_gsm_authen_imei_err)
  vsub->imei[0] == 0
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - test_gsm_authen_imei_err: now used by 1 (active-conn)
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- MS replies with an Identity Response, VLR sends the IMEI to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_ID_RESP
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_ID_RESP
DMM IDENTITY RESPONSE: IMEI-423423423423420
DVLR set IMEI on subscriber; IMSI=901700000004620 IMEI=42342342342342
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_ID_IMEI
GSUP --> HLR: OSMO_GSUP_MSGT_CHECK_IMEI_REQUEST: 30010809710000004026f0500807244332244332240a0101
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- HLR can't parse the message and returns ERR
<-- GSUP rx OSMO_GSUP_MSGT_CHECK_IMEI_ERROR: 31010809710000004026f00201600a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071) Check_IMEI_VLR failed; gmm_cause: Invalid mandatory information
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_HLR_IMEI_NACK
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_IMEI}: Received Event LU_COMPL_VLR_E_IMEI_CHECK_NACK
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_IMEI}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_FAILURE
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Deallocated
- sending LU Reject for IMSI-901700000004620:MSISDN-46071:GERAN-A:LU, cause 6
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_CN_CLOSE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - lu: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (active-conn,vlr_gsup_rx,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,vlr_gsup_rx,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,vlr_gsup_rx,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_CHECK_IMEI_ERROR: vlr_gsupc_read_cb() returns 0
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DMSC msub(IMSI-901700000004620:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - active-conn: now used by 0 (-)
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071) freeing VLR subscr (max total use count was 4)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
===== test_gsm_authen_imei_err: SUCCESS

===== test_gsm_authen_tmsi_imei
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000004620 LU-type=IMSI-ATTACH
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 001-868-1
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: rev=GSM net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000004620 id=901700000004620
DVLR New subscr, IMSI: 901700000004620
DVLR VLR subscr IMSI-901700000004620 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000004620 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000004026f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000004026f003222010585df1ae287f6e273dce07090d61320b21042d8b2c3e220861855fb81fc2a8000322201012aca96fb4ffdea5c985cbafa9b6e18b210420bde240220807fa7502e07e1c0003222010e7c03ba7cf0e2fde82b2dc4d63077d422104a29514ae2208e2b234f80788640003222010fa8f20b781b5881329d4fea26b1a3c5121045afc8d7222082392f14f709ae000032220100fd4cc8dbe8715d1f439e304edfd68dc2104bc8d1c5b2208da7cdd6bfe2d70000a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000004620) Received 5 auth tuples
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x1)
- sending GSM Auth Request for IMSI-901700000004620:GERAN-A:LU: tuple use_count=1 key_seq=0 auth_types=0x1 and...
- ...rand=585df1ae287f6e273dce07090d61320b
- ...expecting sres=2d8b2c3e
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- If the HLR were to send a GSUP _UPDATE_LOCATION_RESULT we'd still reject
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Event VLR_ULA_E_HLR_LU_RES not permitted
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends GSUP LU Req to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = 2d8b2c3e)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000004620) AUTH on GERAN received SRES/RES: 2d8b2c3e (4 bytes)
DVLR SUBSCR(IMSI-901700000004620) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000004026f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000004026f00804036470f10a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000004620 has MSISDN:46071
DMSC msub(IMSI-901700000004620:MSISDN-46071) VLR: update for IMSI=901700000004620 (MSISDN=46071)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT, and we send an ID Request for the IMEI to the MS
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_IMEI_TMSI
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_ID_REQ
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_ID_REQ: 051802
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR upd_hlr_vlr_fsm(IMSI-901700000004620:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
- We will only do business when the IMEI is known
  llist_count(&msub_list) == 1
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + test_gsm_authen_tmsi_imei: now used by 2 (active-conn,test_gsm_authen_tmsi_imei)
  vsub->imei[0] == 0
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 - test_gsm_authen_tmsi_imei: now used by 1 (active-conn)
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- MS replies with an Identity Response, VLR sends the IMEI to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_ID_RESP
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_ID_RESP
DMM IDENTITY RESPONSE: IMEI-423423423423420
DVLR set IMEI on subscriber; IMSI=901700000004620 IMEI=42342342342342
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_ID_IMEI
GSUP --> HLR: OSMO_GSUP_MSGT_CHECK_IMEI_REQUEST: 30010809710000004026f0500807244332244332240a0101
DREF msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- HLR accepts the IMEI
<-- GSUP rx OSMO_GSUP_MSGT_CHECK_IMEI_RESULT: 32010809710000004026f05101000a0101
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_HLR_IMEI_ACK
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_IMEI_TMSI}: Received Event LU_COMPL_VLR_E_IMEI_CHECK_ACK
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_IMEI_TMSI}: lu_compl_vlr_new_tmsi()
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100) VLR: update for IMSI=901700000004620 (MSISDN=46071)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_IMEI_TMSI}: state_chg to LU_COMPL_VLR_S_WAIT_TMSI_CNF
- sending LU Accept for IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU, with TMSI 0x03020100
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_CHECK_IMEI_RESULT: vlr_gsupc_read_cb() returns 0
- a LU Accept with a new TMSI was sent, waiting for TMSI Realloc Compl
  llist_count(&msub_list) == 1
  lu_result_sent == 1
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- even though the TMSI is not acked, we can already find the subscr with it
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100 + test_gsm_authen_tmsi_imei: now used by 2 (active-conn,test_gsm_authen_tmsi_imei)
  vsub != NULL == 1
  strcmp(vsub->imsi, imsi) == 0
  vsub->tmsi_new == 0x03020100
  vsub->tmsi == 0xffffffff
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100 - test_gsm_authen_tmsi_imei: now used by 1 (active-conn)
- MS sends TMSI Realloc Complete
  MSC <--GERAN-A-- MS: GSM48_MT_MM_TMSI_REALL_COMPL
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_TMSI_REALL_COMPL
DMM msc_a(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: TMSI Reallocation Completed
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSInew-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_NEW_TMSI_ACK
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: Received Event LU_COMPL_VLR_E_NEW_TMSI_ACK
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) VLR: update for IMSI=901700000004620 (MSISDN=46071)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + attached: now used by 2 (active-conn,attached)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000004620:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: - lu: now used by 1 (rx_from_ms)
DVLR vlr_lu_fsm(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){VLR_ULA_S_DONE}: Deallocated
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,attached,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (active-conn,attached)
  bssap_clear_sent == 1
- LU was successful, and the conn has already been closed
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
- Subscriber has the IMEI and TMSI
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + test_gsm_authen_tmsi_imei: now used by 2 (attached,test_gsm_authen_tmsi_imei)
  strcmp(vsub->imei, "42342342342342") == 0
  vsub->tmsi == 0x03020100
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - test_gsm_authen_tmsi_imei: now used by 1 (attached)


- subscriber detaches, using TMSI
  MSC <--GERAN-A-- MS: GSM48_MT_MM_IMSI_DETACH_IND
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_IMSI_DETACH_IND
DMM IMSI DETACH INDICATION: TMSI-0x03020100
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + gsm48_rx_mm_imsi_detach_ind: now used by 2 (attached,gsm48_rx_mm_imsi_detach_ind)
DMM IMSI DETACH for IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + active-conn: now used by 3 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn)
GSUP --> HLR: OSMO_GSUP_MSGT_PURGE_MS_REQUEST: 0c010809710000004026f02801020a0101
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - attached: now used by 2 (gsm48_rx_mm_imsi_detach_ind,active-conn)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - gsm48_rx_mm_imsi_detach_ind: now used by 1 (active-conn)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_CN_CLOSE
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASING}: Releasing: msc_a use is 1 (rx_from_ms)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 2 (active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 2 (active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 2 (rx_from_ms,wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 1 (active-conn)
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASING}: - rx_from_ms: now used by 1 (wait-Clear-Complete)
  bssap_clear_sent == 1
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASED}: max total use count was 2
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE))
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE)
DMSC msub(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100 - active-conn: now used by 0 (-)
DVLR SUBSCR(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100) freeing VLR subscr (max total use count was 4)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE)
DMSC msc_a(IMSI-901700000004620:MSISDN-46071:TMSI-0x03020100:GERAN-A:NONE){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
===== test_gsm_authen_tmsi_imei: SUCCESS

===== test_gsm_milenage_authen
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000010650 LU-type=NORMAL
DMM msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 1665-165-0
DREF msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000010650:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: rev=GSM net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000010650 id=901700000010650
DVLR New subscr, IMSI: 901700000010650
DVLR VLR subscr IMSI-901700000010650 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000010650 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU)
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000000156f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e4103622010c187a53a5e6b9d573cac7c74451fd46d210485aa31302208d3d50a000bf04f6e23101159ec926a50e98c034a6b7d7c9f418d2410df3a03d9ca5335641efc8e36d76cd20b25101843a645b98d00005b2d666af46c45d927087db47cf7f81e4dc703622010efa9c29a9742148d5c9070348716e1bb210469d5f9fb22083df176f0c29f1a3d2310eb50e770ddcc3060101d2f43b6c2b884241076542abce5ff9345b0e8947f4c6e019c2510f9375e6d41e1000096e7fe4ff1c27e392708706f996719ba609c0a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000010650) Received 3 auth tuples
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x3)
- sending GSM Auth Request for IMSI-901700000010650:GERAN-A:LU: tuple use_count=1 key_seq=0 auth_types=0x3 and...
- ...rand=39fa2f4e3d523d8619a73b4f65c3e14d
- ...expecting sres=9b36efdf
DVLR VLR subscr IMSI-901700000010650 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends GSUP LU Req to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = 9b36efdf)
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650) AUTH on GERAN received SRES/RES: 9b36efdf (4 bytes)
DVLR SUBSCR(IMSI-901700000010650) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000000156f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
DVLR VLR_Authenticate(IMSI-901700000010650:GERAN-A:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000000156f00804032443f20a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000010650 has MSISDN:42342
DMSC msub(IMSI-901700000010650:MSISDN-42342) VLR: update for IMSI=901700000010650 (MSISDN=42342)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
- sending LU Accept for IMSI-901700000010650:MSISDN-42342:GERAN-A:LU
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + attached: now used by 3 (active-conn,vlr_gsup_rx,attached)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU))
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Deferring: will deallocate with upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){VLR_ULA_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU))
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: - lu: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + msc_a_fsm_releasing_onenter: now used by 4 (active-conn,vlr_gsup_rx,attached,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + vlr_subscr_cancel_attach_fsm: now used by 5 (active-conn,vlr_gsup_rx,attached,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,vlr_gsup_rx,attached,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - msc_a_fsm_releasing_onenter: now used by 3 (active-conn,vlr_gsup_rx,attached)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){VLR_ULA_S_DONE}: Deferring: will deallocate with upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Deallocated, including all deferred deallocations
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - vlr_gsup_rx: now used by 2 (active-conn,attached)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
  bssap_clear_sent == 1
- LU was successful, and the conn has already been closed
  lu_result_sent == 1
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU)
DMSC msub(IMSI-901700000010650:MSISDN-42342) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- after a while, a new conn sends a CM Service Request. VLR responds with Auth Req, 2nd auth vector
  MSC <--GERAN-A-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=Short-Messaging-Service
DREF msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_sms: now used by 2 (rx_from_ms,cm_service_sms)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=GSM net=GERAN Auth (no Ciph)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=1 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x3)
- sending GSM Auth Request for IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ: tuple use_count=1 key_seq=1 auth_types=0x3 and...
- ...rand=c187a53a5e6b9d573cac7c74451fd46d
- ...expecting sres=85aa3130
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (cm_service_sms)
  cm_service_result_sent == 0
  auth_request_sent == 1
- needs auth, not yet accepted
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- MS sends Authen Response, VLR accepts with a CM Service Accept
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (cm_service_sms,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = 85aa3130)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342) AUTH on GERAN received SRES/RES: 85aa3130 (4 bytes)
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_CM_SERV_ACC
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_CM_SERV_ACC: 0521
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (cm_service_sms)
  cm_service_result_sent == 1
- Concluding CM Service Request
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - cm_service_sms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
  bssap_clear_sent == 1
- all requests serviced, conn has been released
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 2
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000010650:MSISDN-42342) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- an SMS is sent, MS is paged
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + test_gsm_milenage_authen: now used by 2 (attached,test_gsm_milenage_authen)
  llist_count(&vsub->cs.requests) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + SMS-receiver: now used by 3 (attached,test_gsm_milenage_authen,SMS-receiver)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + SMS: now used by 4 (attached,test_gsm_milenage_authen,SMS-receiver,SMS)
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342 callref-0x40000003 tid-0) New transaction
DLSMS SMC(0) instance created for network
DLSMS SMR(0) instance created for network.
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342 callref-0x40000003 tid-0) Going to send a MT SMS
DLSMS SMR(0) message SM-RL-DATA_REQ received in state IDLE
DLSMS SMR(0) TX SMS RP-DATA
DLSMS SMR(0) new RP state IDLE -> WAIT_FOR_RP_ACK
DLSMS SMC(0) message MNSMS-EST-REQ received in state IDLE
DLSMS SMC(0) new CP state IDLE -> MM_CONN_PENDING
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342 callref-0x40000003 tid-0) Initiating Paging due to MMSMS_EST_REQ
DPAG Paging: IMSI-901700000010650:MSISDN-42342 for MT-SMS: Starting paging
  paging request (SIGNALLING_LOW_PRIO) to IMSI-901700000010650:MSISDN-42342 on GERAN-A
  strcmp(paging_expecting_imsi, vsub->imsi) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + Paging: now used by 5 (attached,test_gsm_milenage_authen,SMS-receiver,SMS,Paging)
  llist_count(&vsub->cs.requests) == 1
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - test_gsm_milenage_authen: now used by 4 (attached,SMS-receiver,SMS,Paging)
  paging_sent == 1
- the subscriber and its pending request should remain
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + test_gsm_milenage_authen: now used by 5 (attached,SMS-receiver,SMS,Paging,test_gsm_milenage_authen)
  llist_count(&vsub->cs.requests) == 1
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - test_gsm_milenage_authen: now used by 4 (attached,SMS-receiver,SMS,Paging)
- MS replies with Paging Response, and VLR sends Auth Request with third key
  MSC <--GERAN-A-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: RR GSM48_MT_RR_PAG_RESP
DRR msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Rx PAGING RESPONSE IMSI-901700000010650
DREF msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: + paging-response: now used by 2 (rx_from_ms,paging-response)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: rev=GSM net=GERAN Auth (no Ciph)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + proc_arq_vlr_fn_init: now used by 5 (attached,SMS-receiver,SMS,Paging,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + active-conn: now used by 6 (attached,SMS-receiver,SMS,Paging,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=2 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x3)
- sending GSM Auth Request for IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP: tuple use_count=1 key_seq=2 auth_types=0x3 and...
- ...rand=efa9c29a9742148d5c9070348716e1bb
- ...expecting sres=69d5f9fb
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - proc_arq_vlr_fn_init: now used by 5 (attached,SMS-receiver,SMS,Paging,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (paging-response)
  auth_request_sent == 1
- needs auth, not yet accepted
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
- MS sends Authen Response, VLR accepts and sends pending SMS
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (paging-response,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = 69d5f9fb)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342) AUTH on GERAN received SRES/RES: 69d5f9fb (4 bytes)
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342) AUTH established GSM security context
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DPAG Paging: IMSI-901700000010650:MSISDN-42342 for MT-SMS: Paging Response action (success)
DPAG Paging: IMSI-901700000010650:MSISDN-42342 for MT-SMS: Removing Paging Request
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342 callref-0x40000003 tid-0) mmsms_paging_cb(success)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + sms: now used by 3 (paging-response,rx_from_ms,sms)
DLSMS SMC(0) message MMSMS-EST-CNF received in state MM_CONN_PENDING
DLSMS SMC(0) send CP data
DLSMS SMC(0) new CP state MM_CONN_PENDING -> WAIT_CP_ACK
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP callref-0x40000003 tid-0) sending CP message (trans=0)
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP callref-0x40000003 tid-0) GSM4.11 TX 09 01 58 01 00 07 91 44 77 58 10 06 50 00 4c 00 05 80 24 43 f2 00 00 07 10 10 00 00 00 00 44 50 79 da 1e 1e e7 41 69 37 48 5e 9e a7 c9 65 37 3d 1d 66 83 c2 70 38 3b 3d 0e d3 d3 6f f7 1c 94 9e 83 c2 20 72 79 9e 96 87 c5 ec 32 a8 1d 96 af cb f4 b4 fb 0c 7a c3 e9 e9 b7 db 05 
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Sending DTAP: SMS SMS:0x01
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: SMS:0x01: 09015801000791447758100650004c0005802443f2000007101000000000445079da1e1ee7416937485e9ea7c965373d1d6683c270383b3d0ed3d36ff71c949e83c22072799e9687c5ec32a81d96afcbf4b4fb0c7ac3e9e9b7db05
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - Paging: now used by 4 (attached,SMS-receiver,SMS,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - paging-response: now used by 2 (rx_from_ms,sms)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (sms)
  dtap_tx_confirmed == 1
- SMS was delivered, no requests pending for subscr
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + test_gsm_milenage_authen: now used by 5 (attached,SMS-receiver,SMS,active-conn,test_gsm_milenage_authen)
  llist_count(&vsub->cs.requests) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - test_gsm_milenage_authen: now used by 4 (attached,SMS-receiver,SMS,active-conn)
- conn is still open to wait for SMS ack dance
  llist_count(&msub_list) == 1
- MS replies with CP-ACK for received SMS
  MSC <--GERAN-A-- MS: SMS:0x04
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (sms,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: SMS SMS:0x04
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP callref-0x40000003 tid-0) receiving SMS message SMS:0x04
DLSMS SMC(0) message MMSMS-DATA-IND (CP ACK) received in state WAIT_CP_ACK
DLSMS SMC(0) received CP-ACK
DLSMS SMC(0) new CP state WAIT_CP_ACK -> MM_ESTABLISHED
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (sms)
  llist_count(&msub_list) == 1
- MS also sends RP-ACK, MSC in turn sends CP-ACK for that
  MSC <--GERAN-A-- MS: SMS:0x01
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (sms,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: SMS SMS:0x01
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP callref-0x40000003 tid-0) receiving SMS message SMS:0x01
DLSMS SMC(0) message MMSMS-DATA-IND (CP DATA) received in state MM_ESTABLISHED
DLSMS SMC(0) received CP-DATA
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP callref-0x40000003 tid-0) sending CP message (trans=0)
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP callref-0x40000003 tid-0) GSM4.11 TX 09 04 
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Sending DTAP: SMS SMS:0x04
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: SMS:0x04: 0904
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP callref-0x40000003 tid-0) MNSMS-DATA/EST-IND
DLSMS SMR(0) message MNSMS-DATA-IND received in state WAIT_FOR_RP_ACK
DLSMS SMR(0) RX SMS RP-ACK
DLSMS SMR(0) new RP state WAIT_FOR_RP_ACK -> IDLE
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP callref-0x40000003 tid-0) RX SMS RP-ACK (MO)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - SMS-receiver: now used by 3 (attached,SMS,active-conn)
DLSMS SMR(0) TX: MNSMS-REL-REQ
DLSMS SMC(0) message MNSMS-REL-REQ received in state MM_ESTABLISHED
DLSMS SMC(0) new CP state MM_ESTABLISHED -> IDLE
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP callref-0x40000003 tid-0) Got MMSMS_REL_REQ, destroying transaction.
DLSMS trans(SMS IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP callref-0x40000003 tid-0) Freeing transaction
DLSMS SMR(0) clearing SMR instance
DLSMS SMC(0) clearing instance
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - SMS: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - sms: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
  dtap_tx_confirmed == 1
  bssap_clear_sent == 1
- SMS is done, conn is gone
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP)
DMSC msub(IMSI-901700000010650:MSISDN-42342) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- subscriber detaches
  MSC <--GERAN-A-- MS: GSM48_MT_MM_IMSI_DETACH_IND
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_IMSI_DETACH_IND
DMM IMSI DETACH INDICATION: IMSI-901700000010650
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + gsm48_rx_mm_imsi_detach_ind: now used by 2 (attached,gsm48_rx_mm_imsi_detach_ind)
DMM IMSI DETACH for IMSI-901700000010650:MSISDN-42342
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + active-conn: now used by 3 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,gsm48_rx_mm_imsi_detach_ind,active-conn)
GSUP --> HLR: OSMO_GSUP_MSGT_PURGE_MS_REQUEST: 0c010809710000000156f02801020a0101
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - attached: now used by 2 (gsm48_rx_mm_imsi_detach_ind,active-conn)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - gsm48_rx_mm_imsi_detach_ind: now used by 1 (active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_CN_CLOSE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASING}: Releasing: msc_a use is 1 (rx_from_ms)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + msc_a_fsm_releasing_onenter: now used by 2 (active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - vlr_subscr_cancel_attach_fsm: now used by 2 (active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 2 (rx_from_ms,wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - msc_a_fsm_releasing_onenter: now used by 1 (active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASING}: - rx_from_ms: now used by 1 (wait-Clear-Complete)
  bssap_clear_sent == 1
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASED}: max total use count was 2
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE)
DMSC msub(IMSI-901700000010650:MSISDN-42342) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - active-conn: now used by 0 (-)
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342) freeing VLR subscr (max total use count was 6)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:GERAN-A:NONE){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
===== test_gsm_milenage_authen: SUCCESS

===== test_wrong_sres_length
- Total time passed: 0.000000 s
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000004620 LU-type=IMSI-ATTACH
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 001-868-1
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: rev=GSM net=GERAN Auth (no Ciph)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000004620 id=901700000004620
DVLR New subscr, IMSI: 901700000004620
DVLR VLR subscr IMSI-901700000004620 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000004620 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000004026f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000004026f003222010585df1ae287f6e273dce07090d61320b21042d8b2c3e220861855fb81fc2a8000322201012aca96fb4ffdea5c985cbafa9b6e18b210420bde240220807fa7502e07e1c0003222010e7c03ba7cf0e2fde82b2dc4d63077d422104a29514ae2208e2b234f80788640003222010fa8f20b781b5881329d4fea26b1a3c5121045afc8d7222082392f14f709ae000032220100fd4cc8dbe8715d1f439e304edfd68dc2104bc8d1c5b2208da7cdd6bfe2d70000a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000004620) Received 5 auth tuples
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use GSM AKA (is_r99=no, at->vec.auth_types=0x1)
- sending GSM Auth Request for IMSI-901700000004620:GERAN-A:LU: tuple use_count=1 key_seq=0 auth_types=0x1 and...
- ...rand=585df1ae287f6e273dce07090d61320b
- ...expecting sres=2d8b2c3e
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- If the HLR were to send a GSUP _UPDATE_LOCATION_RESULT we'd still reject
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000004026f00a0101
DVLR VLR subscr IMSI-901700000004620 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Event VLR_ULA_E_HLR_LU_RES not permitted
DVLR VLR subscr IMSI-901700000004620 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
msc_a_is_accepted() == false
  requests shall be thwarted
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_CC_SETUP
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: unknown 0x33
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: RR GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: GSM48_MT_RR_SYSINFO_1
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: SMS SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Message not permitted for initial conn: SMS:0x01
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode error (rc=-13) for DTAP from MSC-I
  lu_result_sent == 0
- MS sends Authen Response with too short SRES data, auth is thwarted.
  MSC <--GERAN-A-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: MM AUTHENTICATION RESPONSE: l3 length invalid: 5
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: MM AUTHENTICATION RESPONSE: invalid: parsing GSM AKA Auth Response failed with rc=-22; dispatching zero length SRES/RES to trigger failure
DMM msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: MM GSM AUTHENTICATION RESPONSE (sres = )
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000004620) AUTH on GERAN received SRES/RES:  (0 bytes)
DVLR SUBSCR(IMSI-901700000004620) AUTH SRES/RES missing
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result FAILURE, cause ILLEGAL_MS
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTH_FAILED
GSUP --> HLR: OSMO_GSUP_MSGT_AUTH_FAIL_REPORT: 0b010809710000004026f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTH_FAILED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTH_FAILED}: Removing from parent vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_FAILURE
- sending LU Reject for IMSI-901700000004620:GERAN-A:LU, cause 3
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU))
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000004620:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_CN_CLOSE
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - lu: now used by 1 (rx_from_ms)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 1 (rx_from_ms)
DVLR VLR subscr IMSI-901700000004620 + msc_a_fsm_releasing_onenter: now used by 2 (active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000004620 + vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000004620 - vlr_subscr_cancel_attach_fsm: now used by 2 (active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 2 (rx_from_ms,wait-Clear-Complete)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000004620:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000004620 - msc_a_fsm_releasing_onenter: now used by 1 (active-conn)
DVLR vlr_lu_fsm(IMSI-901700000004620:GERAN-A:LU){VLR_ULA_S_DONE}: Deferring: will deallocate with VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU)
DVLR VLR_Authenticate(IMSI-901700000004620:GERAN-A:LU){VLR_SUB_AS_AUTH_FAILED}: Deallocated, including all deferred deallocations
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASING}: - rx_from_ms: now used by 1 (wait-Clear-Complete)
  lu_result_sent == 2
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000004620) MSC-A terminated
DMSC msub(IMSI-901700000004620) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000004620:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:GERAN-A:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000004620:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000004620:GERAN-A:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000004620:GERAN-A:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000004620:GERAN-A:LU)
DMSC msub(IMSI-901700000004620) Free
DVLR VLR subscr IMSI-901700000004620 - active-conn: now used by 0 (-)
DVLR SUBSCR(IMSI-901700000004620) freeing VLR subscr (max total use count was 3)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000004620:GERAN-A:LU)
DMSC msc_a(IMSI-901700000004620:GERAN-A:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
===== test_wrong_sres_length: SUCCESS

