libosmovty 1.13.1.1-afb4 Osmocom VTY library

Macros | Functions
tdef_vty.h File Reference
Tnnn timer VTY configuration

API to configure osmo_tdef Tnnn timers from VTY configuration. More...

`#include <stdint.h>`
`#include <stdarg.h>`
`#include <osmocom/vty/command.h>`

Go to the source code of this file.

## Macros
#define | OSMO_TDEF_VTY_ARG_T "TNNNN"
#define | OSMO_TDEF_VTY_DOC_T
#define | OSMO_TDEF_VTY_ARG_T_OPTIONAL "[" OSMO_TDEF_VTY_ARG_T "]"
#define | OSMO_TDEF_VTY_ARG_VAL "(<0-2147483647>|default)"
#define | OSMO_TDEF_VTY_DOC_VAL "New timer value\n" "Set to default timer value\n"
#define | OSMO_TDEF_VTY_ARG_VAL_OPTIONAL "[" OSMO_TDEF_VTY_ARG_VAL "]"
#define | OSMO_TDEF_VTY_ARG_SET OSMO_TDEF_VTY_ARG_T " " OSMO_TDEF_VTY_ARG_VAL
#define | OSMO_TDEF_VTY_DOC_SET OSMO_TDEF_VTY_DOC_T OSMO_TDEF_VTY_DOC_VAL
#define | OSMO_TDEF_VTY_ARG_SET_OPTIONAL OSMO_TDEF_VTY_ARG_T_OPTIONAL " " OSMO_TDEF_VTY_ARG_VAL_OPTIONAL

## Functions
int | osmo_tdef_vty_set_cmd (struct vty *vty, struct osmo_tdef *tdefs, const char **args)
| Apply a timer configuration from VTY argument strings. More...
int | osmo_tdef_vty_show_cmd (struct vty *vty, struct osmo_tdef *tdefs, const char *T_arg, const char *prefix_fmt,...)
| Output one or all timers to the VTY, as for a VTY command like 'show timer [TNNNN]'. More...
void | osmo_tdef_vty_write (struct vty *vty, struct osmo_tdef *tdefs, const char *prefix_fmt,...)
| Write current timer configuration arguments to the vty. More...
void | osmo_tdef_vty_out_one (struct vty *vty, struct osmo_tdef *t, const char *prefix_fmt,...)
| Write to VTY the current status of one timer. More...
void | osmo_tdef_vty_out_all (struct vty *vty, struct osmo_tdef *tdefs, const char *prefix_fmt,...)
| Write to VTY the current status of all given timers. More...
void | osmo_tdef_vty_out_one_va (struct vty *vty, struct osmo_tdef *t, const char *prefix_fmt, va_list va)
| Write to VTY the current status of one timer. More...
void | osmo_tdef_vty_out_all_va (struct vty *vty, struct osmo_tdef *tdefs, const char *prefix_fmt, va_list va)
| Write to VTY the current status of all given timers. More...
struct osmo_tdef * | osmo_tdef_vty_parse_T_arg (struct vty *vty, struct osmo_tdef *tdefs, const char *T_str)
| Parse an argument like "1234", "T1234", "t1234", or "X1234", "x1234", as from OSMO_TDEF_VTY_ARG_T. More...
unsigned long | osmo_tdef_vty_parse_val_arg (const char *val_arg, unsigned long default_val)
| Parse an argument of the form "(0-2147483647|default)", as from OSMO_TDEF_VTY_ARG_VAL. More...
void | osmo_tdef_vty_groups_init (unsigned int parent_cfg_node, struct osmo_tdef_group *groups)
| Convenience implementation for keeping a fixed set of timer groups in a program. More...
void | osmo_tdef_vty_groups_write (struct vty *vty, const char *indent)
| Write the global osmo_tdef_group configuration to VTY, as previously passed to osmo_tdef_vty_groups_init(). More...

## Detailed Description

API to configure osmo_tdef Tnnn timers from VTY configuration.