\doxysection{osmo\+\_\+gad\+\_\+ell\+\_\+point\+\_\+alt Struct Reference}
\label{structosmo__gad__ell__point__alt}\index{osmo\_gad\_ell\_point\_alt@{osmo\_gad\_ell\_point\_alt}}


{\ttfamily \#include $<$gad.\+h$>$}

\doxysubsection*{Data Fields}
\begin{DoxyCompactItemize}
\item 
int32\+\_\+t \textbf{ lat}
\begin{DoxyCompactList}\small\item\em latitude in micro degrees (degrees $\ast$ 1e6), -\/90\textquotesingle{}000\textquotesingle{}000 (S) . \end{DoxyCompactList}\item 
int32\+\_\+t \textbf{ lon}
\begin{DoxyCompactList}\small\item\em longitude in micro degrees (degrees $\ast$ 1e6), -\/180\textquotesingle{}000\textquotesingle{}000 (W) . \end{DoxyCompactList}\item 
int16\+\_\+t \textbf{ alt}
\begin{DoxyCompactList}\small\item\em Altitude in meters, -\/32767 (depth) . \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Field Documentation}
\mbox{\label{structosmo__gad__ell__point__alt_aa77520c5451e9c13c2b65e015ffda116}} 
\index{osmo\_gad\_ell\_point\_alt@{osmo\_gad\_ell\_point\_alt}!alt@{alt}}
\index{alt@{alt}!osmo\_gad\_ell\_point\_alt@{osmo\_gad\_ell\_point\_alt}}
\doxysubsubsection{alt}
{\footnotesize\ttfamily int16\+\_\+t osmo\+\_\+gad\+\_\+ell\+\_\+point\+\_\+alt\+::alt}



Altitude in meters, -\/32767 (depth) . 

. 32767 (height) \mbox{\label{structosmo__gad__ell__point__alt_a7be7a58498a718870825fec0bc4d6910}} 
\index{osmo\_gad\_ell\_point\_alt@{osmo\_gad\_ell\_point\_alt}!lat@{lat}}
\index{lat@{lat}!osmo\_gad\_ell\_point\_alt@{osmo\_gad\_ell\_point\_alt}}
\doxysubsubsection{lat}
{\footnotesize\ttfamily int32\+\_\+t osmo\+\_\+gad\+\_\+ell\+\_\+point\+\_\+alt\+::lat}



latitude in micro degrees (degrees $\ast$ 1e6), -\/90\textquotesingle{}000\textquotesingle{}000 (S) . 

. 90\textquotesingle{}000\textquotesingle{}000 (N). \mbox{\label{structosmo__gad__ell__point__alt_ad62f433d8252ebcf781cbd5311d4c753}} 
\index{osmo\_gad\_ell\_point\_alt@{osmo\_gad\_ell\_point\_alt}!lon@{lon}}
\index{lon@{lon}!osmo\_gad\_ell\_point\_alt@{osmo\_gad\_ell\_point\_alt}}
\doxysubsubsection{lon}
{\footnotesize\ttfamily int32\+\_\+t osmo\+\_\+gad\+\_\+ell\+\_\+point\+\_\+alt\+::lon}



longitude in micro degrees (degrees $\ast$ 1e6), -\/180\textquotesingle{}000\textquotesingle{}000 (W) . 

. 180\textquotesingle{}000\textquotesingle{}000 (E). 

The documentation for this struct was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
include/osmocom/gsm/\textbf{ gad.\+h}\end{DoxyCompactItemize}
