\doxysection{gsmtap\+\_\+inst Struct Reference}
\label{structgsmtap__inst}\index{gsmtap\_inst@{gsmtap\_inst}}


one gsmtap instance  


\doxysubsection*{Data Fields}
\begin{DoxyCompactItemize}
\item 
int \textbf{ osmo\+\_\+io\+\_\+mode}
\begin{DoxyCompactList}\small\item\em Indicates whether or not to use Osmo IO mode for message output (thus enabling use of tx queues) \end{DoxyCompactList}\item 
int \textbf{ source\+\_\+fd}
\begin{DoxyCompactList}\small\item\em the gsmtap source FD \end{DoxyCompactList}\item 
struct \textbf{ osmo\+\_\+io\+\_\+fd} $\ast$ \textbf{ out}
\begin{DoxyCompactList}\small\item\em Used when osmo\+\_\+io\+\_\+mode is nonzero. \end{DoxyCompactList}\item 
int \textbf{ sink\+\_\+fd}
\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
one gsmtap instance 

\doxysubsection{Field Documentation}
\mbox{\label{structgsmtap__inst_a7fe635c4078e0c6566e18e853ef16371}} 
\index{gsmtap\_inst@{gsmtap\_inst}!osmo\_io\_mode@{osmo\_io\_mode}}
\index{osmo\_io\_mode@{osmo\_io\_mode}!gsmtap\_inst@{gsmtap\_inst}}
\doxysubsubsection{osmo\_io\_mode}
{\footnotesize\ttfamily int gsmtap\+\_\+inst\+::osmo\+\_\+io\+\_\+mode}



Indicates whether or not to use Osmo IO mode for message output (thus enabling use of tx queues) 

\mbox{\label{structgsmtap__inst_ad390464fdc4dfd3406b8135e10411390}} 
\index{gsmtap\_inst@{gsmtap\_inst}!out@{out}}
\index{out@{out}!gsmtap\_inst@{gsmtap\_inst}}
\doxysubsubsection{out}
{\footnotesize\ttfamily struct \textbf{ osmo\+\_\+io\+\_\+fd}$\ast$ gsmtap\+\_\+inst\+::out}



Used when osmo\+\_\+io\+\_\+mode is nonzero. 

\mbox{\label{structgsmtap__inst_a423830303da2b3c271111c758b47b73e}} 
\index{gsmtap\_inst@{gsmtap\_inst}!sink\_fd@{sink\_fd}}
\index{sink\_fd@{sink\_fd}!gsmtap\_inst@{gsmtap\_inst}}
\doxysubsubsection{sink\_fd}
{\footnotesize\ttfamily int gsmtap\+\_\+inst\+::sink\+\_\+fd}

\mbox{\label{structgsmtap__inst_a1023b915308a780148713fef149c5f7f}} 
\index{gsmtap\_inst@{gsmtap\_inst}!source\_fd@{source\_fd}}
\index{source\_fd@{source\_fd}!gsmtap\_inst@{gsmtap\_inst}}
\doxysubsubsection{source\_fd}
{\footnotesize\ttfamily int gsmtap\+\_\+inst\+::source\+\_\+fd}



the gsmtap source FD 



Referenced by \textbf{ gsmtap\+\_\+inst\+\_\+fd2()}.



The documentation for this struct was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
src/core/\textbf{ gsmtap\+\_\+util.\+c}\end{DoxyCompactItemize}
