\doxysection{osmo\+\_\+gcr\+\_\+parsed Struct Reference}
\label{structosmo__gcr__parsed}\index{osmo\_gcr\_parsed@{osmo\_gcr\_parsed}}


Parsed representation of Global Call Reference, 3GPP TS 29.\+205 Table B 2.\+1.\+9.\+1.  




{\ttfamily \#include $<$gsm29205.\+h$>$}

\doxysubsection*{Data Fields}
\begin{DoxyCompactItemize}
\item 
uint8\+\_\+t \textbf{ net} [5]
\item 
uint8\+\_\+t \textbf{ net\+\_\+len}
\begin{DoxyCompactList}\small\item\em Network ID, ITU-\/T Q.\+1902.\+3. \end{DoxyCompactList}\item 
uint16\+\_\+t \textbf{ node}
\begin{DoxyCompactList}\small\item\em length (3-\/5 octets) of gsm29205\+\_\+gcr\+::net \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ cr} [5]
\begin{DoxyCompactList}\small\item\em Node ID. \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
Parsed representation of Global Call Reference, 3GPP TS 29.\+205 Table B 2.\+1.\+9.\+1. 

The documentation for this struct was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
include/osmocom/gsm/\textbf{ gsm29205.\+h}\end{DoxyCompactItemize}
