libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Fields
info_meas_ind_param Struct Reference

for MEAS MPH-INFO.ind More...

`#include <l1sap.h>`

## Data Fields
uint8_t | chan_nr
| Channel Number (Like RSL) More...
uint32_t | fn
| GSM Frame Number. More...
uint16_t | ber10k
| BER in units of 0.01%. More...
union {
int16_t ta_offs_qbits
| timing advance offset (in qbits) More...
int16_t ta_offs_256bits
| timing advance offset (in 1/256th bits) More...
}; |
int16_t | c_i_cb
| C/I ratio in 0.1 dB. More...
uint8_t | is_sub:1
| flags More...
uint8_t | inv_rssi
| RSSI in dBm * -1. More...

## Detailed Description

for MEAS MPH-INFO.ind

## Field Documentation

## ◆

union { ... } info_meas_ind_param::@22

## ◆ ber10k

uint16_t info_meas_ind_param::ber10k

BER in units of 0.01%.

## ◆ c_i_cb

int16_t info_meas_ind_param::c_i_cb

C/I ratio in 0.1 dB.

## ◆ chan_nr

uint8_t info_meas_ind_param::chan_nr

Channel Number (Like RSL)

## ◆ fn

uint32_t info_meas_ind_param::fn

GSM Frame Number.

## ◆ inv_rssi

uint8_t info_meas_ind_param::inv_rssi

RSSI in dBm * -1.

## ◆ is_sub

uint8_t info_meas_ind_param::is_sub

flags

## ◆ ta_offs_256bits

int16_t info_meas_ind_param::ta_offs_256bits

timing advance offset (in 1/256th bits)

## ◆ ta_offs_qbits

int16_t info_meas_ind_param::ta_offs_qbits

timing advance offset (in qbits)

The documentation for this struct was generated from the following file:

- include/osmocom/gsm/l1sap.h