libosmo-netif 1.7.0.10-3a9e Osmocom network interface library

Modules
Here is a list of all modules:

Osmocom Datagram Socket | This code is intended to abstract any use of datagram type sockets, such as UDP
Osmocom Jitter Buffer |
Osmocom Stream Server | This code is intended to abstract any server-side use of stream-type sockets, such as TCP and SCTP
Osmocom Stream Client | This code is intended to abstract any client use of stream-type sockets, such as TCP and SCTP
Themyscira Wireless RTP jitter buffer implementation | The present twjit layer is an interface mechanism from an incoming RTP stream to an output application that has fixed timing requirements, e.g., the Tx side of GSM Um TCH or a T1/E1 TDM interface
Themyscira Wireless RTP endpoint implementation | Osmo_twrtp is a complete RTP endpoint
Osmocom Multiplex Protocol | This code implements a variety of utility functions related to the OSMUX user-plane multiplexing protocol, an efficient alternative to plain UDP/RTP streams for voice transport in back-haul of cellular networks