libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Fields
ph_tch_param Struct Reference

for TCH. More...

`#include <l1sap.h>`

## Data Fields
uint8_t | chan_nr
| Channel Number (Like RSL) More...
uint32_t | fn
| GSM Frame Number. More...
int8_t | rssi
| RSSI of received indication. More...
uint8_t | marker
| RTP Marker bit (speech onset indicator) More...
uint16_t | ber10k
| BER in units of 0.01%. More...
int16_t | lqual_cb
| Link quality in centiBel. More...
int16_t | ta_offs_256bits
| timing advance offset (in 1/256th bits) More...
uint8_t | is_sub:1
| flags More...

## Detailed Description

for TCH.

{req,ind} | TCH-RTS.ind

## Field Documentation

## ◆ ber10k

uint16_t ph_tch_param::ber10k

BER in units of 0.01%.

## ◆ chan_nr

uint8_t ph_tch_param::chan_nr

Channel Number (Like RSL)

## ◆ fn

uint32_t ph_tch_param::fn

GSM Frame Number.

## ◆ is_sub

uint8_t ph_tch_param::is_sub

flags

## ◆ lqual_cb

int16_t ph_tch_param::lqual_cb

Link quality in centiBel.

## ◆ marker

uint8_t ph_tch_param::marker

RTP Marker bit (speech onset indicator)

## ◆ rssi

int8_t ph_tch_param::rssi

RSSI of received indication.

## ◆ ta_offs_256bits

int16_t ph_tch_param::ta_offs_256bits

timing advance offset (in 1/256th bits)

The documentation for this struct was generated from the following file:

- include/osmocom/gsm/l1sap.h