libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Macros
gsm_09_02.h File Reference

GSM TS 09.02 definitions (MAP). More...

Go to the source code of this file.

## Macros
#define | GSM0902_SS_STATUS_Q_BIT 0x08
#define | GSM0902_SS_STATUS_P_BIT 0x04
#define | GSM0902_SS_STATUS_R_BIT 0x02
#define | GSM0902_SS_STATUS_A_BIT 0x01
#define | GSM0902_SS_DATA_SS_STATUS_TAG 0x84
#define | GSM0902_SS_DATA_NBR_USER 0x85
#define | GSM0902_SS_INFO_FORW_INFO_TAG 0xA0
#define | GSM0902_SS_INFO_CALL_BARR_INFO_TAG 0xA1
#define | GSM0902_SS_INFO_SS_DATA_TAG 0xA3
#define | GSM0902_SS_INTERR_SS_RES_SS_STATUS_TAG 0x80
#define | GSM0902_SS_INTERR_SS_RES_BSG_LIST_TAG 0x81
#define | GSM0902_SS_INTERR_SS_RES_FORW_FEAT_LIST_TAG 0x82
#define | GSM0902_SS_INTERR_SS_RES_GEN_SERV_INFO_TAG 0x83
#define | GSM0902_SS_CODE_ALL_SS 0x00
#define | GSM0902_SS_CODE_ALL_LINE_IDENTIFICATION_SS 0x10
#define | GSM0902_SS_CODE_CLIP 0x11
#define | GSM0902_SS_CODE_CLIR 0x12
#define | GSM0902_SS_CODE_COLP 0x13
#define | GSM0902_SS_CODE_COLR 0x14
#define | GSM0902_SS_CODE_MCI 0x15
#define | GSM0902_SS_CODE_ALL_NAME_IDENTIFICATION_SS 0x18
#define | GSM0902_SS_CODE_CNAP 0x19
#define | GSM0902_SS_CODE_ALL_FORWARDING_SS 0x20
#define | GSM0902_SS_CODE_CFU 0x21
#define | GSM0902_SS_CODE_ALL_COND_FORWARDING_SS 0x28
#define | GSM0902_SS_CODE_CFB 0x29
#define | GSM0902_SS_CODE_CFNRY 0x2A
#define | GSM0902_SS_CODE_CFNRC 0x2B
#define | GSM0902_SS_CODE_CD 0x24
#define | GSM0902_SS_CODE_ALL_CALL_OFFERING_SS 0x30
#define | GSM0902_SS_CODE_ECT 0x31
#define | GSM0902_SS_CODE_MAH 0x32
#define | GSM0902_SS_CODE_ALL_CALL_COMPLETION_SS 0x40
#define | GSM0902_SS_CODE_CW 0x41
#define | GSM0902_SS_CODE_HOLD 0x42
#define | GSM0902_SS_CODE_CCBS_A 0x43
#define | GSM0902_SS_CODE_CCBS_B 0x44
#define | GSM0902_SS_CODE_MC 0x45
#define | GSM0902_SS_CODE_ALL_MULTI_PARTY_SS 0x50
#define | GSM0902_SS_CODE_MULTI_PTY 0x51
#define | GSM0902_SS_CODE_ALL_COMMUNITY_OF_INTEREST_SS 0x60
#define | GSM0902_SS_CODE_CUG 0x61
#define | GSM0902_SS_CODE_ALL_CHARGING_SS 0x70
#define | GSM0902_SS_CODE_AOCI 0x71
#define | GSM0902_SS_CODE_AOCC 0x72
#define | GSM0902_SS_CODE_ALL_ADDITIONAL_INFO_TRANSFER_SS 0x80
#define | GSM0902_SS_CODE_UUS1 0x81
#define | GSM0902_SS_CODE_UUS2 0x82
#define | GSM0902_SS_CODE_UUS3 0x83
#define | GSM0902_SS_CODE_ALL_BARRING_SS 0x90
#define | GSM0902_SS_CODE_BARRING_OF_OUTGOING_CALLS 0x91
#define | GSM0902_SS_CODE_BAOC 0x92
#define | GSM0902_SS_CODE_BOIC 0x93
#define | GSM0902_SS_CODE_BOIC_EX_HC 0x94
#define | GSM0902_SS_CODE_BARRING_OF_INCOMING_CALLS 0x99
#define | GSM0902_SS_CODE_BAIC 0x9A
#define | GSM0902_SS_CODE_BIC_ROAM 0x9B
#define | GSM0902_SS_CODE_ALL_PLMN_SPECIFIC_SS 0xF0
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_1 0xF1
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_2 0xF2
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_3 0xF3
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_4 0xF4
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_5 0xF5
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_6 0xF6
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_7 0xF7
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_8 0xF8
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_9 0xF9
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_A 0xFA
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_B 0xFB
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_C 0xFC
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_D 0xFD
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_E 0xFE
#define | GSM0902_SS_CODE_PLMN_SPECIFIC_SS_F 0xFF
#define | GSM0902_SS_CODE_ALL_CALL_PRIORITY_SS 0xA0
#define | GSM0902_SS_CODE_EMLPP 0xA1
#define | GSM0902_SS_CODE_ALL_LCSPRIVACY_EXCEPTION 0xB0
#define | GSM0902_SS_CODE_UNIVERSAL 0xB1
#define | GSM0902_SS_CODE_CALL_SESSION_RELATED 0xB2
#define | GSM0902_SS_CODE_CALL_SESSION_UNRELATED 0xB3
#define | GSM0902_SS_CODE_PLMNOPERATOR 0xB4
#define | GSM0902_SS_CODE_SERVICE_TYPE 0xB5
#define | GSM0902_SS_CODE_ALL_MOLR_SS 0xC0
#define | GSM0902_SS_CODE_BASIC_SELF_LOCATION 0xC1
#define | GSM0902_SS_CODE_AUTONOMOUS_SELF_LOCATION 0xC2
#define | GSM0902_SS_CODE_TRANSFER_TO_THIRD_PARTY 0xC3
#define | GSM0902_TS_CODE_ALL_TELESERVICES 0x00
#define | GSM0902_TS_CODE_ALL_SPEECH_TRANSMISSION_SERVICES 0x10
#define | GSM0902_TS_CODE_TELEPHONY 0x11
#define | GSM0902_TS_CODE_EMERGENCY_CALLS 0x12
#define | GSM0902_TS_CODE_ALL_SHORT_MESSAGE_SERVICES 0x20
#define | GSM0902_TS_CODE_SHORT_MESSAGE_MT_PP 0x21
#define | GSM0902_TS_CODE_SHORT_MESSAGE_MO_PP 0x22
#define | GSM0902_TS_CODE_ALL_FACSIMILE_TRANSMISSION_SERVICES 0x60
#define | GSM0902_TS_CODE_FACSIMILE_GROUP3AND_ALTER_SPEECH 0x61
#define | GSM0902_TS_CODE_AUTOMATIC_FACSIMILE_GROUP3 0x62
#define | GSM0902_TS_CODE_FACSIMILE_GROUP4 0x63
#define | GSM0902_TS_CODE_ALL_DATA_TELESERVICES 0x70
#define | GSM0902_TS_CODE_ALL_TELESERVICES_EXEPT_SMS 0x80
#define | GSM0902_TS_CODE_ALL_VOICE_GROUP_CALL_SERVICES 0x90
#define | GSM0902_TS_CODE_VOICE_GROUP_CALL 0x91
#define | GSM0902_TS_CODE_VOICE_BROADCAST_CALL 0x92
#define | GSM0902_TS_CODE_ALL_PLMN_SPECIFIC_TS 0xD0
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_1 0xD1
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_2 0xD2
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_3 0xD3
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_4 0xD4
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_5 0xD5
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_6 0xD6
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_7 0xD7
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_8 0xD8
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_9 0xD9
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_A 0xDA
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_B 0xDB
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_C 0xDC
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_D 0xDD
#define | GSM0902_TS_CODE_PLMN_SPECIFIC_TS_E 0xDE

## Detailed Description

GSM TS 09.02 definitions (MAP).

## Macro Definition Documentation

## ◆ GSM0902_SS_CODE_ALL_ADDITIONAL_INFO_TRANSFER_SS

#define GSM0902_SS_CODE_ALL_ADDITIONAL_INFO_TRANSFER_SS 0x80

## ◆ GSM0902_SS_CODE_ALL_BARRING_SS

#define GSM0902_SS_CODE_ALL_BARRING_SS 0x90

## ◆ GSM0902_SS_CODE_ALL_CALL_COMPLETION_SS

#define GSM0902_SS_CODE_ALL_CALL_COMPLETION_SS 0x40

## ◆ GSM0902_SS_CODE_ALL_CALL_OFFERING_SS

#define GSM0902_SS_CODE_ALL_CALL_OFFERING_SS 0x30

## ◆ GSM0902_SS_CODE_ALL_CALL_PRIORITY_SS

#define GSM0902_SS_CODE_ALL_CALL_PRIORITY_SS 0xA0

## ◆ GSM0902_SS_CODE_ALL_CHARGING_SS

#define GSM0902_SS_CODE_ALL_CHARGING_SS 0x70

## ◆ GSM0902_SS_CODE_ALL_COMMUNITY_OF_INTEREST_SS

#define GSM0902_SS_CODE_ALL_COMMUNITY_OF_INTEREST_SS 0x60

## ◆ GSM0902_SS_CODE_ALL_COND_FORWARDING_SS

#define GSM0902_SS_CODE_ALL_COND_FORWARDING_SS 0x28

## ◆ GSM0902_SS_CODE_ALL_FORWARDING_SS

#define GSM0902_SS_CODE_ALL_FORWARDING_SS 0x20

## ◆ GSM0902_SS_CODE_ALL_LCSPRIVACY_EXCEPTION

#define GSM0902_SS_CODE_ALL_LCSPRIVACY_EXCEPTION 0xB0

## ◆ GSM0902_SS_CODE_ALL_LINE_IDENTIFICATION_SS

#define GSM0902_SS_CODE_ALL_LINE_IDENTIFICATION_SS 0x10

## ◆ GSM0902_SS_CODE_ALL_MOLR_SS

#define GSM0902_SS_CODE_ALL_MOLR_SS 0xC0

## ◆ GSM0902_SS_CODE_ALL_MULTI_PARTY_SS

#define GSM0902_SS_CODE_ALL_MULTI_PARTY_SS 0x50

## ◆ GSM0902_SS_CODE_ALL_NAME_IDENTIFICATION_SS

#define GSM0902_SS_CODE_ALL_NAME_IDENTIFICATION_SS 0x18

## ◆ GSM0902_SS_CODE_ALL_PLMN_SPECIFIC_SS

#define GSM0902_SS_CODE_ALL_PLMN_SPECIFIC_SS 0xF0

## ◆ GSM0902_SS_CODE_ALL_SS

#define GSM0902_SS_CODE_ALL_SS 0x00

## ◆ GSM0902_SS_CODE_AOCC

#define GSM0902_SS_CODE_AOCC 0x72

## ◆ GSM0902_SS_CODE_AOCI

#define GSM0902_SS_CODE_AOCI 0x71

## ◆ GSM0902_SS_CODE_AUTONOMOUS_SELF_LOCATION

#define GSM0902_SS_CODE_AUTONOMOUS_SELF_LOCATION 0xC2

## ◆ GSM0902_SS_CODE_BAIC

#define GSM0902_SS_CODE_BAIC 0x9A

## ◆ GSM0902_SS_CODE_BAOC

#define GSM0902_SS_CODE_BAOC 0x92

## ◆ GSM0902_SS_CODE_BARRING_OF_INCOMING_CALLS

#define GSM0902_SS_CODE_BARRING_OF_INCOMING_CALLS 0x99

## ◆ GSM0902_SS_CODE_BARRING_OF_OUTGOING_CALLS

#define GSM0902_SS_CODE_BARRING_OF_OUTGOING_CALLS 0x91

## ◆ GSM0902_SS_CODE_BASIC_SELF_LOCATION

#define GSM0902_SS_CODE_BASIC_SELF_LOCATION 0xC1

## ◆ GSM0902_SS_CODE_BIC_ROAM

#define GSM0902_SS_CODE_BIC_ROAM 0x9B

## ◆ GSM0902_SS_CODE_BOIC

#define GSM0902_SS_CODE_BOIC 0x93

## ◆ GSM0902_SS_CODE_BOIC_EX_HC

#define GSM0902_SS_CODE_BOIC_EX_HC 0x94

## ◆ GSM0902_SS_CODE_CALL_SESSION_RELATED

#define GSM0902_SS_CODE_CALL_SESSION_RELATED 0xB2

## ◆ GSM0902_SS_CODE_CALL_SESSION_UNRELATED

#define GSM0902_SS_CODE_CALL_SESSION_UNRELATED 0xB3

## ◆ GSM0902_SS_CODE_CCBS_A

#define GSM0902_SS_CODE_CCBS_A 0x43

## ◆ GSM0902_SS_CODE_CCBS_B

#define GSM0902_SS_CODE_CCBS_B 0x44

## ◆ GSM0902_SS_CODE_CD

#define GSM0902_SS_CODE_CD 0x24

## ◆ GSM0902_SS_CODE_CFB

#define GSM0902_SS_CODE_CFB 0x29

## ◆ GSM0902_SS_CODE_CFNRC

#define GSM0902_SS_CODE_CFNRC 0x2B

## ◆ GSM0902_SS_CODE_CFNRY

#define GSM0902_SS_CODE_CFNRY 0x2A

## ◆ GSM0902_SS_CODE_CFU

#define GSM0902_SS_CODE_CFU 0x21

## ◆ GSM0902_SS_CODE_CLIP

#define GSM0902_SS_CODE_CLIP 0x11

## ◆ GSM0902_SS_CODE_CLIR

#define GSM0902_SS_CODE_CLIR 0x12

## ◆ GSM0902_SS_CODE_CNAP

#define GSM0902_SS_CODE_CNAP 0x19

## ◆ GSM0902_SS_CODE_COLP

#define GSM0902_SS_CODE_COLP 0x13

## ◆ GSM0902_SS_CODE_COLR

#define GSM0902_SS_CODE_COLR 0x14

## ◆ GSM0902_SS_CODE_CUG

#define GSM0902_SS_CODE_CUG 0x61

## ◆ GSM0902_SS_CODE_CW

#define GSM0902_SS_CODE_CW 0x41

## ◆ GSM0902_SS_CODE_ECT

#define GSM0902_SS_CODE_ECT 0x31

## ◆ GSM0902_SS_CODE_EMLPP

#define GSM0902_SS_CODE_EMLPP 0xA1

## ◆ GSM0902_SS_CODE_HOLD

#define GSM0902_SS_CODE_HOLD 0x42

## ◆ GSM0902_SS_CODE_MAH

#define GSM0902_SS_CODE_MAH 0x32

## ◆ GSM0902_SS_CODE_MC

#define GSM0902_SS_CODE_MC 0x45

## ◆ GSM0902_SS_CODE_MCI

#define GSM0902_SS_CODE_MCI 0x15

## ◆ GSM0902_SS_CODE_MULTI_PTY

#define GSM0902_SS_CODE_MULTI_PTY 0x51

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_1

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_1 0xF1

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_2

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_2 0xF2

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_3

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_3 0xF3

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_4

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_4 0xF4

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_5

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_5 0xF5

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_6

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_6 0xF6

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_7

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_7 0xF7

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_8

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_8 0xF8

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_9

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_9 0xF9

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_A

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_A 0xFA

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_B

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_B 0xFB

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_C

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_C 0xFC

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_D

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_D 0xFD

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_E

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_E 0xFE

## ◆ GSM0902_SS_CODE_PLMN_SPECIFIC_SS_F

#define GSM0902_SS_CODE_PLMN_SPECIFIC_SS_F 0xFF

## ◆ GSM0902_SS_CODE_PLMNOPERATOR

#define GSM0902_SS_CODE_PLMNOPERATOR 0xB4

## ◆ GSM0902_SS_CODE_SERVICE_TYPE

#define GSM0902_SS_CODE_SERVICE_TYPE 0xB5

## ◆ GSM0902_SS_CODE_TRANSFER_TO_THIRD_PARTY

#define GSM0902_SS_CODE_TRANSFER_TO_THIRD_PARTY 0xC3

## ◆ GSM0902_SS_CODE_UNIVERSAL

#define GSM0902_SS_CODE_UNIVERSAL 0xB1

## ◆ GSM0902_SS_CODE_UUS1

#define GSM0902_SS_CODE_UUS1 0x81

## ◆ GSM0902_SS_CODE_UUS2

#define GSM0902_SS_CODE_UUS2 0x82

## ◆ GSM0902_SS_CODE_UUS3

#define GSM0902_SS_CODE_UUS3 0x83

## ◆ GSM0902_SS_DATA_NBR_USER

#define GSM0902_SS_DATA_NBR_USER 0x85

## ◆ GSM0902_SS_DATA_SS_STATUS_TAG

#define GSM0902_SS_DATA_SS_STATUS_TAG 0x84

## ◆ GSM0902_SS_INFO_CALL_BARR_INFO_TAG

#define GSM0902_SS_INFO_CALL_BARR_INFO_TAG 0xA1

## ◆ GSM0902_SS_INFO_FORW_INFO_TAG

#define GSM0902_SS_INFO_FORW_INFO_TAG 0xA0

## ◆ GSM0902_SS_INFO_SS_DATA_TAG

#define GSM0902_SS_INFO_SS_DATA_TAG 0xA3

## ◆ GSM0902_SS_INTERR_SS_RES_BSG_LIST_TAG

#define GSM0902_SS_INTERR_SS_RES_BSG_LIST_TAG 0x81

## ◆ GSM0902_SS_INTERR_SS_RES_FORW_FEAT_LIST_TAG

#define GSM0902_SS_INTERR_SS_RES_FORW_FEAT_LIST_TAG 0x82

## ◆ GSM0902_SS_INTERR_SS_RES_GEN_SERV_INFO_TAG

#define GSM0902_SS_INTERR_SS_RES_GEN_SERV_INFO_TAG 0x83

## ◆ GSM0902_SS_INTERR_SS_RES_SS_STATUS_TAG

#define GSM0902_SS_INTERR_SS_RES_SS_STATUS_TAG 0x80

## ◆ GSM0902_SS_STATUS_A_BIT

#define GSM0902_SS_STATUS_A_BIT 0x01

## ◆ GSM0902_SS_STATUS_P_BIT

#define GSM0902_SS_STATUS_P_BIT 0x04

## ◆ GSM0902_SS_STATUS_Q_BIT

#define GSM0902_SS_STATUS_Q_BIT 0x08

## ◆ GSM0902_SS_STATUS_R_BIT

#define GSM0902_SS_STATUS_R_BIT 0x02

## ◆ GSM0902_TS_CODE_ALL_DATA_TELESERVICES

#define GSM0902_TS_CODE_ALL_DATA_TELESERVICES 0x70

## ◆ GSM0902_TS_CODE_ALL_FACSIMILE_TRANSMISSION_SERVICES

#define GSM0902_TS_CODE_ALL_FACSIMILE_TRANSMISSION_SERVICES 0x60

## ◆ GSM0902_TS_CODE_ALL_PLMN_SPECIFIC_TS

#define GSM0902_TS_CODE_ALL_PLMN_SPECIFIC_TS 0xD0

## ◆ GSM0902_TS_CODE_ALL_SHORT_MESSAGE_SERVICES

#define GSM0902_TS_CODE_ALL_SHORT_MESSAGE_SERVICES 0x20

## ◆ GSM0902_TS_CODE_ALL_SPEECH_TRANSMISSION_SERVICES

#define GSM0902_TS_CODE_ALL_SPEECH_TRANSMISSION_SERVICES 0x10

## ◆ GSM0902_TS_CODE_ALL_TELESERVICES

#define GSM0902_TS_CODE_ALL_TELESERVICES 0x00

## ◆ GSM0902_TS_CODE_ALL_TELESERVICES_EXEPT_SMS

#define GSM0902_TS_CODE_ALL_TELESERVICES_EXEPT_SMS 0x80

## ◆ GSM0902_TS_CODE_ALL_VOICE_GROUP_CALL_SERVICES

#define GSM0902_TS_CODE_ALL_VOICE_GROUP_CALL_SERVICES 0x90

## ◆ GSM0902_TS_CODE_AUTOMATIC_FACSIMILE_GROUP3

#define GSM0902_TS_CODE_AUTOMATIC_FACSIMILE_GROUP3 0x62

## ◆ GSM0902_TS_CODE_EMERGENCY_CALLS

#define GSM0902_TS_CODE_EMERGENCY_CALLS 0x12

## ◆ GSM0902_TS_CODE_FACSIMILE_GROUP3AND_ALTER_SPEECH

#define GSM0902_TS_CODE_FACSIMILE_GROUP3AND_ALTER_SPEECH 0x61

## ◆ GSM0902_TS_CODE_FACSIMILE_GROUP4

#define GSM0902_TS_CODE_FACSIMILE_GROUP4 0x63

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_1

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_1 0xD1

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_2

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_2 0xD2

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_3

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_3 0xD3

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_4

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_4 0xD4

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_5

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_5 0xD5

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_6

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_6 0xD6

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_7

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_7 0xD7

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_8

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_8 0xD8

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_9

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_9 0xD9

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_A

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_A 0xDA

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_B

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_B 0xDB

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_C

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_C 0xDC

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_D

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_D 0xDD

## ◆ GSM0902_TS_CODE_PLMN_SPECIFIC_TS_E

#define GSM0902_TS_CODE_PLMN_SPECIFIC_TS_E 0xDE

## ◆ GSM0902_TS_CODE_SHORT_MESSAGE_MO_PP

#define GSM0902_TS_CODE_SHORT_MESSAGE_MO_PP 0x22

## ◆ GSM0902_TS_CODE_SHORT_MESSAGE_MT_PP

#define GSM0902_TS_CODE_SHORT_MESSAGE_MT_PP 0x21

## ◆ GSM0902_TS_CODE_TELEPHONY

#define GSM0902_TS_CODE_TELEPHONY 0x11

## ◆ GSM0902_TS_CODE_VOICE_BROADCAST_CALL

#define GSM0902_TS_CODE_VOICE_BROADCAST_CALL 0x92

## ◆ GSM0902_TS_CODE_VOICE_GROUP_CALL

#define GSM0902_TS_CODE_VOICE_GROUP_CALL 0x91