libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Structures | Enumerations | Functions
oap.h File Reference
Osmocom Authentication Protocol
`#include <stdint.h>`
`#include <osmocom/core/msgb.h>`
`#include <osmocom/gsm/protocol/gsm_04_08_gprs.h>`

Go to the source code of this file.

## Data Structures
struct | osmo_oap_message
| Parsed/decoded OAP protocol message. More...

## Enumerations
enum | osmo_oap_iei { OAP_CAUSE_IE = 0x02 , OAP_RAND_IE = 0x20 , OAP_AUTN_IE = 0x23 , OAP_XRES_IE = 0x24 , OAP_AUTS_IE = 0x25 , OAP_CLIENT_ID_IE = 0x30 }
| Information Element Identifiers for OAP IEs. More...
enum | osmo_oap_message_type { OAP_MSGT_REGISTER_REQUEST = 0b00000100 , OAP_MSGT_REGISTER_ERROR = 0b00000101 , OAP_MSGT_REGISTER_RESULT = 0b00000110 , OAP_MSGT_CHALLENGE_REQUEST = 0b00001000 , OAP_MSGT_CHALLENGE_ERROR = 0b00001001 , OAP_MSGT_CHALLENGE_RESULT = 0b00001010 , OAP_MSGT_SYNC_REQUEST = 0b00001100 , OAP_MSGT_SYNC_ERROR = 0b00001101 , OAP_MSGT_SYNC_RESULT = 0b00001110 }
| OAP message types. More...

## Functions
int | osmo_oap_decode (struct osmo_oap_message *oap_msg, const uint8_t *const_data, size_t data_len)
| Decode OAP message data. More...
void | osmo_oap_encode (struct msgb *msg, const struct osmo_oap_message *oap_msg)
| Compose OAP message data. More...