libosmogsm 1.13.1.1-afb4 Osmocom GSM library

gsm29205.h
Go to the documentation of this file.
1
4/*
5 * (C) 2018 by sysmocom - s.f.m.c. GmbH
6 * All Rights Reserved
7 *
8 * This program is free software; you can redistribute it and/or modify
9 * it under the terms of the GNU General Public License as published by
10 * the Free Software Foundation; either version 2 of the License, or
11 * (at your option) any later version.
12 *
13 * This program is distributed in the hope that it will be useful,
14 * but WITHOUT ANY WARRANTY; without even the implied warranty of
15 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
16 * GNU General Public License for more details.
17 *
18 */
19
20#pragma once
21
22#include <osmocom/core/msgb.h>
23
24#include <stdint.h>
25
26#define OSMO_GCR_MIN_LEN 13
27
29 struct osmo_gcr_parsed {
30 uint8_t net[5];
31 uint8_t net_len;
32 uint16_t node;
33 uint8_t cr[5];
34};
35
36uint8_t osmo_enc_gcr(struct msgb *msg, const struct osmo_gcr_parsed *g);
37 int osmo_dec_gcr(struct osmo_gcr_parsed *gcr, const uint8_t *elem, uint8_t len);
38 bool osmo_gcr_eq(const struct osmo_gcr_parsed *gcr1, const struct osmo_gcr_parsed *gcr2);
g
struct osmo_tdef_group * g
osmo_enc_gcr
uint8_t osmo_enc_gcr(struct msgb *msg, const struct osmo_gcr_parsed *g)
Create Global Call Reference.
Definition: gsm29205.c:40
osmo_gcr_parsed::cr
uint8_t cr[5]
Node ID.
Definition: gsm29205.h:33
osmo_dec_gcr
int osmo_dec_gcr(struct osmo_gcr_parsed *gcr, const uint8_t *elem, uint8_t len)
Decode Global Call Reference, 3GPP TS 29.205 Table B 2.1.9.1.
Definition: gsm29205.c:66
osmo_gcr_eq
bool osmo_gcr_eq(const struct osmo_gcr_parsed *gcr1, const struct osmo_gcr_parsed *gcr2)
Compare two GCR structs.
Definition: gsm29205.c:98
osmo_gcr_parsed::net_len
uint8_t net_len
Network ID, ITU-T Q.1902.3.
Definition: gsm29205.h:31
osmo_gcr_parsed::node
uint16_t node
length (3-5 octets) of gsm29205_gcr::net
Definition: gsm29205.h:32
osmo_gcr_parsed::net
uint8_t net[5]
Definition: gsm29205.h:30
len
uint8_t len
Definition: gsm_04_11.h:0
msg
uint8_t msg[0]
Definition: gsm_08_08.h:8
msgb.h
msgb
osmo_gcr_parsed
Parsed representation of Global Call Reference, 3GPP TS 29.205 Table B 2.1.9.1.
Definition: gsm29205.h:29