libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Structures | Macros | Functions | Variables
gsm_03_41.h File Reference

GSM TS 03.41 definitions also TS 23.041. More...

`#include <stdint.h>`
`#include <osmocom/core/endian.h>`
`#include <osmocom/gsm/protocol/gsm_04_12.h>`

Go to the source code of this file.

## Data Structures
struct | gsm341_ms_message
struct | gsm341_etws_message

## Macros
#define | OSMO_IS_LITTLE_ENDIAN 0
#define | GSM341_MAX_PAYLOAD (GSM412_MSG_LEN-sizeof(struct gsm341_ms_message))
#define | GSM341_MAX_CHARS (GSM341_MAX_PAYLOAD*8/7)
#define | GSM341_7BIT_PADDING '\r'
#define | GSM341_MSG_CODE(ms) ((ms)->serial.code_lo | ((ms)->serial.code_hi << 4))
#define | GSM341_GS_CELL_WIDE_IMMED 0
#define | GSM341_GS_PLMN_WIDE 1
#define | GSM341_GS_LA_WIDE 2
#define | GSM341_GS_CELL_WIDE 3
#define | GSM341_MSGID_EOTD_ASSISTANCE 0x03E8
#define | GSM341_MSGID_DGPS_CORRECTION 0x03E9
#define | GSM341_MSGID_DGPS_EPH_CLOCK_COR 0x03EA
#define | GSM341_MSGID_GPS_ALMANAC_OTHER 0x03EB
#define | GSM341_MSGID_ETWS_EARTHQUAKE 0x1100
#define | GSM341_MSGID_ETWS_TSUNAMI 0x1101
#define | GSM341_MSGID_ETWS_QUAKE_AND_TSUNAMI 0x1102
#define | GSM341_MSGID_ETWS_TEST 0x1103
#define | GSM341_MSGID_ETWS_OTHER 0x1104
#define | GSM341_MSGID_ETWS_CMAS_PRESIDENTIAL 0x1112
#define | GSM341_MSGID_ETWS_CMAS_EXTREME_IMM_OBSERVED 0x1113
#define | GSM341_MSGID_ETWS_CMAS_EXTREME_IMM_LIKELY 0x1114
#define | GSM341_MSGID_ETWS_CMAS_EXTREME_EXP_OBSERVED 0x1115
#define | GSM341_MSGID_ETWS_CMAS_EXTREME_EXP_LIKELY 0x1116
#define | GSM341_MSGID_ETWS_CMAS_SEVERE_IMM_OBSERVED 0x1117
#define | GSM341_MSGID_ETWS_CMAS_SEVERE_IMM_LIKELY 0x1118
#define | GSM341_MSGID_ETWS_CMAS_SEVERE_EXP_OBSERVED 0x1119
#define | GSM341_MSGID_ETWS_CMAS_SEVERE_EXP_LIKELY 0x111A
#define | GSM341_MSGID_ETWS_CMAS_AMBER 0x111B
#define | GSM341_MSGID_ETWS_CMAS_MONTHLY_TEST 0x111C
#define | GSM341_MSGID_ETWS_CMAS_EXERCISE 0x111D
#define | GSM341_MSGID_ETWS_CMAS_OPERATOR_DEFINED 0x111E
#define | GSM341_MSGID_ETWS_CMAS_PRESIDENTIAL_AL 0x111F
#define | GSM341_MSGID_ETWS_CMAS_EXTREME_IMM_OBSERVED_AL 0x1120
#define | GSM341_MSGID_ETWS_CMAS_EXTREME_IMM_LIKELY_AL 0x1121
#define | GSM341_MSGID_ETWS_CMAS_EXTREME_EXP_OBSERVED_AL 0x1122
#define | GSM341_MSGID_ETWS_CMAS_EXTREME_EXP_LIKELY_AL 0x1123
#define | GSM341_MSGID_ETWS_CMAS_SEVERE_IMM_OBSERVED_AL 0x1124
#define | GSM341_MSGID_ETWS_CMAS_SEVERE_IMM_LIKELY_AL 0x1125
#define | GSM341_MSGID_ETWS_CMAS_SEVERE_EXP_OBSERVED_AL 0x1126
#define | GSM341_MSGID_ETWS_CMAS_SEVERE_EXP_LIKELY_AL 0x1127
#define | GSM341_MSGID_ETWS_CMAS_AMBER_AL 0x1128
#define | GSM341_MSGID_ETWS_CMAS_MONTHLY_TEST_AL 0x1129
#define | GSM341_MSGID_ETWS_CMAS_EXERCISE_AL 0x112A
#define | GSM341_MSGID_ETWS_CMAS_OPERATOR_DEFINED_AL 0x112B
#define | GSM341_MSGID_ETWS_EU_INFO_LOCAL_LANGUAGE 0x1900

## Functions
struct gsm341_ms_message | __attribute__ ((packed))

## Variables
struct {
} | serial
uint16_t | msg_id
struct {
} | dcs
struct {
} | page
uint8_t | data [0]
uint16_t | warning_type

## Detailed Description

GSM TS 03.41 definitions also TS 23.041.

## Macro Definition Documentation

## ◆ GSM341_7BIT_PADDING

#define GSM341_7BIT_PADDING '\r'

## ◆ GSM341_GS_CELL_WIDE

#define GSM341_GS_CELL_WIDE 3

## ◆ GSM341_GS_CELL_WIDE_IMMED

#define GSM341_GS_CELL_WIDE_IMMED 0

## ◆ GSM341_GS_LA_WIDE

#define GSM341_GS_LA_WIDE 2

## ◆ GSM341_GS_PLMN_WIDE

#define GSM341_GS_PLMN_WIDE 1

## ◆ GSM341_MAX_CHARS

#define GSM341_MAX_CHARS (GSM341_MAX_PAYLOAD*8/7)

## ◆ GSM341_MAX_PAYLOAD

#define GSM341_MAX_PAYLOAD (GSM412_MSG_LEN-sizeof(struct gsm341_ms_message))

## ◆ GSM341_MSG_CODE

#define GSM341_MSG_CODE | ( |  | ms | ) | ((ms)->serial.code_lo | ((ms)->serial.code_hi << 4))

## ◆ GSM341_MSGID_DGPS_CORRECTION

#define GSM341_MSGID_DGPS_CORRECTION 0x03E9

## ◆ GSM341_MSGID_DGPS_EPH_CLOCK_COR

#define GSM341_MSGID_DGPS_EPH_CLOCK_COR 0x03EA

## ◆ GSM341_MSGID_EOTD_ASSISTANCE

#define GSM341_MSGID_EOTD_ASSISTANCE 0x03E8

## ◆ GSM341_MSGID_ETWS_CMAS_AMBER

#define GSM341_MSGID_ETWS_CMAS_AMBER 0x111B

## ◆ GSM341_MSGID_ETWS_CMAS_AMBER_AL

#define GSM341_MSGID_ETWS_CMAS_AMBER_AL 0x1128

## ◆ GSM341_MSGID_ETWS_CMAS_EXERCISE

#define GSM341_MSGID_ETWS_CMAS_EXERCISE 0x111D

## ◆ GSM341_MSGID_ETWS_CMAS_EXERCISE_AL

#define GSM341_MSGID_ETWS_CMAS_EXERCISE_AL 0x112A

## ◆ GSM341_MSGID_ETWS_CMAS_EXTREME_EXP_LIKELY

#define GSM341_MSGID_ETWS_CMAS_EXTREME_EXP_LIKELY 0x1116

## ◆ GSM341_MSGID_ETWS_CMAS_EXTREME_EXP_LIKELY_AL

#define GSM341_MSGID_ETWS_CMAS_EXTREME_EXP_LIKELY_AL 0x1123

## ◆ GSM341_MSGID_ETWS_CMAS_EXTREME_EXP_OBSERVED

#define GSM341_MSGID_ETWS_CMAS_EXTREME_EXP_OBSERVED 0x1115

## ◆ GSM341_MSGID_ETWS_CMAS_EXTREME_EXP_OBSERVED_AL

#define GSM341_MSGID_ETWS_CMAS_EXTREME_EXP_OBSERVED_AL 0x1122

## ◆ GSM341_MSGID_ETWS_CMAS_EXTREME_IMM_LIKELY

#define GSM341_MSGID_ETWS_CMAS_EXTREME_IMM_LIKELY 0x1114

## ◆ GSM341_MSGID_ETWS_CMAS_EXTREME_IMM_LIKELY_AL

#define GSM341_MSGID_ETWS_CMAS_EXTREME_IMM_LIKELY_AL 0x1121

## ◆ GSM341_MSGID_ETWS_CMAS_EXTREME_IMM_OBSERVED

#define GSM341_MSGID_ETWS_CMAS_EXTREME_IMM_OBSERVED 0x1113

## ◆ GSM341_MSGID_ETWS_CMAS_EXTREME_IMM_OBSERVED_AL

#define GSM341_MSGID_ETWS_CMAS_EXTREME_IMM_OBSERVED_AL 0x1120

## ◆ GSM341_MSGID_ETWS_CMAS_MONTHLY_TEST

#define GSM341_MSGID_ETWS_CMAS_MONTHLY_TEST 0x111C

## ◆ GSM341_MSGID_ETWS_CMAS_MONTHLY_TEST_AL

#define GSM341_MSGID_ETWS_CMAS_MONTHLY_TEST_AL 0x1129

## ◆ GSM341_MSGID_ETWS_CMAS_OPERATOR_DEFINED

#define GSM341_MSGID_ETWS_CMAS_OPERATOR_DEFINED 0x111E

## ◆ GSM341_MSGID_ETWS_CMAS_OPERATOR_DEFINED_AL

#define GSM341_MSGID_ETWS_CMAS_OPERATOR_DEFINED_AL 0x112B

## ◆ GSM341_MSGID_ETWS_CMAS_PRESIDENTIAL

#define GSM341_MSGID_ETWS_CMAS_PRESIDENTIAL 0x1112

## ◆ GSM341_MSGID_ETWS_CMAS_PRESIDENTIAL_AL

#define GSM341_MSGID_ETWS_CMAS_PRESIDENTIAL_AL 0x111F

## ◆ GSM341_MSGID_ETWS_CMAS_SEVERE_EXP_LIKELY

#define GSM341_MSGID_ETWS_CMAS_SEVERE_EXP_LIKELY 0x111A

## ◆ GSM341_MSGID_ETWS_CMAS_SEVERE_EXP_LIKELY_AL

#define GSM341_MSGID_ETWS_CMAS_SEVERE_EXP_LIKELY_AL 0x1127

## ◆ GSM341_MSGID_ETWS_CMAS_SEVERE_EXP_OBSERVED

#define GSM341_MSGID_ETWS_CMAS_SEVERE_EXP_OBSERVED 0x1119

## ◆ GSM341_MSGID_ETWS_CMAS_SEVERE_EXP_OBSERVED_AL

#define GSM341_MSGID_ETWS_CMAS_SEVERE_EXP_OBSERVED_AL 0x1126

## ◆ GSM341_MSGID_ETWS_CMAS_SEVERE_IMM_LIKELY

#define GSM341_MSGID_ETWS_CMAS_SEVERE_IMM_LIKELY 0x1118

## ◆ GSM341_MSGID_ETWS_CMAS_SEVERE_IMM_LIKELY_AL

#define GSM341_MSGID_ETWS_CMAS_SEVERE_IMM_LIKELY_AL 0x1125

## ◆ GSM341_MSGID_ETWS_CMAS_SEVERE_IMM_OBSERVED

#define GSM341_MSGID_ETWS_CMAS_SEVERE_IMM_OBSERVED 0x1117

## ◆ GSM341_MSGID_ETWS_CMAS_SEVERE_IMM_OBSERVED_AL

#define GSM341_MSGID_ETWS_CMAS_SEVERE_IMM_OBSERVED_AL 0x1124

## ◆ GSM341_MSGID_ETWS_EARTHQUAKE

#define GSM341_MSGID_ETWS_EARTHQUAKE 0x1100

## ◆ GSM341_MSGID_ETWS_EU_INFO_LOCAL_LANGUAGE

#define GSM341_MSGID_ETWS_EU_INFO_LOCAL_LANGUAGE 0x1900

## ◆ GSM341_MSGID_ETWS_OTHER

#define GSM341_MSGID_ETWS_OTHER 0x1104

## ◆ GSM341_MSGID_ETWS_QUAKE_AND_TSUNAMI

#define GSM341_MSGID_ETWS_QUAKE_AND_TSUNAMI 0x1102

## ◆ GSM341_MSGID_ETWS_TEST

#define GSM341_MSGID_ETWS_TEST 0x1103

## ◆ GSM341_MSGID_ETWS_TSUNAMI

#define GSM341_MSGID_ETWS_TSUNAMI 0x1101

## ◆ GSM341_MSGID_GPS_ALMANAC_OTHER

#define GSM341_MSGID_GPS_ALMANAC_OTHER 0x03EB

## ◆ OSMO_IS_LITTLE_ENDIAN

#define OSMO_IS_LITTLE_ENDIAN 0

## Variable Documentation

## ◆ data

uint8_t data[0]

## ◆ dcs

uint8_t dcs

Referenced by gsm0341_build_msg(), gsm338_get_sms_alphabet(), and parse_process_uss_req().

## ◆ msg_id

uint16_t msg_id

Referenced by gsm0341_build_msg().

## ◆

struct { ... } page

Referenced by cbsp_dec_write_repl().

## ◆

struct { ... } serial

## ◆ warning_type

uint16_t warning_type