libosmo-netif 1.7.0.10-3a9e Osmocom network interface library

Macros | Functions
osmux_output.c File Reference
Osmocom Multiplex Protocol

Osmocom multiplex protocol helpers (output) More...

`#include <stdio.h>`
`#include <string.h>`
`#include <osmocom/core/msgb.h>`
`#include <osmocom/core/timer.h>`
`#include <osmocom/core/timer_compat.h>`
`#include <osmocom/core/select.h>`
`#include <osmocom/core/talloc.h>`
`#include <osmocom/core/logging.h>`
`#include <osmocom/netif/amr.h>`
`#include <osmocom/netif/rtp.h>`
`#include <osmocom/netif/osmux.h>`
`#include <arpa/inet.h>`

## Macros
#define | DELTA_RTP_MSG 20000
#define | DELTA_RTP_TIMESTAMP 160

## Functions
struct osmux_hdr * | osmux_xfrm_output_pull (struct msgb *msg)
int | osmux_xfrm_output_sched (struct osmux_out_handle *h, struct osmux_hdr *osmuxh)
| Generate RTP packets from osmux frame AMR payload set and schedule them for transmission at appropriate time. More...
void | osmux_xfrm_output_flush (struct osmux_out_handle *h)
| Flush all scheduled RTP packets still pending to be transmitted. More...
struct osmux_out_handle * | osmux_xfrm_output_alloc (void *ctx)
| Allocate a new osmux out handle. More...
void | osmux_xfrm_output_init2 (struct osmux_out_handle *h, uint32_t rtp_ssrc, uint8_t rtp_payload_type) OSMO_DEPRECATED("Use osmux_xfrm_output_alloc() and osmux_xfrm_output_set_rtp_*() instead")
void | osmux_xfrm_output_init (struct osmux_out_handle *h, uint32_t rtp_ssrc) OSMO_DEPRECATED("Use osmux_xfrm_output_alloc() and osmux_xfrm_output_set_rtp_*() instead")
void | osmux_xfrm_output_set_tx_cb (struct osmux_out_handle *h, void(*tx_cb)(struct msgb *msg, void *data), void *data)
| Set transmission callback to call when a generated RTP packet is to be transmitted. More...
void | osmux_xfrm_output_set_rtp_msgb_alloc_cb (struct osmux_out_handle *h, rtp_msgb_alloc_cb_t cb, void *cb_data)
| Set callback to call when an RTP packet to be generated is to be allocated. More...
void | osmux_xfrm_output_set_rtp_ssrc (struct osmux_out_handle *h, uint32_t rtp_ssrc)
| Set SSRC of generated RTP packets from Osmux frames. More...
void | osmux_xfrm_output_set_rtp_pl_type (struct osmux_out_handle *h, uint32_t rtp_payload_type)
| Set Payload Type of generated RTP packets from Osmux frames. More...

## Detailed Description

Osmocom multiplex protocol helpers (output)