\doxysection{include/osmocom/gmr1/l1/ccch.h File Reference}
\label{ccch_8h}\index{include/osmocom/gmr1/l1/ccch.h@{include/osmocom/gmr1/l1/ccch.h}}


Osmocom GMR-\/1 CCCH (PCH/\+AGCH) channel coding header.  


{\ttfamily \#include $<$stdint.\+h$>$}\newline
{\ttfamily \#include $<$osmocom/core/bits.\+h$>$}\newline
\doxysubsection*{Functions}
\begin{DoxyCompactItemize}
\item 
void \textbf{ gmr1\+\_\+ccch\+\_\+encode} (\textbf{ ubit\+\_\+t} $\ast$bits\+\_\+e, const uint8\+\_\+t $\ast$l2)
\begin{DoxyCompactList}\small\item\em Stateless GMR-\/1 CCCH channel coder. \end{DoxyCompactList}\item 
int \textbf{ gmr1\+\_\+ccch\+\_\+decode} (uint8\+\_\+t $\ast$l2, const \textbf{ sbit\+\_\+t} $\ast$bits\+\_\+e, int $\ast$conv\+\_\+rv)
\begin{DoxyCompactList}\small\item\em Stateless GMR-\/1 CCCH channel decoder. \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
Osmocom GMR-\/1 CCCH (PCH/\+AGCH) channel coding header. 

