What:		/sys/bus/iio/devices/iio:deviceX/out_temp_raw
Date:		August 2021
KernelVersion:	5.15
Contact:	Andreas Klinger <ak@it-klinger.de>
Description:
		Set the temperature. This value is sent to the sensor for
		temperature compensation.
		Default value: 25000 (25 °C)

What:		/sys/bus/iio/devices/iio:deviceX/out_humidityrelative_raw
Date:		August 2021
KernelVersion:	5.15
Contact:	Andreas Klinger <ak@it-klinger.de>
Description:
		Set the relative humidity. This value is sent to the sensor for
		humidity compensation.
		Default value: 50000 (50 % relative humidity)
